(kicad_symbol_lib
	(version 20231120)
	(generator "kicad_symbol_editor")
	(generator_version "8.0")
	(symbol "Compute_Module_5_Functional"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 4.826 4.318 0)
			(effects
				(font
					(size 1.524 1.524)
				)
				(justify left)
			)
		)
		(property "Value" "Compute_Module_5_Functional"
			(at 4.826 6.858 0)
			(effects
				(font
					(size 1.524 1.524)
				)
				(justify left)
			)
		)
		(property "Footprint" "CM5:CM5"
			(at 4.826 9.398 0)
			(effects
				(font
					(size 1.524 1.524)
				)
				(justify left)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 5.08 -3.81 0)
			(effects
				(font
					(size 1.524 1.524)
				)
				(justify left)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "Compute_Module_5_Functional_1_0"
			(text "Power"
				(at 21.59 -13.97 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
		)
		(symbol "Compute_Module_5_Functional_1_1"
			(rectangle
				(start 5.08 2.54)
				(end 38.1 -15.24)
				(stroke
					(width 0)
					(type solid)
				)
				(fill
					(type background)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "107"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "108"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "113"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "114"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "119"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "120"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "125"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "126"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "131"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "132"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "137"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "138"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "144"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "150"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "155"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "156"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "161"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "162"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "167"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "168"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "173"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "174"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "179"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "180"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "185"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "186"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "191"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "192"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "197"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "198"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "32"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "33"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "42"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "43"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "52"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "53"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "59"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "60"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "65"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "66"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "71"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "74"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 1.27 0)
				(length 5.08)
				(name "+5V"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "77"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -1.27 0)
				(length 5.08)
				(name "+5V"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "79"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -3.81 0)
				(length 5.08)
				(name "+5V"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "81"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -6.35 0)
				(length 5.08)
				(name "+5V"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "83"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 43.18 -2.54 180)
				(length 5.08)
				(name "CM4_3.3V_Out_1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "84"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -8.89 0)
				(length 5.08)
				(name "+5V"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "85"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 43.18 -5.08 180)
				(length 5.08)
				(name "CM4_3.3V_Out_2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "86"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -11.43 0)
				(length 5.08)
				(name "+5V"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "87"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 43.18 -7.62 180)
				(length 5.08)
				(name "CM4_1.8V_Out_1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "88"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 43.18 -10.16 180)
				(length 5.08)
				(name "CM4_1.8V_Out_2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "90"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 0)
				(length 5.08)
				(name "GND[51]"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "98"
					(effects
						(font
							(size 0 0)
						)
					)
				)
			)
		)
		(symbol "Compute_Module_5_Functional_2_0"
			(text "GPIO"
				(at 7.62 -69.85 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
		)
		(symbol "Compute_Module_5_Functional_2_1"
			(rectangle
				(start 5.08 2.54)
				(end 30.48 -71.12)
				(stroke
					(width 0)
					(type solid)
				)
				(fill
					(type background)
				)
			)
			(pin passive line
				(at 35.56 0 180)
				(length 5.08)
				(name "GPIO26"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 35.56 -2.54 180)
				(length 5.08)
				(name "GPIO21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "25"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 35.56 -5.08 180)
				(length 5.08)
				(name "GPIO19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "26"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 35.56 -7.62 180)
				(length 5.08)
				(name "GPIO20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "27"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 35.56 -10.16 180)
				(length 5.08)
				(name "GPIO13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "28"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 35.56 -12.7 180)
				(length 5.08)
				(name "GPIO16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "29"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 35.56 -15.24 180)
				(length 5.08)
				(name "GPIO6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "30"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 35.56 -17.78 180)
				(length 5.08)
				(name "GPIO12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "31"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 35.56 -20.32 180)
				(length 5.08)
				(name "GPIO5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "34"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 35.56 -22.86 180)
				(length 5.08)
				(name "ID_SC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "35"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 35.56 -25.4 180)
				(length 5.08)
				(name "ID_SD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "36"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 35.56 -27.94 180)
				(length 5.08)
				(name "GPIO7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "37"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 35.56 -30.48 180)
				(length 5.08)
				(name "GPIO11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "38"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 35.56 -33.02 180)
				(length 5.08)
				(name "GPIO8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "39"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 35.56 -35.56 180)
				(length 5.08)
				(name "GPIO9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "40"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 35.56 -38.1 180)
				(length 5.08)
				(name "GPIO25"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "41"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 35.56 -40.64 180)
				(length 5.08)
				(name "GPIO10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "44"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 35.56 -43.18 180)
				(length 5.08)
				(name "GPIO24"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "45"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 35.56 -45.72 180)
				(length 5.08)
				(name "GPIO22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "46"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 35.56 -48.26 180)
				(length 5.08)
				(name "GPIO23"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "47"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 35.56 -50.8 180)
				(length 5.08)
				(name "GPIO27"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "48"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 35.56 -53.34 180)
				(length 5.08)
				(name "GPIO18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "49"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 35.56 -55.88 180)
				(length 5.08)
				(name "GPIO17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "50"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 35.56 -58.42 180)
				(length 5.08)
				(name "GPIO15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "51"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 35.56 -60.96 180)
				(length 5.08)
				(name "GPIO4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "54"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 35.56 -63.5 180)
				(length 5.08)
				(name "GPIO14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "55"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 35.56 -66.04 180)
				(length 5.08)
				(name "GPIO3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "56"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 35.56 -68.58 180)
				(length 5.08)
				(name "GPIO2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "58"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -33.02 0)
				(length 5.08)
				(name "GPIO_VREF"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "78"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "Compute_Module_5_Functional_3_0"
			(text "Ethernet"
				(at 9.652 -18.796 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
		)
		(symbol "Compute_Module_5_Functional_3_1"
			(rectangle
				(start 5.08 2.54)
				(end 45.72 -20.32)
				(stroke
					(width 0)
					(type solid)
				)
				(fill
					(type background)
				)
			)
			(pin passive line
				(at 50.8 -12.7 180)
				(length 5.08)
				(name "Ethernet_Pair0_N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 50.8 -15.24 180)
				(length 5.08)
				(name "Ethernet_Pair2_P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 50.8 -17.78 180)
				(length 5.08)
				(name "Ethernet_Pair0_P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 0 -5.08 0)
				(length 5.08)
				(name "~{Ethernet_nLED3}"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 0 -2.54 0)
				(length 5.08)
				(name "~{Ethernet_nLED2}"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 0 0 0)
				(length 5.08)
				(name "Ethernet_SYNC_OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 50.8 0 180)
				(length 5.08)
				(name "Ethernet_Pair3_P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 50.8 -2.54 180)
				(length 5.08)
				(name "Ethernet_Pair1_P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 50.8 -5.08 180)
				(length 5.08)
				(name "Ethernet_Pair3_N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 50.8 -7.62 180)
				(length 5.08)
				(name "Ethernet_Pair1_N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 50.8 -10.16 180)
				(length 5.08)
				(name "Ethernet_Pair2_N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "Compute_Module_5_Functional_4_0"
			(text "USB"
				(at 7.62 -6.35 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
		)
		(symbol "Compute_Module_5_Functional_4_1"
			(rectangle
				(start 5.08 2.54)
				(end 20.32 -7.62)
				(stroke
					(width 0)
					(type solid)
				)
				(fill
					(type background)
				)
			)
			(pin input line
				(at 25.4 0 180)
				(length 5.08)
				(name "USB_OTG_ID"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "101"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "USB_N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "103"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "USB_P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "105"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "Compute_Module_5_Functional_5_0"
			(text "PCI-E"
				(at 8.89 -19.05 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
		)
		(symbol "Compute_Module_5_Functional_5_1"
			(rectangle
				(start 5.08 8.89)
				(end 25.4 -20.32)
				(stroke
					(width 0)
					(type solid)
				)
				(fill
					(type background)
				)
			)
			(pin input line
				(at 30.48 0 180)
				(length 5.08)
				(name "~{PCIe_CLK_nREQ}"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "102"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PCIE_DET_nWAKE"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "104"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PCIE_PWR_EN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "106"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "~{PCIe_nRST}"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "109"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PCIe_CLK_P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "110"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PCIe_CLK_N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "112"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PCIe_RX_P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "116"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PCIe_RX_N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "118"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PCIe_TX_P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "122"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PCIe_TX_N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "124"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "Compute_Module_5_Functional_6_0"
			(text "Display / Cam"
				(at 12.7 -25.908 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
		)
		(symbol "Compute_Module_5_Functional_6_1"
			(rectangle
				(start 5.08 2.54)
				(end 20.32 -27.94)
				(stroke
					(width 0)
					(type solid)
				)
				(fill
					(type background)
				)
			)
			(pin input line
				(at 25.4 0 180)
				(length 5.08)
				(name "MIPI0_D0_N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "115"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "MIPI0_D0_P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "117"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "MIPI0_D1_N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "121"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "MIPI0_D1_P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "123"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "MIPI0_C_N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "127"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "MIPI0_C_P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "129"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "MIPI0_D2_N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "133"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "MIPI0_D2_P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "135"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 25.4 -20.32 180)
				(length 5.08)
				(name "MIPI0_D3_N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "139"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "MIPI0_D3_P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "141"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "Compute_Module_5_Functional_7_0"
			(text "HDMI"
				(at 7.62 -39.37 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
		)
		(symbol "Compute_Module_5_Functional_7_1"
			(rectangle
				(start 5.08 2.54)
				(end 43.18 -40.64)
				(stroke
					(width 0)
					(type solid)
				)
				(fill
					(type background)
				)
			)
			(pin input line
				(at 0 -10.16 0)
				(length 5.08)
				(name "HDMI1_HOTPLUG"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "143"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -12.7 0)
				(length 5.08)
				(name "HDMI1_SDA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "145"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 48.26 0 180)
				(length 5.08)
				(name "HDMI1_TX2_P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "146"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin open_collector line
				(at 0 -15.24 0)
				(length 5.08)
				(name "HDMI1_SCL"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "147"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 48.26 -2.54 180)
				(length 5.08)
				(name "HDMI1_TX2_N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "148"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin open_collector line
				(at 0 -17.78 0)
				(length 5.08)
				(name "HDMI1_CEC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "149"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin open_collector line
				(at 0 -20.32 0)
				(length 5.08)
				(name "HDMI0_CEC"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "151"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 48.26 -5.08 180)
				(length 5.08)
				(name "HDMI1_TX1_P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "152"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 0 -22.86 0)
				(length 5.08)
				(name "HDMI0_HOTPLUG"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "153"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 48.26 -7.62 180)
				(length 5.08)
				(name "HDMI1_TX1_N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "154"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 48.26 -10.16 180)
				(length 5.08)
				(name "HDMI1_TX0_P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "158"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 48.26 -12.7 180)
				(length 5.08)
				(name "HDMI1_TX0_N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "160"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 48.26 -15.24 180)
				(length 5.08)
				(name "HDMI1_CLK_P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "164"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 48.26 -17.78 180)
				(length 5.08)
				(name "HDMI1_CLK_N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "166"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 48.26 -20.32 180)
				(length 5.08)
				(name "HDMI0_TX2_P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "170"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 48.26 -22.86 180)
				(length 5.08)
				(name "HDMI0_TX2_N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "172"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 48.26 -25.4 180)
				(length 5.08)
				(name "HDMI0_TX1_P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "176"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 48.26 -27.94 180)
				(length 5.08)
				(name "HDMI0_TX1_N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "178"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 48.26 -30.48 180)
				(length 5.08)
				(name "HDMI0_TX0_P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "182"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 48.26 -33.02 180)
				(length 5.08)
				(name "HDMI0_TX0_N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "184"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 48.26 -35.56 180)
				(length 5.08)
				(name "HDMI0_CLK_P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "188"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 48.26 -38.1 180)
				(length 5.08)
				(name "HDMI0_CLK_N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "190"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -25.4 0)
				(length 5.08)
				(name "HDMI0_SDA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "199"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin open_collector line
				(at 0 -27.94 0)
				(length 5.08)
				(name "HDMI0_SCL"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "200"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "Compute_Module_5_Functional_8_0"
			(text "Display / Cam"
				(at 12.446 -40.64 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
		)
		(symbol "Compute_Module_5_Functional_8_1"
			(rectangle
				(start 5.08 -12.7)
				(end 20.32 -41.91)
				(stroke
					(width 0)
					(type solid)
				)
				(fill
					(type background)
				)
			)
			(pin output line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "MIPI1_D0_N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "175"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "MIPI1_D0_P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "177"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 25.4 -20.32 180)
				(length 5.08)
				(name "MIPI1_D1_N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "181"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "MIPI1_D1_P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "183"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "MIPI1_C_N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "187"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "MIPI1_C_P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "189"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "MIPI1_D2_N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "193"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 25.4 -33.02 180)
				(length 5.08)
				(name "MIPI1_D3_N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "194"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 25.4 -35.56 180)
				(length 5.08)
				(name "MIPI1_D2_P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "195"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 25.4 -38.1 180)
				(length 5.08)
				(name "MIPI1_D3_P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "196"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "Compute_Module_5_Functional_9_0"
			(text "SD Card"
				(at 10.16 -26.67 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
		)
		(symbol "Compute_Module_5_Functional_9_1"
			(rectangle
				(start 5.08 2.54)
				(end 43.18 -27.94)
				(stroke
					(width 0)
					(type solid)
				)
				(fill
					(type background)
				)
			)
			(pin passive line
				(at 48.26 0 180)
				(length 5.08)
				(name "SD_CLK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "57"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 48.26 -2.54 180)
				(length 5.08)
				(name "SD_DAT3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "61"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 48.26 -5.08 180)
				(length 5.08)
				(name "SD_CMD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "62"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 48.26 -7.62 180)
				(length 5.08)
				(name "SD_DAT0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "63"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 48.26 -10.16 180)
				(length 5.08)
				(name "SD_DAT5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "64"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 48.26 -12.7 180)
				(length 5.08)
				(name "SD_DAT1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "67"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 48.26 -15.24 180)
				(length 5.08)
				(name "SD_DAT4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "68"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 48.26 -17.78 180)
				(length 5.08)
				(name "SD_DAT2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "69"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 48.26 -20.32 180)
				(length 5.08)
				(name "SD_DAT7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "70"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 48.26 -22.86 180)
				(length 5.08)
				(name "SD_DAT6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "72"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 0 -12.7 0)
				(length 5.08)
				(name "SD_VDD_Override"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "73"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 48.26 -25.4 180)
				(length 5.08)
				(name "SD_PWR_ON"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "75"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "Compute_Module_5_Functional_10_0"
			(text "Miscellaneous"
				(at 12.7 -39.37 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
		)
		(symbol "Compute_Module_5_Functional_10_1"
			(rectangle
				(start 5.08 2.54)
				(end 43.18 -40.64)
				(stroke
					(width 0)
					(type solid)
				)
				(fill
					(type background)
				)
			)
			(pin input line
				(at 0 -10.16 0)
				(length 5.08)
				(name "CAM_GPIO1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "100"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 48.26 -21.59 180)
				(length 5.08)
				(name "Fan_tacho"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 48.26 -24.13 180)
				(length 5.08)
				(name "Fan_PWM"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 0 -16.51 0)
				(length 5.08)
				(name "EEPROM_nWP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin open_collector line
				(at 48.26 -2.54 180)
				(length 5.08)
				(name "~{Pi_nLED_Activity}"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 0 -36.83 0)
				(length 5.08)
				(name "VBAT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "76"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 48.26 -31.75 180)
				(length 5.08)
				(name "I2C_SCL0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "80"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 48.26 -34.29 180)
				(length 5.08)
				(name "I2C_SDA0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "82"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 0 0 0)
				(length 5.08)
				(name "~{WL_nDisable}"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "89"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 0 -2.54 0)
				(length 5.08)
				(name "~{BT_nDisable}"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "91"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 48.26 -11.43 180)
				(length 5.08)
				(name "PWR_Button"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "92"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 0 -21.59 0)
				(length 5.08)
				(name "~{nRPIBOOT}"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "93"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -29.21 0)
				(length 5.08)
				(name "CC1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "94"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 48.26 -6.35 180)
				(length 5.08)
				(name "~{PI_LED_nPWR}"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "95"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 0 -31.75 0)
				(length 5.08)
				(name "CC2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "96"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 0 -7.62 0)
				(length 5.08)
				(name "CAM_GPIO0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "97"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 0 -24.13 0)
				(length 5.08)
				(name "PMIC_ENABLE"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "99"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "Compute_Module_5_Functional_11_0"
			(text "USB 3.0"
				(at 30.226 -20.32 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
		)
		(symbol "Compute_Module_5_Functional_11_1"
			(rectangle
				(start 21.59 2.54)
				(end 38.1 -21.59)
				(stroke
					(width 0)
					(type solid)
				)
				(fill
					(type background)
				)
			)
			(pin input line
				(at 43.18 -17.78 180)
				(length 5.08)
				(name "VBUS_EN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "111"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 43.18 0 180)
				(length 5.08)
				(name "USB3-0-RX_N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "128"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 43.18 -2.54 180)
				(length 5.08)
				(name "USB3-0-RX_P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "130"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 43.18 -5.08 180)
				(length 5.08)
				(name "USB3-0-DP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "134"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 43.18 -7.62 180)
				(length 5.08)
				(name "USB3-0-DM"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "136"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 43.18 -10.16 180)
				(length 5.08)
				(name "USB3-0-TX_N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "140"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 43.18 -12.7 180)
				(length 5.08)
				(name "USB3-0-TX_P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "142"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "Compute_Module_5_Functional_12_0"
			(text "USB 3.0"
				(at 30.988 -16.256 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
		)
		(symbol "Compute_Module_5_Functional_12_1"
			(rectangle
				(start 21.59 2.54)
				(end 38.1 -17.78)
				(stroke
					(width 0)
					(type solid)
				)
				(fill
					(type background)
				)
			)
			(pin input line
				(at 43.18 0 180)
				(length 5.08)
				(name "USB3-1-RX_N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "157"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 43.18 -2.54 180)
				(length 5.08)
				(name "USB3-1-RX_P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "159"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 43.18 -5.08 180)
				(length 5.08)
				(name "USB3-1-DP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "163"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin bidirectional line
				(at 43.18 -7.62 180)
				(length 5.08)
				(name "USB3-1-DM"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "165"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 43.18 -10.16 180)
				(length 5.08)
				(name "USB3-1-TX_N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "169"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin output line
				(at 43.18 -12.7 180)
				(length 5.08)
				(name "USB3-1-TX_P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "171"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
	)
)
