(export (version "E")
  (design
    (source "/Users/sam1902/Documents/CustomDJ/CDJ-MainBoard/CDJ-MainBoard.kicad_sch")
    (date "2026-03-20T16:02:50+0100")
    (tool "Eeschema 9.0.7")
    (sheet (number "1") (name "/") (tstamps "/")
      (title_block
        (title "CustomDJ")
        (company "xXxXxXxXxX DJ Rookmachine B.V. XxXxXxXxXx")
        (rev "v1")
        (date "2026-02-08")
        (source "CDJ-MainBoard.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value ""))))
    (sheet (number "2") (name "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/")
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source "audio_outputs.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value ""))))
    (sheet (number "3") (name "/Test Points/") (tstamps "/51b1dfb5-ef32-4d46-aca8-09c1f86f56e0/")
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source "test_points.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value ""))))
    (sheet (number "4") (name "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/")
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source "usb_dj_ports.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value ""))))
    (sheet (number "5") (name "/HDMI and Ethernet/") (tstamps "/97e2c747-925a-451b-94c7-ccaeac2c14a8/")
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source "hdmi.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value ""))))
    (sheet (number "6") (name "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/")
      (title_block
        (title "Power Delivery (20V @ 3A = 60W, peak draw 2.12A / 42.4W)")
        (company)
        (rev)
        (date)
        (source "power.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value ""))))
    (sheet (number "7") (name "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/")
      (title_block
        (title "Arduino MIDI IO part with muxers")
        (company)
        (rev)
        (date "2026-03-11")
        (source "arduino_midi.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value ""))))
    (sheet (number "8") (name "/Compute Module/") (tstamps "/1698d124-b773-4573-99c0-ad09fa2fae4f/")
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source "cm5.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value ""))))
    (sheet (number "9") (name "/Sim_Buck/") (tstamps "/2c58c456-80df-4d51-9833-733db3c5a28f/")
      (title_block
        (title "Simulation SPICE of the buck converter")
        (company)
        (rev)
        (date "2026-03-11")
        (source "sim_buck.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value ""))))
    (sheet (number "10") (name "/Sim_DAC/") (tstamps "/b78ec0ce-0ea7-4e81-bc06-3286ad54835a/")
      (title_block
        (title "Simulation of the DAC module in SPICE")
        (company)
        (rev)
        (date "2026-03-11")
        (source "sim_dac.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value "")))))
  (components
    (comp (ref "C2")
      (value "2.2uF")
      (footprint "PCM_JLCPCB:C_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05A225MQ5NSNC_C12530.pdf")
      (description "6.3V 2.2uF X5R ±20% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
      (fields
        (field (name "LCSC") "C12530")
        (field (name "Stock") "4528431")
        (field (name "Price") "0.006USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT")
        (field (name "Manufacturer") "Samsung Electro-Mechanics")
        (field (name "Part") "CL05A225MQ5NSNC")
        (field (name "Voltage Rated") "6.3V")
        (field (name "Tolerance") "±20%")
        (field (name "Capacitance") "2.2uF")
        (field (name "Temperature Coefficient") "X5R")
        (field (name "Footprint") "PCM_JLCPCB:C_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05A225MQ5NSNC_C12530.pdf")
        (field (name "Description") "6.3V 2.2uF X5R ±20% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (libsource (lib "PCM_JLCPCB-Capacitors") (part "0402,2.2uF") (description "6.3V 2.2uF X5R ±20% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (property (name "LCSC") (value "C12530"))
      (property (name "Stock") (value "4528431"))
      (property (name "Price") (value "0.006USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT"))
      (property (name "Manufacturer") (value "Samsung Electro-Mechanics"))
      (property (name "Part") (value "CL05A225MQ5NSNC"))
      (property (name "Voltage Rated") (value "6.3V"))
      (property (name "Tolerance") (value "±20%"))
      (property (name "Capacitance") (value "2.2uF"))
      (property (name "Temperature Coefficient") (value "X5R"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "1aec9ef3-1d43-4480-b3e1-6a138398df8c"))
    (comp (ref "C3")
      (value "100nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "c260e480-2c5d-4e45-b8e0-b11d915de7d4"))
    (comp (ref "C4")
      (value "10µF")
      (footprint "Capacitor_SMD:C_0805_2012Metric")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0805_2012Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "bd9696e1-d478-4f32-b68f-06fac59537ec"))
    (comp (ref "C5")
      (value "100nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "4f661c28-4201-4914-992b-643824c79e39"))
    (comp (ref "C6")
      (value "1µF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "fff78815-9d5f-4b3c-90ec-7f2950b9fd4f"))
    (comp (ref "C7")
      (value "1µF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "04c3f33a-6fbc-4a33-818e-05b243110513"))
    (comp (ref "C8")
      (value "2.2uF")
      (footprint "PCM_JLCPCB:C_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05A225MQ5NSNC_C12530.pdf")
      (description "6.3V 2.2uF X5R ±20% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
      (fields
        (field (name "LCSC") "C12530")
        (field (name "Stock") "4528431")
        (field (name "Price") "0.006USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT")
        (field (name "Manufacturer") "Samsung Electro-Mechanics")
        (field (name "Part") "CL05A225MQ5NSNC")
        (field (name "Voltage Rated") "6.3V")
        (field (name "Tolerance") "±20%")
        (field (name "Capacitance") "2.2uF")
        (field (name "Temperature Coefficient") "X5R")
        (field (name "Footprint") "PCM_JLCPCB:C_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05A225MQ5NSNC_C12530.pdf")
        (field (name "Description") "6.3V 2.2uF X5R ±20% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (libsource (lib "PCM_JLCPCB-Capacitors") (part "0402,2.2uF") (description "6.3V 2.2uF X5R ±20% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (property (name "LCSC") (value "C12530"))
      (property (name "Stock") (value "4528431"))
      (property (name "Price") (value "0.006USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT"))
      (property (name "Manufacturer") (value "Samsung Electro-Mechanics"))
      (property (name "Part") (value "CL05A225MQ5NSNC"))
      (property (name "Voltage Rated") (value "6.3V"))
      (property (name "Tolerance") (value "±20%"))
      (property (name "Capacitance") (value "2.2uF"))
      (property (name "Temperature Coefficient") (value "X5R"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "8d618956-9d25-40a2-af1e-fa0d9496e6aa"))
    (comp (ref "C9")
      (value "2.2uF")
      (footprint "PCM_JLCPCB:C_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05A225MQ5NSNC_C12530.pdf")
      (description "6.3V 2.2uF X5R ±20% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
      (fields
        (field (name "LCSC") "C12530")
        (field (name "Stock") "4528431")
        (field (name "Price") "0.006USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT")
        (field (name "Manufacturer") "Samsung Electro-Mechanics")
        (field (name "Part") "CL05A225MQ5NSNC")
        (field (name "Voltage Rated") "6.3V")
        (field (name "Tolerance") "±20%")
        (field (name "Capacitance") "2.2uF")
        (field (name "Temperature Coefficient") "X5R")
        (field (name "Footprint") "PCM_JLCPCB:C_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05A225MQ5NSNC_C12530.pdf")
        (field (name "Description") "6.3V 2.2uF X5R ±20% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (libsource (lib "PCM_JLCPCB-Capacitors") (part "0402,2.2uF") (description "6.3V 2.2uF X5R ±20% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (property (name "LCSC") (value "C12530"))
      (property (name "Stock") (value "4528431"))
      (property (name "Price") (value "0.006USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT"))
      (property (name "Manufacturer") (value "Samsung Electro-Mechanics"))
      (property (name "Part") (value "CL05A225MQ5NSNC"))
      (property (name "Voltage Rated") (value "6.3V"))
      (property (name "Tolerance") (value "±20%"))
      (property (name "Capacitance") (value "2.2uF"))
      (property (name "Temperature Coefficient") (value "X5R"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "159e1c2d-480e-443e-bfbd-4c2c798168cf"))
    (comp (ref "C10")
      (value "100nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "40ef6e82-9c3c-44d8-bd56-9bf044af3525"))
    (comp (ref "C11")
      (value "2.2nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "efb48ce7-aacb-44df-8d4b-f2ecf7890d24"))
    (comp (ref "C12")
      (value "2.2uF")
      (footprint "PCM_JLCPCB:C_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05A225MQ5NSNC_C12530.pdf")
      (description "6.3V 2.2uF X5R ±20% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
      (fields
        (field (name "LCSC") "C12530")
        (field (name "Stock") "4528431")
        (field (name "Price") "0.006USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT")
        (field (name "Manufacturer") "Samsung Electro-Mechanics")
        (field (name "Part") "CL05A225MQ5NSNC")
        (field (name "Voltage Rated") "6.3V")
        (field (name "Tolerance") "±20%")
        (field (name "Capacitance") "2.2uF")
        (field (name "Temperature Coefficient") "X5R")
        (field (name "Footprint") "PCM_JLCPCB:C_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05A225MQ5NSNC_C12530.pdf")
        (field (name "Description") "6.3V 2.2uF X5R ±20% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (libsource (lib "PCM_JLCPCB-Capacitors") (part "0402,2.2uF") (description "6.3V 2.2uF X5R ±20% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (property (name "LCSC") (value "C12530"))
      (property (name "Stock") (value "4528431"))
      (property (name "Price") (value "0.006USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT"))
      (property (name "Manufacturer") (value "Samsung Electro-Mechanics"))
      (property (name "Part") (value "CL05A225MQ5NSNC"))
      (property (name "Voltage Rated") (value "6.3V"))
      (property (name "Tolerance") (value "±20%"))
      (property (name "Capacitance") (value "2.2uF"))
      (property (name "Temperature Coefficient") (value "X5R"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "3982897a-ee04-471e-8d36-2e7f43b2013e"))
    (comp (ref "C13")
      (value "2.2nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "0098216d-cafd-4381-a194-cc23ac8e3f25"))
    (comp (ref "C60")
      (value "10uF")
      (footprint "PCM_JLCPCB:C_0805")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2411041759_Murata-Electronics-GRM21BR61H106KE43L_C440198.pdf")
      (description "50V 10uF X5R ±10% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
      (fields
        (field (name "LCSC") "C440198")
        (field (name "Stock") "1422246")
        (field (name "Price") "0.066USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "5")
        (field (name "Attrition Qty") "4")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT")
        (field (name "Manufacturer") "Murata Electronics")
        (field (name "Part") "GRM21BR61H106KE43L")
        (field (name "Voltage Rated") "50V")
        (field (name "Tolerance") "±10%")
        (field (name "Capacitance") "10uF")
        (field (name "Temperature Coefficient") "X5R")
        (field (name "Footprint") "PCM_JLCPCB:C_0805")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2411041759_Murata-Electronics-GRM21BR61H106KE43L_C440198.pdf")
        (field (name "Description") "50V 10uF X5R ±10% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (libsource (lib "PCM_JLCPCB-Capacitors") (part "0805,10uF,(2)") (description "50V 10uF X5R ±10% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (property (name "LCSC") (value "C440198"))
      (property (name "Stock") (value "1422246"))
      (property (name "Price") (value "0.066USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "5"))
      (property (name "Attrition Qty") (value "4"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT"))
      (property (name "Manufacturer") (value "Murata Electronics"))
      (property (name "Part") (value "GRM21BR61H106KE43L"))
      (property (name "Voltage Rated") (value "50V"))
      (property (name "Tolerance") (value "±10%"))
      (property (name "Capacitance") (value "10uF"))
      (property (name "Temperature Coefficient") (value "X5R"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "d964bfdd-3598-4f3c-ad34-ba8e211880ce"))
    (comp (ref "FB1")
      (value "~")
      (footprint "PCM_JLCPCB:FB_0603")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2310301640_Sunlord-GZ1608D601TF_C1002.pdf")
      (description "450mΩ ±25% 600Ω@100MHz 0603 Ferrite Beads ROHS")
      (fields
        (field (name "LCSC") "C1002")
        (field (name "Stock") "789150")
        (field (name "Price") "0.010USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "6")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Filters/EMI Optimization,Ferrite Beads")
        (field (name "Manufacturer") "Sunlord")
        (field (name "Part") "GZ1608D601TF")
        (field (name "DC Resistance") "450mΩ")
        (field (name "Impedance @ Frequency") "600Ω@100MHz")
        (field (name "Circuits") "1")
        (field (name "Current Rating") "200mA")
        (field (name "Tolerance") "±25%")
        (field (name "Footprint") "PCM_JLCPCB:FB_0603")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2310301640_Sunlord-GZ1608D601TF_C1002.pdf")
        (field (name "Description") "450mΩ ±25% 600Ω@100MHz 0603 Ferrite Beads ROHS"))
      (libsource (lib "PCM_JLCPCB-Inductors") (part "Ferrite,0603") (description "450mΩ ±25% 600Ω@100MHz 0603 Ferrite Beads ROHS"))
      (property (name "LCSC") (value "C1002"))
      (property (name "Stock") (value "789150"))
      (property (name "Price") (value "0.010USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "6"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Filters/EMI Optimization,Ferrite Beads"))
      (property (name "Manufacturer") (value "Sunlord"))
      (property (name "Part") (value "GZ1608D601TF"))
      (property (name "DC Resistance") (value "450mΩ"))
      (property (name "Impedance @ Frequency") (value "600Ω@100MHz"))
      (property (name "Circuits") (value "1"))
      (property (name "Current Rating") (value "200mA"))
      (property (name "Tolerance") (value "±25%"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_fp_filters") (value "FB_*"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "23f23e2b-67f5-4f99-baa1-294ed0c04cb4"))
    (comp (ref "J2")
      (value "PJ-611E 6.35mm jack")
      (footprint "JLC2KiCad_lib-footprints:AUDIO-TH_PJ-611E_1")
      (datasheet "https://item.szlcsc.com/datasheet/PJ-611E/292943.html?spm=sc.it.xds.a&lcsc_vid=EVMNBFVWTlcKUQUCQ1FdVFJSRgcNXgJXE1BbX1ACQlgxVlNQQ1NcUF1RR1VcXjsOAxUeFF5JWA0NAgAHWQIASA%3D%3D")
      (fields
        (field (name "LCSC") "C309282")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:AUDIO-TH_PJ-611E_1")
        (field (name "Datasheet") "https://item.szlcsc.com/datasheet/PJ-611E/292943.html?spm=sc.it.xds.a&lcsc_vid=EVMNBFVWTlcKUQUCQ1FdVFJSRgcNXgJXE1BbX1ACQlgxVlNQQ1NcUF1RR1VcXjsOAxUeFF5JWA0NAgAHWQIASA%3D%3D")
        (field (name "Description")))
      (libsource (lib "PJ-611E jack 6.35mm") (part "PJ-611E") (description ""))
      (property (name "LCSC") (value "C309282"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_keywords") (value "C309282"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "d8972c84-be5a-41b1-a667-1e70daa636ac"))
    (comp (ref "J3")
      (value "J_RCA_L (white)")
      (footprint "JLC2KiCad_lib-footprints:CONN-TH_AV-5")
      (fields
        (field (name "MF") "Same Sky")
        (field (name "Description_1") "Metal Right-Angle, SMT RCA Jack, White Insulator")
        (field (name "Package") "None")
        (field (name "Price") "None")
        (field (name "Check_prices") "https://www.snapeda.com/parts/RCJ-013-SMT-TR/Same+Sky/view-part/?ref=eda")
        (field (name "PART_REV") "B")
        (field (name "STANDARD") "Manufacturer recommendations")
        (field (name "SnapEDA_Link") "https://www.snapeda.com/parts/RCJ-013-SMT-TR/Same+Sky/view-part/?ref=snap")
        (field (name "MP") "RCJ-013-SMT-TR")
        (field (name "Purchase-URL") "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=1316562&manufacturer=Same Sky&part_name=RCJ-013-SMT-TR&search_term=rca jack pcb mount")
        (field (name "Availability") "In Stock")
        (field (name "MANUFACTURER") "CUI Inc")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:CONN-TH_AV-5")
        (field (name "Datasheet"))
        (field (name "Description")))
      (libsource (lib "rca-jack-white") (part "RCJ-013-SMT") (description ""))
      (property (name "MF") (value "Same Sky"))
      (property (name "Description_1") (value "Metal Right-Angle, SMT RCA Jack, White Insulator"))
      (property (name "Package") (value "None"))
      (property (name "Price") (value "None"))
      (property (name "Check_prices") (value "https://www.snapeda.com/parts/RCJ-013-SMT-TR/Same+Sky/view-part/?ref=eda"))
      (property (name "PART_REV") (value "B"))
      (property (name "STANDARD") (value "Manufacturer recommendations"))
      (property (name "SnapEDA_Link") (value "https://www.snapeda.com/parts/RCJ-013-SMT-TR/Same+Sky/view-part/?ref=snap"))
      (property (name "MP") (value "RCJ-013-SMT-TR"))
      (property (name "Purchase-URL") (value "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=1316562&manufacturer=Same Sky&part_name=RCJ-013-SMT-TR&search_term=rca jack pcb mount"))
      (property (name "Availability") (value "In Stock"))
      (property (name "MANUFACTURER") (value "CUI Inc"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "a588bdb6-f08f-42bc-807f-4bfb60c077dd"))
    (comp (ref "J4")
      (value "J_RCA_R (red)")
      (footprint "JLC2KiCad_lib-footprints:CONN-TH_AV-5")
      (fields
        (field (name "MF") "Same Sky")
        (field (name "Description_1") "Metal Right-Angle, SMT RCA Jack, Red Insulator")
        (field (name "Package") "None")
        (field (name "Price") "None")
        (field (name "Check_prices") "https://www.snapeda.com/parts/RCJ-012-SMT-TR/Same+Sky/view-part/?ref=eda")
        (field (name "PART_REV") "B")
        (field (name "STANDARD") "Manufacturer recommendations")
        (field (name "SnapEDA_Link") "https://www.snapeda.com/parts/RCJ-012-SMT-TR/Same+Sky/view-part/?ref=snap")
        (field (name "MP") "RCJ-012-SMT-TR")
        (field (name "Purchase-URL") "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=1316485&manufacturer=Same Sky&part_name=RCJ-012-SMT-TR&search_term=rca jack pcb mount")
        (field (name "Availability") "In Stock")
        (field (name "MANUFACTURER") "CUI Inc")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:CONN-TH_AV-5")
        (field (name "Datasheet"))
        (field (name "Description")))
      (libsource (lib "rca-jack-red") (part "RCJ-012-SMT") (description ""))
      (property (name "MF") (value "Same Sky"))
      (property (name "Description_1") (value "Metal Right-Angle, SMT RCA Jack, Red Insulator"))
      (property (name "Package") (value "None"))
      (property (name "Price") (value "None"))
      (property (name "Check_prices") (value "https://www.snapeda.com/parts/RCJ-012-SMT-TR/Same+Sky/view-part/?ref=eda"))
      (property (name "PART_REV") (value "B"))
      (property (name "STANDARD") (value "Manufacturer recommendations"))
      (property (name "SnapEDA_Link") (value "https://www.snapeda.com/parts/RCJ-012-SMT-TR/Same+Sky/view-part/?ref=snap"))
      (property (name "MP") (value "RCJ-012-SMT-TR"))
      (property (name "Purchase-URL") (value "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=1316485&manufacturer=Same Sky&part_name=RCJ-012-SMT-TR&search_term=rca jack pcb mount"))
      (property (name "Availability") (value "In Stock"))
      (property (name "MANUFACTURER") (value "CUI Inc"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "0fe64348-9aaa-42ab-87f8-1d2a60e96301"))
    (comp (ref "J5")
      (value "PJ-320D 3.5mm jack")
      (footprint "JLC2KiCad_lib-footprints:AUDIO-SMD_PJ-320D-1")
      (datasheet "https://atta.szlcsc.com/upload/public/pdf/source/20190925/C431535_8B274506621F6117FB020BF07A197848.pdf")
      (fields
        (field (name "LCSC") "C431535")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:AUDIO-SMD_PJ-320D-1")
        (field (name "Datasheet") "https://atta.szlcsc.com/upload/public/pdf/source/20190925/C431535_8B274506621F6117FB020BF07A197848.pdf")
        (field (name "Description")))
      (libsource (lib "PJ-320D jack 3.5mm") (part "PJ-320D") (description ""))
      (property (name "LCSC") (value "C431535"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_keywords") (value "C431535"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "0c486586-4411-4e6a-82f2-92c1d239706d"))
    (comp (ref "R11")
      (value "47kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "1c3caf85-5cf5-41bb-b440-f9ff940fc829"))
    (comp (ref "R12")
      (value "470Ω")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "7e8e8b16-edef-4204-bc6b-9180e174626c"))
    (comp (ref "R13")
      (value "470Ω")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "ccb187a4-79e3-46e5-8f34-b2e6d3e85dd4"))
    (comp (ref "U2")
      (value "PCM5122PW")
      (footprint "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm")
      (datasheet "http://www.ti.com/lit/ds/symlink/pcm5122.pdf")
      (description "2VRMS DirectPath, 112dB Audio Stereo DAC with 32-bit, 384kHz PCM Interface, TSSOP-28")
      (fields
        (field (name "Footprint") "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm")
        (field (name "Datasheet") "http://www.ti.com/lit/ds/symlink/pcm5122.pdf")
        (field (name "Description") "2VRMS DirectPath, 112dB Audio Stereo DAC with 32-bit, 384kHz PCM Interface, TSSOP-28"))
      (libsource (lib "Audio") (part "PCM5122PW") (description "2VRMS DirectPath, 112dB Audio Stereo DAC with 32-bit, 384kHz PCM Interface, TSSOP-28"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_keywords") (value "audio dac 2ch 32bit 384kHz"))
      (property (name "ki_fp_filters") (value "TSSOP*4.4x9.7mm*P0.65mm*"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "309d9f76-601e-4cd9-ae2a-b0cb670fc820"))
    (comp (ref "H1")
      (value "MountingHole")
      (footprint "MountingHole:MountingHole_3.2mm_M3")
      (datasheet "~")
      (description "Mounting Hole without connection")
      (fields
        (field (name "Footprint") "MountingHole:MountingHole_3.2mm_M3")
        (field (name "Datasheet") "~")
        (field (name "Description") "Mounting Hole without connection"))
      (libsource (lib "Mechanical") (part "MountingHole") (description "Mounting Hole without connection"))
      (property (name "Sheetname") (value "Test Points"))
      (property (name "Sheetfile") (value "test_points.kicad_sch"))
      (property (name "exclude_from_bom"))
      (property (name "ki_keywords") (value "mounting hole"))
      (property (name "ki_fp_filters") (value "MountingHole*"))
      (sheetpath (names "/Test Points/") (tstamps "/51b1dfb5-ef32-4d46-aca8-09c1f86f56e0/"))
      (tstamps "56f74c51-f794-4317-a013-c2963c2bf83e"))
    (comp (ref "H2")
      (value "MountingHole")
      (footprint "MountingHole:MountingHole_3.2mm_M3")
      (datasheet "~")
      (description "Mounting Hole without connection")
      (fields
        (field (name "Footprint") "MountingHole:MountingHole_3.2mm_M3")
        (field (name "Datasheet") "~")
        (field (name "Description") "Mounting Hole without connection"))
      (libsource (lib "Mechanical") (part "MountingHole") (description "Mounting Hole without connection"))
      (property (name "Sheetname") (value "Test Points"))
      (property (name "Sheetfile") (value "test_points.kicad_sch"))
      (property (name "exclude_from_bom"))
      (property (name "ki_keywords") (value "mounting hole"))
      (property (name "ki_fp_filters") (value "MountingHole*"))
      (sheetpath (names "/Test Points/") (tstamps "/51b1dfb5-ef32-4d46-aca8-09c1f86f56e0/"))
      (tstamps "b29d003e-e50d-47ac-b43b-5653327636e5"))
    (comp (ref "H3")
      (value "MountingHole")
      (footprint "MountingHole:MountingHole_3.2mm_M3")
      (datasheet "~")
      (description "Mounting Hole without connection")
      (fields
        (field (name "Footprint") "MountingHole:MountingHole_3.2mm_M3")
        (field (name "Datasheet") "~")
        (field (name "Description") "Mounting Hole without connection"))
      (libsource (lib "Mechanical") (part "MountingHole") (description "Mounting Hole without connection"))
      (property (name "Sheetname") (value "Test Points"))
      (property (name "Sheetfile") (value "test_points.kicad_sch"))
      (property (name "exclude_from_bom"))
      (property (name "ki_keywords") (value "mounting hole"))
      (property (name "ki_fp_filters") (value "MountingHole*"))
      (sheetpath (names "/Test Points/") (tstamps "/51b1dfb5-ef32-4d46-aca8-09c1f86f56e0/"))
      (tstamps "2709749f-f25d-4c6b-8b75-29bc3049cb5e"))
    (comp (ref "H4")
      (value "MountingHole")
      (footprint "MountingHole:MountingHole_3.2mm_M3")
      (datasheet "~")
      (description "Mounting Hole without connection")
      (fields
        (field (name "Footprint") "MountingHole:MountingHole_3.2mm_M3")
        (field (name "Datasheet") "~")
        (field (name "Description") "Mounting Hole without connection"))
      (libsource (lib "Mechanical") (part "MountingHole") (description "Mounting Hole without connection"))
      (property (name "Sheetname") (value "Test Points"))
      (property (name "Sheetfile") (value "test_points.kicad_sch"))
      (property (name "exclude_from_bom"))
      (property (name "ki_keywords") (value "mounting hole"))
      (property (name "ki_fp_filters") (value "MountingHole*"))
      (sheetpath (names "/Test Points/") (tstamps "/51b1dfb5-ef32-4d46-aca8-09c1f86f56e0/"))
      (tstamps "0653b266-e99c-4ae7-b401-ac460769c694"))
    (comp (ref "J6")
      (value "J_ISP_ATMEGA")
      (footprint "Connector_JST:JST_PH_B6B-PH-K_1x06_P2.00mm_Vertical")
      (datasheet "~")
      (description "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (fields
        (field (name "Footprint") "Connector_JST:JST_PH_B6B-PH-K_1x06_P2.00mm_Vertical")
        (field (name "Datasheet") "~")
        (field (name "Description") "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (libsource (lib "Connector_Generic") (part "Conn_01x06") (description "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (property (name "Sheetname") (value "Test Points"))
      (property (name "Sheetfile") (value "test_points.kicad_sch"))
      (property (name "ki_keywords") (value "connector"))
      (property (name "ki_fp_filters") (value "Connector*:*_1x??_*"))
      (sheetpath (names "/Test Points/") (tstamps "/51b1dfb5-ef32-4d46-aca8-09c1f86f56e0/"))
      (tstamps "163942d0-20bb-4554-8110-898eb11c0d60"))
    (comp (ref "J7")
      (value "J_I2C")
      (footprint "Connector_JST:JST_PH_B4B-PH-K_1x04_P2.00mm_Vertical")
      (datasheet "~")
      (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (fields
        (field (name "Footprint") "Connector_JST:JST_PH_B4B-PH-K_1x04_P2.00mm_Vertical")
        (field (name "Datasheet") "~")
        (field (name "Description") "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (libsource (lib "Connector_Generic") (part "Conn_01x04") (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (property (name "Sheetname") (value "Test Points"))
      (property (name "Sheetfile") (value "test_points.kicad_sch"))
      (property (name "ki_keywords") (value "connector"))
      (property (name "ki_fp_filters") (value "Connector*:*_1x??_*"))
      (sheetpath (names "/Test Points/") (tstamps "/51b1dfb5-ef32-4d46-aca8-09c1f86f56e0/"))
      (tstamps "902037ab-2e15-4ffa-86c7-cdaf90458176"))
    (comp (ref "TP1")
      (value "TP_20V_USB_RAIL")
      (footprint "TestPoint:TestPoint_Pad_2.0x2.0mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Footprint") "TestPoint:TestPoint_Pad_2.0x2.0mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Sheetname") (value "Test Points"))
      (property (name "Sheetfile") (value "test_points.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Test Points/") (tstamps "/51b1dfb5-ef32-4d46-aca8-09c1f86f56e0/"))
      (tstamps "9b728568-849d-4b2d-b07b-9f5aff9a8a3c"))
    (comp (ref "TP2")
      (value "TP_20V_USB")
      (footprint "TestPoint:TestPoint_Pad_2.0x2.0mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Footprint") "TestPoint:TestPoint_Pad_2.0x2.0mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Sheetname") (value "Test Points"))
      (property (name "Sheetfile") (value "test_points.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Test Points/") (tstamps "/51b1dfb5-ef32-4d46-aca8-09c1f86f56e0/"))
      (tstamps "b3836ea7-1cfe-493c-b6c2-d1b308195380"))
    (comp (ref "TP3")
      (value "TP_3.3_DGTL")
      (footprint "TestPoint:TestPoint_Pad_2.0x2.0mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Footprint") "TestPoint:TestPoint_Pad_2.0x2.0mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Sheetname") (value "Test Points"))
      (property (name "Sheetfile") (value "test_points.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Test Points/") (tstamps "/51b1dfb5-ef32-4d46-aca8-09c1f86f56e0/"))
      (tstamps "bffa881a-28f6-44b8-93c6-251ff3411913"))
    (comp (ref "TP4")
      (value "TP_5V")
      (footprint "TestPoint:TestPoint_Pad_2.0x2.0mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Footprint") "TestPoint:TestPoint_Pad_2.0x2.0mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Sheetname") (value "Test Points"))
      (property (name "Sheetfile") (value "test_points.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Test Points/") (tstamps "/51b1dfb5-ef32-4d46-aca8-09c1f86f56e0/"))
      (tstamps "000c4d62-16fa-4517-8feb-60d44f0a2c5c"))
    (comp (ref "TP5")
      (value "TP_3.3_ANALOG")
      (footprint "TestPoint:TestPoint_Pad_2.0x2.0mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Footprint") "TestPoint:TestPoint_Pad_2.0x2.0mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Sheetname") (value "Test Points"))
      (property (name "Sheetfile") (value "test_points.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Test Points/") (tstamps "/51b1dfb5-ef32-4d46-aca8-09c1f86f56e0/"))
      (tstamps "76099a4f-c44b-4008-b8a7-3315ee307196"))
    (comp (ref "TP6")
      (value "TP_I2C_SDA")
      (footprint "TestPoint:TestPoint_Pad_1.5x1.5mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Footprint") "TestPoint:TestPoint_Pad_1.5x1.5mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Sheetname") (value "Test Points"))
      (property (name "Sheetfile") (value "test_points.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Test Points/") (tstamps "/51b1dfb5-ef32-4d46-aca8-09c1f86f56e0/"))
      (tstamps "c8cffb17-742a-4eb5-a83f-456166104239"))
    (comp (ref "TP7")
      (value "TP_GND")
      (footprint "TestPoint:TestPoint_Pad_2.0x2.0mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Footprint") "TestPoint:TestPoint_Pad_2.0x2.0mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Sheetname") (value "Test Points"))
      (property (name "Sheetfile") (value "test_points.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Test Points/") (tstamps "/51b1dfb5-ef32-4d46-aca8-09c1f86f56e0/"))
      (tstamps "a9cb6750-7855-448a-8fef-5da4eec8b027"))
    (comp (ref "TP8")
      (value "TP_I2C_SCL")
      (footprint "TestPoint:TestPoint_Pad_1.5x1.5mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Footprint") "TestPoint:TestPoint_Pad_1.5x1.5mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Sheetname") (value "Test Points"))
      (property (name "Sheetfile") (value "test_points.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Test Points/") (tstamps "/51b1dfb5-ef32-4d46-aca8-09c1f86f56e0/"))
      (tstamps "8373e821-6e2c-4815-b5f4-083d162ee632"))
    (comp (ref "TP9")
      (value "TP_I2S_BCK")
      (footprint "TestPoint:TestPoint_Pad_1.5x1.5mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Footprint") "TestPoint:TestPoint_Pad_1.5x1.5mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Sheetname") (value "Test Points"))
      (property (name "Sheetfile") (value "test_points.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Test Points/") (tstamps "/51b1dfb5-ef32-4d46-aca8-09c1f86f56e0/"))
      (tstamps "c10537b8-5cc7-4ab7-b68e-2bdbbacbaebe"))
    (comp (ref "TP10")
      (value "TP_I2S_LRCK")
      (footprint "TestPoint:TestPoint_Pad_1.5x1.5mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Footprint") "TestPoint:TestPoint_Pad_1.5x1.5mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Sheetname") (value "Test Points"))
      (property (name "Sheetfile") (value "test_points.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Test Points/") (tstamps "/51b1dfb5-ef32-4d46-aca8-09c1f86f56e0/"))
      (tstamps "5c96c9d8-07a0-4b6b-8b3b-43cd8c67e5d9"))
    (comp (ref "TP11")
      (value "TP_I2S_DIN")
      (footprint "TestPoint:TestPoint_Pad_1.5x1.5mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Footprint") "TestPoint:TestPoint_Pad_1.5x1.5mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Sheetname") (value "Test Points"))
      (property (name "Sheetfile") (value "test_points.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Test Points/") (tstamps "/51b1dfb5-ef32-4d46-aca8-09c1f86f56e0/"))
      (tstamps "c2ef8b36-7158-4909-803c-8d9369519cd3"))
    (comp (ref "C14")
      (value "1µF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "a164dc69-2c12-4ac3-9cc7-239e932f18ad"))
    (comp (ref "C15")
      (value "1µF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "26f44fdb-c055-4df4-bbbe-886627cd7cff"))
    (comp (ref "C16")
      (value "1µF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "dac0d2e6-2158-46fb-b346-b816dce74306"))
    (comp (ref "C17")
      (value "1µF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "9bd8f95e-2099-405d-813b-27e00652ee85"))
    (comp (ref "C18")
      (value "1µF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "d974f2a3-4574-4cf0-9511-6c8ea5d40aa4"))
    (comp (ref "C19")
      (value "1µF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "7e32ea3d-fc47-47a1-a66f-b074d2a27274"))
    (comp (ref "C20")
      (value "100nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "952ac961-d558-4e7f-9815-286604b478e7"))
    (comp (ref "C21")
      (value "100nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "9ff13258-c727-4529-9560-fce4539c02a5"))
    (comp (ref "C22")
      (value "1µF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "1317ff50-e8d1-469f-94a9-ac53cf4dbd3e"))
    (comp (ref "C23")
      (value "1µF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "2a7c94c0-bcdf-420e-aff2-99c492bec02d"))
    (comp (ref "J8")
      (value "AUX POWER USB_A")
      (footprint "JLC2KiCad_lib-footprints:USB-3.0-A-TH_HC-ST-003-010-L15.0-J-K")
      (datasheet "~")
      (description "USB Type A connector used to light up gadgets using this circuit's power")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:USB-3.0-A-TH_HC-ST-003-010-L15.0-J-K")
        (field (name "Datasheet") "~")
        (field (name "Description") "USB Type A connector used to light up gadgets using this circuit's power"))
      (libsource (lib "Connector") (part "USB_A") (description "USB Type A connector"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "connector USB"))
      (property (name "ki_fp_filters") (value "USB*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "473da71d-55a4-488c-b9b7-d8b63cb7cad2"))
    (comp (ref "J9")
      (value "TYPE-C_16PIN_2MD(073)")
      (footprint "JLC2KiCad_lib-footprints:USB-C-SMD_TYPE-C-6PIN-2MD-073")
      (datasheet "https://atta.szlcsc.com/upload/public/pdf/source/20210409/C2765186_34D42616F62DF94D17C4D63D74D9FD03.pdf")
      (description "USB-C Data USB2.0")
      (fields
        (field (name "LCSC") "C2765186")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:USB-C-SMD_TYPE-C-6PIN-2MD-073")
        (field (name "Datasheet") "https://atta.szlcsc.com/upload/public/pdf/source/20210409/C2765186_34D42616F62DF94D17C4D63D74D9FD03.pdf")
        (field (name "Description") "USB-C Data USB2.0"))
      (libsource (lib "jlc_TYPE-C_16PIN_2MD(073)") (part "TYPE-C_16PIN_2MD(073)") (description ""))
      (property (name "LCSC") (value "C2765186"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "C2765186"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "f3002b94-c727-457d-8fd7-41e607fe1802"))
    (comp (ref "J10")
      (value "USB_DJ_STICK (USB3_A)")
      (footprint "JLC2KiCad_lib-footprints:USB-3.0-A-TH_HC-ST-003-010-L15.0-J-K")
      (datasheet "~")
      (description "USB 3.0 A connector")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:USB-3.0-A-TH_HC-ST-003-010-L15.0-J-K")
        (field (name "Datasheet") "~")
        (field (name "Description") "USB 3.0 A connector"))
      (libsource (lib "Connector") (part "USB3_A") (description "USB 3.0 A connector"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "usb universal serial bus"))
      (property (name "ki_fp_filters") (value "USB3*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "ef5a3171-3d0c-4174-b3a5-dc9ee025bc31"))
    (comp (ref "J11")
      (value "USB_SCREEN (USB3_A)")
      (footprint "JLC2KiCad_lib-footprints:USB-3.0-A-TH_HC-ST-003-010-L15.0-J-K")
      (datasheet "~")
      (description "USB 3.0 A connector")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:USB-3.0-A-TH_HC-ST-003-010-L15.0-J-K")
        (field (name "Datasheet") "~")
        (field (name "Description") "USB 3.0 A connector"))
      (libsource (lib "Connector") (part "USB3_A") (description "USB 3.0 A connector"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "usb universal serial bus"))
      (property (name "ki_fp_filters") (value "USB3*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "680b1526-22ae-42ac-8b8d-6241e707f287"))
    (comp (ref "R14")
      (value "100kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "44273459-1582-47a4-84ae-f05de514277f"))
    (comp (ref "R15")
      (value "10kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "d9ff175a-2704-4c17-acd6-6dd3e5c3c4db"))
    (comp (ref "R16")
      (value "10kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "3dc7a99a-09e3-4aa1-b347-d0e84ab48181"))
    (comp (ref "R17")
      (value "100kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "c6ad4673-9612-44de-9ef5-c550341af4d6"))
    (comp (ref "R18")
      (value "10kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "18dae2b8-cdad-475c-b519-28ab9f92aa9d"))
    (comp (ref "R19")
      (value "100kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "2619be51-8473-49aa-ba0e-7068ac1941d6"))
    (comp (ref "R20")
      (value "10kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "b13c1d57-75cd-4096-82d9-b5d0b9885562"))
    (comp (ref "R21")
      (value "5.1kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "ad3b56e0-772d-4498-b1ff-75f301d3d7e5"))
    (comp (ref "R22")
      (value "5.1kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "e2d8225a-ae82-49b0-a512-f4430a13d329"))
    (comp (ref "R23")
      (value "100kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "3022c101-6b08-44e5-bc77-3ad3540171b2"))
    (comp (ref "R24")
      (value "10kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "14d8051b-bbc0-493f-8fe0-f901aeb5ae0e"))
    (comp (ref "U1")
      (value "Compute_Module_5_Functional")
      (footprint "kicad-thirdparty-footprints:CM5")
      (fields
        (field (name "Footprint") "kicad-thirdparty-footprints:CM5")
        (field (name "Datasheet"))
        (field (name "Description")))
      (libsource (lib "rpi-cm-5") (part "Compute_Module_5_Functional") (description ""))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "6d3d3746-e7c4-4300-a51b-7415f722c2b5" "4417d12c-776a-4ae2-b0ac-7c19d5361bd6" "0a37b576-4847-42fa-ade4-9f579e85d0c2"))
    (comp (ref "U3")
      (value "AP2553W6-7")
      (footprint "JLC2KiCad_lib-footprints:SOT-26_L3.0-W1.6-P0.95-LS2.8-BL")
      (datasheet "https://item.szlcsc.com/211080.html")
      (fields
        (field (name "LCSC") "C212302")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:SOT-26_L3.0-W1.6-P0.95-LS2.8-BL")
        (field (name "Datasheet") "https://item.szlcsc.com/211080.html")
        (field (name "Description")))
      (libsource (lib "AP2553W6-7") (part "AP2553W6-7") (description ""))
      (property (name "LCSC") (value "C212302"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "C212302"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "ffd0b6bb-d454-4460-bd18-11768c1d3bdc"))
    (comp (ref "U4")
      (value "AP2553W6-7")
      (footprint "JLC2KiCad_lib-footprints:SOT-26_L3.0-W1.6-P0.95-LS2.8-BL")
      (datasheet "https://item.szlcsc.com/211080.html")
      (fields
        (field (name "LCSC") "C212302")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:SOT-26_L3.0-W1.6-P0.95-LS2.8-BL")
        (field (name "Datasheet") "https://item.szlcsc.com/211080.html")
        (field (name "Description")))
      (libsource (lib "AP2553W6-7") (part "AP2553W6-7") (description ""))
      (property (name "LCSC") (value "C212302"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "C212302"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "c6477ae5-d171-4636-97f7-c43bebb35b68"))
    (comp (ref "U5")
      (value "AP2553W6-7")
      (footprint "JLC2KiCad_lib-footprints:SOT-26_L3.0-W1.6-P0.95-LS2.8-BL")
      (datasheet "https://item.szlcsc.com/211080.html")
      (fields
        (field (name "LCSC") "C212302")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:SOT-26_L3.0-W1.6-P0.95-LS2.8-BL")
        (field (name "Datasheet") "https://item.szlcsc.com/211080.html")
        (field (name "Description")))
      (libsource (lib "AP2553W6-7") (part "AP2553W6-7") (description ""))
      (property (name "LCSC") (value "C212302"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "C212302"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "6630d2a6-2dc3-4f86-ae72-a320e95cf006"))
    (comp (ref "U6")
      (value "USBLC6-2SC6-ES")
      (footprint "footprint:SOT-23-6_L2.9-W1.6-P0.95-LS2.8-BR")
      (datasheet "https://item.szlcsc.com/169042.html")
      (fields
        (field (name "LCSC") "C5180249")
        (field (name "Footprint") "footprint:SOT-23-6_L2.9-W1.6-P0.95-LS2.8-BR")
        (field (name "Datasheet") "https://item.szlcsc.com/169042.html")
        (field (name "Description")))
      (libsource (lib "jlc_USBLC6-2SC6-ES") (part "USBLC6-2SC6-ES") (description ""))
      (property (name "LCSC") (value "C5180249"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "C5180249"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "168f8e4d-528a-43db-ac4f-ab0898c18a2a"))
    (comp (ref "U8")
      (value "USBLC6-2SC6-ES")
      (footprint "footprint:SOT-23-6_L2.9-W1.6-P0.95-LS2.8-BR")
      (datasheet "https://item.szlcsc.com/169042.html")
      (fields
        (field (name "LCSC") "C5180249")
        (field (name "Footprint") "footprint:SOT-23-6_L2.9-W1.6-P0.95-LS2.8-BR")
        (field (name "Datasheet") "https://item.szlcsc.com/169042.html")
        (field (name "Description")))
      (libsource (lib "jlc_USBLC6-2SC6-ES") (part "USBLC6-2SC6-ES") (description ""))
      (property (name "LCSC") (value "C5180249"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "C5180249"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "22a1f263-4fcf-4968-971c-8fb11e86a3cf"))
    (comp (ref "U9")
      (value "AP2553W6-7")
      (footprint "JLC2KiCad_lib-footprints:SOT-26_L3.0-W1.6-P0.95-LS2.8-BL")
      (datasheet "https://item.szlcsc.com/211080.html")
      (fields
        (field (name "LCSC") "C212302")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:SOT-26_L3.0-W1.6-P0.95-LS2.8-BL")
        (field (name "Datasheet") "https://item.szlcsc.com/211080.html")
        (field (name "Description")))
      (libsource (lib "AP2553W6-7") (part "AP2553W6-7") (description ""))
      (property (name "LCSC") (value "C212302"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "C212302"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "47e62c68-9807-4713-881f-5759cfe0c360"))
    (comp (ref "U22")
      (value "USBLC6-2SC6-ES")
      (footprint "footprint:SOT-23-6_L2.9-W1.6-P0.95-LS2.8-BR")
      (datasheet "https://item.szlcsc.com/169042.html")
      (fields
        (field (name "LCSC") "C5180249")
        (field (name "Footprint") "footprint:SOT-23-6_L2.9-W1.6-P0.95-LS2.8-BR")
        (field (name "Datasheet") "https://item.szlcsc.com/169042.html")
        (field (name "Description")))
      (libsource (lib "jlc_USBLC6-2SC6-ES") (part "USBLC6-2SC6-ES") (description ""))
      (property (name "LCSC") (value "C5180249"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "C5180249"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "28a0d64d-4244-4f11-a685-52ae0c027c48"))
    (comp (ref "J12")
      (value "HR911130A")
      (footprint "JLC2KiCad_lib-footprints:RJ45-TH_HR911130A")
      (datasheet "https://item.szlcsc.com/55426.html")
      (fields
        (field (name "LCSC") "C54408")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:RJ45-TH_HR911130A")
        (field (name "Datasheet") "https://item.szlcsc.com/55426.html")
        (field (name "Description")))
      (libsource (lib "") (part "HR911130A_1") (description ""))
      (property (name "LCSC") (value "C54408"))
      (property (name "Sheetname") (value "HDMI and Ethernet"))
      (property (name "Sheetfile") (value "hdmi.kicad_sch"))
      (property (name "ki_keywords") (value "C54408"))
      (sheetpath (names "/HDMI and Ethernet/") (tstamps "/97e2c747-925a-451b-94c7-ccaeac2c14a8/"))
      (tstamps "64a918de-2451-421d-9eae-24ca1970d9ff"))
    (comp (ref "J13")
      (value "PI HDMI_0 (HDMI_D_1.4 micro)")
      (footprint "JLC2KiCad_lib-footprints:HDMI-SMD_HDMI-101S")
      (datasheet "http://pinoutguide.com/PortableDevices/micro_hdmi_type_d_pinout.shtml")
      (description "HDMI 1.4+ type D connector")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:HDMI-SMD_HDMI-101S")
        (field (name "Datasheet") "http://pinoutguide.com/PortableDevices/micro_hdmi_type_d_pinout.shtml")
        (field (name "Description") "HDMI 1.4+ type D connector"))
      (libsource (lib "Connector") (part "HDMI_D_1.4") (description "HDMI 1.4+ type D connector"))
      (property (name "Sheetname") (value "HDMI and Ethernet"))
      (property (name "Sheetfile") (value "hdmi.kicad_sch"))
      (property (name "ki_keywords") (value "hdmi conn"))
      (property (name "ki_fp_filters") (value "HDMI*D*"))
      (sheetpath (names "/HDMI and Ethernet/") (tstamps "/97e2c747-925a-451b-94c7-ccaeac2c14a8/"))
      (tstamps "49c01394-e7c0-48a0-adc0-5a338f4ebfd9"))
    (comp (ref "J14")
      (value "PI HDMI_0 (HDMI_D_1.4 micro)")
      (footprint "JLC2KiCad_lib-footprints:HDMI-SMD_HDMI-101S")
      (datasheet "http://pinoutguide.com/PortableDevices/micro_hdmi_type_d_pinout.shtml")
      (description "HDMI 1.4+ type D connector")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:HDMI-SMD_HDMI-101S")
        (field (name "Datasheet") "http://pinoutguide.com/PortableDevices/micro_hdmi_type_d_pinout.shtml")
        (field (name "Description") "HDMI 1.4+ type D connector"))
      (libsource (lib "Connector") (part "HDMI_D_1.4") (description "HDMI 1.4+ type D connector"))
      (property (name "Sheetname") (value "HDMI and Ethernet"))
      (property (name "Sheetfile") (value "hdmi.kicad_sch"))
      (property (name "ki_keywords") (value "hdmi conn"))
      (property (name "ki_fp_filters") (value "HDMI*D*"))
      (sheetpath (names "/HDMI and Ethernet/") (tstamps "/97e2c747-925a-451b-94c7-ccaeac2c14a8/"))
      (tstamps "762e5660-f9ca-4878-8c8d-fe0d1e6ae217"))
    (comp (ref "R25")
      (value "270Ω")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "HDMI and Ethernet"))
      (property (name "Sheetfile") (value "hdmi.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/HDMI and Ethernet/") (tstamps "/97e2c747-925a-451b-94c7-ccaeac2c14a8/"))
      (tstamps "06ab9de6-e22d-4745-97ea-244260c32cc3"))
    (comp (ref "R26")
      (value "270Ω")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "HDMI and Ethernet"))
      (property (name "Sheetfile") (value "hdmi.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/HDMI and Ethernet/") (tstamps "/97e2c747-925a-451b-94c7-ccaeac2c14a8/"))
      (tstamps "bcacd027-4321-4fa4-a645-21ca24d1c515"))
    (comp (ref "C24")
      (value "100nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "fd27a5cf-ad66-4de4-9476-d5d177325ff3"))
    (comp (ref "C25")
      (value "1uF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized CERAMIC capacitor")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized CERAMIC capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "a32ba231-ee1d-4dc4-85c6-62b5bb173f38"))
    (comp (ref "C26")
      (value "1uF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized CERAMIC capacitor")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized CERAMIC capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "4ab2f267-88b6-4e5a-a319-e73dafbab2e1"))
    (comp (ref "C27")
      (value "100nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "9f879c2e-d42d-4e69-a0ff-3bf00fb76da0"))
    (comp (ref "C28")
      (value "100nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "a4572058-4832-4939-a61e-b7b8c5b75e10"))
    (comp (ref "C29")
      (value "100nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "72849b12-8f14-45a9-a4b8-c90fd974d959"))
    (comp (ref "C30")
      (value "100nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "2c8c9716-88dd-473a-ac06-b3960f3973a2"))
    (comp (ref "C31")
      (value "1uF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized CERAMIC capacitor")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized CERAMIC capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "18c7cf92-2c72-4fde-a923-6a92f6eb27fa"))
    (comp (ref "C32")
      (value "1uF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized CERAMIC capacitor")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized CERAMIC capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "f1a4d73a-00ef-4cd9-91e4-dcc4fb9c8771"))
    (comp (ref "C33")
      (value "100nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "944c08c3-81ef-45f5-96c2-11d541ef3edb"))
    (comp (ref "C34")
      (value "100nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "ef64d47f-2653-4782-b4aa-e691d42b97a6"))
    (comp (ref "C35")
      (value "100nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "5847a6db-e430-4d77-a224-31efd6343252"))
    (comp (ref "C36")
      (value "1µF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "b27266aa-f803-4983-8e02-af9e829e835f"))
    (comp (ref "C37")
      (value "10µF/35V")
      (footprint "Capacitor_SMD:C_0805_2012Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0805_2012Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "0527da60-5b8e-4909-a33d-e9d57c569d7b"))
    (comp (ref "C38")
      (value "100nF/50V")
      (footprint "Capacitor_SMD:C_0603_1608Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0603_1608Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "161aeb7f-2540-4455-b6ae-ce406024cbf2"))
    (comp (ref "C39")
      (value "22uF")
      (footprint "PCM_JLCPCB:C_0805")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL21A226MAQNNNE_C45783.pdf")
      (description "25V 22uF X5R ±20% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
      (fields
        (field (name "LCSC") "C45783")
        (field (name "Stock") "6479946")
        (field (name "Price") "0.027USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "8")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT")
        (field (name "Manufacturer") "Samsung Electro-Mechanics")
        (field (name "Part") "CL21A226MAQNNNE")
        (field (name "Voltage Rated") "25V")
        (field (name "Tolerance") "±20%")
        (field (name "Capacitance") "22uF")
        (field (name "Temperature Coefficient") "X5R")
        (field (name "Footprint") "PCM_JLCPCB:C_0805")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL21A226MAQNNNE_C45783.pdf")
        (field (name "Description") "25V 22uF X5R ±20% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (libsource (lib "PCM_JLCPCB-Capacitors") (part "0805,22uF") (description "25V 22uF X5R ±20% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (property (name "LCSC") (value "C45783"))
      (property (name "Stock") (value "6479946"))
      (property (name "Price") (value "0.027USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "8"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT"))
      (property (name "Manufacturer") (value "Samsung Electro-Mechanics"))
      (property (name "Part") (value "CL21A226MAQNNNE"))
      (property (name "Voltage Rated") (value "25V"))
      (property (name "Tolerance") (value "±20%"))
      (property (name "Capacitance") (value "22uF"))
      (property (name "Temperature Coefficient") (value "X5R"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "9ad3a4cc-8677-4446-9f58-006e97e88c86"))
    (comp (ref "C40")
      (value "22uF")
      (footprint "PCM_JLCPCB:C_0805")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL21A226MAQNNNE_C45783.pdf")
      (description "25V 22uF X5R ±20% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
      (fields
        (field (name "LCSC") "C45783")
        (field (name "Stock") "6479946")
        (field (name "Price") "0.027USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "8")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT")
        (field (name "Manufacturer") "Samsung Electro-Mechanics")
        (field (name "Part") "CL21A226MAQNNNE")
        (field (name "Voltage Rated") "25V")
        (field (name "Tolerance") "±20%")
        (field (name "Capacitance") "22uF")
        (field (name "Temperature Coefficient") "X5R")
        (field (name "Footprint") "PCM_JLCPCB:C_0805")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL21A226MAQNNNE_C45783.pdf")
        (field (name "Description") "25V 22uF X5R ±20% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (libsource (lib "PCM_JLCPCB-Capacitors") (part "0805,22uF") (description "25V 22uF X5R ±20% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (property (name "LCSC") (value "C45783"))
      (property (name "Stock") (value "6479946"))
      (property (name "Price") (value "0.027USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "8"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT"))
      (property (name "Manufacturer") (value "Samsung Electro-Mechanics"))
      (property (name "Part") (value "CL21A226MAQNNNE"))
      (property (name "Voltage Rated") (value "25V"))
      (property (name "Tolerance") (value "±20%"))
      (property (name "Capacitance") (value "22uF"))
      (property (name "Temperature Coefficient") (value "X5R"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "f54bafbe-eef3-4880-9bc6-730e409d4f06"))
    (comp (ref "C41")
      (value "22uF")
      (footprint "PCM_JLCPCB:C_0805")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL21A226MAQNNNE_C45783.pdf")
      (description "25V 22uF X5R ±20% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
      (fields
        (field (name "LCSC") "C45783")
        (field (name "Stock") "6479946")
        (field (name "Price") "0.027USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "8")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT")
        (field (name "Manufacturer") "Samsung Electro-Mechanics")
        (field (name "Part") "CL21A226MAQNNNE")
        (field (name "Voltage Rated") "25V")
        (field (name "Tolerance") "±20%")
        (field (name "Capacitance") "22uF")
        (field (name "Temperature Coefficient") "X5R")
        (field (name "Footprint") "PCM_JLCPCB:C_0805")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL21A226MAQNNNE_C45783.pdf")
        (field (name "Description") "25V 22uF X5R ±20% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (libsource (lib "PCM_JLCPCB-Capacitors") (part "0805,22uF") (description "25V 22uF X5R ±20% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (property (name "LCSC") (value "C45783"))
      (property (name "Stock") (value "6479946"))
      (property (name "Price") (value "0.027USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "8"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT"))
      (property (name "Manufacturer") (value "Samsung Electro-Mechanics"))
      (property (name "Part") (value "CL21A226MAQNNNE"))
      (property (name "Voltage Rated") (value "25V"))
      (property (name "Tolerance") (value "±20%"))
      (property (name "Capacitance") (value "22uF"))
      (property (name "Temperature Coefficient") (value "X5R"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "73cb35d7-831b-4b4f-8db7-09756dff78f7"))
    (comp (ref "C42")
      (value "10uF")
      (footprint "PCM_JLCPCB:C_0805")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2411041759_Murata-Electronics-GRM21BR61H106KE43L_C440198.pdf")
      (description "50V 10uF X5R ±10% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
      (fields
        (field (name "LCSC") "C440198")
        (field (name "Stock") "1422246")
        (field (name "Price") "0.066USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "5")
        (field (name "Attrition Qty") "4")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT")
        (field (name "Manufacturer") "Murata Electronics")
        (field (name "Part") "GRM21BR61H106KE43L")
        (field (name "Voltage Rated") "50V")
        (field (name "Tolerance") "±10%")
        (field (name "Capacitance") "10uF")
        (field (name "Temperature Coefficient") "X5R")
        (field (name "Footprint") "PCM_JLCPCB:C_0805")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2411041759_Murata-Electronics-GRM21BR61H106KE43L_C440198.pdf")
        (field (name "Description") "50V 10uF X5R ±10% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (libsource (lib "PCM_JLCPCB-Capacitors") (part "0805,10uF,(2)") (description "50V 10uF X5R ±10% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (property (name "LCSC") (value "C440198"))
      (property (name "Stock") (value "1422246"))
      (property (name "Price") (value "0.066USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "5"))
      (property (name "Attrition Qty") (value "4"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT"))
      (property (name "Manufacturer") (value "Murata Electronics"))
      (property (name "Part") (value "GRM21BR61H106KE43L"))
      (property (name "Voltage Rated") (value "50V"))
      (property (name "Tolerance") (value "±10%"))
      (property (name "Capacitance") (value "10uF"))
      (property (name "Temperature Coefficient") (value "X5R"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "dea176c5-2154-4356-9b5b-f6e9bd958275"))
    (comp (ref "C43")
      (value "10uF")
      (footprint "PCM_JLCPCB:C_0805")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2411041759_Murata-Electronics-GRM21BR61H106KE43L_C440198.pdf")
      (description "50V 10uF X5R ±10% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
      (fields
        (field (name "LCSC") "C440198")
        (field (name "Stock") "1422246")
        (field (name "Price") "0.066USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "5")
        (field (name "Attrition Qty") "4")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT")
        (field (name "Manufacturer") "Murata Electronics")
        (field (name "Part") "GRM21BR61H106KE43L")
        (field (name "Voltage Rated") "50V")
        (field (name "Tolerance") "±10%")
        (field (name "Capacitance") "10uF")
        (field (name "Temperature Coefficient") "X5R")
        (field (name "Footprint") "PCM_JLCPCB:C_0805")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2411041759_Murata-Electronics-GRM21BR61H106KE43L_C440198.pdf")
        (field (name "Description") "50V 10uF X5R ±10% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (libsource (lib "PCM_JLCPCB-Capacitors") (part "0805,10uF,(2)") (description "50V 10uF X5R ±10% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (property (name "LCSC") (value "C440198"))
      (property (name "Stock") (value "1422246"))
      (property (name "Price") (value "0.066USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "5"))
      (property (name "Attrition Qty") (value "4"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT"))
      (property (name "Manufacturer") (value "Murata Electronics"))
      (property (name "Part") (value "GRM21BR61H106KE43L"))
      (property (name "Voltage Rated") (value "50V"))
      (property (name "Tolerance") (value "±10%"))
      (property (name "Capacitance") (value "10uF"))
      (property (name "Temperature Coefficient") (value "X5R"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "9f808e14-6a86-4527-9ea2-726561d40961"))
    (comp (ref "C44")
      (value "100nF")
      (footprint "PCM_JLCPCB:C_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05B104KB54PNC_C307331.pdf")
      (description "50V 100nF X7R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
      (fields
        (field (name "LCSC") "C307331")
        (field (name "Stock") "8389599")
        (field (name "Price") "0.008USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT")
        (field (name "Manufacturer") "Samsung Electro-Mechanics")
        (field (name "Part") "CL05B104KB54PNC")
        (field (name "Voltage Rated") "50V")
        (field (name "Tolerance") "±10%")
        (field (name "Capacitance") "100nF")
        (field (name "Temperature Coefficient") "X7R")
        (field (name "Footprint") "PCM_JLCPCB:C_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05B104KB54PNC_C307331.pdf")
        (field (name "Description") "50V 100nF X7R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (libsource (lib "PCM_JLCPCB-Capacitors") (part "0402,100nF,(2)") (description "50V 100nF X7R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (property (name "LCSC") (value "C307331"))
      (property (name "Stock") (value "8389599"))
      (property (name "Price") (value "0.008USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT"))
      (property (name "Manufacturer") (value "Samsung Electro-Mechanics"))
      (property (name "Part") (value "CL05B104KB54PNC"))
      (property (name "Voltage Rated") (value "50V"))
      (property (name "Tolerance") (value "±10%"))
      (property (name "Capacitance") (value "100nF"))
      (property (name "Temperature Coefficient") (value "X7R"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "24db408b-d71f-4208-a0c3-316afac55655"))
    (comp (ref "C45")
      (value "1uF")
      (footprint "PCM_JLCPCB:C_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05A105KA5NQNC_C52923.pdf")
      (description "25V 1uF X5R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
      (fields
        (field (name "LCSC") "C52923")
        (field (name "Stock") "7021828")
        (field (name "Price") "0.006USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT")
        (field (name "Manufacturer") "Samsung Electro-Mechanics")
        (field (name "Part") "CL05A105KA5NQNC")
        (field (name "Voltage Rated") "25V")
        (field (name "Tolerance") "±10%")
        (field (name "Capacitance") "1uF")
        (field (name "Temperature Coefficient") "X5R")
        (field (name "Footprint") "PCM_JLCPCB:C_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05A105KA5NQNC_C52923.pdf")
        (field (name "Description") "25V 1uF X5R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (libsource (lib "PCM_JLCPCB-Capacitors") (part "0402,1uF") (description "25V 1uF X5R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (property (name "LCSC") (value "C52923"))
      (property (name "Stock") (value "7021828"))
      (property (name "Price") (value "0.006USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT"))
      (property (name "Manufacturer") (value "Samsung Electro-Mechanics"))
      (property (name "Part") (value "CL05A105KA5NQNC"))
      (property (name "Voltage Rated") (value "25V"))
      (property (name "Tolerance") (value "±10%"))
      (property (name "Capacitance") (value "1uF"))
      (property (name "Temperature Coefficient") (value "X5R"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "53c7997d-7e56-47f3-b140-1a5a9341c465"))
    (comp (ref "C46")
      (value "22uF")
      (footprint "PCM_JLCPCB:C_0805")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL21A226MAQNNNE_C45783.pdf")
      (description "25V 22uF X5R ±20% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
      (fields
        (field (name "LCSC") "C45783")
        (field (name "Stock") "6479946")
        (field (name "Price") "0.027USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "8")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT")
        (field (name "Manufacturer") "Samsung Electro-Mechanics")
        (field (name "Part") "CL21A226MAQNNNE")
        (field (name "Voltage Rated") "25V")
        (field (name "Tolerance") "±20%")
        (field (name "Capacitance") "22uF")
        (field (name "Temperature Coefficient") "X5R")
        (field (name "Footprint") "PCM_JLCPCB:C_0805")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL21A226MAQNNNE_C45783.pdf")
        (field (name "Description") "25V 22uF X5R ±20% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (libsource (lib "PCM_JLCPCB-Capacitors") (part "0805,22uF") (description "25V 22uF X5R ±20% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (property (name "LCSC") (value "C45783"))
      (property (name "Stock") (value "6479946"))
      (property (name "Price") (value "0.027USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "8"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT"))
      (property (name "Manufacturer") (value "Samsung Electro-Mechanics"))
      (property (name "Part") (value "CL21A226MAQNNNE"))
      (property (name "Voltage Rated") (value "25V"))
      (property (name "Tolerance") (value "±20%"))
      (property (name "Capacitance") (value "22uF"))
      (property (name "Temperature Coefficient") (value "X5R"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "927bb68e-2ff6-4fef-ba87-571e1a209e64"))
    (comp (ref "C47")
      (value "100pF")
      (footprint "PCM_JLCPCB:C_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_FH--Guangdong-Fenghua-Advanced-Tech-0402CG101J500NT_C1546.pdf")
      (description "50V 100pF C0G ±5% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
      (fields
        (field (name "LCSC") "C1546")
        (field (name "Stock") "2554383")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT")
        (field (name "Manufacturer") "FH(Guangdong Fenghua Advanced Tech)")
        (field (name "Part") "0402CG101J500NT")
        (field (name "Voltage Rated") "50V")
        (field (name "Tolerance") "±5%")
        (field (name "Capacitance") "100pF")
        (field (name "Temperature Coefficient") "C0G")
        (field (name "Footprint") "PCM_JLCPCB:C_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_FH--Guangdong-Fenghua-Advanced-Tech-0402CG101J500NT_C1546.pdf")
        (field (name "Description") "50V 100pF C0G ±5% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (libsource (lib "PCM_JLCPCB-Capacitors") (part "0402,100pF") (description "50V 100pF C0G ±5% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (property (name "LCSC") (value "C1546"))
      (property (name "Stock") (value "2554383"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT"))
      (property (name "Manufacturer") (value "FH(Guangdong Fenghua Advanced Tech)"))
      (property (name "Part") (value "0402CG101J500NT"))
      (property (name "Voltage Rated") (value "50V"))
      (property (name "Tolerance") (value "±5%"))
      (property (name "Capacitance") (value "100pF"))
      (property (name "Temperature Coefficient") (value "C0G"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "86a75b04-5225-4e5d-853a-516bc67504b1"))
    (comp (ref "C48")
      (value "100nF/50V")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "1af27551-7b77-435a-afb7-88eac174520c"))
    (comp (ref "D3")
      (value "KT-0603R")
      (footprint "JLC2KiCad_lib-footprints:LED0603-RD")
      (datasheet "https://item.szlcsc.com/347874.html")
      (fields
        (field (name "LCSC") "C2286")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:LED0603-RD")
        (field (name "Datasheet") "https://item.szlcsc.com/347874.html")
        (field (name "Description")))
      (libsource (lib "KT-0603R") (part "KT-0603R") (description ""))
      (property (name "LCSC") (value "C2286"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "C2286"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "0b7c3e22-e0e1-462a-9cb1-f31aacaab848"))
    (comp (ref "D4")
      (value "BZT52C3V3S")
      (footprint "PCM_JLCPCB:D_SOD-323")
      (datasheet "https://wmsc.lcsc.com/wmsc/upload/file/pdf/v2/lcsc/2403280505_hongjiacheng-BZT52C3V3S_C19077437.pdf")
      (description "Independent Type 200mW 3.1V~3.5V 3.3V SOD-323 Zener Diodes ROHS")
      (fields
        (field (name "LCSC") "C19077437")
        (field (name "Stock") "229387")
        (field (name "Price") "0.018USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Preferred Component")
        (field (name "Category") "Diodes,Zener Diodes")
        (field (name "Manufacturer") "hongjiacheng")
        (field (name "Part") "BZT52C3V3S")
        (field (name "Footprint") "PCM_JLCPCB:D_SOD-323")
        (field (name "Datasheet") "https://wmsc.lcsc.com/wmsc/upload/file/pdf/v2/lcsc/2403280505_hongjiacheng-BZT52C3V3S_C19077437.pdf")
        (field (name "Description") "Independent Type 200mW 3.1V~3.5V 3.3V SOD-323 Zener Diodes ROHS"))
      (libsource (lib "PCM_JLCPCB-Diodes") (part "Zener,BZT52C3V3S") (description "Independent Type 200mW 3.1V~3.5V 3.3V SOD-323 Zener Diodes ROHS"))
      (property (name "LCSC") (value "C19077437"))
      (property (name "Stock") (value "229387"))
      (property (name "Price") (value "0.018USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Preferred Component"))
      (property (name "Category") (value "Diodes,Zener Diodes"))
      (property (name "Manufacturer") (value "hongjiacheng"))
      (property (name "Part") (value "BZT52C3V3S"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_fp_filters") (value "D_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "01bcc9ee-0ab4-46ec-954f-bbf0146285a7"))
    (comp (ref "D5")
      (value "PSC-1608U52GC-G4")
      (footprint "JLC2KiCad_lib-footprints:LED0603-RD_GREEN")
      (datasheet "https://atta.szlcsc.com/upload/public/pdf/source/20190115/C264450_D840E7E570138F41CCE67133F241C738.pdf")
      (fields
        (field (name "LCSC") "C22371297")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:LED0603-RD_GREEN")
        (field (name "Datasheet") "https://atta.szlcsc.com/upload/public/pdf/source/20190115/C264450_D840E7E570138F41CCE67133F241C738.pdf")
        (field (name "Description")))
      (libsource (lib "PSC-1608U52GC-G4") (part "PSC-1608U52GC-G4") (description ""))
      (property (name "LCSC") (value "C22371297"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "C22371297"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "b681a82d-fc87-48e5-b309-360d34beb59e"))
    (comp (ref "D6")
      (value "KT-0603R")
      (footprint "JLC2KiCad_lib-footprints:LED0603-RD")
      (datasheet "https://item.szlcsc.com/347874.html")
      (fields
        (field (name "LCSC") "C2286")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:LED0603-RD")
        (field (name "Datasheet") "https://item.szlcsc.com/347874.html")
        (field (name "Description")))
      (libsource (lib "KT-0603R") (part "KT-0603R") (description ""))
      (property (name "LCSC") (value "C2286"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "C2286"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "77e40ba0-0b44-4d46-a1ed-e27504b457b8"))
    (comp (ref "J15")
      (value "TYPE-C-31-M-12")
      (footprint "JLC2KiCad_lib-footprints:USB-C_SMD-TYPE-C-31-M-12_1")
      (datasheet "https://item.szlcsc.com/datasheet/TYPE-C-31-M-12/177331.html?spm=sc.gbn.xds.a___sc.gbn.hd.ss&lcsc_vid=RgMNUVYEQARbV1xTElVcVwIAFFBXVwBfEQdfX1UCRAcxVlNTQFBcUlFXT1hYVTsOAxUeFF5JWA0NAgAHWQIASA%3D%3D")
      (description "USB-C Power C165948")
      (fields
        (field (name "LCSC") "C165948")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:USB-C_SMD-TYPE-C-31-M-12_1")
        (field (name "Datasheet") "https://item.szlcsc.com/datasheet/TYPE-C-31-M-12/177331.html?spm=sc.gbn.xds.a___sc.gbn.hd.ss&lcsc_vid=RgMNUVYEQARbV1xTElVcVwIAFFBXVwBfEQdfX1UCRAcxVlNTQFBcUlFXT1hYVTsOAxUeFF5JWA0NAgAHWQIASA%3D%3D")
        (field (name "Description") "USB-C Power C165948"))
      (libsource (lib "TYPE-C-31-M-12") (part "TYPE-C-31-M-12") (description ""))
      (property (name "LCSC") (value "C165948"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "C165948"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "d00fe3b6-1d5f-415a-a4c5-5a4aad471803"))
    (comp (ref "L1")
      (value "SL1040-2R2M")
      (footprint "JLC2KiCad_lib-footprints:IND-SMD_SL1040-R47M")
      (datasheet "https://atta.szlcsc.com/upload/public/pdf/source/20240611/8DE7D6BE1273F2E871C82A6D5C20B08D.pdf")
      (fields
        (field (name "LCSC") "C22463836")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:IND-SMD_SL1040-R47M")
        (field (name "Datasheet") "https://atta.szlcsc.com/upload/public/pdf/source/20240611/8DE7D6BE1273F2E871C82A6D5C20B08D.pdf")
        (field (name "Description")))
      (libsource (lib "SL1040-2R2M") (part "SL1040-2R2M") (description ""))
      (property (name "LCSC") (value "C22463836"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "C22463836"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "167f41e6-7955-4ce1-9c4c-81a3b240f3d7"))
    (comp (ref "R27")
      (value "3.3kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "cd0ffe8b-f9a6-48b6-acd9-a50a5d190c21"))
    (comp (ref "R28")
      (value "3.3kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "LCSC") "C22978")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "LCSC") (value "C22978"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "4d123850-2a3f-4e48-8856-e7d170a708b8"))
    (comp (ref "R29")
      (value "1kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "e2046b71-aa3b-4796-8874-d1b096bfde74"))
    (comp (ref "R30")
      (value "100kΩ")
      (footprint "PCM_JLCPCB:R_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010100_UNI-ROYAL-Uniroyal-Elec-0402WGF1003TCE_C25741.pdf")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 100kΩ 0402 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C25741")
        (field (name "Stock") "6969783")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF1003TCE")
        (field (name "Resistance") "100kΩ")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010100_UNI-ROYAL-Uniroyal-Elec-0402WGF1003TCE_C25741.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 100kΩ 0402 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0402,100kΩ") (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 100kΩ 0402 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C25741"))
      (property (name "Stock") (value "6969783"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0402WGF1003TCE"))
      (property (name "Resistance") (value "100kΩ"))
      (property (name "Power(Watts)") (value "62.5mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "50V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±100ppm/°C"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "5c2260b7-4fcf-4a8d-8658-4b9c34b49021"))
    (comp (ref "R31")
      (value "18kΩ")
      (footprint "PCM_JLCPCB:R_0603")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010045_UNI-ROYAL-Uniroyal-Elec-0603WAF1802T5E_C25810.pdf")
      (description "100mW Thick Film Resistors 75V ±100ppm/°C ±1% 18kΩ 0603 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C25810")
        (field (name "Stock") "574660")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0603WAF1802T5E")
        (field (name "Resistance") "18kΩ")
        (field (name "Power(Watts)") "100mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "75V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0603")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010045_UNI-ROYAL-Uniroyal-Elec-0603WAF1802T5E_C25810.pdf")
        (field (name "Description") "100mW Thick Film Resistors 75V ±100ppm/°C ±1% 18kΩ 0603 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0603,18kΩ") (description "100mW Thick Film Resistors 75V ±100ppm/°C ±1% 18kΩ 0603 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C25810"))
      (property (name "Stock") (value "574660"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0603WAF1802T5E"))
      (property (name "Resistance") (value "18kΩ"))
      (property (name "Power(Watts)") (value "100mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "75V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±100ppm/°C"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "4a7830e6-10c1-403b-ae48-959667f701c6"))
    (comp (ref "R32")
      (value "10Ω")
      (footprint "PCM_JLCPCB:R_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2411221126_UNI-ROYAL-Uniroyal-Elec-0402WGF100JTCE_C25077.pdf")
      (description "62.5mW Thick Film Resistors 50V ±1% ±200ppm/°C 10Ω 0402 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C25077")
        (field (name "Stock") "4873481")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF100JTCE")
        (field (name "Resistance") "10Ω")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±200ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2411221126_UNI-ROYAL-Uniroyal-Elec-0402WGF100JTCE_C25077.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±1% ±200ppm/°C 10Ω 0402 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0402,10Ω") (description "62.5mW Thick Film Resistors 50V ±1% ±200ppm/°C 10Ω 0402 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C25077"))
      (property (name "Stock") (value "4873481"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0402WGF100JTCE"))
      (property (name "Resistance") (value "10Ω"))
      (property (name "Power(Watts)") (value "62.5mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "50V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±200ppm/°C"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "8d584352-3510-4b24-9048-9fbd1d85a987"))
    (comp (ref "R33")
      (value "510Ω")
      (footprint "PCM_JLCPCB:R_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF5100TCE_C25123.pdf")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 510Ω 0402 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C25123")
        (field (name "Stock") "2434473")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "12")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF5100TCE")
        (field (name "Resistance") "510Ω")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF5100TCE_C25123.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 510Ω 0402 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0402,510Ω") (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 510Ω 0402 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C25123"))
      (property (name "Stock") (value "2434473"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "12"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0402WGF5100TCE"))
      (property (name "Resistance") (value "510Ω"))
      (property (name "Power(Watts)") (value "62.5mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "50V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±100ppm/°C"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "388c0a69-40e6-408e-b558-59bb7a55cc83"))
    (comp (ref "R34")
      (value "200kΩ")
      (footprint "PCM_JLCPCB:R_0603")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010045_UNI-ROYAL-Uniroyal-Elec-0603WAF2003T5E_C25811.pdf")
      (description "100mW Thick Film Resistors 75V ±100ppm/°C ±1% 200kΩ 0603 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C25811")
        (field (name "Stock") "1426208")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0603WAF2003T5E")
        (field (name "Resistance") "200kΩ")
        (field (name "Power(Watts)") "100mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "75V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0603")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010045_UNI-ROYAL-Uniroyal-Elec-0603WAF2003T5E_C25811.pdf")
        (field (name "Description") "100mW Thick Film Resistors 75V ±100ppm/°C ±1% 200kΩ 0603 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0603,200kΩ") (description "100mW Thick Film Resistors 75V ±100ppm/°C ±1% 200kΩ 0603 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C25811"))
      (property (name "Stock") (value "1426208"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0603WAF2003T5E"))
      (property (name "Resistance") (value "200kΩ"))
      (property (name "Power(Watts)") (value "100mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "75V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±100ppm/°C"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "aa8cb6b9-b6db-462e-9782-82fe90959cb0"))
    (comp (ref "R35")
      (value "27kΩ")
      (footprint "PCM_JLCPCB:R_0603")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010130_UNI-ROYAL-Uniroyal-Elec-0603WAF2702T5E_C22967.pdf")
      (description "100mW Thick Film Resistors 75V ±100ppm/°C ±1% 27kΩ 0603 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C22967")
        (field (name "Stock") "708507")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0603WAF2702T5E")
        (field (name "Resistance") "27kΩ")
        (field (name "Power(Watts)") "100mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "75V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0603")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010130_UNI-ROYAL-Uniroyal-Elec-0603WAF2702T5E_C22967.pdf")
        (field (name "Description") "100mW Thick Film Resistors 75V ±100ppm/°C ±1% 27kΩ 0603 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0603,27kΩ") (description "100mW Thick Film Resistors 75V ±100ppm/°C ±1% 27kΩ 0603 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C22967"))
      (property (name "Stock") (value "708507"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0603WAF2702T5E"))
      (property (name "Resistance") (value "27kΩ"))
      (property (name "Power(Watts)") (value "100mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "75V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±100ppm/°C"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "ed5ce352-bf7e-4d1c-858b-2674fd5586dd"))
    (comp (ref "SW3")
      (value "SW_MAIN_POWER")
      (footprint "JLC2KiCad_lib-footprints:SW-TH_PS-22E05")
      (datasheet "https://atta.szlcsc.com/upload/public/pdf/source/20210825/03FED21E2D4F2980BA08F4ED04C13B40.pdf")
      (fields
        (field (name "LCSC") "C19190928")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:SW-TH_PS-22E05")
        (field (name "Datasheet") "https://atta.szlcsc.com/upload/public/pdf/source/20210825/03FED21E2D4F2980BA08F4ED04C13B40.pdf")
        (field (name "Description")))
      (libsource (lib "PS-22E05-S-O-001") (part "PS-22E05-S-O-001") (description ""))
      (property (name "LCSC") (value "C19190928"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "C19190928"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "ad778893-c1fb-4dad-8d17-c591559144e4"))
    (comp (ref "U10")
      (value "AP2112K-3.3 DIGITAL PSU LDO")
      (footprint "JLC2KiCad_lib-footprints:SOT-23-5_L2.9-W1.6-P0.95-LS2.8-BR")
      (datasheet "https://www.diodes.com/assets/Datasheets/AP2112.pdf")
      (description "600mA low dropout linear regulator, with enable pin, 3.8V-6V input voltage range, 3.3V fixed positive output, SOT-23-5")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:SOT-23-5_L2.9-W1.6-P0.95-LS2.8-BR")
        (field (name "Datasheet") "https://www.diodes.com/assets/Datasheets/AP2112.pdf")
        (field (name "Description") "600mA low dropout linear regulator, with enable pin, 3.8V-6V input voltage range, 3.3V fixed positive output, SOT-23-5"))
      (libsource (lib "Regulator_Linear") (part "AP2112K-3.3") (description "600mA low dropout linear regulator, with enable pin, 3.8V-6V input voltage range, 3.3V fixed positive output, SOT-23-5"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "linear regulator ldo fixed positive"))
      (property (name "ki_fp_filters") (value "SOT?23?5*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "297d4d38-3986-4bca-b131-1d4a2b954165"))
    (comp (ref "U11")
      (value "AP2112K-3.3 ANALOG AUDIO LDO")
      (footprint "JLC2KiCad_lib-footprints:SOT-23-5_L2.9-W1.6-P0.95-LS2.8-BR")
      (datasheet "https://www.diodes.com/assets/Datasheets/AP2112.pdf")
      (description "clean analog, for PCM5242 analog section only -- 600mA low dropout linear regulator, with enable pin, 3.8V-6V input voltage range, 3.3V fixed positive output, SOT-23-5")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:SOT-23-5_L2.9-W1.6-P0.95-LS2.8-BR")
        (field (name "Datasheet") "https://www.diodes.com/assets/Datasheets/AP2112.pdf")
        (field (name "Description") "clean analog, for PCM5242 analog section only -- 600mA low dropout linear regulator, with enable pin, 3.8V-6V input voltage range, 3.3V fixed positive output, SOT-23-5"))
      (libsource (lib "Regulator_Linear") (part "AP2112K-3.3") (description "600mA low dropout linear regulator, with enable pin, 3.8V-6V input voltage range, 3.3V fixed positive output, SOT-23-5"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "linear regulator ldo fixed positive"))
      (property (name "ki_fp_filters") (value "SOT?23?5*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "e85fefb2-4c9b-413a-9140-54d0ffc66788"))
    (comp (ref "U12")
      (value "CH224K")
      (footprint "JLC2KiCad_lib-footprints:ESSOP-10_L4.9-W3.9-P1.0-LS6.0-TL-EP")
      (datasheet "https://www.wch.cn/downloads/file/301.html")
      (description "100W USB Type-C PD3.0/2.0, BC1.2 Sink Controller, SSOP-10")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:ESSOP-10_L4.9-W3.9-P1.0-LS6.0-TL-EP")
        (field (name "Datasheet") "https://www.wch.cn/downloads/file/301.html")
        (field (name "Description") "100W USB Type-C PD3.0/2.0, BC1.2 Sink Controller, SSOP-10"))
      (libsource (lib "Interface_USB") (part "CH224K") (description "100W USB Type-C PD3.0/2.0, BC1.2 Sink Controller, SSOP-10"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "USB-C WCH powered-device"))
      (property (name "ki_fp_filters") (value "SSOP*3.9x4.9mm*P1mm*EP2.1x3.3mm*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "d4cab4f1-520c-4755-b9d4-abd2cd18705b"))
    (comp (ref "U13")
      (value "SY8368AQQC")
      (footprint "JLC2KiCad_lib-footprints:QFN-12_L3.0-W3.0-P0.45-TL-EP")
      (datasheet "https://atta.szlcsc.com/upload/public/pdf/source/20180224/C178253_15194367790221363788.pdf")
      (fields
        (field (name "LCSC") "C207642")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:QFN-12_L3.0-W3.0-P0.45-TL-EP")
        (field (name "Datasheet") "https://atta.szlcsc.com/upload/public/pdf/source/20180224/C178253_15194367790221363788.pdf")
        (field (name "Description")))
      (libsource (lib "SY8368AQQC") (part "SY8368AQQC") (description ""))
      (property (name "LCSC") (value "C207642"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "C207642"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "ad0dd509-8300-48a3-9905-1b707b086243"))
    (comp (ref "C49")
      (value "15pF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "0a98cc2a-2f3d-477e-858b-9056b4fff403"))
    (comp (ref "C50")
      (value "15pF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "a397d297-62d5-4c44-9d38-68510deb7179"))
    (comp (ref "C51")
      (value "100nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "7d6b3185-27bd-45c4-9bb8-ec34f3d1a8c6"))
    (comp (ref "C52")
      (value "10nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, a trick to reduce ADC noise further. Not massively useful but 0.1 cents addition")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, a trick to reduce ADC noise further. Not massively useful but 0.1 cents addition"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "869a6ff0-2778-49c4-a7d2-469b592af6f1"))
    (comp (ref "C53")
      (value "100nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "567e92ac-416d-4662-a5cf-7d3b393490bd"))
    (comp (ref "C54")
      (value "1uF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "980bc064-5e1e-4f0d-9ec7-dbae45398075"))
    (comp (ref "C55")
      (value "1uF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "b26b00f8-47d3-4d14-a4dc-caf61af2b366"))
    (comp (ref "C56")
      (value "100nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "e817a6f3-7c4e-420b-a318-deadfe3abe38"))
    (comp (ref "C57")
      (value "100nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "f016868c-76f1-4e20-9fb1-468a42b6e24f"))
    (comp (ref "C58")
      (value "22nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "cae2631b-631a-4ca4-a33a-12f65aa24d88"))
    (comp (ref "C61")
      (value "100nF")
      (footprint "PCM_JLCPCB:C_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05B104KB54PNC_C307331.pdf")
      (description "50V 100nF X7R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
      (fields
        (field (name "LCSC") "C307331")
        (field (name "Stock") "8389599")
        (field (name "Price") "0.008USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT")
        (field (name "Manufacturer") "Samsung Electro-Mechanics")
        (field (name "Part") "CL05B104KB54PNC")
        (field (name "Voltage Rated") "50V")
        (field (name "Tolerance") "±10%")
        (field (name "Capacitance") "100nF")
        (field (name "Temperature Coefficient") "X7R")
        (field (name "Footprint") "PCM_JLCPCB:C_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05B104KB54PNC_C307331.pdf")
        (field (name "Description") "50V 100nF X7R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (libsource (lib "PCM_JLCPCB-Capacitors") (part "0402,100nF,(2)") (description "50V 100nF X7R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (property (name "LCSC") (value "C307331"))
      (property (name "Stock") (value "8389599"))
      (property (name "Price") (value "0.008USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT"))
      (property (name "Manufacturer") (value "Samsung Electro-Mechanics"))
      (property (name "Part") (value "CL05B104KB54PNC"))
      (property (name "Voltage Rated") (value "50V"))
      (property (name "Tolerance") (value "±10%"))
      (property (name "Capacitance") (value "100nF"))
      (property (name "Temperature Coefficient") (value "X7R"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "5b89257e-a2b5-4599-997c-fade112e4f32"))
    (comp (ref "C62")
      (value "100nF")
      (footprint "PCM_JLCPCB:C_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05B104KB54PNC_C307331.pdf")
      (description "50V 100nF X7R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
      (fields
        (field (name "LCSC") "C307331")
        (field (name "Stock") "8389599")
        (field (name "Price") "0.008USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT")
        (field (name "Manufacturer") "Samsung Electro-Mechanics")
        (field (name "Part") "CL05B104KB54PNC")
        (field (name "Voltage Rated") "50V")
        (field (name "Tolerance") "±10%")
        (field (name "Capacitance") "100nF")
        (field (name "Temperature Coefficient") "X7R")
        (field (name "Footprint") "PCM_JLCPCB:C_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05B104KB54PNC_C307331.pdf")
        (field (name "Description") "50V 100nF X7R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (libsource (lib "PCM_JLCPCB-Capacitors") (part "0402,100nF,(2)") (description "50V 100nF X7R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (property (name "LCSC") (value "C307331"))
      (property (name "Stock") (value "8389599"))
      (property (name "Price") (value "0.008USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT"))
      (property (name "Manufacturer") (value "Samsung Electro-Mechanics"))
      (property (name "Part") (value "CL05B104KB54PNC"))
      (property (name "Voltage Rated") (value "50V"))
      (property (name "Tolerance") (value "±10%"))
      (property (name "Capacitance") (value "100nF"))
      (property (name "Temperature Coefficient") (value "X7R"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "6f53bb50-da42-490e-9d63-10e6b4d95913"))
    (comp (ref "C63")
      (value "100nF")
      (footprint "PCM_JLCPCB:C_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05B104KB54PNC_C307331.pdf")
      (description "50V 100nF X7R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
      (fields
        (field (name "LCSC") "C307331")
        (field (name "Stock") "8389599")
        (field (name "Price") "0.008USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT")
        (field (name "Manufacturer") "Samsung Electro-Mechanics")
        (field (name "Part") "CL05B104KB54PNC")
        (field (name "Voltage Rated") "50V")
        (field (name "Tolerance") "±10%")
        (field (name "Capacitance") "100nF")
        (field (name "Temperature Coefficient") "X7R")
        (field (name "Footprint") "PCM_JLCPCB:C_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05B104KB54PNC_C307331.pdf")
        (field (name "Description") "50V 100nF X7R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (libsource (lib "PCM_JLCPCB-Capacitors") (part "0402,100nF,(2)") (description "50V 100nF X7R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (property (name "LCSC") (value "C307331"))
      (property (name "Stock") (value "8389599"))
      (property (name "Price") (value "0.008USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT"))
      (property (name "Manufacturer") (value "Samsung Electro-Mechanics"))
      (property (name "Part") (value "CL05B104KB54PNC"))
      (property (name "Voltage Rated") (value "50V"))
      (property (name "Tolerance") (value "±10%"))
      (property (name "Capacitance") (value "100nF"))
      (property (name "Temperature Coefficient") (value "X7R"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "2fdd5823-911e-40ff-bfc4-cb9b2b205d40"))
    (comp (ref "J16")
      (value "J_JOGWHEEL")
      (footprint "Connector_JST:JST_PH_B5B-PH-K_1x05_P2.00mm_Vertical")
      (datasheet "~")
      (description "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (fields
        (field (name "Footprint") "Connector_JST:JST_PH_B5B-PH-K_1x05_P2.00mm_Vertical")
        (field (name "Datasheet") "~")
        (field (name "Description") "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (libsource (lib "Connector_Generic") (part "Conn_01x05") (description "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "connector"))
      (property (name "ki_fp_filters") (value "Connector*:*_1x??_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "7cadb305-af68-4b94-9b28-7bd1b523b340"))
    (comp (ref "J17")
      (value "J_HOTCUES")
      (footprint "Connector_JST:JST_PH_B8B-PH-K_1x08_P2.00mm_Vertical")
      (datasheet "~")
      (description "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (fields
        (field (name "Footprint") "Connector_JST:JST_PH_B8B-PH-K_1x08_P2.00mm_Vertical")
        (field (name "Datasheet") "~")
        (field (name "Description") "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (libsource (lib "Connector_Generic") (part "Conn_01x08") (description "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "connector"))
      (property (name "ki_fp_filters") (value "Connector*:*_1x??_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "413eb8b1-3541-4044-b3e7-9dc08377ff42"))
    (comp (ref "J18")
      (value "J_LEFT_CTRLS")
      (footprint "Connector_JST:JST_PH_B10B-PH-K_1x10_P2.00mm_Vertical")
      (datasheet "~")
      (description "Generic connector, single row, 01x10, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (fields
        (field (name "Footprint") "Connector_JST:JST_PH_B10B-PH-K_1x10_P2.00mm_Vertical")
        (field (name "Datasheet") "~")
        (field (name "Description") "Generic connector, single row, 01x10, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (libsource (lib "Connector_Generic") (part "Conn_01x10") (description "Generic connector, single row, 01x10, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "connector"))
      (property (name "ki_fp_filters") (value "Connector*:*_1x??_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "6cf6eac8-1cb7-49f6-b263-efc956cf518c"))
    (comp (ref "J19")
      (value "J_RIGHT_CTRLS")
      (footprint "Connector_JST:JST_PH_B12B-PH-K_1x12_P2.00mm_Vertical")
      (datasheet "~")
      (description "Generic connector, single row, 01x12, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (fields
        (field (name "Footprint") "Connector_JST:JST_PH_B12B-PH-K_1x12_P2.00mm_Vertical")
        (field (name "Datasheet") "~")
        (field (name "Description") "Generic connector, single row, 01x12, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (libsource (lib "Connector_Generic") (part "Conn_01x12") (description "Generic connector, single row, 01x12, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "connector"))
      (property (name "ki_fp_filters") (value "Connector*:*_1x??_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "f1579707-df32-40d2-aaf9-14ec5434fcfb"))
    (comp (ref "J20")
      (value "J_TOP_LEFT")
      (footprint "Connector_JST:JST_PH_B10B-PH-K_1x10_P2.00mm_Vertical")
      (datasheet "~")
      (description "Generic connector, single row, 01x10, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (fields
        (field (name "Footprint") "Connector_JST:JST_PH_B10B-PH-K_1x10_P2.00mm_Vertical")
        (field (name "Datasheet") "~")
        (field (name "Description") "Generic connector, single row, 01x10, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (libsource (lib "Connector_Generic") (part "Conn_01x10") (description "Generic connector, single row, 01x10, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "connector"))
      (property (name "ki_fp_filters") (value "Connector*:*_1x??_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "59a3dbc1-2522-4174-bab0-bd9a80e55fe1"))
    (comp (ref "J21")
      (value "J_TOP_RIGHT")
      (footprint "Connector_JST:JST_PH_B8B-PH-K_1x08_P2.00mm_Vertical")
      (datasheet "~")
      (description "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (fields
        (field (name "Footprint") "Connector_JST:JST_PH_B8B-PH-K_1x08_P2.00mm_Vertical")
        (field (name "Datasheet") "~")
        (field (name "Description") "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (libsource (lib "Connector_Generic") (part "Conn_01x08") (description "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "connector"))
      (property (name "ki_fp_filters") (value "Connector*:*_1x??_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "418900b3-8e8b-477b-acc1-47306f9ad027"))
    (comp (ref "R36")
      (value "10kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "d530e05f-1d28-4927-849c-921096553a85"))
    (comp (ref "R37")
      (value "22kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor pull up")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor pull up"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "a85aa449-029f-4c47-9326-1c2ea337825a"))
    (comp (ref "R41")
      (value "10kΩ")
      (footprint "PCM_JLCPCB:R_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2411221126_UNI-ROYAL-Uniroyal-Elec-0402WGF1002TCE_C25744.pdf")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 10kΩ 0402 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C25744")
        (field (name "Stock") "24372091")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF1002TCE")
        (field (name "Resistance") "10kΩ")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2411221126_UNI-ROYAL-Uniroyal-Elec-0402WGF1002TCE_C25744.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 10kΩ 0402 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0402,10kΩ") (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 10kΩ 0402 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C25744"))
      (property (name "Stock") (value "24372091"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0402WGF1002TCE"))
      (property (name "Resistance") (value "10kΩ"))
      (property (name "Power(Watts)") (value "62.5mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "50V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±100ppm/°C"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "3a208929-d73d-44db-a537-c33272aa17fe"))
    (comp (ref "R52")
      (value "10kΩ")
      (footprint "PCM_JLCPCB:R_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2411221126_UNI-ROYAL-Uniroyal-Elec-0402WGF1002TCE_C25744.pdf")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 10kΩ 0402 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C25744")
        (field (name "Stock") "24372091")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF1002TCE")
        (field (name "Resistance") "10kΩ")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2411221126_UNI-ROYAL-Uniroyal-Elec-0402WGF1002TCE_C25744.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 10kΩ 0402 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0402,10kΩ") (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 10kΩ 0402 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C25744"))
      (property (name "Stock") (value "24372091"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0402WGF1002TCE"))
      (property (name "Resistance") (value "10kΩ"))
      (property (name "Power(Watts)") (value "62.5mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "50V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±100ppm/°C"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "4dfbc347-769c-4dc9-8362-964f85ab7c29"))
    (comp (ref "R53")
      (value "4.7kΩ")
      (footprint "PCM_JLCPCB:R_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010045_UNI-ROYAL-Uniroyal-Elec-0402WGF4701TCE_C25900.pdf")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 4.7kΩ 0402 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C25900")
        (field (name "Stock") "7644059")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF4701TCE")
        (field (name "Resistance") "4.7kΩ")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010045_UNI-ROYAL-Uniroyal-Elec-0402WGF4701TCE_C25900.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 4.7kΩ 0402 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0402,4.7kΩ") (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 4.7kΩ 0402 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C25900"))
      (property (name "Stock") (value "7644059"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0402WGF4701TCE"))
      (property (name "Resistance") (value "4.7kΩ"))
      (property (name "Power(Watts)") (value "62.5mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "50V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±100ppm/°C"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "59fc6875-ab45-4617-9d77-ddcdf1fd395e"))
    (comp (ref "R54")
      (value "4.7kΩ")
      (footprint "PCM_JLCPCB:R_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010045_UNI-ROYAL-Uniroyal-Elec-0402WGF4701TCE_C25900.pdf")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 4.7kΩ 0402 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C25900")
        (field (name "Stock") "7644059")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF4701TCE")
        (field (name "Resistance") "4.7kΩ")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010045_UNI-ROYAL-Uniroyal-Elec-0402WGF4701TCE_C25900.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 4.7kΩ 0402 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0402,4.7kΩ") (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 4.7kΩ 0402 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C25900"))
      (property (name "Stock") (value "7644059"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0402WGF4701TCE"))
      (property (name "Resistance") (value "4.7kΩ"))
      (property (name "Power(Watts)") (value "62.5mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "50V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±100ppm/°C"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "b594d692-f1f9-4569-bcd0-090a22f59d6b"))
    (comp (ref "R55")
      (value "10kΩ")
      (footprint "PCM_JLCPCB:R_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2411221126_UNI-ROYAL-Uniroyal-Elec-0402WGF1002TCE_C25744.pdf")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 10kΩ 0402 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C25744")
        (field (name "Stock") "24372091")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF1002TCE")
        (field (name "Resistance") "10kΩ")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2411221126_UNI-ROYAL-Uniroyal-Elec-0402WGF1002TCE_C25744.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 10kΩ 0402 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0402,10kΩ") (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 10kΩ 0402 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C25744"))
      (property (name "Stock") (value "24372091"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0402WGF1002TCE"))
      (property (name "Resistance") (value "10kΩ"))
      (property (name "Power(Watts)") (value "62.5mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "50V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±100ppm/°C"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "fc890b0d-7b61-45a9-a42f-79ef907251b3"))
    (comp (ref "R56")
      (value "330Ω")
      (footprint "PCM_JLCPCB:R_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF3300TCE_C25104.pdf")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C25104")
        (field (name "Stock") "1159127")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF3300TCE")
        (field (name "Resistance") "330Ω")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF3300TCE_C25104.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0402,330Ω") (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C25104"))
      (property (name "Stock") (value "1159127"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0402WGF3300TCE"))
      (property (name "Resistance") (value "330Ω"))
      (property (name "Power(Watts)") (value "62.5mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "50V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±100ppm/°C"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "5c638ea1-a626-4b17-8339-0113ed7c27f4"))
    (comp (ref "R57")
      (value "330Ω")
      (footprint "PCM_JLCPCB:R_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF3300TCE_C25104.pdf")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C25104")
        (field (name "Stock") "1159127")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF3300TCE")
        (field (name "Resistance") "330Ω")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF3300TCE_C25104.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0402,330Ω") (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C25104"))
      (property (name "Stock") (value "1159127"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0402WGF3300TCE"))
      (property (name "Resistance") (value "330Ω"))
      (property (name "Power(Watts)") (value "62.5mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "50V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±100ppm/°C"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "39262d57-533d-4924-bdb7-648bb2201939"))
    (comp (ref "R58")
      (value "330Ω")
      (footprint "PCM_JLCPCB:R_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF3300TCE_C25104.pdf")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C25104")
        (field (name "Stock") "1159127")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF3300TCE")
        (field (name "Resistance") "330Ω")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF3300TCE_C25104.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0402,330Ω") (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C25104"))
      (property (name "Stock") (value "1159127"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0402WGF3300TCE"))
      (property (name "Resistance") (value "330Ω"))
      (property (name "Power(Watts)") (value "62.5mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "50V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±100ppm/°C"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "03dbbadc-1d1b-4f69-b308-c7c86d85947d"))
    (comp (ref "R59")
      (value "330Ω")
      (footprint "PCM_JLCPCB:R_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF3300TCE_C25104.pdf")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C25104")
        (field (name "Stock") "1159127")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF3300TCE")
        (field (name "Resistance") "330Ω")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF3300TCE_C25104.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0402,330Ω") (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C25104"))
      (property (name "Stock") (value "1159127"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0402WGF3300TCE"))
      (property (name "Resistance") (value "330Ω"))
      (property (name "Power(Watts)") (value "62.5mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "50V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±100ppm/°C"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "40ad3fb4-ceb9-40fd-b79b-b704579284a1"))
    (comp (ref "R60")
      (value "330Ω")
      (footprint "PCM_JLCPCB:R_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF3300TCE_C25104.pdf")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C25104")
        (field (name "Stock") "1159127")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF3300TCE")
        (field (name "Resistance") "330Ω")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF3300TCE_C25104.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0402,330Ω") (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C25104"))
      (property (name "Stock") (value "1159127"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0402WGF3300TCE"))
      (property (name "Resistance") (value "330Ω"))
      (property (name "Power(Watts)") (value "62.5mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "50V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±100ppm/°C"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "bdcae60f-a53b-4bed-a5f8-6eaf715bec8f"))
    (comp (ref "R61")
      (value "330Ω")
      (footprint "PCM_JLCPCB:R_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF3300TCE_C25104.pdf")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C25104")
        (field (name "Stock") "1159127")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF3300TCE")
        (field (name "Resistance") "330Ω")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF3300TCE_C25104.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0402,330Ω") (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C25104"))
      (property (name "Stock") (value "1159127"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0402WGF3300TCE"))
      (property (name "Resistance") (value "330Ω"))
      (property (name "Power(Watts)") (value "62.5mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "50V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±100ppm/°C"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "e6690af1-e203-4bd8-9ade-2da23b5de33e"))
    (comp (ref "R62")
      (value "330Ω")
      (footprint "PCM_JLCPCB:R_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF3300TCE_C25104.pdf")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C25104")
        (field (name "Stock") "1159127")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF3300TCE")
        (field (name "Resistance") "330Ω")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF3300TCE_C25104.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0402,330Ω") (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C25104"))
      (property (name "Stock") (value "1159127"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0402WGF3300TCE"))
      (property (name "Resistance") (value "330Ω"))
      (property (name "Power(Watts)") (value "62.5mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "50V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±100ppm/°C"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "8f4bbfde-6a21-4a26-8218-dd874786aa59"))
    (comp (ref "R63")
      (value "330Ω")
      (footprint "PCM_JLCPCB:R_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF3300TCE_C25104.pdf")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C25104")
        (field (name "Stock") "1159127")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF3300TCE")
        (field (name "Resistance") "330Ω")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF3300TCE_C25104.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0402,330Ω") (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C25104"))
      (property (name "Stock") (value "1159127"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0402WGF3300TCE"))
      (property (name "Resistance") (value "330Ω"))
      (property (name "Power(Watts)") (value "62.5mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "50V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±100ppm/°C"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "51f476cb-7c03-451d-98d9-fd83b4d99256"))
    (comp (ref "R64")
      (value "330Ω")
      (footprint "PCM_JLCPCB:R_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF3300TCE_C25104.pdf")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C25104")
        (field (name "Stock") "1159127")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF3300TCE")
        (field (name "Resistance") "330Ω")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF3300TCE_C25104.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0402,330Ω") (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C25104"))
      (property (name "Stock") (value "1159127"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0402WGF3300TCE"))
      (property (name "Resistance") (value "330Ω"))
      (property (name "Power(Watts)") (value "62.5mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "50V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±100ppm/°C"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "afc25615-125c-4aed-a31f-2239b81d2515"))
    (comp (ref "R65")
      (value "330Ω")
      (footprint "PCM_JLCPCB:R_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF3300TCE_C25104.pdf")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C25104")
        (field (name "Stock") "1159127")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF3300TCE")
        (field (name "Resistance") "330Ω")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF3300TCE_C25104.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0402,330Ω") (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C25104"))
      (property (name "Stock") (value "1159127"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0402WGF3300TCE"))
      (property (name "Resistance") (value "330Ω"))
      (property (name "Power(Watts)") (value "62.5mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "50V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±100ppm/°C"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "f8862ab9-6376-4955-b982-89f71970cb4b"))
    (comp (ref "R66")
      (value "330Ω")
      (footprint "PCM_JLCPCB:R_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF3300TCE_C25104.pdf")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C25104")
        (field (name "Stock") "1159127")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF3300TCE")
        (field (name "Resistance") "330Ω")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF3300TCE_C25104.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0402,330Ω") (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C25104"))
      (property (name "Stock") (value "1159127"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0402WGF3300TCE"))
      (property (name "Resistance") (value "330Ω"))
      (property (name "Power(Watts)") (value "62.5mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "50V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±100ppm/°C"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "f1f1c958-d0b8-4da4-ac0d-e85ae0d7cee8"))
    (comp (ref "R67")
      (value "330Ω")
      (footprint "PCM_JLCPCB:R_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF3300TCE_C25104.pdf")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C25104")
        (field (name "Stock") "1159127")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF3300TCE")
        (field (name "Resistance") "330Ω")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF3300TCE_C25104.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0402,330Ω") (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C25104"))
      (property (name "Stock") (value "1159127"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0402WGF3300TCE"))
      (property (name "Resistance") (value "330Ω"))
      (property (name "Power(Watts)") (value "62.5mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "50V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±100ppm/°C"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "f94cea44-43dd-42d1-8882-92ad75ce9208"))
    (comp (ref "R68")
      (value "330Ω")
      (footprint "PCM_JLCPCB:R_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF3300TCE_C25104.pdf")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C25104")
        (field (name "Stock") "1159127")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF3300TCE")
        (field (name "Resistance") "330Ω")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF3300TCE_C25104.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0402,330Ω") (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C25104"))
      (property (name "Stock") (value "1159127"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0402WGF3300TCE"))
      (property (name "Resistance") (value "330Ω"))
      (property (name "Power(Watts)") (value "62.5mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "50V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±100ppm/°C"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "d91df0ab-a638-45c6-9799-eff65fc1f574"))
    (comp (ref "SW4")
      (value "RESET_BTN")
      (footprint "PCM_JLCPCB:SW_TS-1088-AR02016")
      (datasheet "~")
      (description "Push button switch, generic, two pins")
      (fields
        (field (name "Footprint") "PCM_JLCPCB:SW_TS-1088-AR02016")
        (field (name "Datasheet") "~")
        (field (name "Description") "Push button switch, generic, two pins"))
      (libsource (lib "Switch") (part "SW_Push") (description "Push button switch, generic, two pins"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "switch normally-open pushbutton push-button"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "c28e212b-0b2e-4b16-8343-2d0b8792eb69"))
    (comp (ref "TP12")
      (value "PF7")
      (footprint "TestPoint:TestPoint_Pad_2.0x2.0mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Footprint") "TestPoint:TestPoint_Pad_2.0x2.0mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "00d128ce-6aa0-4b0e-be34-0943da7ff95f"))
    (comp (ref "TP13")
      (value "PF6")
      (footprint "TestPoint:TestPoint_Pad_2.0x2.0mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Footprint") "TestPoint:TestPoint_Pad_2.0x2.0mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "8645f3ac-8e28-42e5-8384-cd2c35deb4dd"))
    (comp (ref "TP14")
      (value "PF5")
      (footprint "TestPoint:TestPoint_Pad_2.0x2.0mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Footprint") "TestPoint:TestPoint_Pad_2.0x2.0mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "de4f1ee8-c373-4aaa-abb8-ebcb9f9fe13f"))
    (comp (ref "TP15")
      (value "PF4")
      (footprint "TestPoint:TestPoint_Pad_2.0x2.0mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Footprint") "TestPoint:TestPoint_Pad_2.0x2.0mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "193a1e08-51ea-4d10-9ba5-c19d1d106199"))
    (comp (ref "TP16")
      (value "PF1")
      (footprint "TestPoint:TestPoint_Pad_2.0x2.0mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Footprint") "TestPoint:TestPoint_Pad_2.0x2.0mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "9f1ea6a8-7970-4850-a547-070b2c43a75f"))
    (comp (ref "TP18")
      (value "PC7")
      (footprint "TestPoint:TestPoint_Pad_2.0x2.0mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Footprint") "TestPoint:TestPoint_Pad_2.0x2.0mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "5e9f6541-523c-42e3-89bf-7f602c3e4093"))
    (comp (ref "TP24")
      (value "I2C_SDA_ARDUINO")
      (footprint "TestPoint:TestPoint_Pad_1.5x1.5mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Footprint") "TestPoint:TestPoint_Pad_1.5x1.5mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "df4c1f7d-9c02-42e4-93d7-e311077d80e6"))
    (comp (ref "TP25")
      (value "I2C_SCL_ARDUINO")
      (footprint "TestPoint:TestPoint_Pad_1.5x1.5mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Footprint") "TestPoint:TestPoint_Pad_1.5x1.5mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "15c56689-972b-4837-b7d8-10411990ef89"))
    (comp (ref "U14")
      (value "ATmega32U4-A (Arduino MIDI controller)")
      (footprint "JLC2KiCad_lib-footprints:VQFN-44_L7.0-W7.0-P0.50-BL-EP5.2")
      (datasheet "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-7766-8-bit-AVR-ATmega16U4-32U4_Datasheet.pdf")
      (description "16MHz, 32kB Flash, 2.5kB SRAM, 1kB EEPROM, USB 2.0, TQFP-44")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:VQFN-44_L7.0-W7.0-P0.50-BL-EP5.2")
        (field (name "Datasheet") "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-7766-8-bit-AVR-ATmega16U4-32U4_Datasheet.pdf")
        (field (name "Description") "16MHz, 32kB Flash, 2.5kB SRAM, 1kB EEPROM, USB 2.0, TQFP-44"))
      (libsource (lib "MCU_Microchip_ATmega") (part "ATmega32U4-A") (description "16MHz, 32kB Flash, 2.5kB SRAM, 1kB EEPROM, USB 2.0, TQFP-44"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "AVR 8bit Microcontroller MegaAVR USB"))
      (property (name "ki_fp_filters") (value "TQFP*10x10mm*P0.8mm*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "776493bf-cc4f-41f2-8e7a-632ad96677db"))
    (comp (ref "U16")
      (value "74HC4067PW,118")
      (footprint "JLC2KiCad_lib-footprints:TSSOP-28_L9.8-W6.6-P0.65-BL")
      (datasheet "https://item.szlcsc.com/6601.html")
      (fields
        (field (name "LCSC") "C179326")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:TSSOP-28_L9.8-W6.6-P0.65-BL")
        (field (name "Datasheet") "https://item.szlcsc.com/6601.html")
        (field (name "Description")))
      (libsource (lib "74HC4067PW,118") (part "74HC4067PW,118") (description ""))
      (property (name "LCSC") (value "C179326"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "C179326"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "036597f5-b576-4627-a6a3-2e425506ccfc"))
    (comp (ref "U18")
      (value "MCP23017T-E/SS")
      (footprint "JLC2KiCad_lib-footprints:SSOP-28_L10.2-W5.3-P0.65-LS7.8-BL")
      (datasheet "https://item.szlcsc.com/397275.html")
      (description "MCP1_BTNS")
      (fields
        (field (name "LCSC") "C558584")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:SSOP-28_L10.2-W5.3-P0.65-LS7.8-BL")
        (field (name "Datasheet") "https://item.szlcsc.com/397275.html")
        (field (name "Description") "MCP1_BTNS"))
      (libsource (lib "MCP23017T-E/SS") (part "MCP23017T-E/SS") (description ""))
      (property (name "LCSC") (value "C558584"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "C558584"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "d0a9b269-23c1-49cf-bf36-790ead9d69a2"))
    (comp (ref "U19")
      (value "MCP23017T-E/SS")
      (footprint "JLC2KiCad_lib-footprints:SSOP-28_L10.2-W5.3-P0.65-LS7.8-BL")
      (datasheet "https://item.szlcsc.com/397275.html")
      (description "MCP2_LEDS")
      (fields
        (field (name "LCSC") "C558584")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:SSOP-28_L10.2-W5.3-P0.65-LS7.8-BL")
        (field (name "Datasheet") "https://item.szlcsc.com/397275.html")
        (field (name "Description") "MCP2_LEDS"))
      (libsource (lib "MCP23017T-E/SS") (part "MCP23017T-E/SS") (description ""))
      (property (name "LCSC") (value "C558584"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "C558584"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "d1229cf1-7a42-4bbb-84ae-c0d7de4d0808"))
    (comp (ref "X1")
      (value "X322516MLB4SI")
      (footprint "PCM_JLCPCB:OSC-SMD_4P-L3.2-W2.5-BL")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2403291504_YXC-Crystal-Oscillators-X322516MLB4SI_C13738.pdf")
      (description "16MHz Surface Mount Crystal 9pF ±10ppm ±20ppm SMD3225-4P Crystals ROHS")
      (fields
        (field (name "LCSC") "C13738")
        (field (name "Stock") "162087")
        (field (name "Price") "0.068USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "5")
        (field (name "Attrition Qty") "4")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Crystals/Oscillators/Resonators,Crystals")
        (field (name "Manufacturer") "Yangxing Tech")
        (field (name "Part") "X322516MLB4SI")
        (field (name "Frequency") "16MHz")
        (field (name "Frequency Stability") "±20ppm")
        (field (name "Operating Temperature") "-40°C~+85°C")
        (field (name "Frequency Tolerance") "±10ppm")
        (field (name "Crystal Type") "SMD Crystal Resonator")
        (field (name "Load Capacitance") "9pF")
        (field (name "Normal Temperature Frequency Tolerance") "±10ppm")
        (field (name "Type") "Surface Mount Crystal")
        (field (name "Footprint") "PCM_JLCPCB:OSC-SMD_4P-L3.2-W2.5-BL")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2403291504_YXC-Crystal-Oscillators-X322516MLB4SI_C13738.pdf")
        (field (name "Description") "16MHz Surface Mount Crystal 9pF ±10ppm ±20ppm SMD3225-4P Crystals ROHS"))
      (libsource (lib "PCM_JLCPCB-Crystals") (part "Crystal, 16MHz, 9pF") (description "16MHz Surface Mount Crystal 9pF ±10ppm ±20ppm SMD3225-4P Crystals ROHS"))
      (property (name "LCSC") (value "C13738"))
      (property (name "Stock") (value "162087"))
      (property (name "Price") (value "0.068USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "5"))
      (property (name "Attrition Qty") (value "4"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Crystals/Oscillators/Resonators,Crystals"))
      (property (name "Manufacturer") (value "Yangxing Tech"))
      (property (name "Part") (value "X322516MLB4SI"))
      (property (name "Frequency") (value "16MHz"))
      (property (name "Frequency Stability") (value "±20ppm"))
      (property (name "Operating Temperature") (value "-40°C~+85°C"))
      (property (name "Frequency Tolerance") (value "±10ppm"))
      (property (name "Crystal Type") (value "SMD Crystal Resonator"))
      (property (name "Load Capacitance") (value "9pF"))
      (property (name "Normal Temperature Frequency Tolerance") (value "±10ppm"))
      (property (name "Type") (value "Surface Mount Crystal"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "C13738"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "802b01d0-2016-4734-838a-ab91987a3f82"))
    (comp (ref "BT1")
      (value "CR2032-BS-6-1")
      (footprint "JLC2KiCad_lib-footprints:BAT-TH_CR2032-BS-6-1")
      (datasheet "https://item.szlcsc.com/71472.html")
      (fields
        (field (name "LCSC") "C70377")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:BAT-TH_CR2032-BS-6-1")
        (field (name "Datasheet") "https://item.szlcsc.com/71472.html")
        (field (name "Description")))
      (libsource (lib "CR2032-BS-6-1") (part "CR2032-BS-6-1") (description ""))
      (property (name "LCSC") (value "C70377"))
      (property (name "Sheetname") (value "Compute Module"))
      (property (name "Sheetfile") (value "cm5.kicad_sch"))
      (property (name "ki_keywords") (value "C70377"))
      (sheetpath (names "/Compute Module/") (tstamps "/1698d124-b773-4573-99c0-ad09fa2fae4f/"))
      (tstamps "11eda74e-925a-453a-8338-744d6c79ca06"))
    (comp (ref "C1")
      (value "100nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Compute Module"))
      (property (name "Sheetfile") (value "cm5.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Compute Module/") (tstamps "/1698d124-b773-4573-99c0-ad09fa2fae4f/"))
      (tstamps "0eeed2c4-5957-435c-877d-1d6f7a507e90"))
    (comp (ref "C65")
      (value "100nF")
      (footprint "PCM_JLCPCB:C_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05B104KO5NNNC_C1525.pdf")
      (description "16V 100nF X7R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
      (fields
        (field (name "LCSC") "C1525")
        (field (name "Stock") "20208285")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT")
        (field (name "Manufacturer") "Samsung Electro-Mechanics")
        (field (name "Part") "CL05B104KO5NNNC")
        (field (name "Voltage Rated") "16V")
        (field (name "Tolerance") "±10%")
        (field (name "Capacitance") "100nF")
        (field (name "Temperature Coefficient") "X7R")
        (field (name "Footprint") "PCM_JLCPCB:C_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05B104KO5NNNC_C1525.pdf")
        (field (name "Description") "16V 100nF X7R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (libsource (lib "PCM_JLCPCB-Capacitors") (part "0402,100nF") (description "16V 100nF X7R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (property (name "LCSC") (value "C1525"))
      (property (name "Stock") (value "20208285"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT"))
      (property (name "Manufacturer") (value "Samsung Electro-Mechanics"))
      (property (name "Part") (value "CL05B104KO5NNNC"))
      (property (name "Voltage Rated") (value "16V"))
      (property (name "Tolerance") (value "±10%"))
      (property (name "Capacitance") (value "100nF"))
      (property (name "Temperature Coefficient") (value "X7R"))
      (property (name "Sheetname") (value "Compute Module"))
      (property (name "Sheetfile") (value "cm5.kicad_sch"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Compute Module/") (tstamps "/1698d124-b773-4573-99c0-ad09fa2fae4f/"))
      (tstamps "5cfbb848-ab61-4c2a-ac6f-90f0a273f2b2"))
    (comp (ref "C66")
      (value "100nF")
      (footprint "PCM_JLCPCB:C_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05B104KO5NNNC_C1525.pdf")
      (description "16V 100nF X7R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
      (fields
        (field (name "LCSC") "C1525")
        (field (name "Stock") "20208285")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT")
        (field (name "Manufacturer") "Samsung Electro-Mechanics")
        (field (name "Part") "CL05B104KO5NNNC")
        (field (name "Voltage Rated") "16V")
        (field (name "Tolerance") "±10%")
        (field (name "Capacitance") "100nF")
        (field (name "Temperature Coefficient") "X7R")
        (field (name "Footprint") "PCM_JLCPCB:C_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05B104KO5NNNC_C1525.pdf")
        (field (name "Description") "16V 100nF X7R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (libsource (lib "PCM_JLCPCB-Capacitors") (part "0402,100nF") (description "16V 100nF X7R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (property (name "LCSC") (value "C1525"))
      (property (name "Stock") (value "20208285"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT"))
      (property (name "Manufacturer") (value "Samsung Electro-Mechanics"))
      (property (name "Part") (value "CL05B104KO5NNNC"))
      (property (name "Voltage Rated") (value "16V"))
      (property (name "Tolerance") (value "±10%"))
      (property (name "Capacitance") (value "100nF"))
      (property (name "Temperature Coefficient") (value "X7R"))
      (property (name "Sheetname") (value "Compute Module"))
      (property (name "Sheetfile") (value "cm5.kicad_sch"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Compute Module/") (tstamps "/1698d124-b773-4573-99c0-ad09fa2fae4f/"))
      (tstamps "a6ed2c66-1ce6-47ed-9874-410d9ef7e9b6"))
    (comp (ref "C75")
      (value "100nF")
      (footprint "PCM_JLCPCB:C_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05B104KO5NNNC_C1525.pdf")
      (description "16V 100nF X7R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
      (fields
        (field (name "LCSC") "C1525")
        (field (name "Stock") "20208285")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT")
        (field (name "Manufacturer") "Samsung Electro-Mechanics")
        (field (name "Part") "CL05B104KO5NNNC")
        (field (name "Voltage Rated") "16V")
        (field (name "Tolerance") "±10%")
        (field (name "Capacitance") "100nF")
        (field (name "Temperature Coefficient") "X7R")
        (field (name "Footprint") "PCM_JLCPCB:C_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05B104KO5NNNC_C1525.pdf")
        (field (name "Description") "16V 100nF X7R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (libsource (lib "PCM_JLCPCB-Capacitors") (part "0402,100nF") (description "16V 100nF X7R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (property (name "LCSC") (value "C1525"))
      (property (name "Stock") (value "20208285"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT"))
      (property (name "Manufacturer") (value "Samsung Electro-Mechanics"))
      (property (name "Part") (value "CL05B104KO5NNNC"))
      (property (name "Voltage Rated") (value "16V"))
      (property (name "Tolerance") (value "±10%"))
      (property (name "Capacitance") (value "100nF"))
      (property (name "Temperature Coefficient") (value "X7R"))
      (property (name "Sheetname") (value "Compute Module"))
      (property (name "Sheetfile") (value "cm5.kicad_sch"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Compute Module/") (tstamps "/1698d124-b773-4573-99c0-ad09fa2fae4f/"))
      (tstamps "2d2ae385-0dc7-4a5a-b006-ddef6fed3b0d"))
    (comp (ref "C76")
      (value "10uF")
      (footprint "PCM_JLCPCB:C_0805")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL21A106KAYNNNE_C15850.pdf")
      (description "25V 10uF X5R ±10% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
      (fields
        (field (name "LCSC") "C15850")
        (field (name "Stock") "6525809")
        (field (name "Price") "0.014USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT")
        (field (name "Manufacturer") "Samsung Electro-Mechanics")
        (field (name "Part") "CL21A106KAYNNNE")
        (field (name "Voltage Rated") "25V")
        (field (name "Tolerance") "±10%")
        (field (name "Capacitance") "10uF")
        (field (name "Temperature Coefficient") "X5R")
        (field (name "Footprint") "PCM_JLCPCB:C_0805")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL21A106KAYNNNE_C15850.pdf")
        (field (name "Description") "25V 10uF X5R ±10% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (libsource (lib "PCM_JLCPCB-Capacitors") (part "0805,10uF") (description "25V 10uF X5R ±10% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (property (name "LCSC") (value "C15850"))
      (property (name "Stock") (value "6525809"))
      (property (name "Price") (value "0.014USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT"))
      (property (name "Manufacturer") (value "Samsung Electro-Mechanics"))
      (property (name "Part") (value "CL21A106KAYNNNE"))
      (property (name "Voltage Rated") (value "25V"))
      (property (name "Tolerance") (value "±10%"))
      (property (name "Capacitance") (value "10uF"))
      (property (name "Temperature Coefficient") (value "X5R"))
      (property (name "Sheetname") (value "Compute Module"))
      (property (name "Sheetfile") (value "cm5.kicad_sch"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Compute Module/") (tstamps "/1698d124-b773-4573-99c0-ad09fa2fae4f/"))
      (tstamps "e69da19a-0e2a-43c6-9f1f-1d2cfa9b773a"))
    (comp (ref "D1")
      (value "PSC-1608U52GC-G4")
      (footprint "JLC2KiCad_lib-footprints:LED0603-RD_GREEN")
      (datasheet "https://atta.szlcsc.com/upload/public/pdf/source/20190115/C264450_D840E7E570138F41CCE67133F241C738.pdf")
      (description "green led 780mcd")
      (fields
        (field (name "LCSC") "C22371297")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:LED0603-RD_GREEN")
        (field (name "Datasheet") "https://atta.szlcsc.com/upload/public/pdf/source/20190115/C264450_D840E7E570138F41CCE67133F241C738.pdf")
        (field (name "Description") "green led 780mcd"))
      (libsource (lib "PSC-1608U52GC-G4") (part "PSC-1608U52GC-G4") (description ""))
      (property (name "LCSC") (value "C22371297"))
      (property (name "Sheetname") (value "Compute Module"))
      (property (name "Sheetfile") (value "cm5.kicad_sch"))
      (property (name "ki_keywords") (value "C22371297"))
      (sheetpath (names "/Compute Module/") (tstamps "/1698d124-b773-4573-99c0-ad09fa2fae4f/"))
      (tstamps "dd446156-56f3-4c7b-b2d8-65127bb03476"))
    (comp (ref "D2")
      (value "XL-1608UBC-04")
      (footprint "JLC2KiCad_lib-footprints:LED0603-RD_BLUE")
      (datasheet "https://atta.szlcsc.com/upload/public/pdf/source/20210617/C2837377_50FC585D376FE0CDA016E524346528FF.pdf")
      (fields
        (field (name "LCSC") "C965807")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:LED0603-RD_BLUE")
        (field (name "Datasheet") "https://atta.szlcsc.com/upload/public/pdf/source/20210617/C2837377_50FC585D376FE0CDA016E524346528FF.pdf")
        (field (name "Description")))
      (libsource (lib "XL-1608UBC-04") (part "XL-1608UBC-04") (description ""))
      (property (name "LCSC") (value "C965807"))
      (property (name "Sheetname") (value "Compute Module"))
      (property (name "Sheetfile") (value "cm5.kicad_sch"))
      (property (name "ki_keywords") (value "C965807"))
      (sheetpath (names "/Compute Module/") (tstamps "/1698d124-b773-4573-99c0-ad09fa2fae4f/"))
      (tstamps "7dcaef86-a358-43ee-9ba9-a98c96e1dd84"))
    (comp (ref "J1")
      (value "J_FAN_PWM")
      (footprint "Connector_JST:JST_PH_B4B-PH-K_1x04_P2.00mm_Vertical")
      (datasheet "~")
      (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (fields
        (field (name "Footprint") "Connector_JST:JST_PH_B4B-PH-K_1x04_P2.00mm_Vertical")
        (field (name "Datasheet") "~")
        (field (name "Description") "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (libsource (lib "Connector_Generic") (part "Conn_01x04") (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (property (name "Sheetname") (value "Compute Module"))
      (property (name "Sheetfile") (value "cm5.kicad_sch"))
      (property (name "ki_keywords") (value "connector"))
      (property (name "ki_fp_filters") (value "Connector*:*_1x??_*"))
      (sheetpath (names "/Compute Module/") (tstamps "/1698d124-b773-4573-99c0-ad09fa2fae4f/"))
      (tstamps "d2475d13-fe58-408b-b741-4adff211bb67"))
    (comp (ref "Q1")
      (value "AO3400A NFET")
      (footprint "PCM_JLCPCB:Q_SOT-23")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_1811081213_Alpha---Omega-Semicon-AO3400A_C20917.pdf")
      (description "30V 5.7A 26.5mΩ@10V,5.7A 1.4W 1.5V@250uA 1 N-Channel SOT-23-3L MOSFETs ROHS")
      (fields
        (field (name "LCSC") "C20917")
        (field (name "Stock") "463122")
        (field (name "Price") "0.074USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "5")
        (field (name "Attrition Qty") "4")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Transistors,MOSFETs")
        (field (name "Manufacturer") "Alpha & Omega Semicon")
        (field (name "Part") "AO3400A")
        (field (name "Continuous Drain Current (Id)") "5.7A")
        (field (name "Input Capacitance (Ciss@Vds)") "630pF@15V")
        (field (name "Operating Temperature") "-55°C~+150°C@(Tj)")
        (field (name "Type") "1 N-channel")
        (field (name "Drain Source Voltage (Vdss)") "30V")
        (field (name "Power Dissipation (Pd)") "1.4W")
        (field (name "Gate Threshold Voltage (Vgs(th)@Id)") "1.5V@250uA")
        (field (name "Drain Source On Resistance (RDS(on)@Vgs,Id)") "26.5mΩ@10V,5.7A")
        (field (name "Total Gate Charge (Qg@Vgs)") "7nC@4.5V")
        (field (name "Footprint") "PCM_JLCPCB:Q_SOT-23")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_1811081213_Alpha---Omega-Semicon-AO3400A_C20917.pdf")
        (field (name "Description") "30V 5.7A 26.5mΩ@10V,5.7A 1.4W 1.5V@250uA 1 N-Channel SOT-23-3L MOSFETs ROHS"))
      (libsource (lib "PCM_JLCPCB-Transistors") (part "NMOS,AO3400A") (description "30V 5.7A 26.5mΩ@10V,5.7A 1.4W 1.5V@250uA 1 N-Channel SOT-23-3L MOSFETs ROHS"))
      (property (name "LCSC") (value "C20917"))
      (property (name "Stock") (value "463122"))
      (property (name "Price") (value "0.074USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "5"))
      (property (name "Attrition Qty") (value "4"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Transistors,MOSFETs"))
      (property (name "Manufacturer") (value "Alpha & Omega Semicon"))
      (property (name "Part") (value "AO3400A"))
      (property (name "Continuous Drain Current (Id)") (value "5.7A"))
      (property (name "Input Capacitance (Ciss@Vds)") (value "630pF@15V"))
      (property (name "Operating Temperature") (value "-55°C~+150°C@(Tj)"))
      (property (name "Type") (value "1 N-channel"))
      (property (name "Drain Source Voltage (Vdss)") (value "30V"))
      (property (name "Power Dissipation (Pd)") (value "1.4W"))
      (property (name "Gate Threshold Voltage (Vgs(th)@Id)") (value "1.5V@250uA"))
      (property (name "Drain Source On Resistance (RDS(on)@Vgs,Id)") (value "26.5mΩ@10V,5.7A"))
      (property (name "Total Gate Charge (Qg@Vgs)") (value "7nC@4.5V"))
      (property (name "Sheetname") (value "Compute Module"))
      (property (name "Sheetfile") (value "cm5.kicad_sch"))
      (property (name "ki_fp_filters") (value "Q_*"))
      (sheetpath (names "/Compute Module/") (tstamps "/1698d124-b773-4573-99c0-ad09fa2fae4f/"))
      (tstamps "e1406856-a399-4f49-86d1-7e636c71a930"))
    (comp (ref "Q2")
      (value "SI2301CDS-T1-GE3 P-FET")
      (footprint "PCM_JLCPCB:Q_SOT-23")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_1808272021_Vishay-Intertech-SI2301CDS-T1-GE3_C10487.pdf")
      (description "20V 3.1A 112mΩ@4.5V,2.8A 1V@250uA 1 Piece P-Channel SOT-23 MOSFETs ROHS")
      (fields
        (field (name "LCSC") "C10487")
        (field (name "Stock") "476267")
        (field (name "Price") "0.058USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "5")
        (field (name "Attrition Qty") "4")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Transistors,MOSFETs")
        (field (name "Manufacturer") "Vishay Intertech")
        (field (name "Part") "SI2301CDS-T1-GE3")
        (field (name "Continuous Drain Current (Id)") "2.3A")
        (field (name "Input Capacitance (Ciss@Vds)") "405pF@10V")
        (field (name "Operating Temperature") "-55°C~+150°C")
        (field (name "Type") "1 Piece P-Channel")
        (field (name "Drain Source Voltage (Vdss)") "20V")
        (field (name "Power Dissipation (Pd)") "0.86W")
        (field (name "Gate Threshold Voltage (Vgs(th)@Id)") "1V@250uA")
        (field (name "Reverse Transfer Capacitance (Crss@Vds)") "55pF@10V")
        (field (name "Drain Source On Resistance (RDS(on)@Vgs,Id)") "0.112Ω@4.5V,2.8A")
        (field (name "Total Gate Charge (Qg@Vgs)") "3.3nC@10V")
        (field (name "Footprint") "PCM_JLCPCB:Q_SOT-23")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_1808272021_Vishay-Intertech-SI2301CDS-T1-GE3_C10487.pdf")
        (field (name "Description") "20V 3.1A 112mΩ@4.5V,2.8A 1V@250uA 1 Piece P-Channel SOT-23 MOSFETs ROHS"))
      (libsource (lib "PCM_JLCPCB-Transistors") (part "PMOS,SI2301CDS-T1-GE3") (description "20V 3.1A 112mΩ@4.5V,2.8A 1V@250uA 1 Piece P-Channel SOT-23 MOSFETs ROHS"))
      (property (name "LCSC") (value "C10487"))
      (property (name "Stock") (value "476267"))
      (property (name "Price") (value "0.058USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "5"))
      (property (name "Attrition Qty") (value "4"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Transistors,MOSFETs"))
      (property (name "Manufacturer") (value "Vishay Intertech"))
      (property (name "Part") (value "SI2301CDS-T1-GE3"))
      (property (name "Continuous Drain Current (Id)") (value "2.3A"))
      (property (name "Input Capacitance (Ciss@Vds)") (value "405pF@10V"))
      (property (name "Operating Temperature") (value "-55°C~+150°C"))
      (property (name "Type") (value "1 Piece P-Channel"))
      (property (name "Drain Source Voltage (Vdss)") (value "20V"))
      (property (name "Power Dissipation (Pd)") (value "0.86W"))
      (property (name "Gate Threshold Voltage (Vgs(th)@Id)") (value "1V@250uA"))
      (property (name "Reverse Transfer Capacitance (Crss@Vds)") (value "55pF@10V"))
      (property (name "Drain Source On Resistance (RDS(on)@Vgs,Id)") (value "0.112Ω@4.5V,2.8A"))
      (property (name "Total Gate Charge (Qg@Vgs)") (value "3.3nC@10V"))
      (property (name "Sheetname") (value "Compute Module"))
      (property (name "Sheetfile") (value "cm5.kicad_sch"))
      (property (name "ki_fp_filters") (value "Q_*"))
      (sheetpath (names "/Compute Module/") (tstamps "/1698d124-b773-4573-99c0-ad09fa2fae4f/"))
      (tstamps "b4675fce-85c1-429b-942f-13f43df60639"))
    (comp (ref "R1")
      (value "10kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Compute Module"))
      (property (name "Sheetfile") (value "cm5.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Compute Module/") (tstamps "/1698d124-b773-4573-99c0-ad09fa2fae4f/"))
      (tstamps "940f0796-96ca-40eb-b2d9-bd78898c4cc6"))
    (comp (ref "R2")
      (value "5.1kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Compute Module"))
      (property (name "Sheetfile") (value "cm5.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Compute Module/") (tstamps "/1698d124-b773-4573-99c0-ad09fa2fae4f/"))
      (tstamps "fb8ba5bd-0e97-4a46-8628-ff0214a6dfa2"))
    (comp (ref "R3")
      (value "5.1kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Compute Module"))
      (property (name "Sheetfile") (value "cm5.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Compute Module/") (tstamps "/1698d124-b773-4573-99c0-ad09fa2fae4f/"))
      (tstamps "8663eea9-57be-469f-aeb0-7b60a4ecd127"))
    (comp (ref "R4")
      (value "220Ω")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Compute Module"))
      (property (name "Sheetfile") (value "cm5.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Compute Module/") (tstamps "/1698d124-b773-4573-99c0-ad09fa2fae4f/"))
      (tstamps "3cc517e8-ca8a-41cb-9c02-1005b114990d"))
    (comp (ref "R5")
      (value "2.2kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Compute Module"))
      (property (name "Sheetfile") (value "cm5.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Compute Module/") (tstamps "/1698d124-b773-4573-99c0-ad09fa2fae4f/"))
      (tstamps "aae294f9-b3d1-46c3-906a-bfd623ec1b0d"))
    (comp (ref "R6")
      (value "220Ω")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Compute Module"))
      (property (name "Sheetfile") (value "cm5.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Compute Module/") (tstamps "/1698d124-b773-4573-99c0-ad09fa2fae4f/"))
      (tstamps "e92bb50a-f91d-4b2c-b448-1c0076131190"))
    (comp (ref "R7")
      (value "2.2kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Compute Module"))
      (property (name "Sheetfile") (value "cm5.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Compute Module/") (tstamps "/1698d124-b773-4573-99c0-ad09fa2fae4f/"))
      (tstamps "25dc006a-5bcf-4b1a-9319-0f09ecfcf89a"))
    (comp (ref "R8")
      (value "100Ω")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Compute Module"))
      (property (name "Sheetfile") (value "cm5.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Compute Module/") (tstamps "/1698d124-b773-4573-99c0-ad09fa2fae4f/"))
      (tstamps "06f4b706-1555-4f31-bf9f-b82ae96d189a"))
    (comp (ref "R9")
      (value "2.2kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Compute Module"))
      (property (name "Sheetfile") (value "cm5.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Compute Module/") (tstamps "/1698d124-b773-4573-99c0-ad09fa2fae4f/"))
      (tstamps "a1e64fd2-67c3-4b19-8a84-02841be4d63c"))
    (comp (ref "R10")
      (value "3.3kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Compute Module"))
      (property (name "Sheetfile") (value "cm5.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Compute Module/") (tstamps "/1698d124-b773-4573-99c0-ad09fa2fae4f/"))
      (tstamps "42fcc5db-8a46-45d4-a04e-79c52a30d140"))
    (comp (ref "R69")
      (value "33Ω")
      (footprint "PCM_JLCPCB:R_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF330JTCE_C25105.pdf")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 33Ω 0402 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C25105")
        (field (name "Stock") "2122900")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF330JTCE")
        (field (name "Resistance") "33Ω")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF330JTCE_C25105.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 33Ω 0402 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0402,33Ω") (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 33Ω 0402 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C25105"))
      (property (name "Stock") (value "2122900"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0402WGF330JTCE"))
      (property (name "Resistance") (value "33Ω"))
      (property (name "Power(Watts)") (value "62.5mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "50V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±100ppm/°C"))
      (property (name "Sheetname") (value "Compute Module"))
      (property (name "Sheetfile") (value "cm5.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Compute Module/") (tstamps "/1698d124-b773-4573-99c0-ad09fa2fae4f/"))
      (tstamps "05d1efaf-f0d3-4b78-aa42-195f5fc3bcca"))
    (comp (ref "R70")
      (value "10kΩ")
      (footprint "PCM_JLCPCB:R_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2411221126_UNI-ROYAL-Uniroyal-Elec-0402WGF1002TCE_C25744.pdf")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 10kΩ 0402 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C25744")
        (field (name "Stock") "24372091")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF1002TCE")
        (field (name "Resistance") "10kΩ")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2411221126_UNI-ROYAL-Uniroyal-Elec-0402WGF1002TCE_C25744.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 10kΩ 0402 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0402,10kΩ") (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 10kΩ 0402 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C25744"))
      (property (name "Stock") (value "24372091"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0402WGF1002TCE"))
      (property (name "Resistance") (value "10kΩ"))
      (property (name "Power(Watts)") (value "62.5mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "50V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±100ppm/°C"))
      (property (name "Sheetname") (value "Compute Module"))
      (property (name "Sheetfile") (value "cm5.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Compute Module/") (tstamps "/1698d124-b773-4573-99c0-ad09fa2fae4f/"))
      (tstamps "9d48e713-446a-447d-9149-6309415bce74"))
    (comp (ref "R71")
      (value "10kΩ")
      (footprint "PCM_JLCPCB:R_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2411221126_UNI-ROYAL-Uniroyal-Elec-0402WGF1002TCE_C25744.pdf")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 10kΩ 0402 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C25744")
        (field (name "Stock") "24372091")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF1002TCE")
        (field (name "Resistance") "10kΩ")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2411221126_UNI-ROYAL-Uniroyal-Elec-0402WGF1002TCE_C25744.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 10kΩ 0402 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0402,10kΩ") (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 10kΩ 0402 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C25744"))
      (property (name "Stock") (value "24372091"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0402WGF1002TCE"))
      (property (name "Resistance") (value "10kΩ"))
      (property (name "Power(Watts)") (value "62.5mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "50V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±100ppm/°C"))
      (property (name "Sheetname") (value "Compute Module"))
      (property (name "Sheetfile") (value "cm5.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Compute Module/") (tstamps "/1698d124-b773-4573-99c0-ad09fa2fae4f/"))
      (tstamps "5d905ad5-7501-43c4-b3c5-4a6cc83f11c1"))
    (comp (ref "R72")
      (value "10kΩ")
      (footprint "PCM_JLCPCB:R_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2411221126_UNI-ROYAL-Uniroyal-Elec-0402WGF1002TCE_C25744.pdf")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 10kΩ 0402 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C25744")
        (field (name "Stock") "24372091")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF1002TCE")
        (field (name "Resistance") "10kΩ")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2411221126_UNI-ROYAL-Uniroyal-Elec-0402WGF1002TCE_C25744.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 10kΩ 0402 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0402,10kΩ") (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 10kΩ 0402 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C25744"))
      (property (name "Stock") (value "24372091"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0402WGF1002TCE"))
      (property (name "Resistance") (value "10kΩ"))
      (property (name "Power(Watts)") (value "62.5mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "50V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±100ppm/°C"))
      (property (name "Sheetname") (value "Compute Module"))
      (property (name "Sheetfile") (value "cm5.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Compute Module/") (tstamps "/1698d124-b773-4573-99c0-ad09fa2fae4f/"))
      (tstamps "027aec58-d8dd-43c7-a0f2-20a1a244fc55"))
    (comp (ref "R73")
      (value "10kΩ")
      (footprint "PCM_JLCPCB:R_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2411221126_UNI-ROYAL-Uniroyal-Elec-0402WGF1002TCE_C25744.pdf")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 10kΩ 0402 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C25744")
        (field (name "Stock") "24372091")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF1002TCE")
        (field (name "Resistance") "10kΩ")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2411221126_UNI-ROYAL-Uniroyal-Elec-0402WGF1002TCE_C25744.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 10kΩ 0402 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0402,10kΩ") (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 10kΩ 0402 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C25744"))
      (property (name "Stock") (value "24372091"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0402WGF1002TCE"))
      (property (name "Resistance") (value "10kΩ"))
      (property (name "Power(Watts)") (value "62.5mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "50V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±100ppm/°C"))
      (property (name "Sheetname") (value "Compute Module"))
      (property (name "Sheetfile") (value "cm5.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Compute Module/") (tstamps "/1698d124-b773-4573-99c0-ad09fa2fae4f/"))
      (tstamps "d02f5c27-b0f4-4d70-a2bc-e123a013fa62"))
    (comp (ref "R74")
      (value "10kΩ")
      (footprint "PCM_JLCPCB:R_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2411221126_UNI-ROYAL-Uniroyal-Elec-0402WGF1002TCE_C25744.pdf")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 10kΩ 0402 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C25744")
        (field (name "Stock") "24372091")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF1002TCE")
        (field (name "Resistance") "10kΩ")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2411221126_UNI-ROYAL-Uniroyal-Elec-0402WGF1002TCE_C25744.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 10kΩ 0402 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0402,10kΩ") (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 10kΩ 0402 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C25744"))
      (property (name "Stock") (value "24372091"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0402WGF1002TCE"))
      (property (name "Resistance") (value "10kΩ"))
      (property (name "Power(Watts)") (value "62.5mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "50V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±100ppm/°C"))
      (property (name "Sheetname") (value "Compute Module"))
      (property (name "Sheetfile") (value "cm5.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Compute Module/") (tstamps "/1698d124-b773-4573-99c0-ad09fa2fae4f/"))
      (tstamps "1fa07890-667b-4195-a7a6-2b92afe479fc"))
    (comp (ref "R75")
      (value "10kΩ")
      (footprint "PCM_JLCPCB:R_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2411221126_UNI-ROYAL-Uniroyal-Elec-0402WGF1002TCE_C25744.pdf")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 10kΩ 0402 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C25744")
        (field (name "Stock") "24372091")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF1002TCE")
        (field (name "Resistance") "10kΩ")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2411221126_UNI-ROYAL-Uniroyal-Elec-0402WGF1002TCE_C25744.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 10kΩ 0402 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0402,10kΩ") (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 10kΩ 0402 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C25744"))
      (property (name "Stock") (value "24372091"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0402WGF1002TCE"))
      (property (name "Resistance") (value "10kΩ"))
      (property (name "Power(Watts)") (value "62.5mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "50V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±100ppm/°C"))
      (property (name "Sheetname") (value "Compute Module"))
      (property (name "Sheetfile") (value "cm5.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Compute Module/") (tstamps "/1698d124-b773-4573-99c0-ad09fa2fae4f/"))
      (tstamps "4cd10ffe-648b-46eb-bbf7-49b900487863"))
    (comp (ref "R76")
      (value "10kΩ")
      (footprint "PCM_JLCPCB:R_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2411221126_UNI-ROYAL-Uniroyal-Elec-0402WGF1002TCE_C25744.pdf")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 10kΩ 0402 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C25744")
        (field (name "Stock") "24372091")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF1002TCE")
        (field (name "Resistance") "10kΩ")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2411221126_UNI-ROYAL-Uniroyal-Elec-0402WGF1002TCE_C25744.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 10kΩ 0402 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0402,10kΩ") (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 10kΩ 0402 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C25744"))
      (property (name "Stock") (value "24372091"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0402WGF1002TCE"))
      (property (name "Resistance") (value "10kΩ"))
      (property (name "Power(Watts)") (value "62.5mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "50V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±100ppm/°C"))
      (property (name "Sheetname") (value "Compute Module"))
      (property (name "Sheetfile") (value "cm5.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Compute Module/") (tstamps "/1698d124-b773-4573-99c0-ad09fa2fae4f/"))
      (tstamps "2385c96c-201c-4f76-94b9-38442926b84a"))
    (comp (ref "SW1")
      (value "DSWB05LHGET")
      (footprint "JLC2KiCad_lib-footprints:SW-TH_DSWB05LHGET")
      (datasheet "https://so.szlcsc.com/global.html?c=&k=C126889")
      (fields
        (field (name "LCSC") "C126889")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:SW-TH_DSWB05LHGET")
        (field (name "Datasheet") "https://so.szlcsc.com/global.html?c=&k=C126889")
        (field (name "Description")))
      (libsource (lib "DSWB05LHGET") (part "DSWB05LHGET") (description ""))
      (property (name "LCSC") (value "C126889"))
      (property (name "Sheetname") (value "Compute Module"))
      (property (name "Sheetfile") (value "cm5.kicad_sch"))
      (property (name "ki_keywords") (value "C126889"))
      (sheetpath (names "/Compute Module/") (tstamps "/1698d124-b773-4573-99c0-ad09fa2fae4f/"))
      (tstamps "9e2b7235-cac5-470e-a1c7-5df13cf42503"))
    (comp (ref "SW2")
      (value "PWR_BUT_CM5")
      (footprint "PCM_JLCPCB:SW_TS-1088-AR02016")
      (datasheet "~")
      (description "Push button switch, generic, two pins")
      (fields
        (field (name "Footprint") "PCM_JLCPCB:SW_TS-1088-AR02016")
        (field (name "Datasheet") "~")
        (field (name "Description") "Push button switch, generic, two pins"))
      (libsource (lib "Switch") (part "SW_Push") (description "Push button switch, generic, two pins"))
      (property (name "Sheetname") (value "Compute Module"))
      (property (name "Sheetfile") (value "cm5.kicad_sch"))
      (property (name "ki_keywords") (value "switch normally-open pushbutton push-button"))
      (sheetpath (names "/Compute Module/") (tstamps "/1698d124-b773-4573-99c0-ad09fa2fae4f/"))
      (tstamps "d097adbb-1382-4027-acfa-fed5463824eb"))
    (comp (ref "U7")
      (value "USBLC6-2SC6-ES")
      (footprint "footprint:SOT-23-6_L2.9-W1.6-P0.95-LS2.8-BR")
      (datasheet "https://item.szlcsc.com/169042.html")
      (fields
        (field (name "LCSC") "C5180249")
        (field (name "Footprint") "footprint:SOT-23-6_L2.9-W1.6-P0.95-LS2.8-BR")
        (field (name "Datasheet") "https://item.szlcsc.com/169042.html")
        (field (name "Description")))
      (libsource (lib "jlc_USBLC6-2SC6-ES") (part "USBLC6-2SC6-ES") (description ""))
      (property (name "LCSC") (value "C5180249"))
      (property (name "Sheetname") (value "Compute Module"))
      (property (name "Sheetfile") (value "cm5.kicad_sch"))
      (property (name "ki_keywords") (value "C5180249"))
      (sheetpath (names "/Compute Module/") (tstamps "/1698d124-b773-4573-99c0-ad09fa2fae4f/"))
      (tstamps "20bb5f16-ccb1-4977-97da-96f1cb6c16d6"))
    (comp (ref "U20")
      (value "TF-15×15")
      (footprint "footprint:TF-SMD_TF-15-15")
      (datasheet "https://item.szlcsc.com/112422.html")
      (fields
        (field (name "LCSC") "C111196")
        (field (name "Footprint") "footprint:TF-SMD_TF-15-15")
        (field (name "Datasheet") "https://item.szlcsc.com/112422.html")
        (field (name "Description")))
      (libsource (lib "TF-15×15") (part "TF-15×15") (description ""))
      (property (name "LCSC") (value "C111196"))
      (property (name "Sheetname") (value "Compute Module"))
      (property (name "Sheetfile") (value "cm5.kicad_sch"))
      (property (name "ki_keywords") (value "C111196"))
      (sheetpath (names "/Compute Module/") (tstamps "/1698d124-b773-4573-99c0-ad09fa2fae4f/"))
      (tstamps "aa15bee3-febf-4436-9f10-448433163983"))
    (comp (ref "U21")
      (value "USBLC6-2SC6-ES")
      (footprint "footprint:SOT-23-6_L2.9-W1.6-P0.95-LS2.8-BR")
      (datasheet "https://item.szlcsc.com/169042.html")
      (fields
        (field (name "LCSC") "C5180249")
        (field (name "Footprint") "footprint:SOT-23-6_L2.9-W1.6-P0.95-LS2.8-BR")
        (field (name "Datasheet") "https://item.szlcsc.com/169042.html")
        (field (name "Description")))
      (libsource (lib "jlc_USBLC6-2SC6-ES") (part "USBLC6-2SC6-ES") (description ""))
      (property (name "LCSC") (value "C5180249"))
      (property (name "Sheetname") (value "Compute Module"))
      (property (name "Sheetfile") (value "cm5.kicad_sch"))
      (property (name "ki_keywords") (value "C5180249"))
      (sheetpath (names "/Compute Module/") (tstamps "/1698d124-b773-4573-99c0-ad09fa2fae4f/"))
      (tstamps "986abe16-f07e-4971-8e88-0200e1d140d5"))
    (comp (ref "U23")
      (value "USBLC6-2SC6-ES")
      (footprint "footprint:SOT-23-6_L2.9-W1.6-P0.95-LS2.8-BR")
      (datasheet "https://item.szlcsc.com/169042.html")
      (fields
        (field (name "LCSC") "C5180249")
        (field (name "Footprint") "footprint:SOT-23-6_L2.9-W1.6-P0.95-LS2.8-BR")
        (field (name "Datasheet") "https://item.szlcsc.com/169042.html")
        (field (name "Description")))
      (libsource (lib "jlc_USBLC6-2SC6-ES") (part "USBLC6-2SC6-ES") (description ""))
      (property (name "LCSC") (value "C5180249"))
      (property (name "Sheetname") (value "Compute Module"))
      (property (name "Sheetfile") (value "cm5.kicad_sch"))
      (property (name "ki_keywords") (value "C5180249"))
      (sheetpath (names "/Compute Module/") (tstamps "/1698d124-b773-4573-99c0-ad09fa2fae4f/"))
      (tstamps "bd069648-049d-412b-828f-f9bd333e0884"))
    (comp (ref "C67")
      (value "10u")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Sim_Buck"))
      (property (name "Sheetfile") (value "sim_buck.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Sim_Buck/") (tstamps "/2c58c456-80df-4d51-9833-733db3c5a28f/"))
      (tstamps "d45692f7-4406-41a3-8060-51d3ca35b544"))
    (comp (ref "C68")
      (value "10u")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Sim_Buck"))
      (property (name "Sheetfile") (value "sim_buck.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Sim_Buck/") (tstamps "/2c58c456-80df-4d51-9833-733db3c5a28f/"))
      (tstamps "77302528-f6f2-4c98-89f7-bf99b6ff69b0"))
    (comp (ref "C69")
      (value "100n")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Sim_Buck"))
      (property (name "Sheetfile") (value "sim_buck.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Sim_Buck/") (tstamps "/2c58c456-80df-4d51-9833-733db3c5a28f/"))
      (tstamps "b629349a-4cd6-4082-a3dc-cfb78f7c0cff"))
    (comp (ref "C70")
      (value "22u")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Sim_Buck"))
      (property (name "Sheetfile") (value "sim_buck.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Sim_Buck/") (tstamps "/2c58c456-80df-4d51-9833-733db3c5a28f/"))
      (tstamps "59bef483-eb8a-48f8-a4e1-c409622200c8"))
    (comp (ref "C71")
      (value "22u")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Sim_Buck"))
      (property (name "Sheetfile") (value "sim_buck.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Sim_Buck/") (tstamps "/2c58c456-80df-4d51-9833-733db3c5a28f/"))
      (tstamps "b28ef218-e1ab-4ef2-b746-950edda62462"))
    (comp (ref "C72")
      (value "22u")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Sim_Buck"))
      (property (name "Sheetfile") (value "sim_buck.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Sim_Buck/") (tstamps "/2c58c456-80df-4d51-9833-733db3c5a28f/"))
      (tstamps "3b6316c1-8f55-4368-9b2d-e1de8c5a6fca"))
    (comp (ref "C73")
      (value "100p")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Sim_Buck"))
      (property (name "Sheetfile") (value "sim_buck.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Sim_Buck/") (tstamps "/2c58c456-80df-4d51-9833-733db3c5a28f/"))
      (tstamps "87e09eb3-d24d-4afb-86ba-9d389d50839f"))
    (comp (ref "C74")
      (value "1u")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Sim_Buck"))
      (property (name "Sheetfile") (value "sim_buck.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Sim_Buck/") (tstamps "/2c58c456-80df-4d51-9833-733db3c5a28f/"))
      (tstamps "22de3a36-acc8-4d22-a9c9-90bcdf86cbf0"))
    (comp (ref "D8")
      (value "LED")
      (datasheet "~")
      (description "Light emitting diode")
      (fields
        (field (name "Sim.Pins") "1=K 2=A")
        (field (name "Sim.Library") "LED.lib")
        (field (name "Sim.Name") "LED")
        (field (name "Sim.Device") "D")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Light emitting diode"))
      (libsource (lib "Device") (part "LED") (description "Light emitting diode"))
      (property (name "Sim.Pins") (value "1=K 2=A"))
      (property (name "Sim.Library") (value "LED.lib"))
      (property (name "Sim.Name") (value "LED"))
      (property (name "Sim.Device") (value "D"))
      (property (name "Sheetname") (value "Sim_Buck"))
      (property (name "Sheetfile") (value "sim_buck.kicad_sch"))
      (property (name "ki_keywords") (value "LED diode"))
      (property (name "ki_fp_filters") (value "LED* LED_SMD:* LED_THT:*"))
      (sheetpath (names "/Sim_Buck/") (tstamps "/2c58c456-80df-4d51-9833-733db3c5a28f/"))
      (tstamps "42073023-0197-435c-a5b4-9c7bcd7728a4"))
    (comp (ref "L3")
      (value "2.2µ")
      (datasheet "~")
      (description "Inductor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Inductor"))
      (libsource (lib "Device") (part "L") (description "Inductor"))
      (property (name "Sheetname") (value "Sim_Buck"))
      (property (name "Sheetfile") (value "sim_buck.kicad_sch"))
      (property (name "ki_keywords") (value "inductor choke coil reactor magnetic"))
      (property (name "ki_fp_filters") (value "Choke_* *Coil* Inductor_* L_*"))
      (sheetpath (names "/Sim_Buck/") (tstamps "/2c58c456-80df-4d51-9833-733db3c5a28f/"))
      (tstamps "64dd8f89-bbf5-4586-97ca-b731d9ad15a5"))
    (comp (ref "R38")
      (value "1m")
      (datasheet "~")
      (description "ESR")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "ESR"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Sim_Buck"))
      (property (name "Sheetfile") (value "sim_buck.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Sim_Buck/") (tstamps "/2c58c456-80df-4d51-9833-733db3c5a28f/"))
      (tstamps "3606604e-fa90-4ee7-bdb6-aa84690d4cbf"))
    (comp (ref "R44")
      (value "100k")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Sim_Buck"))
      (property (name "Sheetfile") (value "sim_buck.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Sim_Buck/") (tstamps "/2c58c456-80df-4d51-9833-733db3c5a28f/"))
      (tstamps "0248405c-89ba-4589-9969-45e41ee82192"))
    (comp (ref "R45")
      (value "18k")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Sim_Buck"))
      (property (name "Sheetfile") (value "sim_buck.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Sim_Buck/") (tstamps "/2c58c456-80df-4d51-9833-733db3c5a28f/"))
      (tstamps "e42de3bc-78c9-40e1-af5f-5dd5f2a2905c"))
    (comp (ref "R46")
      (value "510")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Sim_Buck"))
      (property (name "Sheetfile") (value "sim_buck.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Sim_Buck/") (tstamps "/2c58c456-80df-4d51-9833-733db3c5a28f/"))
      (tstamps "71e963c1-bd81-434b-903b-069cd6347af1"))
    (comp (ref "R47")
      (value "10")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Sim_Buck"))
      (property (name "Sheetfile") (value "sim_buck.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Sim_Buck/") (tstamps "/2c58c456-80df-4d51-9833-733db3c5a28f/"))
      (tstamps "80003390-4d25-42fd-bf17-50fadf00c9b5"))
    (comp (ref "R48")
      (value "200k")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Sim_Buck"))
      (property (name "Sheetfile") (value "sim_buck.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Sim_Buck/") (tstamps "/2c58c456-80df-4d51-9833-733db3c5a28f/"))
      (tstamps "2349e1f0-d85a-4988-9ece-00e4d1e1bfc6"))
    (comp (ref "R49")
      (value "27k")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Sim_Buck"))
      (property (name "Sheetfile") (value "sim_buck.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Sim_Buck/") (tstamps "/2c58c456-80df-4d51-9833-733db3c5a28f/"))
      (tstamps "af9f9504-e933-40e5-bad4-f96792b9eac3"))
    (comp (ref "R50")
      (value "1.25")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Sim_Buck"))
      (property (name "Sheetfile") (value "sim_buck.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Sim_Buck/") (tstamps "/2c58c456-80df-4d51-9833-733db3c5a28f/"))
      (tstamps "e16d18d2-b9f2-473c-9249-a3da0a214fbf"))
    (comp (ref "U15")
      (value "SY8368AQQC")
      (footprint "footprint:QFN-12_L3.0-W3.0-P0.45-TL-EP")
      (datasheet "https://atta.szlcsc.com/upload/public/pdf/source/20180224/C178253_15194367790221363788.pdf")
      (fields
        (field (name "LCSC") "C207642")
        (field (name "Sim.Library") "SY8368AQQC.lib")
        (field (name "Sim.Name") "SY8368AQQC")
        (field (name "Sim.Device") "SUBCKT")
        (field (name "Sim.Pins") "1=GND1 2=LX 3=GND2 4=IN1 5=IN2 6=IN3 7=BS 8=VCC 9=FB 10=ILMT 11=PG 12=EN")
        (field (name "Footprint") "footprint:QFN-12_L3.0-W3.0-P0.45-TL-EP")
        (field (name "Datasheet") "https://atta.szlcsc.com/upload/public/pdf/source/20180224/C178253_15194367790221363788.pdf")
        (field (name "Description")))
      (libsource (lib "SY8368AQQC") (part "SY8368AQQC") (description ""))
      (property (name "LCSC") (value "C207642"))
      (property (name "Sim.Library") (value "SY8368AQQC.lib"))
      (property (name "Sim.Name") (value "SY8368AQQC"))
      (property (name "Sim.Device") (value "SUBCKT"))
      (property (name "Sim.Pins") (value "1=GND1 2=LX 3=GND2 4=IN1 5=IN2 6=IN3 7=BS 8=VCC 9=FB 10=ILMT 11=PG 12=EN"))
      (property (name "Sheetname") (value "Sim_Buck"))
      (property (name "Sheetfile") (value "sim_buck.kicad_sch"))
      (property (name "ki_keywords") (value "C207642"))
      (sheetpath (names "/Sim_Buck/") (tstamps "/2c58c456-80df-4d51-9833-733db3c5a28f/"))
      (tstamps "9dff4de0-5de0-4c65-b9a2-5b19c969a39d"))
    (comp (ref "V1")
      (value "20")
      (datasheet "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#sec_Independent_Sources_for")
      (description "Voltage source, DC")
      (fields
        (field (name "Sim.Pins") "1=+ 2=-")
        (field (name "Sim.Type") "DC")
        (field (name "Sim.Device") "V")
        (field (name "Footprint"))
        (field (name "Datasheet") "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#sec_Independent_Sources_for")
        (field (name "Description") "Voltage source, DC"))
      (libsource (lib "Simulation_SPICE") (part "VDC") (description "Voltage source, DC"))
      (property (name "Sim.Pins") (value "1=+ 2=-"))
      (property (name "Sim.Type") (value "DC"))
      (property (name "Sim.Device") (value "V"))
      (property (name "Sheetname") (value "Sim_Buck"))
      (property (name "Sheetfile") (value "sim_buck.kicad_sch"))
      (property (name "ki_keywords") (value "simulation"))
      (sheetpath (names "/Sim_Buck/") (tstamps "/2c58c456-80df-4d51-9833-733db3c5a28f/"))
      (tstamps "0c9228f7-a1de-41be-936a-8e588386f2cc"))
    (comp (ref "C59")
      (value "10u")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Sim_DAC"))
      (property (name "Sheetfile") (value "sim_dac.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Sim_DAC/") (tstamps "/b78ec0ce-0ea7-4e81-bc06-3286ad54835a/"))
      (tstamps "2be23cad-f07c-4a5f-ae1d-e05ae37e0584"))
    (comp (ref "C79")
      (value "2.2u")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Sim_DAC"))
      (property (name "Sheetfile") (value "sim_dac.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Sim_DAC/") (tstamps "/b78ec0ce-0ea7-4e81-bc06-3286ad54835a/"))
      (tstamps "983d2d16-21e3-430e-bf8d-79529a974a88"))
    (comp (ref "C80")
      (value "100n")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Sim_DAC"))
      (property (name "Sheetfile") (value "sim_dac.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Sim_DAC/") (tstamps "/b78ec0ce-0ea7-4e81-bc06-3286ad54835a/"))
      (tstamps "1c8f7006-47aa-4ded-b347-8dff593e0a17"))
    (comp (ref "C81")
      (value "10u")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Sim_DAC"))
      (property (name "Sheetfile") (value "sim_dac.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Sim_DAC/") (tstamps "/b78ec0ce-0ea7-4e81-bc06-3286ad54835a/"))
      (tstamps "5f208268-34f0-4566-a0ba-da394a4df4e2"))
    (comp (ref "C82")
      (value "100n")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Sim_DAC"))
      (property (name "Sheetfile") (value "sim_dac.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Sim_DAC/") (tstamps "/b78ec0ce-0ea7-4e81-bc06-3286ad54835a/"))
      (tstamps "9f4b4737-c8e0-49c4-a84d-5abe63168631"))
    (comp (ref "C83")
      (value "1u")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Sim_DAC"))
      (property (name "Sheetfile") (value "sim_dac.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Sim_DAC/") (tstamps "/b78ec0ce-0ea7-4e81-bc06-3286ad54835a/"))
      (tstamps "5debdfdb-b83d-4309-b086-aef3c276ded2"))
    (comp (ref "C84")
      (value "100n")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Sim_DAC"))
      (property (name "Sheetfile") (value "sim_dac.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Sim_DAC/") (tstamps "/b78ec0ce-0ea7-4e81-bc06-3286ad54835a/"))
      (tstamps "1647250c-3e29-429b-aebb-c9b6eb702007"))
    (comp (ref "C85")
      (value "2.2u")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Sim_DAC"))
      (property (name "Sheetfile") (value "sim_dac.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Sim_DAC/") (tstamps "/b78ec0ce-0ea7-4e81-bc06-3286ad54835a/"))
      (tstamps "4d7fe4bc-5ed3-4e12-9aa0-84dc7321d045"))
    (comp (ref "C86")
      (value "1u")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Sim_DAC"))
      (property (name "Sheetfile") (value "sim_dac.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Sim_DAC/") (tstamps "/b78ec0ce-0ea7-4e81-bc06-3286ad54835a/"))
      (tstamps "6d64b973-082f-4eff-b61d-03d83bcada23"))
    (comp (ref "C87")
      (value "2.2u")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Sim_DAC"))
      (property (name "Sheetfile") (value "sim_dac.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Sim_DAC/") (tstamps "/b78ec0ce-0ea7-4e81-bc06-3286ad54835a/"))
      (tstamps "f8b25f81-ce3a-4315-8622-f8b05b28b1cd"))
    (comp (ref "C88")
      (value "2.2n")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Sim_DAC"))
      (property (name "Sheetfile") (value "sim_dac.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Sim_DAC/") (tstamps "/b78ec0ce-0ea7-4e81-bc06-3286ad54835a/"))
      (tstamps "daa48d22-ae21-419e-a342-f2f2e718445f"))
    (comp (ref "C89")
      (value "2.2u")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Sim_DAC"))
      (property (name "Sheetfile") (value "sim_dac.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Sim_DAC/") (tstamps "/b78ec0ce-0ea7-4e81-bc06-3286ad54835a/"))
      (tstamps "3935d4d7-854d-4830-8d3c-3d309c451cbc"))
    (comp (ref "C90")
      (value "2.2n")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Sim_DAC"))
      (property (name "Sheetfile") (value "sim_dac.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Sim_DAC/") (tstamps "/b78ec0ce-0ea7-4e81-bc06-3286ad54835a/"))
      (tstamps "733e41fb-0ecc-4b1a-9970-31fa61510f9e"))
    (comp (ref "FEB3")
      (value "200m")
      (datasheet "~")
      (description "Ferrite bead")
      (fields
        (field (name "Sim.Library") "FERRITE_BEAD.lib")
        (field (name "Sim.Name") "FERRITE_BEAD")
        (field (name "Sim.Device") "SUBCKT")
        (field (name "Sim.Pins") "1=1 2=2")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Ferrite bead"))
      (libsource (lib "Device") (part "FerriteBead") (description "Ferrite bead"))
      (property (name "Sim.Library") (value "FERRITE_BEAD.lib"))
      (property (name "Sim.Name") (value "FERRITE_BEAD"))
      (property (name "Sim.Device") (value "SUBCKT"))
      (property (name "Sim.Pins") (value "1=1 2=2"))
      (property (name "Sheetname") (value "Sim_DAC"))
      (property (name "Sheetfile") (value "sim_dac.kicad_sch"))
      (property (name "ki_keywords") (value "L ferrite bead inductor filter"))
      (property (name "ki_fp_filters") (value "Inductor_* L_* *Ferrite*"))
      (sheetpath (names "/Sim_DAC/") (tstamps "/b78ec0ce-0ea7-4e81-bc06-3286ad54835a/"))
      (tstamps "b315bdef-cba1-4916-8591-860f88e01c92"))
    (comp (ref "R39")
      (value "10k")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Sim_DAC"))
      (property (name "Sheetfile") (value "sim_dac.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Sim_DAC/") (tstamps "/b78ec0ce-0ea7-4e81-bc06-3286ad54835a/"))
      (tstamps "3c20b020-917b-41a2-8e0a-bc7c9c51bae6"))
    (comp (ref "R40")
      (value "10k")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Sim_DAC"))
      (property (name "Sheetfile") (value "sim_dac.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Sim_DAC/") (tstamps "/b78ec0ce-0ea7-4e81-bc06-3286ad54835a/"))
      (tstamps "41c44e2b-91b1-460b-bd73-52f75b72e0ab"))
    (comp (ref "R42")
      (value "47k")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Sim_DAC"))
      (property (name "Sheetfile") (value "sim_dac.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Sim_DAC/") (tstamps "/b78ec0ce-0ea7-4e81-bc06-3286ad54835a/"))
      (tstamps "59f52a35-21f0-4c33-9c8a-1724c9e6a0e6"))
    (comp (ref "R43")
      (value "470")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Sim_DAC"))
      (property (name "Sheetfile") (value "sim_dac.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Sim_DAC/") (tstamps "/b78ec0ce-0ea7-4e81-bc06-3286ad54835a/"))
      (tstamps "20143882-bcc9-4347-8168-925f114be670"))
    (comp (ref "R51")
      (value "470")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Sim_DAC"))
      (property (name "Sheetfile") (value "sim_dac.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Sim_DAC/") (tstamps "/b78ec0ce-0ea7-4e81-bc06-3286ad54835a/"))
      (tstamps "5ae78283-944b-472d-a5ff-9ab1f3241f2d"))
    (comp (ref "U17")
      (value "PCM5122PW")
      (footprint "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm")
      (datasheet "http://www.ti.com/lit/ds/symlink/pcm5122.pdf")
      (description "2VRMS DirectPath, 112dB Audio Stereo DAC with 32-bit, 384kHz PCM Interface, TSSOP-28")
      (fields
        (field (name "Sim.Library") "PCM5122.lib")
        (field (name "Sim.Name") "PCM5122")
        (field (name "Sim.Device") "SUBCKT")
        (field (name "Sim.Pins") "1=CPVDD 2=CAPP 3=CPGND 4=CAPM 5=VNEG 6=OUTL 7=OUTR 8=AVDD 9=AGND 10=VCOM_DEMP 11=SDA 12=SCL 13=GPIO5 14=GPIO4 15=GPIO3 16=ADR2 17=MODE1 18=MODE2 19=GPIO6 20=SCK 21=BCK 22=DIN 23=LRCK 24=ADR1 25=XSMT 26=LDOO 27=DGND 28=DVDD")
        (field (name "Footprint") "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm")
        (field (name "Datasheet") "http://www.ti.com/lit/ds/symlink/pcm5122.pdf")
        (field (name "Description") "2VRMS DirectPath, 112dB Audio Stereo DAC with 32-bit, 384kHz PCM Interface, TSSOP-28"))
      (libsource (lib "Audio") (part "PCM5122PW") (description "2VRMS DirectPath, 112dB Audio Stereo DAC with 32-bit, 384kHz PCM Interface, TSSOP-28"))
      (property (name "Sim.Library") (value "PCM5122.lib"))
      (property (name "Sim.Name") (value "PCM5122"))
      (property (name "Sim.Device") (value "SUBCKT"))
      (property (name "Sim.Pins") (value "1=CPVDD 2=CAPP 3=CPGND 4=CAPM 5=VNEG 6=OUTL 7=OUTR 8=AVDD 9=AGND 10=VCOM_DEMP 11=SDA 12=SCL 13=GPIO5 14=GPIO4 15=GPIO3 16=ADR2 17=MODE1 18=MODE2 19=GPIO6 20=SCK 21=BCK 22=DIN 23=LRCK 24=ADR1 25=XSMT 26=LDOO 27=DGND 28=DVDD"))
      (property (name "Sheetname") (value "Sim_DAC"))
      (property (name "Sheetfile") (value "sim_dac.kicad_sch"))
      (property (name "ki_keywords") (value "audio dac 2ch 32bit 384kHz"))
      (property (name "ki_fp_filters") (value "TSSOP*4.4x9.7mm*P0.65mm*"))
      (sheetpath (names "/Sim_DAC/") (tstamps "/b78ec0ce-0ea7-4e81-bc06-3286ad54835a/"))
      (tstamps "a28fe143-003b-4f87-983b-6d0f83a62b63"))
    (comp (ref "V2")
      (value "3.3")
      (datasheet "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#sec_Independent_Sources_for")
      (description "Voltage source, DC")
      (fields
        (field (name "Sim.Pins") "1=+ 2=-")
        (field (name "Sim.Type") "DC")
        (field (name "Sim.Device") "V")
        (field (name "Footprint"))
        (field (name "Datasheet") "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#sec_Independent_Sources_for")
        (field (name "Description") "Voltage source, DC"))
      (libsource (lib "Simulation_SPICE") (part "VDC") (description "Voltage source, DC"))
      (property (name "Sim.Pins") (value "1=+ 2=-"))
      (property (name "Sim.Type") (value "DC"))
      (property (name "Sim.Device") (value "V"))
      (property (name "Sheetname") (value "Sim_DAC"))
      (property (name "Sheetfile") (value "sim_dac.kicad_sch"))
      (property (name "ki_keywords") (value "simulation"))
      (sheetpath (names "/Sim_DAC/") (tstamps "/b78ec0ce-0ea7-4e81-bc06-3286ad54835a/"))
      (tstamps "49af8029-e2a1-48bf-922c-6c381ee6746a"))
    (comp (ref "V3")
      (value "3.3")
      (datasheet "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#sec_Independent_Sources_for")
      (description "Voltage source, DC")
      (fields
        (field (name "Sim.Pins") "1=+ 2=-")
        (field (name "Sim.Type") "DC")
        (field (name "Sim.Device") "V")
        (field (name "Footprint"))
        (field (name "Datasheet") "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#sec_Independent_Sources_for")
        (field (name "Description") "Voltage source, DC"))
      (libsource (lib "Simulation_SPICE") (part "VDC") (description "Voltage source, DC"))
      (property (name "Sim.Pins") (value "1=+ 2=-"))
      (property (name "Sim.Type") (value "DC"))
      (property (name "Sim.Device") (value "V"))
      (property (name "Sheetname") (value "Sim_DAC"))
      (property (name "Sheetfile") (value "sim_dac.kicad_sch"))
      (property (name "ki_keywords") (value "simulation"))
      (sheetpath (names "/Sim_DAC/") (tstamps "/b78ec0ce-0ea7-4e81-bc06-3286ad54835a/"))
      (tstamps "b862716e-e8bb-4d55-8145-9046f4ef8360"))
    (comp (ref "V4")
      (value "VSIN")
      (datasheet "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#sec_Independent_Sources_for")
      (description "Voltage source, sinusoidal")
      (fields
        (field (name "Sim.Pins") "1=+ 2=-")
        (field (name "Sim.Params") "dc=0 ampl=10m f=800k ac=0")
        (field (name "Sim.Type") "SIN")
        (field (name "Sim.Device") "V")
        (field (name "Footprint"))
        (field (name "Datasheet") "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#sec_Independent_Sources_for")
        (field (name "Description") "Voltage source, sinusoidal"))
      (libsource (lib "Simulation_SPICE") (part "VSIN") (description "Voltage source, sinusoidal"))
      (property (name "Sim.Pins") (value "1=+ 2=-"))
      (property (name "Sim.Params") (value "dc=0 ampl=10m f=800k ac=0"))
      (property (name "Sim.Type") (value "SIN"))
      (property (name "Sim.Device") (value "V"))
      (property (name "Sheetname") (value "Sim_DAC"))
      (property (name "Sheetfile") (value "sim_dac.kicad_sch"))
      (property (name "ki_keywords") (value "simulation ac vac"))
      (sheetpath (names "/Sim_DAC/") (tstamps "/b78ec0ce-0ea7-4e81-bc06-3286ad54835a/"))
      (tstamps "e5466045-0377-4dbf-acf1-237db9fa9c3a")))
  (libparts
    (libpart (lib "") (part "HR911130A_1")
      (docs "https://item.szlcsc.com/55426.html")
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "HR911130A")
        (field (name "Footprint") "footprint:RJ45-TH_HR911130A")
        (field (name "Datasheet") "https://item.szlcsc.com/55426.html")
        (field (name "Description"))
        (field (name "LCSC") "C54408"))
      (pins
        (pin (num "1") (name "P1") (type "output"))
        (pin (num "2") (name "MDI0+") (type "input"))
        (pin (num "3") (name "MDI0-") (type "input"))
        (pin (num "4") (name "MDI1+") (type "input"))
        (pin (num "5") (name "MDI2+") (type "input"))
        (pin (num "6") (name "MDI2-") (type "input"))
        (pin (num "7") (name "MDI1-") (type "input"))
        (pin (num "8") (name "MDI3+") (type "input"))
        (pin (num "9") (name "MDI3-") (type "input"))
        (pin (num "10") (name "P10") (type "power_in"))
        (pin (num "11") (name "11") (type "passive"))
        (pin (num "12") (name "12") (type "passive"))
        (pin (num "13") (name "13") (type "passive"))
        (pin (num "14") (name "14") (type "passive"))
        (pin (num "SHIELD0") (name "SHIELD0") (type "passive"))
        (pin (num "SHIELD1") (name "SHIELD1") (type "passive"))))
    (libpart (lib "74HC4067PW,118") (part "74HC4067PW,118")
      (docs "https://item.szlcsc.com/6601.html")
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "74HC4067PW,118")
        (field (name "Footprint") "footprint:TSSOP-24_L7.8-W4.4-P0.65-LS6.4-BL")
        (field (name "Datasheet") "https://item.szlcsc.com/6601.html")
        (field (name "Description"))
        (field (name "LCSC") "C179326"))
      (pins
        (pin (num "1") (name "Z") (type "unspecified"))
        (pin (num "2") (name "Y7") (type "unspecified"))
        (pin (num "3") (name "Y6") (type "unspecified"))
        (pin (num "4") (name "Y5") (type "unspecified"))
        (pin (num "5") (name "Y4") (type "unspecified"))
        (pin (num "6") (name "Y3") (type "unspecified"))
        (pin (num "7") (name "Y2") (type "unspecified"))
        (pin (num "8") (name "Y1") (type "unspecified"))
        (pin (num "9") (name "Y0") (type "unspecified"))
        (pin (num "10") (name "S0") (type "unspecified"))
        (pin (num "11") (name "S1") (type "unspecified"))
        (pin (num "12") (name "GND") (type "unspecified"))
        (pin (num "13") (name "S3") (type "unspecified"))
        (pin (num "14") (name "S2") (type "unspecified"))
        (pin (num "15") (name "E#") (type "unspecified"))
        (pin (num "16") (name "Y15") (type "unspecified"))
        (pin (num "17") (name "Y14") (type "unspecified"))
        (pin (num "18") (name "Y13") (type "unspecified"))
        (pin (num "19") (name "Y12") (type "unspecified"))
        (pin (num "20") (name "Y11") (type "unspecified"))
        (pin (num "21") (name "Y10") (type "unspecified"))
        (pin (num "22") (name "Y9") (type "unspecified"))
        (pin (num "23") (name "Y8") (type "unspecified"))
        (pin (num "24") (name "VCC") (type "unspecified"))))
    (libpart (lib "AP2553W6-7") (part "AP2553W6-7")
      (docs "https://item.szlcsc.com/211080.html")
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "AP2553W6-7")
        (field (name "Footprint") "footprint:SOT-26_L3.0-W1.6-P0.95-LS2.8-BL")
        (field (name "Datasheet") "https://item.szlcsc.com/211080.html")
        (field (name "Description"))
        (field (name "LCSC") "C212302"))
      (pins
        (pin (num "1") (name "IN") (type "unspecified"))
        (pin (num "2") (name "GND") (type "unspecified"))
        (pin (num "3") (name "EN") (type "unspecified"))
        (pin (num "4") (name "FAULT") (type "unspecified"))
        (pin (num "5") (name "ILIM") (type "unspecified"))
        (pin (num "6") (name "OUT") (type "unspecified"))))
    (libpart (lib "Audio") (part "PCM5122PW")
      (description "2VRMS DirectPath, 112dB Audio Stereo DAC with 32-bit, 384kHz PCM Interface, TSSOP-28")
      (docs "http://www.ti.com/lit/ds/symlink/pcm5122.pdf")
      (footprints
        (fp "TSSOP*4.4x9.7mm*P0.65mm*"))
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "PCM5122PW")
        (field (name "Footprint") "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm")
        (field (name "Datasheet") "http://www.ti.com/lit/ds/symlink/pcm5122.pdf")
        (field (name "Description") "2VRMS DirectPath, 112dB Audio Stereo DAC with 32-bit, 384kHz PCM Interface, TSSOP-28"))
      (pins
        (pin (num "1") (name "CPVDD") (type "power_in"))
        (pin (num "2") (name "CAPP") (type "passive"))
        (pin (num "3") (name "CPGND") (type "power_in"))
        (pin (num "4") (name "CAPM") (type "passive"))
        (pin (num "5") (name "VNEG") (type "passive"))
        (pin (num "6") (name "OUTL") (type "output"))
        (pin (num "7") (name "OUTR") (type "output"))
        (pin (num "8") (name "AVDD") (type "power_in"))
        (pin (num "9") (name "AGND") (type "power_in"))
        (pin (num "10") (name "VCOM/DEMP") (type "bidirectional"))
        (pin (num "11") (name "SDA/MOSI/ATT2") (type "bidirectional"))
        (pin (num "12") (name "SCL/MC/ATT1") (type "input"))
        (pin (num "13") (name "GPIO5/ATT0") (type "bidirectional"))
        (pin (num "14") (name "GPIO4/MAST") (type "bidirectional"))
        (pin (num "15") (name "GPIO3/AGNS") (type "bidirectional"))
        (pin (num "16") (name "ADR2/GPIO2/DOUT") (type "bidirectional"))
        (pin (num "17") (name "MODE1") (type "input"))
        (pin (num "18") (name "MODE2/MS") (type "input"))
        (pin (num "19") (name "GPIO6/FLT") (type "bidirectional"))
        (pin (num "20") (name "SCK") (type "input"))
        (pin (num "21") (name "BCK") (type "bidirectional"))
        (pin (num "22") (name "DIN") (type "input"))
        (pin (num "23") (name "LRCK") (type "bidirectional"))
        (pin (num "24") (name "ADR1/MISO/FMT") (type "bidirectional"))
        (pin (num "25") (name "XSMT") (type "input"))
        (pin (num "26") (name "LDOO") (type "passive"))
        (pin (num "27") (name "DGND") (type "power_in"))
        (pin (num "28") (name "DVDD") (type "power_in"))))
    (libpart (lib "CR2032-BS-6-1") (part "CR2032-BS-6-1")
      (docs "https://item.szlcsc.com/71472.html")
      (fields
        (field (name "Reference") "B")
        (field (name "Value") "CR2032-BS-6-1")
        (field (name "Footprint") "footprint:BAT-TH_CR2032-BS-6-1")
        (field (name "Datasheet") "https://item.szlcsc.com/71472.html")
        (field (name "Description"))
        (field (name "LCSC") "C70377"))
      (pins
        (pin (num "1") (name "1") (type "input"))
        (pin (num "2") (name "2") (type "input"))))
    (libpart (lib "Connector") (part "HDMI_D_1.4")
      (description "HDMI 1.4+ type D connector")
      (docs "http://pinoutguide.com/PortableDevices/micro_hdmi_type_d_pinout.shtml")
      (footprints
        (fp "HDMI*D*"))
      (fields
        (field (name "Reference") "J")
        (field (name "Value") "HDMI_D_1.4")
        (field (name "Footprint"))
        (field (name "Datasheet") "http://pinoutguide.com/PortableDevices/micro_hdmi_type_d_pinout.shtml")
        (field (name "Description") "HDMI 1.4+ type D connector"))
      (pins
        (pin (num "1") (name "HPD/HEAC-") (type "passive"))
        (pin (num "2") (name "UTILITY/HEAC+") (type "passive"))
        (pin (num "3") (name "D2+") (type "passive"))
        (pin (num "4") (name "D2S") (type "power_in"))
        (pin (num "5") (name "D2-") (type "passive"))
        (pin (num "6") (name "D1+") (type "passive"))
        (pin (num "7") (name "D1S") (type "power_in"))
        (pin (num "8") (name "D1-") (type "passive"))
        (pin (num "9") (name "D0+") (type "passive"))
        (pin (num "10") (name "D0S") (type "power_in"))
        (pin (num "11") (name "D0-") (type "passive"))
        (pin (num "12") (name "CK+") (type "passive"))
        (pin (num "13") (name "CKS") (type "power_in"))
        (pin (num "14") (name "CK-") (type "passive"))
        (pin (num "15") (name "CEC") (type "bidirectional"))
        (pin (num "16") (name "GND") (type "power_in"))
        (pin (num "17") (name "SCL") (type "passive"))
        (pin (num "18") (name "SDA") (type "bidirectional"))
        (pin (num "19") (name "+5V") (type "power_in"))
        (pin (num "SH") (name "SH") (type "passive"))))
    (libpart (lib "Connector") (part "TestPoint")
      (description "test point")
      (docs "~")
      (footprints
        (fp "Pin*")
        (fp "Test*"))
      (fields
        (field (name "Reference") "TP")
        (field (name "Value") "TestPoint")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (pins
        (pin (num "1") (name "1") (type "passive"))))
    (libpart (lib "Connector") (part "USB3_A")
      (description "USB 3.0 A connector")
      (docs "~")
      (footprints
        (fp "USB3*"))
      (fields
        (field (name "Reference") "J")
        (field (name "Value") "USB3_A")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "USB 3.0 A connector"))
      (pins
        (pin (num "1") (name "VBUS") (type "power_in"))
        (pin (num "2") (name "D-") (type "bidirectional"))
        (pin (num "3") (name "D+") (type "bidirectional"))
        (pin (num "4") (name "GND") (type "power_in"))
        (pin (num "5") (name "SSRX-") (type "output"))
        (pin (num "6") (name "SSRX+") (type "output"))
        (pin (num "7") (name "DRAIN") (type "passive"))
        (pin (num "8") (name "SSTX-") (type "input"))
        (pin (num "9") (name "SSTX+") (type "input"))
        (pin (num "10") (name "SHIELD") (type "passive"))))
    (libpart (lib "Connector") (part "USB_A")
      (description "USB Type A connector")
      (docs "~")
      (footprints
        (fp "USB*"))
      (fields
        (field (name "Reference") "J")
        (field (name "Value") "USB_A")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "USB Type A connector"))
      (pins
        (pin (num "1") (name "VBUS") (type "power_in"))
        (pin (num "2") (name "D-") (type "bidirectional"))
        (pin (num "3") (name "D+") (type "bidirectional"))
        (pin (num "4") (name "GND") (type "power_in"))
        (pin (num "5") (name "Shield") (type "passive"))))
    (libpart (lib "Connector_Generic") (part "Conn_01x04")
      (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs "~")
      (footprints
        (fp "Connector*:*_1x??_*"))
      (fields
        (field (name "Reference") "J")
        (field (name "Value") "Conn_01x04")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (pins
        (pin (num "1") (name "Pin_1") (type "passive"))
        (pin (num "2") (name "Pin_2") (type "passive"))
        (pin (num "3") (name "Pin_3") (type "passive"))
        (pin (num "4") (name "Pin_4") (type "passive"))))
    (libpart (lib "Connector_Generic") (part "Conn_01x05")
      (description "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs "~")
      (footprints
        (fp "Connector*:*_1x??_*"))
      (fields
        (field (name "Reference") "J")
        (field (name "Value") "Conn_01x05")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (pins
        (pin (num "1") (name "Pin_1") (type "passive"))
        (pin (num "2") (name "Pin_2") (type "passive"))
        (pin (num "3") (name "Pin_3") (type "passive"))
        (pin (num "4") (name "Pin_4") (type "passive"))
        (pin (num "5") (name "Pin_5") (type "passive"))))
    (libpart (lib "Connector_Generic") (part "Conn_01x06")
      (description "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs "~")
      (footprints
        (fp "Connector*:*_1x??_*"))
      (fields
        (field (name "Reference") "J")
        (field (name "Value") "Conn_01x06")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (pins
        (pin (num "1") (name "Pin_1") (type "passive"))
        (pin (num "2") (name "Pin_2") (type "passive"))
        (pin (num "3") (name "Pin_3") (type "passive"))
        (pin (num "4") (name "Pin_4") (type "passive"))
        (pin (num "5") (name "Pin_5") (type "passive"))
        (pin (num "6") (name "Pin_6") (type "passive"))))
    (libpart (lib "Connector_Generic") (part "Conn_01x08")
      (description "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs "~")
      (footprints
        (fp "Connector*:*_1x??_*"))
      (fields
        (field (name "Reference") "J")
        (field (name "Value") "Conn_01x08")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (pins
        (pin (num "1") (name "Pin_1") (type "passive"))
        (pin (num "2") (name "Pin_2") (type "passive"))
        (pin (num "3") (name "Pin_3") (type "passive"))
        (pin (num "4") (name "Pin_4") (type "passive"))
        (pin (num "5") (name "Pin_5") (type "passive"))
        (pin (num "6") (name "Pin_6") (type "passive"))
        (pin (num "7") (name "Pin_7") (type "passive"))
        (pin (num "8") (name "Pin_8") (type "passive"))))
    (libpart (lib "Connector_Generic") (part "Conn_01x10")
      (description "Generic connector, single row, 01x10, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs "~")
      (footprints
        (fp "Connector*:*_1x??_*"))
      (fields
        (field (name "Reference") "J")
        (field (name "Value") "Conn_01x10")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Generic connector, single row, 01x10, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (pins
        (pin (num "1") (name "Pin_1") (type "passive"))
        (pin (num "2") (name "Pin_2") (type "passive"))
        (pin (num "3") (name "Pin_3") (type "passive"))
        (pin (num "4") (name "Pin_4") (type "passive"))
        (pin (num "5") (name "Pin_5") (type "passive"))
        (pin (num "6") (name "Pin_6") (type "passive"))
        (pin (num "7") (name "Pin_7") (type "passive"))
        (pin (num "8") (name "Pin_8") (type "passive"))
        (pin (num "9") (name "Pin_9") (type "passive"))
        (pin (num "10") (name "Pin_10") (type "passive"))))
    (libpart (lib "Connector_Generic") (part "Conn_01x12")
      (description "Generic connector, single row, 01x12, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs "~")
      (footprints
        (fp "Connector*:*_1x??_*"))
      (fields
        (field (name "Reference") "J")
        (field (name "Value") "Conn_01x12")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Generic connector, single row, 01x12, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (pins
        (pin (num "1") (name "Pin_1") (type "passive"))
        (pin (num "2") (name "Pin_2") (type "passive"))
        (pin (num "3") (name "Pin_3") (type "passive"))
        (pin (num "4") (name "Pin_4") (type "passive"))
        (pin (num "5") (name "Pin_5") (type "passive"))
        (pin (num "6") (name "Pin_6") (type "passive"))
        (pin (num "7") (name "Pin_7") (type "passive"))
        (pin (num "8") (name "Pin_8") (type "passive"))
        (pin (num "9") (name "Pin_9") (type "passive"))
        (pin (num "10") (name "Pin_10") (type "passive"))
        (pin (num "11") (name "Pin_11") (type "passive"))
        (pin (num "12") (name "Pin_12") (type "passive"))))
    (libpart (lib "DSWB05LHGET") (part "DSWB05LHGET")
      (docs "https://so.szlcsc.com/global.html?c=&k=C126889")
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "DSWB05LHGET")
        (field (name "Footprint") "footprint:SW-TH_DSWB05LHGET")
        (field (name "Datasheet") "https://so.szlcsc.com/global.html?c=&k=C126889")
        (field (name "Description"))
        (field (name "LCSC") "C126889"))
      (pins
        (pin (num "1") (name "A1") (type "input"))
        (pin (num "2") (name "A2") (type "input"))
        (pin (num "3") (name "A3") (type "input"))
        (pin (num "4") (name "A4") (type "input"))
        (pin (num "5") (name "A5") (type "input"))
        (pin (num "6") (name "B5") (type "input"))
        (pin (num "7") (name "B4") (type "input"))
        (pin (num "8") (name "B3") (type "input"))
        (pin (num "9") (name "B2") (type "input"))
        (pin (num "10") (name "B1") (type "input"))))
    (libpart (lib "Device") (part "C")
      (description "Unpolarized capacitor")
      (docs "~")
      (footprints
        (fp "C_*"))
      (fields
        (field (name "Reference") "C")
        (field (name "Value") "C")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "Device") (part "C_Small")
      (description "Unpolarized capacitor, small symbol")
      (docs "~")
      (footprints
        (fp "C_*"))
      (fields
        (field (name "Reference") "C")
        (field (name "Value") "C_Small")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "Device") (part "FerriteBead")
      (description "Ferrite bead")
      (docs "~")
      (footprints
        (fp "Inductor_*")
        (fp "L_*")
        (fp "*Ferrite*"))
      (fields
        (field (name "Reference") "FB")
        (field (name "Value") "FerriteBead")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Ferrite bead"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "Device") (part "L")
      (description "Inductor")
      (docs "~")
      (footprints
        (fp "Choke_*")
        (fp "*Coil*")
        (fp "Inductor_*")
        (fp "L_*"))
      (fields
        (field (name "Reference") "L")
        (field (name "Value") "L")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Inductor"))
      (pins
        (pin (num "1") (name "1") (type "passive"))
        (pin (num "2") (name "2") (type "passive"))))
    (libpart (lib "Device") (part "LED")
      (description "Light emitting diode")
      (docs "~")
      (footprints
        (fp "LED*")
        (fp "LED_SMD:*")
        (fp "LED_THT:*"))
      (fields
        (field (name "Reference") "D")
        (field (name "Value") "LED")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Light emitting diode")
        (field (name "Sim.Pins") "1=K 2=A"))
      (pins
        (pin (num "1") (name "K") (type "passive"))
        (pin (num "2") (name "A") (type "passive"))))
    (libpart (lib "Device") (part "R")
      (description "Resistor")
      (docs "~")
      (footprints
        (fp "R_*"))
      (fields
        (field (name "Reference") "R")
        (field (name "Value") "R")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "Interface_USB") (part "CH224K")
      (description "100W USB Type-C PD3.0/2.0, BC1.2 Sink Controller, SSOP-10")
      (docs "https://www.wch.cn/downloads/file/301.html")
      (footprints
        (fp "SSOP*3.9x4.9mm*P1mm*EP2.1x3.3mm*"))
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "CH224K")
        (field (name "Footprint") "Package_SO:SSOP-10-1EP_3.9x4.9mm_P1mm_EP2.1x3.3mm")
        (field (name "Datasheet") "https://www.wch.cn/downloads/file/301.html")
        (field (name "Description") "100W USB Type-C PD3.0/2.0, BC1.2 Sink Controller, SSOP-10"))
      (pins
        (pin (num "1") (name "VDD") (type "power_in"))
        (pin (num "2") (name "CFG2") (type "passive"))
        (pin (num "3") (name "CFG3") (type "passive"))
        (pin (num "4") (name "DP") (type "bidirectional"))
        (pin (num "5") (name "DM") (type "bidirectional"))
        (pin (num "6") (name "CC2") (type "bidirectional"))
        (pin (num "7") (name "CC1") (type "bidirectional"))
        (pin (num "8") (name "VBUS") (type "passive"))
        (pin (num "9") (name "CFG1") (type "passive"))
        (pin (num "10") (name "PG") (type "open_collector"))
        (pin (num "11") (name "GND") (type "power_in"))))
    (libpart (lib "KT-0603R") (part "KT-0603R")
      (docs "https://item.szlcsc.com/347874.html")
      (fields
        (field (name "Reference") "LED")
        (field (name "Value") "KT-0603R")
        (field (name "Footprint") "footprint:LED0603-RD")
        (field (name "Datasheet") "https://item.szlcsc.com/347874.html")
        (field (name "Description"))
        (field (name "LCSC") "C2286"))
      (pins
        (pin (num "1") (name "K") (type "unspecified"))
        (pin (num "2") (name "A") (type "unspecified"))))
    (libpart (lib "MCP23017T-E/SS") (part "MCP23017T-E/SS")
      (docs "https://item.szlcsc.com/397275.html")
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "MCP23017T-E{slash}SS")
        (field (name "Footprint") "footprint:SSOP-28_L10.2-W5.3-P0.65-LS7.8-BL")
        (field (name "Datasheet") "https://item.szlcsc.com/397275.html")
        (field (name "Description"))
        (field (name "LCSC") "C558584"))
      (pins
        (pin (num "1") (name "GPB0") (type "unspecified"))
        (pin (num "2") (name "GPB1") (type "unspecified"))
        (pin (num "3") (name "GPB2") (type "unspecified"))
        (pin (num "4") (name "GPB3") (type "unspecified"))
        (pin (num "5") (name "GPB4") (type "unspecified"))
        (pin (num "6") (name "GPB5") (type "unspecified"))
        (pin (num "7") (name "GPB6") (type "unspecified"))
        (pin (num "8") (name "GPB7") (type "unspecified"))
        (pin (num "9") (name "VDD") (type "unspecified"))
        (pin (num "10") (name "VSS") (type "unspecified"))
        (pin (num "11") (name "NC") (type "unspecified"))
        (pin (num "12") (name "SCK") (type "unspecified"))
        (pin (num "13") (name "SDA") (type "unspecified"))
        (pin (num "14") (name "NC") (type "unspecified"))
        (pin (num "15") (name "A0") (type "unspecified"))
        (pin (num "16") (name "A1") (type "unspecified"))
        (pin (num "17") (name "A2") (type "unspecified"))
        (pin (num "18") (name "RESET#") (type "unspecified"))
        (pin (num "19") (name "INTB") (type "unspecified"))
        (pin (num "20") (name "INTA") (type "unspecified"))
        (pin (num "21") (name "GPA0") (type "unspecified"))
        (pin (num "22") (name "GPA1") (type "unspecified"))
        (pin (num "23") (name "GPA2") (type "unspecified"))
        (pin (num "24") (name "GPA3") (type "unspecified"))
        (pin (num "25") (name "GPA4") (type "unspecified"))
        (pin (num "26") (name "GPA5") (type "unspecified"))
        (pin (num "27") (name "GPA6") (type "unspecified"))
        (pin (num "28") (name "GPA7") (type "unspecified"))))
    (libpart (lib "MCU_Microchip_ATmega") (part "ATmega32U4-A")
      (description "16MHz, 32kB Flash, 2.5kB SRAM, 1kB EEPROM, USB 2.0, TQFP-44")
      (docs "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-7766-8-bit-AVR-ATmega16U4-32U4_Datasheet.pdf")
      (footprints
        (fp "TQFP*10x10mm*P0.8mm*"))
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "ATmega32U4-A")
        (field (name "Footprint") "Package_QFP:TQFP-44_10x10mm_P0.8mm")
        (field (name "Datasheet") "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-7766-8-bit-AVR-ATmega16U4-32U4_Datasheet.pdf")
        (field (name "Description") "16MHz, 32kB Flash, 2.5kB SRAM, 1kB EEPROM, USB 2.0, TQFP-44"))
      (pins
        (pin (num "1") (name "PE6") (type "bidirectional"))
        (pin (num "2") (name "UVCC") (type "power_in"))
        (pin (num "3") (name "D-") (type "bidirectional"))
        (pin (num "4") (name "D+") (type "bidirectional"))
        (pin (num "5") (name "UGND") (type "passive"))
        (pin (num "6") (name "UCAP") (type "passive"))
        (pin (num "7") (name "VBUS") (type "input"))
        (pin (num "8") (name "PB0") (type "bidirectional"))
        (pin (num "9") (name "PB1") (type "bidirectional"))
        (pin (num "10") (name "PB2") (type "bidirectional"))
        (pin (num "11") (name "PB3") (type "bidirectional"))
        (pin (num "12") (name "PB7") (type "bidirectional"))
        (pin (num "13") (name "~{RESET}") (type "input"))
        (pin (num "14") (name "VCC") (type "power_in"))
        (pin (num "15") (name "GND") (type "power_in"))
        (pin (num "16") (name "XTAL2") (type "output"))
        (pin (num "17") (name "XTAL1") (type "input"))
        (pin (num "18") (name "PD0") (type "bidirectional"))
        (pin (num "19") (name "PD1") (type "bidirectional"))
        (pin (num "20") (name "PD2") (type "bidirectional"))
        (pin (num "21") (name "PD3") (type "bidirectional"))
        (pin (num "22") (name "PD5") (type "bidirectional"))
        (pin (num "23") (name "GND") (type "passive"))
        (pin (num "24") (name "AVCC") (type "power_in"))
        (pin (num "25") (name "PD4") (type "bidirectional"))
        (pin (num "26") (name "PD6") (type "bidirectional"))
        (pin (num "27") (name "PD7") (type "bidirectional"))
        (pin (num "28") (name "PB4") (type "bidirectional"))
        (pin (num "29") (name "PB5") (type "bidirectional"))
        (pin (num "30") (name "PB6") (type "bidirectional"))
        (pin (num "31") (name "PC6") (type "bidirectional"))
        (pin (num "32") (name "PC7") (type "bidirectional"))
        (pin (num "33") (name "~{HWB}/PE2") (type "bidirectional"))
        (pin (num "34") (name "VCC") (type "passive"))
        (pin (num "35") (name "GND") (type "passive"))
        (pin (num "36") (name "PF7") (type "bidirectional"))
        (pin (num "37") (name "PF6") (type "bidirectional"))
        (pin (num "38") (name "PF5") (type "bidirectional"))
        (pin (num "39") (name "PF4") (type "bidirectional"))
        (pin (num "40") (name "PF1") (type "bidirectional"))
        (pin (num "41") (name "PF0") (type "bidirectional"))
        (pin (num "42") (name "AREF") (type "passive"))
        (pin (num "43") (name "GND") (type "passive"))
        (pin (num "44") (name "AVCC") (type "passive"))))
    (libpart (lib "Mechanical") (part "MountingHole")
      (description "Mounting Hole without connection")
      (docs "~")
      (footprints
        (fp "MountingHole*"))
      (fields
        (field (name "Reference") "H")
        (field (name "Value") "MountingHole")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Mounting Hole without connection")))
    (libpart (lib "PCM_JLCPCB-Capacitors") (part "0402,100nF")
      (description "16V 100nF X7R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
      (docs "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05B104KO5NNNC_C1525.pdf")
      (footprints
        (fp "C_*"))
      (fields
        (field (name "Reference") "C")
        (field (name "Value") "100nF")
        (field (name "Footprint") "PCM_JLCPCB:C_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05B104KO5NNNC_C1525.pdf")
        (field (name "Description") "16V 100nF X7R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
        (field (name "LCSC") "C1525")
        (field (name "Stock") "20208285")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT")
        (field (name "Manufacturer") "Samsung Electro-Mechanics")
        (field (name "Part") "CL05B104KO5NNNC")
        (field (name "Voltage Rated") "16V")
        (field (name "Tolerance") "±10%")
        (field (name "Capacitance") "100nF")
        (field (name "Temperature Coefficient") "X7R"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "PCM_JLCPCB-Capacitors") (part "0402,100nF,(2)")
      (description "50V 100nF X7R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
      (docs "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05B104KB54PNC_C307331.pdf")
      (footprints
        (fp "C_*"))
      (fields
        (field (name "Reference") "C")
        (field (name "Value") "100nF")
        (field (name "Footprint") "PCM_JLCPCB:C_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05B104KB54PNC_C307331.pdf")
        (field (name "Description") "50V 100nF X7R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
        (field (name "LCSC") "C307331")
        (field (name "Stock") "8389599")
        (field (name "Price") "0.008USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT")
        (field (name "Manufacturer") "Samsung Electro-Mechanics")
        (field (name "Part") "CL05B104KB54PNC")
        (field (name "Voltage Rated") "50V")
        (field (name "Tolerance") "±10%")
        (field (name "Capacitance") "100nF")
        (field (name "Temperature Coefficient") "X7R"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "PCM_JLCPCB-Capacitors") (part "0402,100pF")
      (description "50V 100pF C0G ±5% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
      (docs "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_FH--Guangdong-Fenghua-Advanced-Tech-0402CG101J500NT_C1546.pdf")
      (footprints
        (fp "C_*"))
      (fields
        (field (name "Reference") "C")
        (field (name "Value") "100pF")
        (field (name "Footprint") "PCM_JLCPCB:C_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_FH--Guangdong-Fenghua-Advanced-Tech-0402CG101J500NT_C1546.pdf")
        (field (name "Description") "50V 100pF C0G ±5% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
        (field (name "LCSC") "C1546")
        (field (name "Stock") "2554383")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT")
        (field (name "Manufacturer") "FH(Guangdong Fenghua Advanced Tech)")
        (field (name "Part") "0402CG101J500NT")
        (field (name "Voltage Rated") "50V")
        (field (name "Tolerance") "±5%")
        (field (name "Capacitance") "100pF")
        (field (name "Temperature Coefficient") "C0G"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "PCM_JLCPCB-Capacitors") (part "0402,1uF")
      (description "25V 1uF X5R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
      (docs "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05A105KA5NQNC_C52923.pdf")
      (footprints
        (fp "C_*"))
      (fields
        (field (name "Reference") "C")
        (field (name "Value") "1uF")
        (field (name "Footprint") "PCM_JLCPCB:C_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05A105KA5NQNC_C52923.pdf")
        (field (name "Description") "25V 1uF X5R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
        (field (name "LCSC") "C52923")
        (field (name "Stock") "7021828")
        (field (name "Price") "0.006USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT")
        (field (name "Manufacturer") "Samsung Electro-Mechanics")
        (field (name "Part") "CL05A105KA5NQNC")
        (field (name "Voltage Rated") "25V")
        (field (name "Tolerance") "±10%")
        (field (name "Capacitance") "1uF")
        (field (name "Temperature Coefficient") "X5R"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "PCM_JLCPCB-Capacitors") (part "0402,2.2uF")
      (description "6.3V 2.2uF X5R ±20% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
      (docs "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05A225MQ5NSNC_C12530.pdf")
      (footprints
        (fp "C_*"))
      (fields
        (field (name "Reference") "C")
        (field (name "Value") "2.2uF")
        (field (name "Footprint") "PCM_JLCPCB:C_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05A225MQ5NSNC_C12530.pdf")
        (field (name "Description") "6.3V 2.2uF X5R ±20% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
        (field (name "LCSC") "C12530")
        (field (name "Stock") "4528431")
        (field (name "Price") "0.006USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT")
        (field (name "Manufacturer") "Samsung Electro-Mechanics")
        (field (name "Part") "CL05A225MQ5NSNC")
        (field (name "Voltage Rated") "6.3V")
        (field (name "Tolerance") "±20%")
        (field (name "Capacitance") "2.2uF")
        (field (name "Temperature Coefficient") "X5R"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "PCM_JLCPCB-Capacitors") (part "0805,10uF")
      (description "25V 10uF X5R ±10% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
      (docs "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL21A106KAYNNNE_C15850.pdf")
      (footprints
        (fp "C_*"))
      (fields
        (field (name "Reference") "C")
        (field (name "Value") "10uF")
        (field (name "Footprint") "PCM_JLCPCB:C_0805")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL21A106KAYNNNE_C15850.pdf")
        (field (name "Description") "25V 10uF X5R ±10% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
        (field (name "LCSC") "C15850")
        (field (name "Stock") "6525809")
        (field (name "Price") "0.014USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT")
        (field (name "Manufacturer") "Samsung Electro-Mechanics")
        (field (name "Part") "CL21A106KAYNNNE")
        (field (name "Voltage Rated") "25V")
        (field (name "Tolerance") "±10%")
        (field (name "Capacitance") "10uF")
        (field (name "Temperature Coefficient") "X5R"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "PCM_JLCPCB-Capacitors") (part "0805,10uF,(2)")
      (description "50V 10uF X5R ±10% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
      (docs "https://www.lcsc.com/datasheet/lcsc_datasheet_2411041759_Murata-Electronics-GRM21BR61H106KE43L_C440198.pdf")
      (footprints
        (fp "C_*"))
      (fields
        (field (name "Reference") "C")
        (field (name "Value") "10uF")
        (field (name "Footprint") "PCM_JLCPCB:C_0805")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2411041759_Murata-Electronics-GRM21BR61H106KE43L_C440198.pdf")
        (field (name "Description") "50V 10uF X5R ±10% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
        (field (name "LCSC") "C440198")
        (field (name "Stock") "1422246")
        (field (name "Price") "0.066USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "5")
        (field (name "Attrition Qty") "4")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT")
        (field (name "Manufacturer") "Murata Electronics")
        (field (name "Part") "GRM21BR61H106KE43L")
        (field (name "Voltage Rated") "50V")
        (field (name "Tolerance") "±10%")
        (field (name "Capacitance") "10uF")
        (field (name "Temperature Coefficient") "X5R"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "PCM_JLCPCB-Capacitors") (part "0805,22uF")
      (description "25V 22uF X5R ±20% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
      (docs "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL21A226MAQNNNE_C45783.pdf")
      (footprints
        (fp "C_*"))
      (fields
        (field (name "Reference") "C")
        (field (name "Value") "22uF")
        (field (name "Footprint") "PCM_JLCPCB:C_0805")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL21A226MAQNNNE_C45783.pdf")
        (field (name "Description") "25V 22uF X5R ±20% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
        (field (name "LCSC") "C45783")
        (field (name "Stock") "6479946")
        (field (name "Price") "0.027USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "8")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT")
        (field (name "Manufacturer") "Samsung Electro-Mechanics")
        (field (name "Part") "CL21A226MAQNNNE")
        (field (name "Voltage Rated") "25V")
        (field (name "Tolerance") "±20%")
        (field (name "Capacitance") "22uF")
        (field (name "Temperature Coefficient") "X5R"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "PCM_JLCPCB-Crystals") (part "Crystal, 16MHz, 9pF")
      (description "16MHz Surface Mount Crystal 9pF ±10ppm ±20ppm SMD3225-4P Crystals ROHS")
      (docs "https://www.lcsc.com/datasheet/lcsc_datasheet_2403291504_YXC-Crystal-Oscillators-X322516MLB4SI_C13738.pdf")
      (fields
        (field (name "Reference") "X")
        (field (name "Value") "X322516MLB4SI")
        (field (name "Footprint") "PCM_JLCPCB:OSC-SMD_4P-L3.2-W2.5-BL")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2403291504_YXC-Crystal-Oscillators-X322516MLB4SI_C13738.pdf")
        (field (name "Description") "16MHz Surface Mount Crystal 9pF ±10ppm ±20ppm SMD3225-4P Crystals ROHS")
        (field (name "LCSC") "C13738")
        (field (name "Stock") "162087")
        (field (name "Price") "0.068USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "5")
        (field (name "Attrition Qty") "4")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Crystals/Oscillators/Resonators,Crystals")
        (field (name "Manufacturer") "Yangxing Tech")
        (field (name "Part") "X322516MLB4SI")
        (field (name "Frequency") "16MHz")
        (field (name "Frequency Stability") "±20ppm")
        (field (name "Operating Temperature") "-40°C~+85°C")
        (field (name "Frequency Tolerance") "±10ppm")
        (field (name "Crystal Type") "SMD Crystal Resonator")
        (field (name "Load Capacitance") "9pF")
        (field (name "Normal Temperature Frequency Tolerance") "±10ppm")
        (field (name "Type") "Surface Mount Crystal"))
      (pins
        (pin (num "1") (name "OSC") (type "unspecified"))
        (pin (num "2") (name "GND") (type "unspecified"))
        (pin (num "3") (name "OSC") (type "unspecified"))
        (pin (num "4") (name "GND") (type "unspecified"))))
    (libpart (lib "PCM_JLCPCB-Diodes") (part "Zener,BZT52C3V3S")
      (description "Independent Type 200mW 3.1V~3.5V 3.3V SOD-323 Zener Diodes ROHS")
      (docs "https://wmsc.lcsc.com/wmsc/upload/file/pdf/v2/lcsc/2403280505_hongjiacheng-BZT52C3V3S_C19077437.pdf")
      (footprints
        (fp "D_*"))
      (fields
        (field (name "Reference") "D")
        (field (name "Value") "BZT52C3V3S")
        (field (name "Footprint") "PCM_JLCPCB:D_SOD-323")
        (field (name "Datasheet") "https://wmsc.lcsc.com/wmsc/upload/file/pdf/v2/lcsc/2403280505_hongjiacheng-BZT52C3V3S_C19077437.pdf")
        (field (name "Description") "Independent Type 200mW 3.1V~3.5V 3.3V SOD-323 Zener Diodes ROHS")
        (field (name "LCSC") "C19077437")
        (field (name "Stock") "229387")
        (field (name "Price") "0.018USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Preferred Component")
        (field (name "Category") "Diodes,Zener Diodes")
        (field (name "Manufacturer") "hongjiacheng")
        (field (name "Part") "BZT52C3V3S"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "PCM_JLCPCB-Inductors") (part "Ferrite,0603")
      (description "450mΩ ±25% 600Ω@100MHz 0603 Ferrite Beads ROHS")
      (docs "https://www.lcsc.com/datasheet/lcsc_datasheet_2310301640_Sunlord-GZ1608D601TF_C1002.pdf")
      (footprints
        (fp "FB_*"))
      (fields
        (field (name "Reference") "FB")
        (field (name "Value"))
        (field (name "Footprint") "PCM_JLCPCB:FB_0603")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2310301640_Sunlord-GZ1608D601TF_C1002.pdf")
        (field (name "Description") "450mΩ ±25% 600Ω@100MHz 0603 Ferrite Beads ROHS")
        (field (name "LCSC") "C1002")
        (field (name "Stock") "789150")
        (field (name "Price") "0.010USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "6")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Filters/EMI Optimization,Ferrite Beads")
        (field (name "Manufacturer") "Sunlord")
        (field (name "Part") "GZ1608D601TF")
        (field (name "DC Resistance") "450mΩ")
        (field (name "Impedance @ Frequency") "600Ω@100MHz")
        (field (name "Circuits") "1")
        (field (name "Current Rating") "200mA")
        (field (name "Tolerance") "±25%"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "PCM_JLCPCB-Resistors") (part "0402,100kΩ")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 100kΩ 0402 Chip Resistor - Surface Mount ROHS")
      (docs "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010100_UNI-ROYAL-Uniroyal-Elec-0402WGF1003TCE_C25741.pdf")
      (footprints
        (fp "R_*"))
      (fields
        (field (name "Reference") "R")
        (field (name "Value") "100kΩ")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010100_UNI-ROYAL-Uniroyal-Elec-0402WGF1003TCE_C25741.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 100kΩ 0402 Chip Resistor - Surface Mount ROHS")
        (field (name "LCSC") "C25741")
        (field (name "Stock") "6969783")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF1003TCE")
        (field (name "Resistance") "100kΩ")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "PCM_JLCPCB-Resistors") (part "0402,10kΩ")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 10kΩ 0402 Chip Resistor - Surface Mount ROHS")
      (docs "https://www.lcsc.com/datasheet/lcsc_datasheet_2411221126_UNI-ROYAL-Uniroyal-Elec-0402WGF1002TCE_C25744.pdf")
      (footprints
        (fp "R_*"))
      (fields
        (field (name "Reference") "R")
        (field (name "Value") "10kΩ")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2411221126_UNI-ROYAL-Uniroyal-Elec-0402WGF1002TCE_C25744.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 10kΩ 0402 Chip Resistor - Surface Mount ROHS")
        (field (name "LCSC") "C25744")
        (field (name "Stock") "24372091")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF1002TCE")
        (field (name "Resistance") "10kΩ")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "PCM_JLCPCB-Resistors") (part "0402,10Ω")
      (description "62.5mW Thick Film Resistors 50V ±1% ±200ppm/°C 10Ω 0402 Chip Resistor - Surface Mount ROHS")
      (docs "https://www.lcsc.com/datasheet/lcsc_datasheet_2411221126_UNI-ROYAL-Uniroyal-Elec-0402WGF100JTCE_C25077.pdf")
      (footprints
        (fp "R_*"))
      (fields
        (field (name "Reference") "R")
        (field (name "Value") "10Ω")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2411221126_UNI-ROYAL-Uniroyal-Elec-0402WGF100JTCE_C25077.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±1% ±200ppm/°C 10Ω 0402 Chip Resistor - Surface Mount ROHS")
        (field (name "LCSC") "C25077")
        (field (name "Stock") "4873481")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF100JTCE")
        (field (name "Resistance") "10Ω")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±200ppm/°C"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "PCM_JLCPCB-Resistors") (part "0402,330Ω")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS")
      (docs "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF3300TCE_C25104.pdf")
      (footprints
        (fp "R_*"))
      (fields
        (field (name "Reference") "R")
        (field (name "Value") "330Ω")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF3300TCE_C25104.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 330Ω 0402 Chip Resistor - Surface Mount ROHS")
        (field (name "LCSC") "C25104")
        (field (name "Stock") "1159127")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF3300TCE")
        (field (name "Resistance") "330Ω")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "PCM_JLCPCB-Resistors") (part "0402,33Ω")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 33Ω 0402 Chip Resistor - Surface Mount ROHS")
      (docs "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF330JTCE_C25105.pdf")
      (footprints
        (fp "R_*"))
      (fields
        (field (name "Reference") "R")
        (field (name "Value") "33Ω")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF330JTCE_C25105.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 33Ω 0402 Chip Resistor - Surface Mount ROHS")
        (field (name "LCSC") "C25105")
        (field (name "Stock") "2122900")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF330JTCE")
        (field (name "Resistance") "33Ω")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "PCM_JLCPCB-Resistors") (part "0402,4.7kΩ")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 4.7kΩ 0402 Chip Resistor - Surface Mount ROHS")
      (docs "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010045_UNI-ROYAL-Uniroyal-Elec-0402WGF4701TCE_C25900.pdf")
      (footprints
        (fp "R_*"))
      (fields
        (field (name "Reference") "R")
        (field (name "Value") "4.7kΩ")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010045_UNI-ROYAL-Uniroyal-Elec-0402WGF4701TCE_C25900.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 4.7kΩ 0402 Chip Resistor - Surface Mount ROHS")
        (field (name "LCSC") "C25900")
        (field (name "Stock") "7644059")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF4701TCE")
        (field (name "Resistance") "4.7kΩ")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "PCM_JLCPCB-Resistors") (part "0402,510Ω")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 510Ω 0402 Chip Resistor - Surface Mount ROHS")
      (docs "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF5100TCE_C25123.pdf")
      (footprints
        (fp "R_*"))
      (fields
        (field (name "Reference") "R")
        (field (name "Value") "510Ω")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF5100TCE_C25123.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 510Ω 0402 Chip Resistor - Surface Mount ROHS")
        (field (name "LCSC") "C25123")
        (field (name "Stock") "2434473")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "12")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF5100TCE")
        (field (name "Resistance") "510Ω")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "PCM_JLCPCB-Resistors") (part "0603,18kΩ")
      (description "100mW Thick Film Resistors 75V ±100ppm/°C ±1% 18kΩ 0603 Chip Resistor - Surface Mount ROHS")
      (docs "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010045_UNI-ROYAL-Uniroyal-Elec-0603WAF1802T5E_C25810.pdf")
      (footprints
        (fp "R_*"))
      (fields
        (field (name "Reference") "R")
        (field (name "Value") "18kΩ")
        (field (name "Footprint") "PCM_JLCPCB:R_0603")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010045_UNI-ROYAL-Uniroyal-Elec-0603WAF1802T5E_C25810.pdf")
        (field (name "Description") "100mW Thick Film Resistors 75V ±100ppm/°C ±1% 18kΩ 0603 Chip Resistor - Surface Mount ROHS")
        (field (name "LCSC") "C25810")
        (field (name "Stock") "574660")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0603WAF1802T5E")
        (field (name "Resistance") "18kΩ")
        (field (name "Power(Watts)") "100mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "75V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "PCM_JLCPCB-Resistors") (part "0603,200kΩ")
      (description "100mW Thick Film Resistors 75V ±100ppm/°C ±1% 200kΩ 0603 Chip Resistor - Surface Mount ROHS")
      (docs "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010045_UNI-ROYAL-Uniroyal-Elec-0603WAF2003T5E_C25811.pdf")
      (footprints
        (fp "R_*"))
      (fields
        (field (name "Reference") "R")
        (field (name "Value") "200kΩ")
        (field (name "Footprint") "PCM_JLCPCB:R_0603")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010045_UNI-ROYAL-Uniroyal-Elec-0603WAF2003T5E_C25811.pdf")
        (field (name "Description") "100mW Thick Film Resistors 75V ±100ppm/°C ±1% 200kΩ 0603 Chip Resistor - Surface Mount ROHS")
        (field (name "LCSC") "C25811")
        (field (name "Stock") "1426208")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0603WAF2003T5E")
        (field (name "Resistance") "200kΩ")
        (field (name "Power(Watts)") "100mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "75V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "PCM_JLCPCB-Resistors") (part "0603,27kΩ")
      (description "100mW Thick Film Resistors 75V ±100ppm/°C ±1% 27kΩ 0603 Chip Resistor - Surface Mount ROHS")
      (docs "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010130_UNI-ROYAL-Uniroyal-Elec-0603WAF2702T5E_C22967.pdf")
      (footprints
        (fp "R_*"))
      (fields
        (field (name "Reference") "R")
        (field (name "Value") "27kΩ")
        (field (name "Footprint") "PCM_JLCPCB:R_0603")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010130_UNI-ROYAL-Uniroyal-Elec-0603WAF2702T5E_C22967.pdf")
        (field (name "Description") "100mW Thick Film Resistors 75V ±100ppm/°C ±1% 27kΩ 0603 Chip Resistor - Surface Mount ROHS")
        (field (name "LCSC") "C22967")
        (field (name "Stock") "708507")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0603WAF2702T5E")
        (field (name "Resistance") "27kΩ")
        (field (name "Power(Watts)") "100mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "75V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "PCM_JLCPCB-Transistors") (part "NMOS,AO3400A")
      (description "30V 5.7A 26.5mΩ@10V,5.7A 1.4W 1.5V@250uA 1 N-Channel SOT-23-3L MOSFETs ROHS")
      (docs "https://www.lcsc.com/datasheet/lcsc_datasheet_1811081213_Alpha---Omega-Semicon-AO3400A_C20917.pdf")
      (footprints
        (fp "Q_*"))
      (fields
        (field (name "Reference") "Q")
        (field (name "Value") "AO3400A")
        (field (name "Footprint") "PCM_JLCPCB:Q_SOT-23")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_1811081213_Alpha---Omega-Semicon-AO3400A_C20917.pdf")
        (field (name "Description") "30V 5.7A 26.5mΩ@10V,5.7A 1.4W 1.5V@250uA 1 N-Channel SOT-23-3L MOSFETs ROHS")
        (field (name "LCSC") "C20917")
        (field (name "Stock") "463122")
        (field (name "Price") "0.074USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "5")
        (field (name "Attrition Qty") "4")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Transistors,MOSFETs")
        (field (name "Manufacturer") "Alpha & Omega Semicon")
        (field (name "Part") "AO3400A")
        (field (name "Continuous Drain Current (Id)") "5.7A")
        (field (name "Input Capacitance (Ciss@Vds)") "630pF@15V")
        (field (name "Operating Temperature") "-55°C~+150°C@(Tj)")
        (field (name "Type") "1 N-channel")
        (field (name "Drain Source Voltage (Vdss)") "30V")
        (field (name "Power Dissipation (Pd)") "1.4W")
        (field (name "Gate Threshold Voltage (Vgs(th)@Id)") "1.5V@250uA")
        (field (name "Drain Source On Resistance (RDS(on)@Vgs,Id)") "26.5mΩ@10V,5.7A")
        (field (name "Total Gate Charge (Qg@Vgs)") "7nC@4.5V"))
      (pins
        (pin (num "1") (name "G") (type "input"))
        (pin (num "2") (name "S") (type "passive"))
        (pin (num "3") (name "D") (type "passive"))))
    (libpart (lib "PCM_JLCPCB-Transistors") (part "PMOS,SI2301CDS-T1-GE3")
      (description "20V 3.1A 112mΩ@4.5V,2.8A 1V@250uA 1 Piece P-Channel SOT-23 MOSFETs ROHS")
      (docs "https://www.lcsc.com/datasheet/lcsc_datasheet_1808272021_Vishay-Intertech-SI2301CDS-T1-GE3_C10487.pdf")
      (footprints
        (fp "Q_*"))
      (fields
        (field (name "Reference") "Q")
        (field (name "Value") "SI2301CDS-T1-GE3")
        (field (name "Footprint") "PCM_JLCPCB:Q_SOT-23")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_1808272021_Vishay-Intertech-SI2301CDS-T1-GE3_C10487.pdf")
        (field (name "Description") "20V 3.1A 112mΩ@4.5V,2.8A 1V@250uA 1 Piece P-Channel SOT-23 MOSFETs ROHS")
        (field (name "LCSC") "C10487")
        (field (name "Stock") "476267")
        (field (name "Price") "0.058USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "5")
        (field (name "Attrition Qty") "4")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Transistors,MOSFETs")
        (field (name "Manufacturer") "Vishay Intertech")
        (field (name "Part") "SI2301CDS-T1-GE3")
        (field (name "Continuous Drain Current (Id)") "2.3A")
        (field (name "Input Capacitance (Ciss@Vds)") "405pF@10V")
        (field (name "Operating Temperature") "-55°C~+150°C")
        (field (name "Type") "1 Piece P-Channel")
        (field (name "Drain Source Voltage (Vdss)") "20V")
        (field (name "Power Dissipation (Pd)") "0.86W")
        (field (name "Gate Threshold Voltage (Vgs(th)@Id)") "1V@250uA")
        (field (name "Reverse Transfer Capacitance (Crss@Vds)") "55pF@10V")
        (field (name "Drain Source On Resistance (RDS(on)@Vgs,Id)") "0.112Ω@4.5V,2.8A")
        (field (name "Total Gate Charge (Qg@Vgs)") "3.3nC@10V"))
      (pins
        (pin (num "1") (name "G") (type "input"))
        (pin (num "2") (name "S") (type "passive"))
        (pin (num "3") (name "D") (type "passive"))))
    (libpart (lib "PJ-320D jack 3.5mm") (part "PJ-320D")
      (docs "https://atta.szlcsc.com/upload/public/pdf/source/20190925/C431535_8B274506621F6117FB020BF07A197848.pdf")
      (fields
        (field (name "Reference") "U10")
        (field (name "Value") "PJ-320D 3.5mm jack")
        (field (name "Footprint") "footprint:AUDIO-SMD_PJ-320D-1")
        (field (name "Datasheet") "https://atta.szlcsc.com/upload/public/pdf/source/20190925/C431535_8B274506621F6117FB020BF07A197848.pdf")
        (field (name "Description"))
        (field (name "LCSC") "C431535"))
      (pins
        (pin (num "1") (name "GND/SHLD") (type "passive"))
        (pin (num "2") (name "LEFT_P") (type "passive"))
        (pin (num "3") (name "RIGHT_P") (type "passive"))
        (pin (num "4") (name "DETECT_GND") (type "passive"))))
    (libpart (lib "PJ-611E jack 6.35mm") (part "PJ-611E")
      (docs "https://item.szlcsc.com/datasheet/PJ-611E/292943.html?spm=sc.it.xds.a&lcsc_vid=EVMNBFVWTlcKUQUCQ1FdVFJSRgcNXgJXE1BbX1ACQlgxVlNQQ1NcUF1RR1VcXjsOAxUeFF5JWA0NAgAHWQIASA%3D%3D")
      (fields
        (field (name "Reference") "J18")
        (field (name "Value") "PJ-611E 6.35mm jack")
        (field (name "Footprint") "footprint:AUDIO-TH_PJ-611E_1")
        (field (name "Datasheet") "https://item.szlcsc.com/datasheet/PJ-611E/292943.html?spm=sc.it.xds.a&lcsc_vid=EVMNBFVWTlcKUQUCQ1FdVFJSRgcNXgJXE1BbX1ACQlgxVlNQQ1NcUF1RR1VcXjsOAxUeFF5JWA0NAgAHWQIASA%3D%3D")
        (field (name "Description"))
        (field (name "LCSC") "C309282"))
      (pins
        (pin (num "2") (name "GND/SHLD") (type "passive"))
        (pin (num "3") (name "DETECT_GND") (type "passive"))
        (pin (num "4") (name "RIGHT_P") (type "passive"))
        (pin (num "5") (name "DETECT_R") (type "passive"))
        (pin (num "6") (name "LEFT_P") (type "passive"))
        (pin (num "7") (name "DETECT_LEFT") (type "passive"))))
    (libpart (lib "PS-22E05-S-O-001") (part "PS-22E05-S-O-001")
      (docs "https://atta.szlcsc.com/upload/public/pdf/source/20210825/03FED21E2D4F2980BA08F4ED04C13B40.pdf")
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "PS-22E05-S-O-001")
        (field (name "Footprint") "footprint:SW-TH_PS-22E05")
        (field (name "Datasheet") "https://atta.szlcsc.com/upload/public/pdf/source/20210825/03FED21E2D4F2980BA08F4ED04C13B40.pdf")
        (field (name "Description"))
        (field (name "LCSC") "C19190928"))
      (pins
        (pin (num "1") (name "1") (type "unspecified"))
        (pin (num "2") (name "2") (type "unspecified"))
        (pin (num "3") (name "3") (type "unspecified"))
        (pin (num "4") (name "4") (type "unspecified"))
        (pin (num "5") (name "5") (type "unspecified"))
        (pin (num "6") (name "6") (type "unspecified"))
        (pin (num "7") (name "7") (type "unspecified"))
        (pin (num "8") (name "8") (type "unspecified"))))
    (libpart (lib "PSC-1608U52GC-G4") (part "PSC-1608U52GC-G4")
      (docs "https://atta.szlcsc.com/upload/public/pdf/source/20190115/C264450_D840E7E570138F41CCE67133F241C738.pdf")
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "PSC-1608U52GC-G4")
        (field (name "Footprint") "footprint:LED0603-RD_GREEN")
        (field (name "Datasheet") "https://atta.szlcsc.com/upload/public/pdf/source/20190115/C264450_D840E7E570138F41CCE67133F241C738.pdf")
        (field (name "Description"))
        (field (name "LCSC") "C22371297"))
      (pins
        (pin (num "1") (name "K") (type "unspecified"))
        (pin (num "2") (name "A") (type "unspecified"))))
    (libpart (lib "Regulator_Linear") (part "AP2112K-3.3")
      (description "600mA low dropout linear regulator, with enable pin, 3.8V-6V input voltage range, 3.3V fixed positive output, SOT-23-5")
      (docs "https://www.diodes.com/assets/Datasheets/AP2112.pdf")
      (footprints
        (fp "SOT?23?5*"))
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "AP2112K-3.3")
        (field (name "Footprint") "Package_TO_SOT_SMD:SOT-23-5")
        (field (name "Datasheet") "https://www.diodes.com/assets/Datasheets/AP2112.pdf")
        (field (name "Description") "600mA low dropout linear regulator, with enable pin, 3.8V-6V input voltage range, 3.3V fixed positive output, SOT-23-5"))
      (pins
        (pin (num "1") (name "VIN") (type "power_in"))
        (pin (num "2") (name "GND") (type "power_in"))
        (pin (num "3") (name "EN") (type "input"))
        (pin (num "4") (name "NC") (type "no_connect"))
        (pin (num "5") (name "VOUT") (type "power_out"))))
    (libpart (lib "SL1040-2R2M") (part "SL1040-2R2M")
      (docs "https://atta.szlcsc.com/upload/public/pdf/source/20240611/8DE7D6BE1273F2E871C82A6D5C20B08D.pdf")
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "SL1040-2R2M")
        (field (name "Footprint") "footprint:IND-SMD_SL1040-R47M")
        (field (name "Datasheet") "https://atta.szlcsc.com/upload/public/pdf/source/20240611/8DE7D6BE1273F2E871C82A6D5C20B08D.pdf")
        (field (name "Description"))
        (field (name "LCSC") "C22463836"))
      (pins
        (pin (num "1") (name "1") (type "unspecified"))
        (pin (num "2") (name "2") (type "unspecified"))))
    (libpart (lib "SY8368AQQC") (part "SY8368AQQC")
      (docs "https://atta.szlcsc.com/upload/public/pdf/source/20180224/C178253_15194367790221363788.pdf")
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "SY8368AQQC")
        (field (name "Footprint") "footprint:QFN-12_L3.0-W3.0-P0.45-TL-EP")
        (field (name "Datasheet") "https://atta.szlcsc.com/upload/public/pdf/source/20180224/C178253_15194367790221363788.pdf")
        (field (name "Description"))
        (field (name "LCSC") "C207642"))
      (pins
        (pin (num "1") (name "GND") (type "unspecified"))
        (pin (num "2") (name "LX") (type "unspecified"))
        (pin (num "3") (name "GND") (type "unspecified"))
        (pin (num "4") (name "IN") (type "unspecified"))
        (pin (num "5") (name "IN") (type "unspecified"))
        (pin (num "6") (name "IN") (type "unspecified"))
        (pin (num "7") (name "BS") (type "unspecified"))
        (pin (num "8") (name "VCC") (type "unspecified"))
        (pin (num "9") (name "FB") (type "unspecified"))
        (pin (num "10") (name "ILMT") (type "unspecified"))
        (pin (num "11") (name "PG") (type "unspecified"))
        (pin (num "12") (name "EN") (type "unspecified"))))
    (libpart (lib "Simulation_SPICE") (part "VDC")
      (description "Voltage source, DC")
      (docs "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#sec_Independent_Sources_for")
      (fields
        (field (name "Reference") "V")
        (field (name "Value") "1")
        (field (name "Footprint"))
        (field (name "Datasheet") "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#sec_Independent_Sources_for")
        (field (name "Description") "Voltage source, DC")
        (field (name "Sim.Pins") "1=+ 2=-")
        (field (name "Sim.Type") "DC")
        (field (name "Sim.Device") "V"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "Simulation_SPICE") (part "VSIN")
      (description "Voltage source, sinusoidal")
      (docs "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#sec_Independent_Sources_for")
      (fields
        (field (name "Reference") "V")
        (field (name "Value") "VSIN")
        (field (name "Footprint"))
        (field (name "Datasheet") "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#sec_Independent_Sources_for")
        (field (name "Description") "Voltage source, sinusoidal")
        (field (name "Sim.Pins") "1=+ 2=-")
        (field (name "Sim.Params") "dc=0 ampl=1 f=1k ac=1")
        (field (name "Sim.Type") "SIN")
        (field (name "Sim.Device") "V"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "Switch") (part "SW_Push")
      (description "Push button switch, generic, two pins")
      (docs "~")
      (fields
        (field (name "Reference") "SW")
        (field (name "Value") "SW_Push")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Push button switch, generic, two pins"))
      (pins
        (pin (num "1") (name "1") (type "passive"))
        (pin (num "2") (name "2") (type "passive"))))
    (libpart (lib "TF-15×15") (part "TF-15×15")
      (docs "https://item.szlcsc.com/112422.html")
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "TF-15×15")
        (field (name "Footprint") "footprint:TF-SMD_TF-15-15")
        (field (name "Datasheet") "https://item.szlcsc.com/112422.html")
        (field (name "Description"))
        (field (name "LCSC") "C111196"))
      (pins
        (pin (num "1") (name "DAT2") (type "input"))
        (pin (num "2") (name "CD/DAT3") (type "input"))
        (pin (num "3") (name "CMD") (type "input"))
        (pin (num "4") (name "VDD") (type "input"))
        (pin (num "5") (name "CLK") (type "input"))
        (pin (num "6") (name "VSS") (type "input"))
        (pin (num "7") (name "DAT0") (type "input"))
        (pin (num "8") (name "DAT1") (type "input"))
        (pin (num "9") (name "CD") (type "input"))
        (pin (num "10") (name "G3") (type "input"))
        (pin (num "11") (name "G4") (type "input"))
        (pin (num "12") (name "G1") (type "input"))
        (pin (num "13") (name "G2") (type "input"))))
    (libpart (lib "TYPE-C-31-M-12") (part "TYPE-C-31-M-12")
      (docs "https://item.szlcsc.com/datasheet/TYPE-C-31-M-12/177331.html?spm=sc.gbn.xds.a___sc.gbn.hd.ss&lcsc_vid=RgMNUVYEQARbV1xTElVcVwIAFFBXVwBfEQdfX1UCRAcxVlNTQFBcUlFXT1hYVTsOAxUeFF5JWA0NAgAHWQIASA%3D%3D")
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "TYPE-C-31-M-12")
        (field (name "Footprint") "footprint:USB-C_SMD-TYPE-C-31-M-12_1")
        (field (name "Datasheet") "https://item.szlcsc.com/datasheet/TYPE-C-31-M-12/177331.html?spm=sc.gbn.xds.a___sc.gbn.hd.ss&lcsc_vid=RgMNUVYEQARbV1xTElVcVwIAFFBXVwBfEQdfX1UCRAcxVlNTQFBcUlFXT1hYVTsOAxUeFF5JWA0NAgAHWQIASA%3D%3D")
        (field (name "Description"))
        (field (name "LCSC") "C165948"))
      (pins
        (pin (num "1") (name "EH") (type "unspecified"))
        (pin (num "2") (name "EH") (type "unspecified"))
        (pin (num "3") (name "EH") (type "unspecified"))
        (pin (num "4") (name "EH") (type "unspecified"))
        (pin (num "A1B12") (name "GND") (type "unspecified"))
        (pin (num "A4B9") (name "VBUS") (type "unspecified"))
        (pin (num "A5") (name "CC1") (type "unspecified"))
        (pin (num "A6") (name "DP1") (type "unspecified"))
        (pin (num "A7") (name "DN1") (type "unspecified"))
        (pin (num "A8") (name "SBU1") (type "unspecified"))
        (pin (num "B1A12") (name "GND") (type "unspecified"))
        (pin (num "B4A9") (name "VBUS") (type "unspecified"))
        (pin (num "B5") (name "CC2") (type "unspecified"))
        (pin (num "B6") (name "DP2") (type "unspecified"))
        (pin (num "B7") (name "DN2") (type "unspecified"))
        (pin (num "B8") (name "SBU2") (type "unspecified"))))
    (libpart (lib "XL-1608UBC-04") (part "XL-1608UBC-04")
      (docs "https://atta.szlcsc.com/upload/public/pdf/source/20210617/C2837377_50FC585D376FE0CDA016E524346528FF.pdf")
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "XL-1608UBC-04")
        (field (name "Footprint") "footprint:LED0603-RD_BLUE")
        (field (name "Datasheet") "https://atta.szlcsc.com/upload/public/pdf/source/20210617/C2837377_50FC585D376FE0CDA016E524346528FF.pdf")
        (field (name "Description"))
        (field (name "LCSC") "C965807"))
      (pins
        (pin (num "1") (name "K") (type "unspecified"))
        (pin (num "2") (name "A") (type "unspecified"))))
    (libpart (lib "jlc_TYPE-C_16PIN_2MD(073)") (part "TYPE-C_16PIN_2MD(073)")
      (docs "https://atta.szlcsc.com/upload/public/pdf/source/20210409/C2765186_34D42616F62DF94D17C4D63D74D9FD03.pdf")
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "TYPE-C_16PIN_2MD(073)")
        (field (name "Footprint") "footprint:USB-C-SMD_TYPE-C-6PIN-2MD-073")
        (field (name "Datasheet") "https://atta.szlcsc.com/upload/public/pdf/source/20210409/C2765186_34D42616F62DF94D17C4D63D74D9FD03.pdf")
        (field (name "Description"))
        (field (name "LCSC") "C2765186"))
      (pins
        (pin (num "1") (name "GND") (type "unspecified"))
        (pin (num "2") (name "VBUS") (type "unspecified"))
        (pin (num "3") (name "SBU2") (type "unspecified"))
        (pin (num "4") (name "CC1") (type "unspecified"))
        (pin (num "5") (name "DN2") (type "unspecified"))
        (pin (num "6") (name "DP1") (type "unspecified"))
        (pin (num "7") (name "DN1") (type "unspecified"))
        (pin (num "8") (name "DP2") (type "unspecified"))
        (pin (num "9") (name "SBU1") (type "unspecified"))
        (pin (num "10") (name "CC2") (type "unspecified"))
        (pin (num "11") (name "VBUS") (type "unspecified"))
        (pin (num "12") (name "GND") (type "unspecified"))
        (pin (num "13") (name "SHELL") (type "unspecified"))
        (pin (num "14") (name "SHELL") (type "unspecified"))))
    (libpart (lib "jlc_USBLC6-2SC6-ES") (part "USBLC6-2SC6-ES")
      (docs "https://item.szlcsc.com/169042.html")
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "USBLC6-2SC6-ES")
        (field (name "Footprint") "footprint:SOT-23-6_L2.9-W1.6-P0.95-LS2.8-BR")
        (field (name "Datasheet") "https://item.szlcsc.com/169042.html")
        (field (name "Description"))
        (field (name "LCSC") "C5180249"))
      (pins
        (pin (num "1") (name "I/O1") (type "input"))
        (pin (num "2") (name "GND") (type "input"))
        (pin (num "3") (name "I/O2") (type "input"))
        (pin (num "4") (name "I/O2") (type "input"))
        (pin (num "5") (name "VCC") (type "input"))
        (pin (num "6") (name "I/O1") (type "input"))))
    (libpart (lib "rca-jack-red") (part "RCJ-012-SMT")
      (fields
        (field (name "Reference") "J7")
        (field (name "Value") "J_RCA_R (red)")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:CONN-TH_AV-5")
        (field (name "Datasheet"))
        (field (name "Description"))
        (field (name "MF") "Same Sky")
        (field (name "Description_1") "Metal Right-Angle, SMT RCA Jack, Red Insulator")
        (field (name "Package") "None")
        (field (name "Price") "None")
        (field (name "Check_prices") "https://www.snapeda.com/parts/RCJ-012-SMT-TR/Same+Sky/view-part/?ref=eda")
        (field (name "PART_REV") "B")
        (field (name "STANDARD") "Manufacturer recommendations")
        (field (name "SnapEDA_Link") "https://www.snapeda.com/parts/RCJ-012-SMT-TR/Same+Sky/view-part/?ref=snap")
        (field (name "MP") "RCJ-012-SMT-TR")
        (field (name "Purchase-URL") "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=1316485&manufacturer=Same Sky&part_name=RCJ-012-SMT-TR&search_term=rca jack pcb mount")
        (field (name "Availability") "In Stock")
        (field (name "MANUFACTURER") "CUI Inc"))
      (pins
        (pin (num "1A") (name "SHLD") (type "passive"))
        (pin (num "1B") (name "SHLD") (type "passive"))
        (pin (num "1C") (name "SHLD") (type "passive"))
        (pin (num "2") (name "SIGNL") (type "passive"))))
    (libpart (lib "rca-jack-white") (part "RCJ-013-SMT")
      (fields
        (field (name "Reference") "J6")
        (field (name "Value") "J_RCA_L (white)")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:CONN-TH_AV-5")
        (field (name "Datasheet"))
        (field (name "Description"))
        (field (name "MF") "Same Sky")
        (field (name "Description_1") "Metal Right-Angle, SMT RCA Jack, White Insulator")
        (field (name "Package") "None")
        (field (name "Price") "None")
        (field (name "Check_prices") "https://www.snapeda.com/parts/RCJ-013-SMT-TR/Same+Sky/view-part/?ref=eda")
        (field (name "PART_REV") "B")
        (field (name "STANDARD") "Manufacturer recommendations")
        (field (name "SnapEDA_Link") "https://www.snapeda.com/parts/RCJ-013-SMT-TR/Same+Sky/view-part/?ref=snap")
        (field (name "MP") "RCJ-013-SMT-TR")
        (field (name "Purchase-URL") "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=1316562&manufacturer=Same Sky&part_name=RCJ-013-SMT-TR&search_term=rca jack pcb mount")
        (field (name "Availability") "In Stock")
        (field (name "MANUFACTURER") "CUI Inc"))
      (pins
        (pin (num "1A") (name "SHLD") (type "passive"))
        (pin (num "1B") (name "SHLD") (type "passive"))
        (pin (num "1C") (name "SHLD") (type "passive"))
        (pin (num "2") (name "SIGNL") (type "passive"))))
    (libpart (lib "rpi-cm-5") (part "Compute_Module_5_Functional")
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "Compute_Module_5_Functional")
        (field (name "Footprint") "CM5:CM5")
        (field (name "Datasheet"))
        (field (name "Description")))
      (pins
        (pin (num "1") (name "GND[51]") (type "power_in"))
        (pin (num "2") (name "GND[51]") (type "power_in"))
        (pin (num "3") (name "Ethernet_Pair3_P") (type "passive"))
        (pin (num "4") (name "Ethernet_Pair1_P") (type "passive"))
        (pin (num "5") (name "Ethernet_Pair3_N") (type "passive"))
        (pin (num "6") (name "Ethernet_Pair1_N") (type "passive"))
        (pin (num "7") (name "GND[51]") (type "power_in"))
        (pin (num "8") (name "GND[51]") (type "power_in"))
        (pin (num "9") (name "Ethernet_Pair2_N") (type "passive"))
        (pin (num "10") (name "Ethernet_Pair0_N") (type "passive"))
        (pin (num "11") (name "Ethernet_Pair2_P") (type "passive"))
        (pin (num "12") (name "Ethernet_Pair0_P") (type "passive"))
        (pin (num "13") (name "GND[51]") (type "power_in"))
        (pin (num "14") (name "GND[51]") (type "power_in"))
        (pin (num "15") (name "~{Ethernet_nLED3}") (type "output"))
        (pin (num "16") (name "Fan_tacho") (type "input"))
        (pin (num "17") (name "~{Ethernet_nLED2}") (type "output"))
        (pin (num "18") (name "Ethernet_SYNC_OUT") (type "input"))
        (pin (num "19") (name "Fan_PWM") (type "output"))
        (pin (num "20") (name "EEPROM_nWP") (type "input"))
        (pin (num "21") (name "~{Pi_nLED_Activity}") (type "open_collector"))
        (pin (num "22") (name "GND[51]") (type "power_in"))
        (pin (num "23") (name "GND[51]") (type "power_in"))
        (pin (num "24") (name "GPIO26") (type "passive"))
        (pin (num "25") (name "GPIO21") (type "passive"))
        (pin (num "26") (name "GPIO19") (type "passive"))
        (pin (num "27") (name "GPIO20") (type "passive"))
        (pin (num "28") (name "GPIO13") (type "passive"))
        (pin (num "29") (name "GPIO16") (type "passive"))
        (pin (num "30") (name "GPIO6") (type "passive"))
        (pin (num "31") (name "GPIO12") (type "passive"))
        (pin (num "32") (name "GND[51]") (type "power_in"))
        (pin (num "33") (name "GND[51]") (type "power_in"))
        (pin (num "34") (name "GPIO5") (type "passive"))
        (pin (num "35") (name "ID_SC") (type "passive"))
        (pin (num "36") (name "ID_SD") (type "passive"))
        (pin (num "37") (name "GPIO7") (type "passive"))
        (pin (num "38") (name "GPIO11") (type "passive"))
        (pin (num "39") (name "GPIO8") (type "passive"))
        (pin (num "40") (name "GPIO9") (type "passive"))
        (pin (num "41") (name "GPIO25") (type "passive"))
        (pin (num "42") (name "GND[51]") (type "power_in"))
        (pin (num "43") (name "GND[51]") (type "power_in"))
        (pin (num "44") (name "GPIO10") (type "passive"))
        (pin (num "45") (name "GPIO24") (type "passive"))
        (pin (num "46") (name "GPIO22") (type "passive"))
        (pin (num "47") (name "GPIO23") (type "passive"))
        (pin (num "48") (name "GPIO27") (type "passive"))
        (pin (num "49") (name "GPIO18") (type "passive"))
        (pin (num "50") (name "GPIO17") (type "passive"))
        (pin (num "51") (name "GPIO15") (type "passive"))
        (pin (num "52") (name "GND[51]") (type "power_in"))
        (pin (num "53") (name "GND[51]") (type "power_in"))
        (pin (num "54") (name "GPIO4") (type "passive"))
        (pin (num "55") (name "GPIO14") (type "passive"))
        (pin (num "56") (name "GPIO3") (type "passive"))
        (pin (num "57") (name "SD_CLK") (type "passive"))
        (pin (num "58") (name "GPIO2") (type "passive"))
        (pin (num "59") (name "GND[51]") (type "power_in"))
        (pin (num "60") (name "GND[51]") (type "power_in"))
        (pin (num "61") (name "SD_DAT3") (type "passive"))
        (pin (num "62") (name "SD_CMD") (type "passive"))
        (pin (num "63") (name "SD_DAT0") (type "passive"))
        (pin (num "64") (name "SD_DAT5") (type "passive"))
        (pin (num "65") (name "GND[51]") (type "power_in"))
        (pin (num "66") (name "GND[51]") (type "power_in"))
        (pin (num "67") (name "SD_DAT1") (type "passive"))
        (pin (num "68") (name "SD_DAT4") (type "passive"))
        (pin (num "69") (name "SD_DAT2") (type "passive"))
        (pin (num "70") (name "SD_DAT7") (type "passive"))
        (pin (num "71") (name "GND[51]") (type "power_in"))
        (pin (num "72") (name "SD_DAT6") (type "passive"))
        (pin (num "73") (name "SD_VDD_Override") (type "input"))
        (pin (num "74") (name "GND[51]") (type "power_in"))
        (pin (num "75") (name "SD_PWR_ON") (type "output"))
        (pin (num "76") (name "VBAT") (type "input"))
        (pin (num "77") (name "+5V") (type "power_in"))
        (pin (num "78") (name "GPIO_VREF") (type "power_in"))
        (pin (num "79") (name "+5V") (type "power_in"))
        (pin (num "80") (name "I2C_SCL0") (type "bidirectional"))
        (pin (num "81") (name "+5V") (type "power_in"))
        (pin (num "82") (name "I2C_SDA0") (type "bidirectional"))
        (pin (num "83") (name "+5V") (type "power_in"))
        (pin (num "84") (name "CM4_3.3V_Out_1") (type "power_out"))
        (pin (num "85") (name "+5V") (type "power_in"))
        (pin (num "86") (name "CM4_3.3V_Out_2") (type "power_out"))
        (pin (num "87") (name "+5V") (type "power_in"))
        (pin (num "88") (name "CM4_1.8V_Out_1") (type "power_out"))
        (pin (num "89") (name "~{WL_nDisable}") (type "input"))
        (pin (num "90") (name "CM4_1.8V_Out_2") (type "power_out"))
        (pin (num "91") (name "~{BT_nDisable}") (type "input"))
        (pin (num "92") (name "PWR_Button") (type "passive"))
        (pin (num "93") (name "~{nRPIBOOT}") (type "input"))
        (pin (num "94") (name "CC1") (type "bidirectional"))
        (pin (num "95") (name "~{PI_LED_nPWR}") (type "output"))
        (pin (num "96") (name "CC2") (type "bidirectional"))
        (pin (num "97") (name "CAM_GPIO0") (type "input"))
        (pin (num "98") (name "GND[51]") (type "power_in"))
        (pin (num "99") (name "PMIC_ENABLE") (type "input"))
        (pin (num "100") (name "CAM_GPIO1") (type "input"))
        (pin (num "101") (name "USB_OTG_ID") (type "input"))
        (pin (num "102") (name "~{PCIe_CLK_nREQ}") (type "input"))
        (pin (num "103") (name "USB_N") (type "passive"))
        (pin (num "104") (name "PCIE_DET_nWAKE") (type "passive"))
        (pin (num "105") (name "USB_P") (type "passive"))
        (pin (num "106") (name "PCIE_PWR_EN") (type "passive"))
        (pin (num "107") (name "GND[51]") (type "power_in"))
        (pin (num "108") (name "GND[51]") (type "power_in"))
        (pin (num "109") (name "~{PCIe_nRST}") (type "output"))
        (pin (num "110") (name "PCIe_CLK_P") (type "output"))
        (pin (num "111") (name "VBUS_EN") (type "input"))
        (pin (num "112") (name "PCIe_CLK_N") (type "output"))
        (pin (num "113") (name "GND[51]") (type "power_in"))
        (pin (num "114") (name "GND[51]") (type "power_in"))
        (pin (num "115") (name "MIPI0_D0_N") (type "input"))
        (pin (num "116") (name "PCIe_RX_P") (type "input"))
        (pin (num "117") (name "MIPI0_D0_P") (type "input"))
        (pin (num "118") (name "PCIe_RX_N") (type "input"))
        (pin (num "119") (name "GND[51]") (type "power_in"))
        (pin (num "120") (name "GND[51]") (type "power_in"))
        (pin (num "121") (name "MIPI0_D1_N") (type "input"))
        (pin (num "122") (name "PCIe_TX_P") (type "output"))
        (pin (num "123") (name "MIPI0_D1_P") (type "input"))
        (pin (num "124") (name "PCIe_TX_N") (type "output"))
        (pin (num "125") (name "GND[51]") (type "power_in"))
        (pin (num "126") (name "GND[51]") (type "power_in"))
        (pin (num "127") (name "MIPI0_C_N") (type "input"))
        (pin (num "128") (name "USB3-0-RX_N") (type "input"))
        (pin (num "129") (name "MIPI0_C_P") (type "input"))
        (pin (num "130") (name "USB3-0-RX_P") (type "input"))
        (pin (num "131") (name "GND[51]") (type "power_in"))
        (pin (num "132") (name "GND[51]") (type "power_in"))
        (pin (num "133") (name "MIPI0_D2_N") (type "input"))
        (pin (num "134") (name "USB3-0-DP") (type "bidirectional"))
        (pin (num "135") (name "MIPI0_D2_P") (type "input"))
        (pin (num "136") (name "USB3-0-DM") (type "bidirectional"))
        (pin (num "137") (name "GND[51]") (type "power_in"))
        (pin (num "138") (name "GND[51]") (type "power_in"))
        (pin (num "139") (name "MIPI0_D3_N") (type "input"))
        (pin (num "140") (name "USB3-0-TX_N") (type "output"))
        (pin (num "141") (name "MIPI0_D3_P") (type "input"))
        (pin (num "142") (name "USB3-0-TX_P") (type "output"))
        (pin (num "143") (name "HDMI1_HOTPLUG") (type "input"))
        (pin (num "144") (name "GND[51]") (type "power_in"))
        (pin (num "145") (name "HDMI1_SDA") (type "bidirectional"))
        (pin (num "146") (name "HDMI1_TX2_P") (type "output"))
        (pin (num "147") (name "HDMI1_SCL") (type "open_collector"))
        (pin (num "148") (name "HDMI1_TX2_N") (type "output"))
        (pin (num "149") (name "HDMI1_CEC") (type "open_collector"))
        (pin (num "150") (name "GND[51]") (type "power_in"))
        (pin (num "151") (name "HDMI0_CEC") (type "open_collector"))
        (pin (num "152") (name "HDMI1_TX1_P") (type "output"))
        (pin (num "153") (name "HDMI0_HOTPLUG") (type "input"))
        (pin (num "154") (name "HDMI1_TX1_N") (type "output"))
        (pin (num "155") (name "GND[51]") (type "power_in"))
        (pin (num "156") (name "GND[51]") (type "power_in"))
        (pin (num "157") (name "USB3-1-RX_N") (type "input"))
        (pin (num "158") (name "HDMI1_TX0_P") (type "output"))
        (pin (num "159") (name "USB3-1-RX_P") (type "input"))
        (pin (num "160") (name "HDMI1_TX0_N") (type "output"))
        (pin (num "161") (name "GND[51]") (type "power_in"))
        (pin (num "162") (name "GND[51]") (type "power_in"))
        (pin (num "163") (name "USB3-1-DP") (type "bidirectional"))
        (pin (num "164") (name "HDMI1_CLK_P") (type "output"))
        (pin (num "165") (name "USB3-1-DM") (type "bidirectional"))
        (pin (num "166") (name "HDMI1_CLK_N") (type "output"))
        (pin (num "167") (name "GND[51]") (type "power_in"))
        (pin (num "168") (name "GND[51]") (type "power_in"))
        (pin (num "169") (name "USB3-1-TX_N") (type "output"))
        (pin (num "170") (name "HDMI0_TX2_P") (type "output"))
        (pin (num "171") (name "USB3-1-TX_P") (type "output"))
        (pin (num "172") (name "HDMI0_TX2_N") (type "output"))
        (pin (num "173") (name "GND[51]") (type "power_in"))
        (pin (num "174") (name "GND[51]") (type "power_in"))
        (pin (num "175") (name "MIPI1_D0_N") (type "output"))
        (pin (num "176") (name "HDMI0_TX1_P") (type "output"))
        (pin (num "177") (name "MIPI1_D0_P") (type "output"))
        (pin (num "178") (name "HDMI0_TX1_N") (type "output"))
        (pin (num "179") (name "GND[51]") (type "power_in"))
        (pin (num "180") (name "GND[51]") (type "power_in"))
        (pin (num "181") (name "MIPI1_D1_N") (type "output"))
        (pin (num "182") (name "HDMI0_TX0_P") (type "output"))
        (pin (num "183") (name "MIPI1_D1_P") (type "output"))
        (pin (num "184") (name "HDMI0_TX0_N") (type "output"))
        (pin (num "185") (name "GND[51]") (type "power_in"))
        (pin (num "186") (name "GND[51]") (type "power_in"))
        (pin (num "187") (name "MIPI1_C_N") (type "output"))
        (pin (num "188") (name "HDMI0_CLK_P") (type "output"))
        (pin (num "189") (name "MIPI1_C_P") (type "output"))
        (pin (num "190") (name "HDMI0_CLK_N") (type "output"))
        (pin (num "191") (name "GND[51]") (type "power_in"))
        (pin (num "192") (name "GND[51]") (type "power_in"))
        (pin (num "193") (name "MIPI1_D2_N") (type "output"))
        (pin (num "194") (name "MIPI1_D3_N") (type "output"))
        (pin (num "195") (name "MIPI1_D2_P") (type "output"))
        (pin (num "196") (name "MIPI1_D3_P") (type "output"))
        (pin (num "197") (name "GND[51]") (type "power_in"))
        (pin (num "198") (name "GND[51]") (type "power_in"))
        (pin (num "199") (name "HDMI0_SDA") (type "bidirectional"))
        (pin (num "200") (name "HDMI0_SCL") (type "open_collector")))))
  (libraries
    (library (logical "74HC4067PW,118")
      (uri "/Users/sam1902/Documents/CustomDJ/JLC2KiCad_lib/symbol/74HC4067PW,118.kicad_sym"))
    (library (logical "AP2553W6-7")
      (uri "/Users/sam1902/Documents/CustomDJ/JLC2KiCad_lib/symbol/AP2553W6-7.kicad_sym"))
    (library (logical "Audio")
      (uri "/Applications/KiCad/KiCad.app/Contents/SharedSupport/symbols//Audio.kicad_sym"))
    (library (logical "CR2032-BS-6-1")
      (uri "/Users/sam1902/Documents/CustomDJ/JLC2KiCad_lib/symbol/CR2032-BS-6-1.kicad_sym"))
    (library (logical "Connector")
      (uri "/Applications/KiCad/KiCad.app/Contents/SharedSupport/symbols//Connector.kicad_sym"))
    (library (logical "Connector_Generic")
      (uri "/Applications/KiCad/KiCad.app/Contents/SharedSupport/symbols//Connector_Generic.kicad_sym"))
    (library (logical "DSWB05LHGET")
      (uri "/Users/sam1902/Documents/CustomDJ/JLC2KiCad_lib/symbol/DSWB05LHGET.kicad_sym"))
    (library (logical "Device")
      (uri "/Applications/KiCad/KiCad.app/Contents/SharedSupport/symbols//Device.kicad_sym"))
    (library (logical "Interface_USB")
      (uri "/Applications/KiCad/KiCad.app/Contents/SharedSupport/symbols//Interface_USB.kicad_sym"))
    (library (logical "KT-0603R")
      (uri "/Users/sam1902/Documents/CustomDJ/JLC2KiCad_lib/symbol/KT-0603R.kicad_sym"))
    (library (logical "MCP23017T-E/SS")
      (uri "/Users/sam1902/Documents/CustomDJ/JLC2KiCad_lib/symbol/MCP23017T-E{slash}SS.kicad_sym"))
    (library (logical "MCU_Microchip_ATmega")
      (uri "/Applications/KiCad/KiCad.app/Contents/SharedSupport/symbols//MCU_Microchip_ATmega.kicad_sym"))
    (library (logical "Mechanical")
      (uri "/Applications/KiCad/KiCad.app/Contents/SharedSupport/symbols//Mechanical.kicad_sym"))
    (library (logical "PCM_JLCPCB-Capacitors")
      (uri "/Users/sam1902/Documents/KiCad/9.0/3rdparty//symbols/com_github_CDFER_JLCPCB-Kicad-Library/JLCPCB-Capacitors.kicad_sym"))
    (library (logical "PCM_JLCPCB-Crystals")
      (uri "/Users/sam1902/Documents/KiCad/9.0/3rdparty//symbols/com_github_CDFER_JLCPCB-Kicad-Library/JLCPCB-Crystals.kicad_sym"))
    (library (logical "PCM_JLCPCB-Diodes")
      (uri "/Users/sam1902/Documents/KiCad/9.0/3rdparty//symbols/com_github_CDFER_JLCPCB-Kicad-Library/JLCPCB-Diodes.kicad_sym"))
    (library (logical "PCM_JLCPCB-Inductors")
      (uri "/Users/sam1902/Documents/KiCad/9.0/3rdparty//symbols/com_github_CDFER_JLCPCB-Kicad-Library/JLCPCB-Inductors.kicad_sym"))
    (library (logical "PCM_JLCPCB-Resistors")
      (uri "/Users/sam1902/Documents/KiCad/9.0/3rdparty//symbols/com_github_CDFER_JLCPCB-Kicad-Library/JLCPCB-Resistors.kicad_sym"))
    (library (logical "PCM_JLCPCB-Transistors")
      (uri "/Users/sam1902/Documents/KiCad/9.0/3rdparty//symbols/com_github_CDFER_JLCPCB-Kicad-Library/JLCPCB-Transistors.kicad_sym"))
    (library (logical "PJ-320D jack 3.5mm")
      (uri "/Users/sam1902/Documents/CustomDJ/JLC2KiCad_lib/symbol/PJ-320D.kicad_sym"))
    (library (logical "PJ-611E jack 6.35mm")
      (uri "/Users/sam1902/Documents/CustomDJ/JLC2KiCad_lib/symbol/PJ-611E.kicad_sym"))
    (library (logical "PS-22E05-S-O-001")
      (uri "/Users/sam1902/Documents/CustomDJ/JLC2KiCad_lib/symbol/PS-22E05-S-O-001.kicad_sym"))
    (library (logical "PSC-1608U52GC-G4")
      (uri "/Users/sam1902/Documents/CustomDJ/JLC2KiCad_lib/symbol/PSC-1608U52GC-G4.kicad_sym"))
    (library (logical "Regulator_Linear")
      (uri "/Applications/KiCad/KiCad.app/Contents/SharedSupport/symbols//Regulator_Linear.kicad_sym"))
    (library (logical "SL1040-2R2M")
      (uri "/Users/sam1902/Documents/CustomDJ/JLC2KiCad_lib/symbol/SL1040-2R2M.kicad_sym"))
    (library (logical "SY8368AQQC")
      (uri "/Users/sam1902/Documents/CustomDJ/JLC2KiCad_lib/symbol/SY8368AQQC.kicad_sym"))
    (library (logical "Simulation_SPICE")
      (uri "/Applications/KiCad/KiCad.app/Contents/SharedSupport/symbols//Simulation_SPICE.kicad_sym"))
    (library (logical "Switch")
      (uri "/Applications/KiCad/KiCad.app/Contents/SharedSupport/symbols//Switch.kicad_sym"))
    (library (logical "TF-15×15")
      (uri "/Users/sam1902/Documents/CustomDJ/JLC2KiCad_lib/symbol/TF-15×15.kicad_sym"))
    (library (logical "TYPE-C-31-M-12")
      (uri "/Users/sam1902/Documents/CustomDJ/JLC2KiCad_lib/symbol/TYPE-C-31-M-12.kicad_sym"))
    (library (logical "XL-1608UBC-04")
      (uri "/Users/sam1902/Documents/CustomDJ/JLC2KiCad_lib/symbol/XL-1608UBC-04.kicad_sym"))
    (library (logical "jlc_TYPE-C_16PIN_2MD(073)")
      (uri "/Users/sam1902/Documents/CustomDJ/JLC2KiCad_lib/symbol/TYPE-C_16PIN_2MD(073).kicad_sym"))
    (library (logical "jlc_USBLC6-2SC6-ES")
      (uri "/Users/sam1902/Documents/CustomDJ/JLC2KiCad_lib/symbol/USBLC6-2SC6-ES.kicad_sym"))
    (library (logical "rca-jack-red")
      (uri "/Users/sam1902/Documents/CustomDJ/kicad-thirdparty-footprints/RCJ-012-SMT.kicad_sym"))
    (library (logical "rca-jack-white")
      (uri "/Users/sam1902/Documents/CustomDJ/kicad-thirdparty-footprints/RCJ-013-SMT.kicad_sym"))
    (library (logical "rpi-cm-5")
      (uri "/Users/sam1902/Documents/CustomDJ/kicad-thirdparty-footprints/CM5.kicad_sym")))
  (nets
    (net (code "1") (name "+3.3V") (class "Default")
      (node (ref "C1") (pin "1") (pintype "passive"))
      (node (ref "C3") (pin "2") (pintype "passive"))
      (node (ref "C31") (pin "1") (pintype "passive"))
      (node (ref "C4") (pin "2") (pintype "passive"))
      (node (ref "C65") (pin "1") (pintype "passive"))
      (node (ref "C66") (pin "1") (pintype "passive"))
      (node (ref "C75") (pin "1") (pintype "passive"))
      (node (ref "J12") (pin "10") (pinfunction "P10") (pintype "power_in"))
      (node (ref "J7") (pin "4") (pinfunction "Pin_4") (pintype "passive"))
      (node (ref "Q2") (pin "2") (pinfunction "S") (pintype "passive"))
      (node (ref "R11") (pin "2") (pintype "passive"))
      (node (ref "R25") (pin "2") (pintype "passive"))
      (node (ref "R26") (pin "2") (pintype "passive"))
      (node (ref "R5") (pin "2") (pintype "passive"))
      (node (ref "R7") (pin "2") (pintype "passive"))
      (node (ref "R70") (pin "1") (pintype "passive"))
      (node (ref "R71") (pin "1") (pintype "passive"))
      (node (ref "R72") (pin "1") (pintype "passive"))
      (node (ref "R73") (pin "1") (pintype "passive"))
      (node (ref "R74") (pin "1") (pintype "passive"))
      (node (ref "R75") (pin "1") (pintype "passive"))
      (node (ref "R76") (pin "1") (pintype "passive"))
      (node (ref "TP3") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U1") (pin "78") (pinfunction "GPIO_VREF") (pintype "power_in"))
      (node (ref "U10") (pin "5") (pinfunction "VOUT") (pintype "power_out"))
      (node (ref "U2") (pin "28") (pinfunction "DVDD") (pintype "power_in"))
      (node (ref "U21") (pin "5") (pinfunction "VCC") (pintype "input"))
      (node (ref "U23") (pin "5") (pinfunction "VCC") (pintype "input"))
      (node (ref "U7") (pin "5") (pinfunction "VCC") (pintype "input")))
    (net (code "2") (name "+3.3V_ANALOG") (class "Default")
      (node (ref "C32") (pin "1") (pintype "passive"))
      (node (ref "C5") (pin "2") (pintype "passive"))
      (node (ref "FB1") (pin "2") (pintype "passive"))
      (node (ref "TP5") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U11") (pin "5") (pinfunction "VOUT") (pintype "power_out"))
      (node (ref "U2") (pin "1") (pinfunction "CPVDD") (pintype "power_in"))
      (node (ref "U2") (pin "8") (pinfunction "AVDD") (pintype "power_in")))
    (net (code "3") (name "+5V") (class "Default")
      (node (ref "C14") (pin "2") (pintype "passive"))
      (node (ref "C16") (pin "2") (pintype "passive"))
      (node (ref "C18") (pin "2") (pintype "passive"))
      (node (ref "C22") (pin "2") (pintype "passive"))
      (node (ref "C24") (pin "1") (pintype "passive"))
      (node (ref "C25") (pin "1") (pintype "passive"))
      (node (ref "C26") (pin "1") (pintype "passive"))
      (node (ref "C27") (pin "1") (pintype "passive"))
      (node (ref "C28") (pin "1") (pintype "passive"))
      (node (ref "C30") (pin "1") (pintype "passive"))
      (node (ref "C34") (pin "1") (pintype "passive"))
      (node (ref "C35") (pin "1") (pintype "passive"))
      (node (ref "C39") (pin "2") (pintype "passive"))
      (node (ref "C40") (pin "2") (pintype "passive"))
      (node (ref "C41") (pin "2") (pintype "passive"))
      (node (ref "C47") (pin "2") (pintype "passive"))
      (node (ref "C55") (pin "2") (pintype "passive"))
      (node (ref "C56") (pin "2") (pintype "passive"))
      (node (ref "C57") (pin "2") (pintype "passive"))
      (node (ref "C61") (pin "1") (pintype "passive"))
      (node (ref "C62") (pin "1") (pintype "passive"))
      (node (ref "C63") (pin "1") (pintype "passive"))
      (node (ref "J1") (pin "2") (pinfunction "Pin_2") (pintype "passive"))
      (node (ref "J13") (pin "19") (pinfunction "+5V") (pintype "power_in"))
      (node (ref "J14") (pin "19") (pinfunction "+5V") (pintype "power_in"))
      (node (ref "J16") (pin "4") (pinfunction "Pin_4") (pintype "passive"))
      (node (ref "J17") (pin "7") (pinfunction "Pin_7") (pintype "passive"))
      (node (ref "J18") (pin "9") (pinfunction "Pin_9") (pintype "passive"))
      (node (ref "J19") (pin "10") (pinfunction "Pin_10") (pintype "passive"))
      (node (ref "J20") (pin "9") (pinfunction "Pin_9") (pintype "passive"))
      (node (ref "J21") (pin "7") (pinfunction "Pin_7") (pintype "passive"))
      (node (ref "J6") (pin "2") (pinfunction "Pin_2") (pintype "passive"))
      (node (ref "L1") (pin "1") (pinfunction "1") (pintype "unspecified"))
      (node (ref "R1") (pin "1") (pintype "passive"))
      (node (ref "R33") (pin "1") (pintype "passive"))
      (node (ref "R34") (pin "2") (pintype "passive"))
      (node (ref "R36") (pin "2") (pintype "passive"))
      (node (ref "R37") (pin "1") (pintype "passive"))
      (node (ref "R52") (pin "2") (pintype "passive"))
      (node (ref "R53") (pin "1") (pintype "passive"))
      (node (ref "R54") (pin "1") (pintype "passive"))
      (node (ref "R55") (pin "2") (pintype "passive"))
      (node (ref "TP4") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U1") (pin "77") (pinfunction "+5V") (pintype "power_in"))
      (node (ref "U1") (pin "79") (pinfunction "+5V") (pintype "power_in"))
      (node (ref "U1") (pin "81") (pinfunction "+5V") (pintype "power_in"))
      (node (ref "U1") (pin "83") (pinfunction "+5V") (pintype "power_in"))
      (node (ref "U1") (pin "85") (pinfunction "+5V") (pintype "power_in"))
      (node (ref "U1") (pin "87") (pinfunction "+5V") (pintype "power_in"))
      (node (ref "U10") (pin "1") (pinfunction "VIN") (pintype "power_in"))
      (node (ref "U10") (pin "3") (pinfunction "EN") (pintype "input"))
      (node (ref "U11") (pin "1") (pinfunction "VIN") (pintype "power_in"))
      (node (ref "U11") (pin "3") (pinfunction "EN") (pintype "input"))
      (node (ref "U14") (pin "14") (pinfunction "VCC") (pintype "power_in"))
      (node (ref "U14") (pin "2") (pinfunction "UVCC") (pintype "power_in"))
      (node (ref "U14") (pin "24") (pinfunction "AVCC") (pintype "power_in"))
      (node (ref "U14") (pin "34") (pinfunction "VCC") (pintype "passive"))
      (node (ref "U14") (pin "44") (pinfunction "AVCC") (pintype "passive"))
      (node (ref "U14") (pin "7") (pinfunction "VBUS") (pintype "input"))
      (node (ref "U16") (pin "24") (pinfunction "VCC") (pintype "unspecified"))
      (node (ref "U18") (pin "9") (pinfunction "VDD") (pintype "unspecified"))
      (node (ref "U19") (pin "15") (pinfunction "A0") (pintype "unspecified"))
      (node (ref "U19") (pin "9") (pinfunction "VDD") (pintype "unspecified"))
      (node (ref "U22") (pin "5") (pinfunction "VCC") (pintype "input"))
      (node (ref "U3") (pin "1") (pinfunction "IN") (pintype "unspecified"))
      (node (ref "U4") (pin "1") (pinfunction "IN") (pintype "unspecified"))
      (node (ref "U5") (pin "1") (pinfunction "IN") (pintype "unspecified"))
      (node (ref "U6") (pin "5") (pinfunction "VCC") (pintype "input"))
      (node (ref "U8") (pin "5") (pinfunction "VCC") (pintype "input"))
      (node (ref "U9") (pin "1") (pinfunction "IN") (pintype "unspecified")))
    (net (code "4") (name "+20V_USB") (class "Default")
      (node (ref "C42") (pin "1") (pintype "passive"))
      (node (ref "C43") (pin "1") (pintype "passive"))
      (node (ref "C46") (pin "2") (pintype "passive"))
      (node (ref "C48") (pin "1") (pintype "passive"))
      (node (ref "R27") (pin "2") (pintype "passive"))
      (node (ref "R30") (pin "1") (pintype "passive"))
      (node (ref "SW3") (pin "1") (pinfunction "1") (pintype "unspecified"))
      (node (ref "TP2") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U13") (pin "4") (pinfunction "IN") (pintype "unspecified"))
      (node (ref "U13") (pin "5") (pinfunction "IN") (pintype "unspecified"))
      (node (ref "U13") (pin "6") (pinfunction "IN") (pintype "unspecified")))
    (net (code "5") (name "+20V_USB_RAIL") (class "Default")
      (node (ref "C37") (pin "1") (pintype "passive"))
      (node (ref "C38") (pin "1") (pintype "passive"))
      (node (ref "J15") (pin "A4B9") (pinfunction "VBUS") (pintype "unspecified"))
      (node (ref "J15") (pin "B4A9") (pinfunction "VBUS") (pintype "unspecified"))
      (node (ref "R28") (pin "1") (pintype "passive"))
      (node (ref "TP1") (pin "1") (pinfunction "1") (pintype "passive")))
    (net (code "6") (name "/Arduino MIDI/BTN_BACK") (class "Default")
      (node (ref "J21") (pin "1") (pinfunction "Pin_1") (pintype "passive"))
      (node (ref "U19") (pin "7") (pinfunction "GPB6") (pintype "unspecified")))
    (net (code "7") (name "/Arduino MIDI/BTN_CUE") (class "Default")
      (node (ref "J18") (pin "2") (pinfunction "Pin_2") (pintype "passive"))
      (node (ref "U18") (pin "22") (pinfunction "GPA1") (pintype "unspecified")))
    (net (code "8") (name "/Arduino MIDI/BTN_DIRECTION") (class "Default")
      (node (ref "J20") (pin "1") (pinfunction "Pin_1") (pintype "passive"))
      (node (ref "U18") (pin "2") (pinfunction "GPB1") (pintype "unspecified")))
    (net (code "9") (name "/Arduino MIDI/BTN_HOTCUE_1") (class "Default")
      (node (ref "J17") (pin "1") (pinfunction "Pin_1") (pintype "passive"))
      (node (ref "U18") (pin "3") (pinfunction "GPB2") (pintype "unspecified")))
    (net (code "10") (name "/Arduino MIDI/BTN_HOTCUE_2") (class "Default")
      (node (ref "J17") (pin "2") (pinfunction "Pin_2") (pintype "passive"))
      (node (ref "U18") (pin "4") (pinfunction "GPB3") (pintype "unspecified")))
    (net (code "11") (name "/Arduino MIDI/BTN_HOTCUE_3") (class "Default")
      (node (ref "J17") (pin "3") (pinfunction "Pin_3") (pintype "passive"))
      (node (ref "U18") (pin "5") (pinfunction "GPB4") (pintype "unspecified")))
    (net (code "12") (name "/Arduino MIDI/BTN_JOG_MODE") (class "Default")
      (node (ref "J19") (pin "4") (pinfunction "Pin_4") (pintype "passive"))
      (node (ref "U19") (pin "21") (pinfunction "GPA0") (pintype "unspecified")))
    (net (code "13") (name "/Arduino MIDI/BTN_LOOP_IN") (class "Default")
      (node (ref "J20") (pin "2") (pinfunction "Pin_2") (pintype "passive"))
      (node (ref "U18") (pin "6") (pinfunction "GPB5") (pintype "unspecified")))
    (net (code "14") (name "/Arduino MIDI/BTN_LOOP_OUT") (class "Default")
      (node (ref "J20") (pin "3") (pinfunction "Pin_3") (pintype "passive"))
      (node (ref "U18") (pin "7") (pinfunction "GPB6") (pintype "unspecified")))
    (net (code "15") (name "/Arduino MIDI/BTN_MTEMPO") (class "Default")
      (node (ref "J19") (pin "2") (pinfunction "Pin_2") (pintype "passive"))
      (node (ref "U18") (pin "24") (pinfunction "GPA3") (pintype "unspecified")))
    (net (code "16") (name "/Arduino MIDI/BTN_PLAY") (class "Default")
      (node (ref "J18") (pin "1") (pinfunction "Pin_1") (pintype "passive"))
      (node (ref "U18") (pin "21") (pinfunction "GPA0") (pintype "unspecified")))
    (net (code "17") (name "/Arduino MIDI/BTN_RELOOP") (class "Default")
      (node (ref "J20") (pin "4") (pinfunction "Pin_4") (pintype "passive"))
      (node (ref "U18") (pin "8") (pinfunction "GPB7") (pintype "unspecified")))
    (net (code "18") (name "/Arduino MIDI/BTN_SEARCH_L") (class "Default")
      (node (ref "J18") (pin "3") (pinfunction "Pin_3") (pintype "passive"))
      (node (ref "U18") (pin "26") (pinfunction "GPA5") (pintype "unspecified")))
    (net (code "19") (name "/Arduino MIDI/BTN_SEARCH_R") (class "Default")
      (node (ref "J18") (pin "4") (pinfunction "Pin_4") (pintype "passive"))
      (node (ref "U18") (pin "27") (pinfunction "GPA6") (pintype "unspecified")))
    (net (code "20") (name "/Arduino MIDI/BTN_TEMPO_RANGE") (class "Default")
      (node (ref "J19") (pin "3") (pinfunction "Pin_3") (pintype "passive"))
      (node (ref "U18") (pin "25") (pinfunction "GPA4") (pintype "unspecified")))
    (net (code "21") (name "/Arduino MIDI/BTN_TEMPO_RST") (class "Default")
      (node (ref "J19") (pin "1") (pinfunction "Pin_1") (pintype "passive"))
      (node (ref "U18") (pin "23") (pinfunction "GPA2") (pintype "unspecified")))
    (net (code "22") (name "/Arduino MIDI/BTN_TRACK_L") (class "Default")
      (node (ref "J18") (pin "5") (pinfunction "Pin_5") (pintype "passive"))
      (node (ref "U18") (pin "28") (pinfunction "GPA7") (pintype "unspecified")))
    (net (code "23") (name "/Arduino MIDI/BTN_TRACK_R") (class "Default")
      (node (ref "J18") (pin "6") (pinfunction "Pin_6") (pintype "passive"))
      (node (ref "U18") (pin "1") (pinfunction "GPB0") (pintype "unspecified")))
    (net (code "24") (name "/Arduino MIDI/FADER_ADIN") (class "Default")
      (node (ref "J19") (pin "9") (pinfunction "Pin_9") (pintype "passive"))
      (node (ref "U16") (pin "9") (pinfunction "Y0") (pintype "unspecified")))
    (net (code "25") (name "/Arduino MIDI/I2C_SCL_ATMEGA") (class "Default")
      (node (ref "R53") (pin "2") (pintype "passive"))
      (node (ref "TP25") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U14") (pin "18") (pinfunction "PD0") (pintype "bidirectional"))
      (node (ref "U18") (pin "12") (pinfunction "SCK") (pintype "unspecified"))
      (node (ref "U19") (pin "12") (pinfunction "SCK") (pintype "unspecified")))
    (net (code "26") (name "/Arduino MIDI/I2C_SDA_ATMEGA") (class "Default")
      (node (ref "R54") (pin "2") (pintype "passive"))
      (node (ref "TP24") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U14") (pin "19") (pinfunction "PD1") (pintype "bidirectional"))
      (node (ref "U18") (pin "13") (pinfunction "SDA") (pintype "unspecified"))
      (node (ref "U19") (pin "13") (pinfunction "SDA") (pintype "unspecified")))
    (net (code "27") (name "/Arduino MIDI/JOG1") (class "Default")
      (node (ref "J16") (pin "1") (pinfunction "Pin_1") (pintype "passive"))
      (node (ref "U14") (pin "8") (pinfunction "PB0") (pintype "bidirectional")))
    (net (code "28") (name "/Arduino MIDI/JOG_TOUCH") (class "Default")
      (node (ref "C58") (pin "1") (pintype "passive"))
      (node (ref "J16") (pin "3") (pinfunction "Pin_3") (pintype "passive"))
      (node (ref "R37") (pin "2") (pintype "passive"))
      (node (ref "U14") (pin "1") (pinfunction "PE6") (pintype "bidirectional")))
    (net (code "29") (name "/Arduino MIDI/LED_CUE") (class "Default")
      (node (ref "J18") (pin "8") (pinfunction "Pin_8") (pintype "passive"))
      (node (ref "R61") (pin "2") (pintype "passive")))
    (net (code "30") (name "/Arduino MIDI/LED_DIRECTION") (class "Default")
      (node (ref "J20") (pin "5") (pinfunction "Pin_5") (pintype "passive"))
      (node (ref "R59") (pin "2") (pintype "passive")))
    (net (code "31") (name "/Arduino MIDI/LED_HOTCUE1") (class "Default")
      (node (ref "J17") (pin "4") (pinfunction "Pin_4") (pintype "passive"))
      (node (ref "R58") (pin "2") (pintype "passive")))
    (net (code "32") (name "/Arduino MIDI/LED_HOTCUE2") (class "Default")
      (node (ref "J17") (pin "5") (pinfunction "Pin_5") (pintype "passive"))
      (node (ref "R57") (pin "2") (pintype "passive")))
    (net (code "33") (name "/Arduino MIDI/LED_HOTCUE3") (class "Default")
      (node (ref "J17") (pin "6") (pinfunction "Pin_6") (pintype "passive"))
      (node (ref "R56") (pin "2") (pintype "passive")))
    (net (code "34") (name "/Arduino MIDI/LED_JOG_MODE_1") (class "Default")
      (node (ref "J19") (pin "5") (pinfunction "Pin_5") (pintype "passive"))
      (node (ref "R66") (pin "1") (pintype "passive")))
    (net (code "35") (name "/Arduino MIDI/LED_JOG_MODE_2") (class "Default")
      (node (ref "J19") (pin "6") (pinfunction "Pin_6") (pintype "passive"))
      (node (ref "R67") (pin "1") (pintype "passive")))
    (net (code "36") (name "/Arduino MIDI/LED_LOOP_IN") (class "Default")
      (node (ref "J20") (pin "6") (pinfunction "Pin_6") (pintype "passive"))
      (node (ref "R63") (pin "1") (pintype "passive")))
    (net (code "37") (name "/Arduino MIDI/LED_LOOP_OUT") (class "Default")
      (node (ref "J20") (pin "7") (pinfunction "Pin_7") (pintype "passive"))
      (node (ref "R64") (pin "1") (pintype "passive")))
    (net (code "38") (name "/Arduino MIDI/LED_MTEMPO") (class "Default")
      (node (ref "J19") (pin "8") (pinfunction "Pin_8") (pintype "passive"))
      (node (ref "R60") (pin "2") (pintype "passive")))
    (net (code "39") (name "/Arduino MIDI/LED_PLAY") (class "Default")
      (node (ref "J18") (pin "7") (pinfunction "Pin_7") (pintype "passive"))
      (node (ref "R62") (pin "2") (pintype "passive")))
    (net (code "40") (name "/Arduino MIDI/LED_RELOOP") (class "Default")
      (node (ref "J20") (pin "8") (pinfunction "Pin_8") (pintype "passive"))
      (node (ref "R65") (pin "1") (pintype "passive")))
    (net (code "41") (name "/Arduino MIDI/LED_TEMPO_RST") (class "Default")
      (node (ref "J19") (pin "7") (pinfunction "Pin_7") (pintype "passive"))
      (node (ref "R68") (pin "1") (pintype "passive")))
    (net (code "42") (name "/Arduino MIDI/MCP1_INT") (class "Default")
      (node (ref "U14") (pin "28") (pinfunction "PB4") (pintype "bidirectional"))
      (node (ref "U18") (pin "19") (pinfunction "INTB") (pintype "unspecified"))
      (node (ref "U18") (pin "20") (pinfunction "INTA") (pintype "unspecified")))
    (net (code "43") (name "/Arduino MIDI/MCP2_INT") (class "Default")
      (node (ref "U14") (pin "29") (pinfunction "PB5") (pintype "bidirectional"))
      (node (ref "U19") (pin "19") (pinfunction "INTB") (pintype "unspecified"))
      (node (ref "U19") (pin "20") (pinfunction "INTA") (pintype "unspecified")))
    (net (code "44") (name "/Arduino MIDI/MUX_S0") (class "Default")
      (node (ref "U14") (pin "25") (pinfunction "PD4") (pintype "bidirectional"))
      (node (ref "U16") (pin "10") (pinfunction "S0") (pintype "unspecified")))
    (net (code "45") (name "/Arduino MIDI/MUX_S1") (class "Default")
      (node (ref "U14") (pin "26") (pinfunction "PD6") (pintype "bidirectional"))
      (node (ref "U16") (pin "11") (pinfunction "S1") (pintype "unspecified")))
    (net (code "46") (name "/Arduino MIDI/MUX_S2") (class "Default")
      (node (ref "U14") (pin "27") (pinfunction "PD7") (pintype "bidirectional"))
      (node (ref "U16") (pin "14") (pinfunction "S2") (pintype "unspecified")))
    (net (code "47") (name "/Arduino MIDI/MUX_S3") (class "Default")
      (node (ref "U14") (pin "22") (pinfunction "PD5") (pintype "bidirectional"))
      (node (ref "U16") (pin "13") (pinfunction "S3") (pintype "unspecified")))
    (net (code "48") (name "/Arduino MIDI/MUX_SIG") (class "Default")
      (node (ref "U14") (pin "41") (pinfunction "PF0") (pintype "bidirectional"))
      (node (ref "U16") (pin "1") (pinfunction "Z") (pintype "unspecified")))
    (net (code "49") (name "/Arduino MIDI/RELEASE_BRAKE_ADIN") (class "Default")
      (node (ref "J21") (pin "6") (pinfunction "Pin_6") (pintype "passive"))
      (node (ref "U16") (pin "7") (pinfunction "Y2") (pintype "unspecified")))
    (net (code "50") (name "/Arduino MIDI/TOUCH_BRAKE_ADIN") (class "Default")
      (node (ref "J21") (pin "5") (pinfunction "Pin_5") (pintype "passive"))
      (node (ref "U16") (pin "8") (pinfunction "Y1") (pintype "unspecified")))
    (net (code "51") (name "/Arduino MIDI/TRACK_ENC_A") (class "Default")
      (node (ref "J21") (pin "2") (pinfunction "Pin_2") (pintype "passive"))
      (node (ref "U14") (pin "30") (pinfunction "PB6") (pintype "bidirectional")))
    (net (code "52") (name "/Arduino MIDI/TRACK_ENC_B") (class "Default")
      (node (ref "J21") (pin "3") (pinfunction "Pin_3") (pintype "passive"))
      (node (ref "U14") (pin "31") (pinfunction "PC6") (pintype "bidirectional")))
    (net (code "53") (name "/Arduino MIDI/TRACK_ENC_PUSH") (class "Default")
      (node (ref "J21") (pin "4") (pinfunction "Pin_4") (pintype "passive"))
      (node (ref "U14") (pin "12") (pinfunction "PB7") (pintype "bidirectional")))
    (net (code "54") (name "/Audio Outputs/RCA_LEFT") (class "Default")
      (node (ref "C13") (pin "1") (pintype "passive"))
      (node (ref "J2") (pin "6") (pinfunction "LEFT_P") (pintype "passive"))
      (node (ref "J3") (pin "2") (pinfunction "SIGNL") (pintype "passive"))
      (node (ref "J5") (pin "2") (pinfunction "LEFT_P") (pintype "passive"))
      (node (ref "R13") (pin "2") (pintype "passive")))
    (net (code "55") (name "/Audio Outputs/RCA_RIGHT") (class "Default")
      (node (ref "C11") (pin "1") (pintype "passive"))
      (node (ref "J2") (pin "4") (pinfunction "RIGHT_P") (pintype "passive"))
      (node (ref "J4") (pin "2") (pinfunction "SIGNL") (pintype "passive"))
      (node (ref "J5") (pin "3") (pinfunction "RIGHT_P") (pintype "passive"))
      (node (ref "R12") (pin "2") (pintype "passive")))
    (net (code "56") (name "/Compute Module/SD_CLK") (class "Default")
      (node (ref "R69") (pin "1") (pintype "passive"))
      (node (ref "U1") (pin "57") (pinfunction "SD_CLK") (pintype "passive"))
      (node (ref "U23") (pin "1") (pinfunction "I/O1") (pintype "input"))
      (node (ref "U23") (pin "6") (pinfunction "I/O1") (pintype "input")))
    (net (code "57") (name "/Compute Module/SD_CMD") (class "Default")
      (node (ref "R70") (pin "2") (pintype "passive"))
      (node (ref "U1") (pin "62") (pinfunction "SD_CMD") (pintype "passive"))
      (node (ref "U20") (pin "3") (pinfunction "CMD") (pintype "input"))
      (node (ref "U23") (pin "3") (pinfunction "I/O2") (pintype "input"))
      (node (ref "U23") (pin "4") (pinfunction "I/O2") (pintype "input")))
    (net (code "58") (name "/Compute Module/SD_DAT0") (class "Default")
      (node (ref "R76") (pin "2") (pintype "passive"))
      (node (ref "U1") (pin "63") (pinfunction "SD_DAT0") (pintype "passive"))
      (node (ref "U20") (pin "7") (pinfunction "DAT0") (pintype "input"))
      (node (ref "U7") (pin "1") (pinfunction "I/O1") (pintype "input"))
      (node (ref "U7") (pin "6") (pinfunction "I/O1") (pintype "input")))
    (net (code "59") (name "/Compute Module/SD_DAT1") (class "Default")
      (node (ref "R75") (pin "2") (pintype "passive"))
      (node (ref "U1") (pin "67") (pinfunction "SD_DAT1") (pintype "passive"))
      (node (ref "U20") (pin "8") (pinfunction "DAT1") (pintype "input"))
      (node (ref "U7") (pin "3") (pinfunction "I/O2") (pintype "input"))
      (node (ref "U7") (pin "4") (pinfunction "I/O2") (pintype "input")))
    (net (code "60") (name "/Compute Module/SD_DAT2") (class "Default")
      (node (ref "R74") (pin "2") (pintype "passive"))
      (node (ref "U1") (pin "69") (pinfunction "SD_DAT2") (pintype "passive"))
      (node (ref "U20") (pin "1") (pinfunction "DAT2") (pintype "input"))
      (node (ref "U21") (pin "3") (pinfunction "I/O2") (pintype "input"))
      (node (ref "U21") (pin "4") (pinfunction "I/O2") (pintype "input")))
    (net (code "61") (name "/Compute Module/SD_DAT3") (class "Default")
      (node (ref "R72") (pin "2") (pintype "passive"))
      (node (ref "U1") (pin "61") (pinfunction "SD_DAT3") (pintype "passive"))
      (node (ref "U20") (pin "2") (pinfunction "CD/DAT3") (pintype "input"))
      (node (ref "U21") (pin "1") (pinfunction "I/O1") (pintype "input"))
      (node (ref "U21") (pin "6") (pinfunction "I/O1") (pintype "input")))
    (net (code "62") (name "/Compute Module/SD_PWR_ON") (class "Default")
      (node (ref "Q1") (pin "1") (pinfunction "G") (pintype "input"))
      (node (ref "R71") (pin "2") (pintype "passive"))
      (node (ref "U1") (pin "75") (pinfunction "SD_PWR_ON") (pintype "output")))
    (net (code "63") (name "/Compute Module/SD_VDD") (class "Default")
      (node (ref "C76") (pin "2") (pintype "passive"))
      (node (ref "Q2") (pin "3") (pinfunction "D") (pintype "passive"))
      (node (ref "U20") (pin "4") (pinfunction "VDD") (pintype "input")))
    (net (code "64") (name "/Compute Module/S_BOOT_GND") (class "Default")
      (node (ref "SW1") (pin "3") (pinfunction "A3") (pintype "input"))
      (node (ref "U1") (pin "93") (pinfunction "~{nRPIBOOT}") (pintype "input")))
    (net (code "65") (name "/Compute Module/S_BT_GND") (class "Default")
      (node (ref "SW1") (pin "2") (pinfunction "A2") (pintype "input"))
      (node (ref "U1") (pin "91") (pinfunction "~{BT_nDisable}") (pintype "input")))
    (net (code "66") (name "/Compute Module/S_EEPROM_WP_GND") (class "Default")
      (node (ref "SW1") (pin "4") (pinfunction "A4") (pintype "input"))
      (node (ref "U1") (pin "20") (pinfunction "EEPROM_nWP") (pintype "input")))
    (net (code "67") (name "/Compute Module/S_WIFI_GND") (class "Default")
      (node (ref "SW1") (pin "1") (pinfunction "A1") (pintype "input"))
      (node (ref "U1") (pin "89") (pinfunction "~{WL_nDisable}") (pintype "input")))
    (net (code "68") (name "/HDMI and Ethernet/eth_nled_2") (class "Default")
      (node (ref "J12") (pin "13") (pinfunction "13") (pintype "passive"))
      (node (ref "U1") (pin "17") (pinfunction "~{Ethernet_nLED2}") (pintype "output")))
    (net (code "69") (name "/HDMI and Ethernet/eth_nled_3") (class "Default")
      (node (ref "J12") (pin "12") (pinfunction "12") (pintype "passive"))
      (node (ref "U1") (pin "15") (pinfunction "~{Ethernet_nLED3}") (pintype "output")))
    (net (code "70") (name "/HDMI and Ethernet/eth_p0_n") (class "Default")
      (node (ref "J12") (pin "3") (pinfunction "MDI0-") (pintype "input"))
      (node (ref "U1") (pin "10") (pinfunction "Ethernet_Pair0_N") (pintype "passive")))
    (net (code "71") (name "/HDMI and Ethernet/eth_p0_p") (class "Default")
      (node (ref "J12") (pin "2") (pinfunction "MDI0+") (pintype "input"))
      (node (ref "U1") (pin "12") (pinfunction "Ethernet_Pair0_P") (pintype "passive")))
    (net (code "72") (name "/HDMI and Ethernet/eth_p1_n") (class "Default")
      (node (ref "J12") (pin "7") (pinfunction "MDI1-") (pintype "input"))
      (node (ref "U1") (pin "6") (pinfunction "Ethernet_Pair1_N") (pintype "passive")))
    (net (code "73") (name "/HDMI and Ethernet/eth_p1_p") (class "Default")
      (node (ref "J12") (pin "4") (pinfunction "MDI1+") (pintype "input"))
      (node (ref "U1") (pin "4") (pinfunction "Ethernet_Pair1_P") (pintype "passive")))
    (net (code "74") (name "/HDMI and Ethernet/eth_p2_n") (class "Default")
      (node (ref "J12") (pin "6") (pinfunction "MDI2-") (pintype "input"))
      (node (ref "U1") (pin "9") (pinfunction "Ethernet_Pair2_N") (pintype "passive")))
    (net (code "75") (name "/HDMI and Ethernet/eth_p2_p") (class "Default")
      (node (ref "J12") (pin "5") (pinfunction "MDI2+") (pintype "input"))
      (node (ref "U1") (pin "11") (pinfunction "Ethernet_Pair2_P") (pintype "passive")))
    (net (code "76") (name "/HDMI and Ethernet/eth_p3_n") (class "Default")
      (node (ref "J12") (pin "9") (pinfunction "MDI3-") (pintype "input"))
      (node (ref "U1") (pin "5") (pinfunction "Ethernet_Pair3_N") (pintype "passive")))
    (net (code "77") (name "/HDMI and Ethernet/eth_p3_p") (class "Default")
      (node (ref "J12") (pin "8") (pinfunction "MDI3+") (pintype "input"))
      (node (ref "U1") (pin "3") (pinfunction "Ethernet_Pair3_P") (pintype "passive")))
    (net (code "78") (name "/Sim_Buck/LX_PIN") (class "Default")
      (node (ref "C69") (pin "1") (pintype "passive"))
      (node (ref "L3") (pin "2") (pinfunction "2") (pintype "passive"))
      (node (ref "U15") (pin "2") (pinfunction "LX") (pintype "unspecified")))
    (net (code "79") (name "/Sim_Buck/VIN") (class "Default")
      (node (ref "C67") (pin "1") (pintype "passive"))
      (node (ref "C68") (pin "1") (pintype "passive"))
      (node (ref "R44") (pin "1") (pintype "passive"))
      (node (ref "U15") (pin "4") (pinfunction "IN") (pintype "unspecified"))
      (node (ref "U15") (pin "5") (pinfunction "IN") (pintype "unspecified"))
      (node (ref "U15") (pin "6") (pinfunction "IN") (pintype "unspecified"))
      (node (ref "V1") (pin "1") (pintype "passive")))
    (net (code "80") (name "/Sim_Buck/VOUT") (class "Default")
      (node (ref "C70") (pin "2") (pintype "passive"))
      (node (ref "C71") (pin "2") (pintype "passive"))
      (node (ref "C72") (pin "2") (pintype "passive"))
      (node (ref "C73") (pin "2") (pintype "passive"))
      (node (ref "R38") (pin "1") (pintype "passive"))
      (node (ref "R46") (pin "1") (pintype "passive"))
      (node (ref "R48") (pin "2") (pintype "passive"))
      (node (ref "R50") (pin "2") (pintype "passive")))
    (net (code "81") (name "/Sim_Buck/VOUT_L") (class "Default")
      (node (ref "L3") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "R38") (pin "2") (pintype "passive")))
    (net (code "82") (name "/Sim_DAC/AVDD") (class "Default")
      (node (ref "C82") (pin "2") (pintype "passive"))
      (node (ref "FEB3") (pin "2") (pintype "passive"))
      (node (ref "R42") (pin "1") (pintype "passive"))
      (node (ref "U17") (pin "1") (pinfunction "CPVDD") (pintype "power_in"))
      (node (ref "U17") (pin "8") (pinfunction "AVDD") (pintype "power_in"))
      (node (ref "V2") (pin "1") (pintype "passive")))
    (net (code "83") (name "/Sim_DAC/COUPLED_L") (class "Default")
      (node (ref "C87") (pin "1") (pintype "passive"))
      (node (ref "R43") (pin "1") (pintype "passive")))
    (net (code "84") (name "/Sim_DAC/COUPLED_R") (class "Default")
      (node (ref "C89") (pin "1") (pintype "passive"))
      (node (ref "R51") (pin "1") (pintype "passive")))
    (net (code "85") (name "/Sim_DAC/DVDD") (class "Default")
      (node (ref "C80") (pin "2") (pintype "passive"))
      (node (ref "C81") (pin "2") (pintype "passive"))
      (node (ref "U17") (pin "28") (pinfunction "DVDD") (pintype "power_in"))
      (node (ref "V4") (pin "1") (pintype "passive")))
    (net (code "86") (name "/Sim_DAC/OUT_L") (class "Default")
      (node (ref "C88") (pin "1") (pintype "passive"))
      (node (ref "R39") (pin "2") (pintype "passive"))
      (node (ref "R43") (pin "2") (pintype "passive")))
    (net (code "87") (name "/Sim_DAC/OUT_R") (class "Default")
      (node (ref "C90") (pin "1") (pintype "passive"))
      (node (ref "R40") (pin "2") (pintype "passive"))
      (node (ref "R51") (pin "2") (pintype "passive")))
    (net (code "88") (name "/USB DJ Ports/USB_AUX_POWR_VBUS") (class "Default")
      (node (ref "C15") (pin "2") (pintype "passive"))
      (node (ref "J8") (pin "1") (pinfunction "VBUS") (pintype "power_in"))
      (node (ref "U3") (pin "6") (pinfunction "OUT") (pintype "unspecified")))
    (net (code "89") (name "/USB DJ Ports/USB_C_DJ_DM") (class "Default")
      (node (ref "U1") (pin "103") (pinfunction "USB_N") (pintype "passive"))
      (node (ref "U22") (pin "3") (pinfunction "I/O2") (pintype "input")))
    (net (code "90") (name "/USB DJ Ports/USB_C_DJ_DP") (class "Default")
      (node (ref "U1") (pin "105") (pinfunction "USB_P") (pintype "passive"))
      (node (ref "U22") (pin "1") (pinfunction "I/O1") (pintype "input")))
    (net (code "91") (name "/USB DJ Ports/USB_C_DJ_VBUS") (class "Default")
      (node (ref "C17") (pin "2") (pintype "passive"))
      (node (ref "J9") (pin "11") (pinfunction "VBUS") (pintype "unspecified"))
      (node (ref "J9") (pin "2") (pinfunction "VBUS") (pintype "unspecified"))
      (node (ref "U4") (pin "6") (pinfunction "OUT") (pintype "unspecified")))
    (net (code "92") (name "/USB DJ Ports/USB_DJ_DM") (class "Default")
      (node (ref "U1") (pin "136") (pinfunction "USB3-0-DM") (pintype "bidirectional"))
      (node (ref "U8") (pin "6") (pinfunction "I/O1") (pintype "input")))
    (net (code "93") (name "/USB DJ Ports/USB_DJ_DP") (class "Default")
      (node (ref "U1") (pin "134") (pinfunction "USB3-0-DP") (pintype "bidirectional"))
      (node (ref "U8") (pin "4") (pinfunction "I/O2") (pintype "input")))
    (net (code "94") (name "/USB DJ Ports/USB_DJ_SSRXM") (class "Default")
      (node (ref "J10") (pin "5") (pinfunction "SSRX-") (pintype "output"))
      (node (ref "U1") (pin "128") (pinfunction "USB3-0-RX_N") (pintype "input")))
    (net (code "95") (name "/USB DJ Ports/USB_DJ_SSRXP") (class "Default")
      (node (ref "J10") (pin "6") (pinfunction "SSRX+") (pintype "output"))
      (node (ref "U1") (pin "130") (pinfunction "USB3-0-RX_P") (pintype "input")))
    (net (code "96") (name "/USB DJ Ports/USB_DJ_SSTXM") (class "Default")
      (node (ref "J10") (pin "8") (pinfunction "SSTX-") (pintype "input"))
      (node (ref "U1") (pin "140") (pinfunction "USB3-0-TX_N") (pintype "output")))
    (net (code "97") (name "/USB DJ Ports/USB_DJ_SSTXP") (class "Default")
      (node (ref "J10") (pin "9") (pinfunction "SSTX+") (pintype "input"))
      (node (ref "U1") (pin "142") (pinfunction "USB3-0-TX_P") (pintype "output")))
    (net (code "98") (name "/USB DJ Ports/USB_DJ_VBUS") (class "Default")
      (node (ref "C19") (pin "2") (pintype "passive"))
      (node (ref "J10") (pin "1") (pinfunction "VBUS") (pintype "power_in"))
      (node (ref "U5") (pin "6") (pinfunction "OUT") (pintype "unspecified")))
    (net (code "99") (name "/USB DJ Ports/USB_DJ_VBUS_EN") (class "Default")
      (node (ref "R17") (pin "2") (pintype "passive"))
      (node (ref "R19") (pin "2") (pintype "passive"))
      (node (ref "U1") (pin "111") (pinfunction "VBUS_EN") (pintype "input"))
      (node (ref "U4") (pin "3") (pinfunction "EN") (pintype "unspecified"))
      (node (ref "U5") (pin "3") (pinfunction "EN") (pintype "unspecified")))
    (net (code "100") (name "/USB DJ Ports/USB_SCR_DM") (class "Default")
      (node (ref "U1") (pin "165") (pinfunction "USB3-1-DM") (pintype "bidirectional"))
      (node (ref "U6") (pin "6") (pinfunction "I/O1") (pintype "input")))
    (net (code "101") (name "/USB DJ Ports/USB_SCR_DP") (class "Default")
      (node (ref "U1") (pin "163") (pinfunction "USB3-1-DP") (pintype "bidirectional"))
      (node (ref "U6") (pin "4") (pinfunction "I/O2") (pintype "input")))
    (net (code "102") (name "/USB DJ Ports/USB_SCR_SSRXM") (class "Default")
      (node (ref "J11") (pin "5") (pinfunction "SSRX-") (pintype "output"))
      (node (ref "U1") (pin "157") (pinfunction "USB3-1-RX_N") (pintype "input")))
    (net (code "103") (name "/USB DJ Ports/USB_SCR_SSRXP") (class "Default")
      (node (ref "J11") (pin "6") (pinfunction "SSRX+") (pintype "output"))
      (node (ref "U1") (pin "159") (pinfunction "USB3-1-RX_P") (pintype "input")))
    (net (code "104") (name "/USB DJ Ports/USB_SCR_SSTXM") (class "Default")
      (node (ref "J11") (pin "8") (pinfunction "SSTX-") (pintype "input"))
      (node (ref "U1") (pin "169") (pinfunction "USB3-1-TX_N") (pintype "output")))
    (net (code "105") (name "/USB DJ Ports/USB_SCR_SSTXP") (class "Default")
      (node (ref "J11") (pin "9") (pinfunction "SSTX+") (pintype "input"))
      (node (ref "U1") (pin "171") (pinfunction "USB3-1-TX_P") (pintype "output")))
    (net (code "106") (name "/USB DJ Ports/USB_SCR_VBUS") (class "Default")
      (node (ref "C23") (pin "2") (pintype "passive"))
      (node (ref "J11") (pin "1") (pinfunction "VBUS") (pintype "power_in"))
      (node (ref "U9") (pin "6") (pinfunction "OUT") (pintype "unspecified")))
    (net (code "107") (name "0") (class "Default")
      (node (ref "C59") (pin "2") (pintype "passive"))
      (node (ref "C67") (pin "2") (pintype "passive"))
      (node (ref "C68") (pin "2") (pintype "passive"))
      (node (ref "C70") (pin "1") (pintype "passive"))
      (node (ref "C71") (pin "1") (pintype "passive"))
      (node (ref "C72") (pin "1") (pintype "passive"))
      (node (ref "C74") (pin "2") (pintype "passive"))
      (node (ref "C79") (pin "1") (pintype "passive"))
      (node (ref "C80") (pin "1") (pintype "passive"))
      (node (ref "C81") (pin "1") (pintype "passive"))
      (node (ref "C82") (pin "1") (pintype "passive"))
      (node (ref "C83") (pin "2") (pintype "passive"))
      (node (ref "C84") (pin "2") (pintype "passive"))
      (node (ref "C86") (pin "1") (pintype "passive"))
      (node (ref "C88") (pin "2") (pintype "passive"))
      (node (ref "C90") (pin "2") (pintype "passive"))
      (node (ref "R39") (pin "1") (pintype "passive"))
      (node (ref "R40") (pin "1") (pintype "passive"))
      (node (ref "R45") (pin "2") (pintype "passive"))
      (node (ref "R49") (pin "2") (pintype "passive"))
      (node (ref "R50") (pin "1") (pintype "passive"))
      (node (ref "U15") (pin "1") (pinfunction "GND") (pintype "unspecified"))
      (node (ref "U15") (pin "10") (pinfunction "ILMT") (pintype "unspecified"))
      (node (ref "U15") (pin "3") (pinfunction "GND") (pintype "unspecified"))
      (node (ref "U17") (pin "27") (pinfunction "DGND") (pintype "power_in"))
      (node (ref "U17") (pin "3") (pinfunction "CPGND") (pintype "power_in"))
      (node (ref "U17") (pin "9") (pinfunction "AGND") (pintype "power_in"))
      (node (ref "V1") (pin "2") (pintype "passive"))
      (node (ref "V2") (pin "2") (pintype "passive"))
      (node (ref "V3") (pin "2") (pintype "passive")))
    (net (code "108") (name "GND") (class "Default")
      (node (ref "BT1") (pin "2") (pinfunction "2") (pintype "input"))
      (node (ref "C1") (pin "2") (pintype "passive"))
      (node (ref "C10") (pin "2") (pintype "passive"))
      (node (ref "C11") (pin "2") (pintype "passive"))
      (node (ref "C13") (pin "2") (pintype "passive"))
      (node (ref "C14") (pin "1") (pintype "passive"))
      (node (ref "C15") (pin "1") (pintype "passive"))
      (node (ref "C16") (pin "1") (pintype "passive"))
      (node (ref "C17") (pin "1") (pintype "passive"))
      (node (ref "C18") (pin "1") (pintype "passive"))
      (node (ref "C19") (pin "1") (pintype "passive"))
      (node (ref "C2") (pin "1") (pintype "passive"))
      (node (ref "C20") (pin "2") (pintype "passive"))
      (node (ref "C21") (pin "2") (pintype "passive"))
      (node (ref "C22") (pin "1") (pintype "passive"))
      (node (ref "C23") (pin "1") (pintype "passive"))
      (node (ref "C24") (pin "2") (pintype "passive"))
      (node (ref "C25") (pin "2") (pintype "passive"))
      (node (ref "C26") (pin "2") (pintype "passive"))
      (node (ref "C27") (pin "2") (pintype "passive"))
      (node (ref "C28") (pin "2") (pintype "passive"))
      (node (ref "C29") (pin "2") (pintype "passive"))
      (node (ref "C3") (pin "1") (pintype "passive"))
      (node (ref "C30") (pin "2") (pintype "passive"))
      (node (ref "C31") (pin "2") (pintype "passive"))
      (node (ref "C32") (pin "2") (pintype "passive"))
      (node (ref "C33") (pin "2") (pintype "passive"))
      (node (ref "C34") (pin "2") (pintype "passive"))
      (node (ref "C35") (pin "2") (pintype "passive"))
      (node (ref "C36") (pin "2") (pintype "passive"))
      (node (ref "C37") (pin "2") (pintype "passive"))
      (node (ref "C38") (pin "2") (pintype "passive"))
      (node (ref "C39") (pin "1") (pintype "passive"))
      (node (ref "C4") (pin "1") (pintype "passive"))
      (node (ref "C40") (pin "1") (pintype "passive"))
      (node (ref "C41") (pin "1") (pintype "passive"))
      (node (ref "C42") (pin "2") (pintype "passive"))
      (node (ref "C43") (pin "2") (pintype "passive"))
      (node (ref "C45") (pin "1") (pintype "passive"))
      (node (ref "C46") (pin "1") (pintype "passive"))
      (node (ref "C48") (pin "2") (pintype "passive"))
      (node (ref "C49") (pin "2") (pintype "passive"))
      (node (ref "C5") (pin "1") (pintype "passive"))
      (node (ref "C50") (pin "1") (pintype "passive"))
      (node (ref "C51") (pin "1") (pintype "passive"))
      (node (ref "C53") (pin "1") (pintype "passive"))
      (node (ref "C54") (pin "2") (pintype "passive"))
      (node (ref "C55") (pin "1") (pintype "passive"))
      (node (ref "C56") (pin "1") (pintype "passive"))
      (node (ref "C57") (pin "1") (pintype "passive"))
      (node (ref "C58") (pin "2") (pintype "passive"))
      (node (ref "C6") (pin "2") (pintype "passive"))
      (node (ref "C60") (pin "2") (pintype "passive"))
      (node (ref "C61") (pin "2") (pintype "passive"))
      (node (ref "C62") (pin "2") (pintype "passive"))
      (node (ref "C63") (pin "2") (pintype "passive"))
      (node (ref "C65") (pin "2") (pintype "passive"))
      (node (ref "C66") (pin "2") (pintype "passive"))
      (node (ref "C7") (pin "2") (pintype "passive"))
      (node (ref "C75") (pin "2") (pintype "passive"))
      (node (ref "C76") (pin "1") (pintype "passive"))
      (node (ref "D1") (pin "1") (pinfunction "K") (pintype "unspecified"))
      (node (ref "D2") (pin "1") (pinfunction "K") (pintype "unspecified"))
      (node (ref "D3") (pin "1") (pinfunction "K") (pintype "unspecified"))
      (node (ref "D4") (pin "1") (pintype "passive"))
      (node (ref "D5") (pin "1") (pinfunction "K") (pintype "unspecified"))
      (node (ref "J1") (pin "1") (pinfunction "Pin_1") (pintype "passive"))
      (node (ref "J10") (pin "10") (pinfunction "SHIELD") (pintype "passive"))
      (node (ref "J10") (pin "4") (pinfunction "GND") (pintype "power_in"))
      (node (ref "J10") (pin "7") (pinfunction "DRAIN") (pintype "passive"))
      (node (ref "J11") (pin "10") (pinfunction "SHIELD") (pintype "passive"))
      (node (ref "J11") (pin "4") (pinfunction "GND") (pintype "power_in"))
      (node (ref "J11") (pin "7") (pinfunction "DRAIN") (pintype "passive"))
      (node (ref "J12") (pin "SHIELD0") (pinfunction "SHIELD0") (pintype "passive"))
      (node (ref "J12") (pin "SHIELD1") (pinfunction "SHIELD1") (pintype "passive"))
      (node (ref "J13") (pin "10") (pinfunction "D0S") (pintype "power_in"))
      (node (ref "J13") (pin "13") (pinfunction "CKS") (pintype "power_in"))
      (node (ref "J13") (pin "16") (pinfunction "GND") (pintype "power_in"))
      (node (ref "J13") (pin "4") (pinfunction "D2S") (pintype "power_in"))
      (node (ref "J13") (pin "7") (pinfunction "D1S") (pintype "power_in"))
      (node (ref "J13") (pin "SH") (pinfunction "SH") (pintype "passive"))
      (node (ref "J14") (pin "10") (pinfunction "D0S") (pintype "power_in"))
      (node (ref "J14") (pin "13") (pinfunction "CKS") (pintype "power_in"))
      (node (ref "J14") (pin "16") (pinfunction "GND") (pintype "power_in"))
      (node (ref "J14") (pin "4") (pinfunction "D2S") (pintype "power_in"))
      (node (ref "J14") (pin "7") (pinfunction "D1S") (pintype "power_in"))
      (node (ref "J14") (pin "SH") (pinfunction "SH") (pintype "passive"))
      (node (ref "J15") (pin "1") (pinfunction "EH") (pintype "unspecified"))
      (node (ref "J15") (pin "2") (pinfunction "EH") (pintype "unspecified"))
      (node (ref "J15") (pin "3") (pinfunction "EH") (pintype "unspecified"))
      (node (ref "J15") (pin "4") (pinfunction "EH") (pintype "unspecified"))
      (node (ref "J15") (pin "A1B12") (pinfunction "GND") (pintype "unspecified"))
      (node (ref "J15") (pin "B1A12") (pinfunction "GND") (pintype "unspecified"))
      (node (ref "J16") (pin "5") (pinfunction "Pin_5") (pintype "passive"))
      (node (ref "J17") (pin "8") (pinfunction "Pin_8") (pintype "passive"))
      (node (ref "J18") (pin "10") (pinfunction "Pin_10") (pintype "passive"))
      (node (ref "J19") (pin "11") (pinfunction "Pin_11") (pintype "passive"))
      (node (ref "J19") (pin "12") (pinfunction "Pin_12") (pintype "passive"))
      (node (ref "J2") (pin "2") (pinfunction "GND/SHLD") (pintype "passive"))
      (node (ref "J20") (pin "10") (pinfunction "Pin_10") (pintype "passive"))
      (node (ref "J21") (pin "8") (pinfunction "Pin_8") (pintype "passive"))
      (node (ref "J3") (pin "1A") (pinfunction "SHLD") (pintype "passive"))
      (node (ref "J3") (pin "1B") (pinfunction "SHLD") (pintype "passive"))
      (node (ref "J3") (pin "1C") (pinfunction "SHLD") (pintype "passive"))
      (node (ref "J4") (pin "1A") (pinfunction "SHLD") (pintype "passive"))
      (node (ref "J4") (pin "1B") (pinfunction "SHLD") (pintype "passive"))
      (node (ref "J4") (pin "1C") (pinfunction "SHLD") (pintype "passive"))
      (node (ref "J5") (pin "1") (pinfunction "GND/SHLD") (pintype "passive"))
      (node (ref "J6") (pin "6") (pinfunction "Pin_6") (pintype "passive"))
      (node (ref "J7") (pin "1") (pinfunction "Pin_1") (pintype "passive"))
      (node (ref "J8") (pin "4") (pinfunction "GND") (pintype "power_in"))
      (node (ref "J8") (pin "5") (pinfunction "Shield") (pintype "passive"))
      (node (ref "J9") (pin "1") (pinfunction "GND") (pintype "unspecified"))
      (node (ref "J9") (pin "12") (pinfunction "GND") (pintype "unspecified"))
      (node (ref "J9") (pin "13") (pinfunction "SHELL") (pintype "unspecified"))
      (node (ref "J9") (pin "14") (pinfunction "SHELL") (pintype "unspecified"))
      (node (ref "Q1") (pin "2") (pinfunction "S") (pintype "passive"))
      (node (ref "R10") (pin "1") (pintype "passive"))
      (node (ref "R14") (pin "1") (pintype "passive"))
      (node (ref "R15") (pin "2") (pintype "passive"))
      (node (ref "R16") (pin "1") (pintype "passive"))
      (node (ref "R17") (pin "1") (pintype "passive"))
      (node (ref "R18") (pin "1") (pintype "passive"))
      (node (ref "R19") (pin "1") (pintype "passive"))
      (node (ref "R2") (pin "1") (pintype "passive"))
      (node (ref "R20") (pin "1") (pintype "passive"))
      (node (ref "R21") (pin "2") (pintype "passive"))
      (node (ref "R22") (pin "2") (pintype "passive"))
      (node (ref "R23") (pin "1") (pintype "passive"))
      (node (ref "R24") (pin "1") (pintype "passive"))
      (node (ref "R3") (pin "1") (pintype "passive"))
      (node (ref "R31") (pin "2") (pintype "passive"))
      (node (ref "R35") (pin "2") (pintype "passive"))
      (node (ref "R41") (pin "2") (pintype "passive"))
      (node (ref "SW1") (pin "10") (pinfunction "B1") (pintype "input"))
      (node (ref "SW1") (pin "6") (pinfunction "B5") (pintype "input"))
      (node (ref "SW1") (pin "7") (pinfunction "B4") (pintype "input"))
      (node (ref "SW1") (pin "8") (pinfunction "B3") (pintype "input"))
      (node (ref "SW1") (pin "9") (pinfunction "B2") (pintype "input"))
      (node (ref "SW2") (pin "2") (pinfunction "2") (pintype "passive"))
      (node (ref "SW4") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "TP7") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U1") (pin "1") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "107") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "108") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "113") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "114") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "119") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "120") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "125") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "126") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "13") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "131") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "132") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "137") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "138") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "14") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "144") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "150") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "155") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "156") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "161") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "162") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "167") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "168") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "173") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "174") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "179") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "180") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "185") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "186") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "191") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "192") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "197") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "198") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "2") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "22") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "23") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "32") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "33") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "42") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "43") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "52") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "53") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "59") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "60") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "65") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "66") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "7") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "71") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "74") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "8") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "98") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U10") (pin "2") (pinfunction "GND") (pintype "power_in"))
      (node (ref "U11") (pin "2") (pinfunction "GND") (pintype "power_in"))
      (node (ref "U12") (pin "11") (pinfunction "GND") (pintype "power_in"))
      (node (ref "U12") (pin "2") (pinfunction "CFG2") (pintype "passive"))
      (node (ref "U12") (pin "9") (pinfunction "CFG1") (pintype "passive"))
      (node (ref "U13") (pin "1") (pinfunction "GND") (pintype "unspecified"))
      (node (ref "U13") (pin "3") (pinfunction "GND") (pintype "unspecified"))
      (node (ref "U14") (pin "15") (pinfunction "GND") (pintype "power_in"))
      (node (ref "U14") (pin "23") (pinfunction "GND") (pintype "passive"))
      (node (ref "U14") (pin "35") (pinfunction "GND") (pintype "passive"))
      (node (ref "U14") (pin "43") (pinfunction "GND") (pintype "passive"))
      (node (ref "U14") (pin "5") (pinfunction "UGND") (pintype "passive"))
      (node (ref "U16") (pin "12") (pinfunction "GND") (pintype "unspecified"))
      (node (ref "U16") (pin "15") (pinfunction "E#") (pintype "unspecified"))
      (node (ref "U18") (pin "10") (pinfunction "VSS") (pintype "unspecified"))
      (node (ref "U18") (pin "15") (pinfunction "A0") (pintype "unspecified"))
      (node (ref "U18") (pin "16") (pinfunction "A1") (pintype "unspecified"))
      (node (ref "U18") (pin "17") (pinfunction "A2") (pintype "unspecified"))
      (node (ref "U19") (pin "10") (pinfunction "VSS") (pintype "unspecified"))
      (node (ref "U19") (pin "16") (pinfunction "A1") (pintype "unspecified"))
      (node (ref "U19") (pin "17") (pinfunction "A2") (pintype "unspecified"))
      (node (ref "U2") (pin "16") (pinfunction "ADR2/GPIO2/DOUT") (pintype "bidirectional"))
      (node (ref "U2") (pin "17") (pinfunction "MODE1") (pintype "input"))
      (node (ref "U2") (pin "18") (pinfunction "MODE2/MS") (pintype "input"))
      (node (ref "U2") (pin "20") (pinfunction "SCK") (pintype "input"))
      (node (ref "U2") (pin "24") (pinfunction "ADR1/MISO/FMT") (pintype "bidirectional"))
      (node (ref "U2") (pin "27") (pinfunction "DGND") (pintype "power_in"))
      (node (ref "U2") (pin "3") (pinfunction "CPGND") (pintype "power_in"))
      (node (ref "U2") (pin "9") (pinfunction "AGND") (pintype "power_in"))
      (node (ref "U20") (pin "10") (pinfunction "G3") (pintype "input"))
      (node (ref "U20") (pin "11") (pinfunction "G4") (pintype "input"))
      (node (ref "U20") (pin "12") (pinfunction "G1") (pintype "input"))
      (node (ref "U20") (pin "13") (pinfunction "G2") (pintype "input"))
      (node (ref "U20") (pin "6") (pinfunction "VSS") (pintype "input"))
      (node (ref "U21") (pin "2") (pinfunction "GND") (pintype "input"))
      (node (ref "U22") (pin "2") (pinfunction "GND") (pintype "input"))
      (node (ref "U23") (pin "2") (pinfunction "GND") (pintype "input"))
      (node (ref "U3") (pin "2") (pinfunction "GND") (pintype "unspecified"))
      (node (ref "U4") (pin "2") (pinfunction "GND") (pintype "unspecified"))
      (node (ref "U5") (pin "2") (pinfunction "GND") (pintype "unspecified"))
      (node (ref "U6") (pin "2") (pinfunction "GND") (pintype "input"))
      (node (ref "U7") (pin "2") (pinfunction "GND") (pintype "input"))
      (node (ref "U8") (pin "2") (pinfunction "GND") (pintype "input"))
      (node (ref "U9") (pin "2") (pinfunction "GND") (pintype "unspecified"))
      (node (ref "X1") (pin "2") (pinfunction "GND") (pintype "unspecified"))
      (node (ref "X1") (pin "4") (pinfunction "GND") (pintype "unspecified")))
    (net (code "109") (name "I2C_SCL") (class "Default")
      (node (ref "J7") (pin "3") (pinfunction "Pin_3") (pintype "passive"))
      (node (ref "R7") (pin "1") (pintype "passive"))
      (node (ref "TP8") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U1") (pin "80") (pinfunction "I2C_SCL0") (pintype "bidirectional"))
      (node (ref "U2") (pin "12") (pinfunction "SCL/MC/ATT1") (pintype "input")))
    (net (code "110") (name "I2C_SDA") (class "Default")
      (node (ref "J7") (pin "2") (pinfunction "Pin_2") (pintype "passive"))
      (node (ref "R5") (pin "1") (pintype "passive"))
      (node (ref "TP6") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U1") (pin "82") (pinfunction "I2C_SDA0") (pintype "bidirectional"))
      (node (ref "U2") (pin "11") (pinfunction "SDA/MOSI/ATT2") (pintype "bidirectional")))
    (net (code "111") (name "I2S_BCK") (class "Default")
      (node (ref "TP9") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U1") (pin "49") (pinfunction "GPIO18") (pintype "passive"))
      (node (ref "U2") (pin "21") (pinfunction "BCK") (pintype "bidirectional")))
    (net (code "112") (name "I2S_DIN") (class "Default")
      (node (ref "TP11") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U1") (pin "25") (pinfunction "GPIO21") (pintype "passive"))
      (node (ref "U2") (pin "22") (pinfunction "DIN") (pintype "input")))
    (net (code "113") (name "I2S_LRCLK") (class "Default")
      (node (ref "TP10") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U1") (pin "26") (pinfunction "GPIO19") (pintype "passive"))
      (node (ref "U2") (pin "23") (pinfunction "LRCK") (pintype "bidirectional")))
    (net (code "114") (name "ISP_MISO") (class "Default")
      (node (ref "J6") (pin "1") (pinfunction "Pin_1") (pintype "passive"))
      (node (ref "U14") (pin "11") (pinfunction "PB3") (pintype "bidirectional")))
    (net (code "115") (name "ISP_MOSI") (class "Default")
      (node (ref "J6") (pin "4") (pinfunction "Pin_4") (pintype "passive"))
      (node (ref "U14") (pin "10") (pinfunction "PB2") (pintype "bidirectional")))
    (net (code "116") (name "ISP_RESET") (class "Default")
      (node (ref "C53") (pin "2") (pintype "passive"))
      (node (ref "J6") (pin "3") (pinfunction "Pin_3") (pintype "passive"))
      (node (ref "R36") (pin "1") (pintype "passive"))
      (node (ref "SW4") (pin "2") (pinfunction "2") (pintype "passive"))
      (node (ref "U14") (pin "13") (pinfunction "~{RESET}") (pintype "input")))
    (net (code "117") (name "ISP_SCK") (class "Default")
      (node (ref "J16") (pin "2") (pinfunction "Pin_2") (pintype "passive"))
      (node (ref "J6") (pin "5") (pinfunction "Pin_5") (pintype "passive"))
      (node (ref "U14") (pin "9") (pinfunction "PB1") (pintype "bidirectional")))
    (net (code "118") (name "Net-(C2-Pad2)") (class "Default")
      (node (ref "C2") (pin "2") (pintype "passive"))
      (node (ref "FB1") (pin "1") (pintype "passive")))
    (net (code "119") (name "Net-(C9-Pad1)") (class "Default")
      (node (ref "C9") (pin "1") (pintype "passive"))
      (node (ref "R12") (pin "1") (pintype "passive")))
    (net (code "120") (name "Net-(C12-Pad1)") (class "Default")
      (node (ref "C12") (pin "1") (pintype "passive"))
      (node (ref "R13") (pin "1") (pintype "passive")))
    (net (code "121") (name "Net-(C47-Pad1)") (class "Default")
      (node (ref "C47") (pin "1") (pintype "passive"))
      (node (ref "R32") (pin "2") (pintype "passive")))
    (net (code "122") (name "Net-(C51-Pad2)") (class "Default")
      (node (ref "C51") (pin "2") (pintype "passive"))
      (node (ref "C52") (pin "1") (pintype "passive")))
    (net (code "123") (name "Net-(C73-Pad1)") (class "Default")
      (node (ref "C73") (pin "1") (pintype "passive"))
      (node (ref "R47") (pin "2") (pintype "passive")))
    (net (code "124") (name "Net-(C79-Pad2)") (class "Default")
      (node (ref "C79") (pin "2") (pintype "passive"))
      (node (ref "FEB3") (pin "1") (pintype "passive")))
    (net (code "125") (name "Net-(D1-A)") (class "Default")
      (node (ref "D1") (pin "2") (pinfunction "A") (pintype "unspecified"))
      (node (ref "R4") (pin "1") (pintype "passive")))
    (net (code "126") (name "Net-(D2-A)") (class "Default")
      (node (ref "D2") (pin "2") (pinfunction "A") (pintype "unspecified"))
      (node (ref "R6") (pin "2") (pintype "passive")))
    (net (code "127") (name "Net-(D3-A)") (class "Default")
      (node (ref "D3") (pin "2") (pinfunction "A") (pintype "unspecified"))
      (node (ref "R27") (pin "1") (pintype "passive")))
    (net (code "128") (name "Net-(D5-A)") (class "Default")
      (node (ref "D5") (pin "2") (pinfunction "A") (pintype "unspecified"))
      (node (ref "R29") (pin "2") (pintype "passive")))
    (net (code "129") (name "Net-(D6-A)") (class "Default")
      (node (ref "D6") (pin "2") (pinfunction "A") (pintype "unspecified"))
      (node (ref "R33") (pin "2") (pintype "passive")))
    (net (code "130") (name "Net-(D6-K)") (class "Default")
      (node (ref "D6") (pin "1") (pinfunction "K") (pintype "unspecified"))
      (node (ref "U13") (pin "11") (pinfunction "PG") (pintype "unspecified")))
    (net (code "131") (name "Net-(D8-A)") (class "Default")
      (node (ref "D8") (pin "2") (pinfunction "A") (pintype "passive"))
      (node (ref "R46") (pin "2") (pintype "passive")))
    (net (code "132") (name "Net-(D8-K)") (class "Default")
      (node (ref "D8") (pin "1") (pinfunction "K") (pintype "passive"))
      (node (ref "U15") (pin "11") (pinfunction "PG") (pintype "unspecified")))
    (net (code "133") (name "Net-(J1-Pin_3)") (class "Default")
      (node (ref "J1") (pin "3") (pinfunction "Pin_3") (pintype "passive"))
      (node (ref "U1") (pin "16") (pinfunction "Fan_tacho") (pintype "input")))
    (net (code "134") (name "Net-(J1-Pin_4)") (class "Default")
      (node (ref "J1") (pin "4") (pinfunction "Pin_4") (pintype "passive"))
      (node (ref "U1") (pin "19") (pinfunction "Fan_PWM") (pintype "output")))
    (net (code "135") (name "Net-(J9-CC1)") (class "Default")
      (node (ref "C21") (pin "1") (pintype "passive"))
      (node (ref "J9") (pin "4") (pinfunction "CC1") (pintype "unspecified"))
      (node (ref "R22") (pin "1") (pintype "passive")))
    (net (code "136") (name "Net-(J9-CC2)") (class "Default")
      (node (ref "C20") (pin "1") (pintype "passive"))
      (node (ref "J9") (pin "10") (pinfunction "CC2") (pintype "unspecified"))
      (node (ref "R21") (pin "1") (pintype "passive")))
    (net (code "137") (name "Net-(J9-DN1)") (class "Default")
      (node (ref "J9") (pin "5") (pinfunction "DN2") (pintype "unspecified"))
      (node (ref "J9") (pin "7") (pinfunction "DN1") (pintype "unspecified"))
      (node (ref "U22") (pin "4") (pinfunction "I/O2") (pintype "input")))
    (net (code "138") (name "Net-(J9-DP1)") (class "Default")
      (node (ref "J9") (pin "6") (pinfunction "DP1") (pintype "unspecified"))
      (node (ref "J9") (pin "8") (pinfunction "DP2") (pintype "unspecified"))
      (node (ref "U22") (pin "6") (pinfunction "I/O1") (pintype "input")))
    (net (code "139") (name "Net-(J10-D+)") (class "Default")
      (node (ref "J10") (pin "3") (pinfunction "D+") (pintype "bidirectional"))
      (node (ref "U8") (pin "3") (pinfunction "I/O2") (pintype "input")))
    (net (code "140") (name "Net-(J10-D-)") (class "Default")
      (node (ref "J10") (pin "2") (pinfunction "D-") (pintype "bidirectional"))
      (node (ref "U8") (pin "1") (pinfunction "I/O1") (pintype "input")))
    (net (code "141") (name "Net-(J11-D+)") (class "Default")
      (node (ref "J11") (pin "3") (pinfunction "D+") (pintype "bidirectional"))
      (node (ref "U6") (pin "3") (pinfunction "I/O2") (pintype "input")))
    (net (code "142") (name "Net-(J11-D-)") (class "Default")
      (node (ref "J11") (pin "2") (pinfunction "D-") (pintype "bidirectional"))
      (node (ref "U6") (pin "1") (pinfunction "I/O1") (pintype "input")))
    (net (code "143") (name "Net-(J12-Pad11)") (class "Default")
      (node (ref "J12") (pin "11") (pinfunction "11") (pintype "passive"))
      (node (ref "R26") (pin "1") (pintype "passive")))
    (net (code "144") (name "Net-(J12-Pad14)") (class "Default")
      (node (ref "J12") (pin "14") (pinfunction "14") (pintype "passive"))
      (node (ref "R25") (pin "1") (pintype "passive")))
    (net (code "145") (name "Net-(J13-CEC)") (class "Default")
      (node (ref "J13") (pin "15") (pinfunction "CEC") (pintype "bidirectional"))
      (node (ref "U1") (pin "151") (pinfunction "HDMI0_CEC") (pintype "open_collector")))
    (net (code "146") (name "Net-(J13-CK+)") (class "Default")
      (node (ref "J13") (pin "12") (pinfunction "CK+") (pintype "passive"))
      (node (ref "U1") (pin "188") (pinfunction "HDMI0_CLK_P") (pintype "output")))
    (net (code "147") (name "Net-(J13-CK-)") (class "Default")
      (node (ref "J13") (pin "14") (pinfunction "CK-") (pintype "passive"))
      (node (ref "U1") (pin "190") (pinfunction "HDMI0_CLK_N") (pintype "output")))
    (net (code "148") (name "Net-(J13-D0+)") (class "Default")
      (node (ref "J13") (pin "9") (pinfunction "D0+") (pintype "passive"))
      (node (ref "U1") (pin "182") (pinfunction "HDMI0_TX0_P") (pintype "output")))
    (net (code "149") (name "Net-(J13-D0-)") (class "Default")
      (node (ref "J13") (pin "11") (pinfunction "D0-") (pintype "passive"))
      (node (ref "U1") (pin "184") (pinfunction "HDMI0_TX0_N") (pintype "output")))
    (net (code "150") (name "Net-(J13-D1+)") (class "Default")
      (node (ref "J13") (pin "6") (pinfunction "D1+") (pintype "passive"))
      (node (ref "U1") (pin "176") (pinfunction "HDMI0_TX1_P") (pintype "output")))
    (net (code "151") (name "Net-(J13-D1-)") (class "Default")
      (node (ref "J13") (pin "8") (pinfunction "D1-") (pintype "passive"))
      (node (ref "U1") (pin "178") (pinfunction "HDMI0_TX1_N") (pintype "output")))
    (net (code "152") (name "Net-(J13-D2+)") (class "Default")
      (node (ref "J13") (pin "3") (pinfunction "D2+") (pintype "passive"))
      (node (ref "U1") (pin "170") (pinfunction "HDMI0_TX2_P") (pintype "output")))
    (net (code "153") (name "Net-(J13-D2-)") (class "Default")
      (node (ref "J13") (pin "5") (pinfunction "D2-") (pintype "passive"))
      (node (ref "U1") (pin "172") (pinfunction "HDMI0_TX2_N") (pintype "output")))
    (net (code "154") (name "Net-(J13-HPD{slash}HEAC-)") (class "Default")
      (node (ref "J13") (pin "1") (pinfunction "HPD/HEAC-") (pintype "passive"))
      (node (ref "U1") (pin "153") (pinfunction "HDMI0_HOTPLUG") (pintype "input")))
    (net (code "155") (name "Net-(J13-SCL)") (class "Default")
      (node (ref "J13") (pin "17") (pinfunction "SCL") (pintype "passive"))
      (node (ref "U1") (pin "200") (pinfunction "HDMI0_SCL") (pintype "open_collector")))
    (net (code "156") (name "Net-(J13-SDA)") (class "Default")
      (node (ref "J13") (pin "18") (pinfunction "SDA") (pintype "bidirectional"))
      (node (ref "U1") (pin "199") (pinfunction "HDMI0_SDA") (pintype "bidirectional")))
    (net (code "157") (name "Net-(J14-CEC)") (class "Default")
      (node (ref "J14") (pin "15") (pinfunction "CEC") (pintype "bidirectional"))
      (node (ref "U1") (pin "149") (pinfunction "HDMI1_CEC") (pintype "open_collector")))
    (net (code "158") (name "Net-(J14-CK+)") (class "Default")
      (node (ref "J14") (pin "12") (pinfunction "CK+") (pintype "passive"))
      (node (ref "U1") (pin "164") (pinfunction "HDMI1_CLK_P") (pintype "output")))
    (net (code "159") (name "Net-(J14-CK-)") (class "Default")
      (node (ref "J14") (pin "14") (pinfunction "CK-") (pintype "passive"))
      (node (ref "U1") (pin "166") (pinfunction "HDMI1_CLK_N") (pintype "output")))
    (net (code "160") (name "Net-(J14-D0+)") (class "Default")
      (node (ref "J14") (pin "9") (pinfunction "D0+") (pintype "passive"))
      (node (ref "U1") (pin "158") (pinfunction "HDMI1_TX0_P") (pintype "output")))
    (net (code "161") (name "Net-(J14-D0-)") (class "Default")
      (node (ref "J14") (pin "11") (pinfunction "D0-") (pintype "passive"))
      (node (ref "U1") (pin "160") (pinfunction "HDMI1_TX0_N") (pintype "output")))
    (net (code "162") (name "Net-(J14-D1+)") (class "Default")
      (node (ref "J14") (pin "6") (pinfunction "D1+") (pintype "passive"))
      (node (ref "U1") (pin "152") (pinfunction "HDMI1_TX1_P") (pintype "output")))
    (net (code "163") (name "Net-(J14-D1-)") (class "Default")
      (node (ref "J14") (pin "8") (pinfunction "D1-") (pintype "passive"))
      (node (ref "U1") (pin "154") (pinfunction "HDMI1_TX1_N") (pintype "output")))
    (net (code "164") (name "Net-(J14-D2+)") (class "Default")
      (node (ref "J14") (pin "3") (pinfunction "D2+") (pintype "passive"))
      (node (ref "U1") (pin "146") (pinfunction "HDMI1_TX2_P") (pintype "output")))
    (net (code "165") (name "Net-(J14-D2-)") (class "Default")
      (node (ref "J14") (pin "5") (pinfunction "D2-") (pintype "passive"))
      (node (ref "U1") (pin "148") (pinfunction "HDMI1_TX2_N") (pintype "output")))
    (net (code "166") (name "Net-(J14-HPD{slash}HEAC-)") (class "Default")
      (node (ref "J14") (pin "1") (pinfunction "HPD/HEAC-") (pintype "passive"))
      (node (ref "U1") (pin "143") (pinfunction "HDMI1_HOTPLUG") (pintype "input")))
    (net (code "167") (name "Net-(J14-SCL)") (class "Default")
      (node (ref "J14") (pin "17") (pinfunction "SCL") (pintype "passive"))
      (node (ref "U1") (pin "147") (pinfunction "HDMI1_SCL") (pintype "open_collector")))
    (net (code "168") (name "Net-(J14-SDA)") (class "Default")
      (node (ref "J14") (pin "18") (pinfunction "SDA") (pintype "bidirectional"))
      (node (ref "U1") (pin "145") (pinfunction "HDMI1_SDA") (pintype "bidirectional")))
    (net (code "169") (name "Net-(J15-CC1)") (class "Default")
      (node (ref "C33") (pin "1") (pintype "passive"))
      (node (ref "J15") (pin "A5") (pinfunction "CC1") (pintype "unspecified"))
      (node (ref "U12") (pin "7") (pinfunction "CC1") (pintype "bidirectional")))
    (net (code "170") (name "Net-(J15-CC2)") (class "Default")
      (node (ref "C29") (pin "1") (pintype "passive"))
      (node (ref "J15") (pin "B5") (pinfunction "CC2") (pintype "unspecified"))
      (node (ref "U12") (pin "6") (pinfunction "CC2") (pintype "bidirectional")))
    (net (code "171") (name "Net-(J15-DN1)") (class "Default")
      (node (ref "J15") (pin "A7") (pinfunction "DN1") (pintype "unspecified"))
      (node (ref "J15") (pin "B7") (pinfunction "DN2") (pintype "unspecified"))
      (node (ref "U12") (pin "5") (pinfunction "DM") (pintype "bidirectional")))
    (net (code "172") (name "Net-(J15-DP1)") (class "Default")
      (node (ref "J15") (pin "A6") (pinfunction "DP1") (pintype "unspecified"))
      (node (ref "J15") (pin "B6") (pinfunction "DP2") (pintype "unspecified"))
      (node (ref "U12") (pin "4") (pinfunction "DP") (pintype "bidirectional")))
    (net (code "173") (name "Net-(Q1-D)") (class "Default")
      (node (ref "Q1") (pin "3") (pinfunction "D") (pintype "passive"))
      (node (ref "Q2") (pin "1") (pinfunction "G") (pintype "input"))
      (node (ref "R73") (pin "2") (pintype "passive")))
    (net (code "174") (name "Net-(U1B-GPIO14)") (class "Default")
      (node (ref "R8") (pin "1") (pintype "passive"))
      (node (ref "U1") (pin "55") (pinfunction "GPIO14") (pintype "passive")))
    (net (code "175") (name "Net-(U1B-GPIO15)") (class "Default")
      (node (ref "R10") (pin "2") (pintype "passive"))
      (node (ref "R9") (pin "1") (pintype "passive"))
      (node (ref "U1") (pin "51") (pinfunction "GPIO15") (pintype "passive")))
    (net (code "176") (name "Net-(U1D-USB_OTG_ID)") (class "Default")
      (node (ref "R15") (pin "1") (pintype "passive"))
      (node (ref "U1") (pin "101") (pinfunction "USB_OTG_ID") (pintype "input")))
    (net (code "177") (name "Net-(U1J-CC1)") (class "USB,Default")
      (node (ref "R3") (pin "2") (pintype "passive"))
      (node (ref "U1") (pin "94") (pinfunction "CC1") (pintype "bidirectional")))
    (net (code "178") (name "Net-(U1J-CC2)") (class "USB,Default")
      (node (ref "R2") (pin "2") (pintype "passive"))
      (node (ref "U1") (pin "96") (pinfunction "CC2") (pintype "bidirectional")))
    (net (code "179") (name "Net-(U1J-PMIC_ENABLE)") (class "Default")
      (node (ref "R1") (pin "2") (pintype "passive"))
      (node (ref "U1") (pin "99") (pinfunction "PMIC_ENABLE") (pintype "input")))
    (net (code "180") (name "Net-(U1J-PWR_Button)") (class "Default")
      (node (ref "SW2") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U1") (pin "92") (pinfunction "PWR_Button") (pintype "passive")))
    (net (code "181") (name "Net-(U1J-VBAT)") (class "Default")
      (node (ref "BT1") (pin "1") (pinfunction "1") (pintype "input"))
      (node (ref "U1") (pin "76") (pinfunction "VBAT") (pintype "input")))
    (net (code "182") (name "Net-(U1J-~{PI_LED_nPWR})") (class "Default")
      (node (ref "R6") (pin "1") (pintype "passive"))
      (node (ref "U1") (pin "95") (pinfunction "~{PI_LED_nPWR}") (pintype "output")))
    (net (code "183") (name "Net-(U1J-~{Pi_nLED_Activity})") (class "Default")
      (node (ref "R4") (pin "2") (pintype "passive"))
      (node (ref "U1") (pin "21") (pinfunction "~{Pi_nLED_Activity}") (pintype "open_collector")))
    (net (code "184") (name "Net-(U2-CAPM)") (class "Default")
      (node (ref "C8") (pin "1") (pintype "passive"))
      (node (ref "U2") (pin "4") (pinfunction "CAPM") (pintype "passive")))
    (net (code "185") (name "Net-(U2-CAPP)") (class "Default")
      (node (ref "C8") (pin "2") (pintype "passive"))
      (node (ref "U2") (pin "2") (pinfunction "CAPP") (pintype "passive")))
    (net (code "186") (name "Net-(U2-LDOO)") (class "Default")
      (node (ref "C10") (pin "1") (pintype "passive"))
      (node (ref "C60") (pin "1") (pintype "passive"))
      (node (ref "U2") (pin "26") (pinfunction "LDOO") (pintype "passive")))
    (net (code "187") (name "Net-(U2-OUTL)") (class "Default")
      (node (ref "C12") (pin "2") (pintype "passive"))
      (node (ref "U2") (pin "6") (pinfunction "OUTL") (pintype "output")))
    (net (code "188") (name "Net-(U2-OUTR)") (class "Default")
      (node (ref "C9") (pin "2") (pintype "passive"))
      (node (ref "U2") (pin "7") (pinfunction "OUTR") (pintype "output")))
    (net (code "189") (name "Net-(U2-VCOM{slash}DEMP)") (class "Default")
      (node (ref "C7") (pin "1") (pintype "passive"))
      (node (ref "U2") (pin "10") (pinfunction "VCOM/DEMP") (pintype "bidirectional")))
    (net (code "190") (name "Net-(U2-VNEG)") (class "Default")
      (node (ref "C6") (pin "1") (pintype "passive"))
      (node (ref "U2") (pin "5") (pinfunction "VNEG") (pintype "passive")))
    (net (code "191") (name "Net-(U2-XSMT)") (class "Default")
      (node (ref "R11") (pin "1") (pintype "passive"))
      (node (ref "U2") (pin "25") (pinfunction "XSMT") (pintype "input")))
    (net (code "192") (name "Net-(U3-EN)") (class "Default")
      (node (ref "R14") (pin "2") (pintype "passive"))
      (node (ref "U3") (pin "3") (pinfunction "EN") (pintype "unspecified")))
    (net (code "193") (name "Net-(U3-ILIM)") (class "Default")
      (node (ref "R16") (pin "2") (pintype "passive"))
      (node (ref "U3") (pin "5") (pinfunction "ILIM") (pintype "unspecified")))
    (net (code "194") (name "Net-(U4-ILIM)") (class "Default")
      (node (ref "R18") (pin "2") (pintype "passive"))
      (node (ref "U4") (pin "5") (pinfunction "ILIM") (pintype "unspecified")))
    (net (code "195") (name "Net-(U5-ILIM)") (class "Default")
      (node (ref "R20") (pin "2") (pintype "passive"))
      (node (ref "U5") (pin "5") (pinfunction "ILIM") (pintype "unspecified")))
    (net (code "196") (name "Net-(U9-EN)") (class "Default")
      (node (ref "R23") (pin "2") (pintype "passive"))
      (node (ref "U9") (pin "3") (pinfunction "EN") (pintype "unspecified")))
    (net (code "197") (name "Net-(U9-ILIM)") (class "Default")
      (node (ref "R24") (pin "2") (pintype "passive"))
      (node (ref "U9") (pin "5") (pinfunction "ILIM") (pintype "unspecified")))
    (net (code "198") (name "Net-(U12-PG)") (class "Default")
      (node (ref "R29") (pin "1") (pintype "passive"))
      (node (ref "U12") (pin "10") (pinfunction "PG") (pintype "open_collector")))
    (net (code "199") (name "Net-(U12-VBUS)") (class "Default")
      (node (ref "SW3") (pin "2") (pinfunction "2") (pintype "unspecified"))
      (node (ref "U12") (pin "8") (pinfunction "VBUS") (pintype "passive")))
    (net (code "200") (name "Net-(U12-VDD)") (class "Default")
      (node (ref "C36") (pin "1") (pintype "passive"))
      (node (ref "D4") (pin "2") (pintype "passive"))
      (node (ref "R28") (pin "2") (pintype "passive"))
      (node (ref "U12") (pin "1") (pinfunction "VDD") (pintype "power_in")))
    (net (code "201") (name "Net-(U13-BS)") (class "Default")
      (node (ref "C44") (pin "2") (pintype "passive"))
      (node (ref "U13") (pin "7") (pinfunction "BS") (pintype "unspecified")))
    (net (code "202") (name "Net-(U13-EN)") (class "Default")
      (node (ref "R30") (pin "2") (pintype "passive"))
      (node (ref "R31") (pin "1") (pintype "passive"))
      (node (ref "U13") (pin "12") (pinfunction "EN") (pintype "unspecified")))
    (net (code "203") (name "Net-(U13-FB)") (class "Default")
      (node (ref "R32") (pin "1") (pintype "passive"))
      (node (ref "R34") (pin "1") (pintype "passive"))
      (node (ref "R35") (pin "1") (pintype "passive"))
      (node (ref "U13") (pin "9") (pinfunction "FB") (pintype "unspecified")))
    (net (code "204") (name "Net-(U13-LX)") (class "Default")
      (node (ref "C44") (pin "1") (pintype "passive"))
      (node (ref "L1") (pin "2") (pinfunction "2") (pintype "unspecified"))
      (node (ref "U13") (pin "2") (pinfunction "LX") (pintype "unspecified")))
    (net (code "205") (name "Net-(U13-VCC)") (class "Default")
      (node (ref "C45") (pin "2") (pintype "passive"))
      (node (ref "U13") (pin "8") (pinfunction "VCC") (pintype "unspecified")))
    (net (code "206") (name "Net-(U14-AREF)") (class "Default")
      (node (ref "C52") (pin "2") (pintype "passive"))
      (node (ref "U14") (pin "42") (pinfunction "AREF") (pintype "passive")))
    (net (code "207") (name "Net-(U14-PC7)") (class "Default")
      (node (ref "TP18") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U14") (pin "32") (pinfunction "PC7") (pintype "bidirectional")))
    (net (code "208") (name "Net-(U14-PF1)") (class "Default")
      (node (ref "TP16") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U14") (pin "40") (pinfunction "PF1") (pintype "bidirectional")))
    (net (code "209") (name "Net-(U14-PF4)") (class "Default")
      (node (ref "TP15") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U14") (pin "39") (pinfunction "PF4") (pintype "bidirectional")))
    (net (code "210") (name "Net-(U14-PF5)") (class "Default")
      (node (ref "TP14") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U14") (pin "38") (pinfunction "PF5") (pintype "bidirectional")))
    (net (code "211") (name "Net-(U14-PF6)") (class "Default")
      (node (ref "TP13") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U14") (pin "37") (pinfunction "PF6") (pintype "bidirectional")))
    (net (code "212") (name "Net-(U14-PF7)") (class "Default")
      (node (ref "TP12") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U14") (pin "36") (pinfunction "PF7") (pintype "bidirectional")))
    (net (code "213") (name "Net-(U14-UCAP)") (class "Default")
      (node (ref "C54") (pin "1") (pintype "passive"))
      (node (ref "U14") (pin "6") (pinfunction "UCAP") (pintype "passive")))
    (net (code "214") (name "Net-(U14-XTAL1)") (class "Default")
      (node (ref "C50") (pin "2") (pintype "passive"))
      (node (ref "U14") (pin "17") (pinfunction "XTAL1") (pintype "input"))
      (node (ref "X1") (pin "3") (pinfunction "OSC") (pintype "unspecified")))
    (net (code "215") (name "Net-(U14-XTAL2)") (class "Default")
      (node (ref "C49") (pin "1") (pintype "passive"))
      (node (ref "U14") (pin "16") (pinfunction "XTAL2") (pintype "output"))
      (node (ref "X1") (pin "1") (pinfunction "OSC") (pintype "unspecified")))
    (net (code "216") (name "Net-(U14-~{HWB}{slash}PE2)") (class "Default")
      (node (ref "R41") (pin "1") (pintype "passive"))
      (node (ref "U14") (pin "33") (pinfunction "~{HWB}/PE2") (pintype "bidirectional")))
    (net (code "217") (name "Net-(U15-BS)") (class "Default")
      (node (ref "C69") (pin "2") (pintype "passive"))
      (node (ref "U15") (pin "7") (pinfunction "BS") (pintype "unspecified")))
    (net (code "218") (name "Net-(U15-EN)") (class "Default")
      (node (ref "R44") (pin "2") (pintype "passive"))
      (node (ref "R45") (pin "1") (pintype "passive"))
      (node (ref "U15") (pin "12") (pinfunction "EN") (pintype "unspecified")))
    (net (code "219") (name "Net-(U15-FB)") (class "Default")
      (node (ref "R47") (pin "1") (pintype "passive"))
      (node (ref "R48") (pin "1") (pintype "passive"))
      (node (ref "R49") (pin "1") (pintype "passive"))
      (node (ref "U15") (pin "9") (pinfunction "FB") (pintype "unspecified")))
    (net (code "220") (name "Net-(U15-VCC)") (class "Default")
      (node (ref "C74") (pin "1") (pintype "passive"))
      (node (ref "U15") (pin "8") (pinfunction "VCC") (pintype "unspecified")))
    (net (code "221") (name "Net-(U17-CAPM)") (class "Default")
      (node (ref "C85") (pin "1") (pintype "passive"))
      (node (ref "U17") (pin "4") (pinfunction "CAPM") (pintype "passive")))
    (net (code "222") (name "Net-(U17-CAPP)") (class "Default")
      (node (ref "C85") (pin "2") (pintype "passive"))
      (node (ref "U17") (pin "2") (pinfunction "CAPP") (pintype "passive")))
    (net (code "223") (name "Net-(U17-LDOO)") (class "Default")
      (node (ref "C59") (pin "1") (pintype "passive"))
      (node (ref "C84") (pin "1") (pintype "passive"))
      (node (ref "U17") (pin "26") (pinfunction "LDOO") (pintype "passive")))
    (net (code "224") (name "Net-(U17-OUTL)") (class "Default")
      (node (ref "C87") (pin "2") (pintype "passive"))
      (node (ref "U17") (pin "6") (pinfunction "OUTL") (pintype "output")))
    (net (code "225") (name "Net-(U17-OUTR)") (class "Default")
      (node (ref "C89") (pin "2") (pintype "passive"))
      (node (ref "U17") (pin "7") (pinfunction "OUTR") (pintype "output")))
    (net (code "226") (name "Net-(U17-VCOM{slash}DEMP)") (class "Default")
      (node (ref "C86") (pin "2") (pintype "passive"))
      (node (ref "U17") (pin "10") (pinfunction "VCOM/DEMP") (pintype "bidirectional")))
    (net (code "227") (name "Net-(U17-VNEG)") (class "Default")
      (node (ref "C83") (pin "1") (pintype "passive"))
      (node (ref "U17") (pin "5") (pinfunction "VNEG") (pintype "passive")))
    (net (code "228") (name "Net-(U17-XSMT)") (class "Default")
      (node (ref "R42") (pin "2") (pintype "passive"))
      (node (ref "U17") (pin "25") (pinfunction "XSMT") (pintype "input")))
    (net (code "229") (name "Net-(U18-RESET#)") (class "Default")
      (node (ref "R52") (pin "1") (pintype "passive"))
      (node (ref "U18") (pin "18") (pinfunction "RESET#") (pintype "unspecified")))
    (net (code "230") (name "Net-(U19-GPA1)") (class "Default")
      (node (ref "R62") (pin "1") (pintype "passive"))
      (node (ref "U19") (pin "22") (pinfunction "GPA1") (pintype "unspecified")))
    (net (code "231") (name "Net-(U19-GPA2)") (class "Default")
      (node (ref "R61") (pin "1") (pintype "passive"))
      (node (ref "U19") (pin "23") (pinfunction "GPA2") (pintype "unspecified")))
    (net (code "232") (name "Net-(U19-GPA3)") (class "Default")
      (node (ref "R60") (pin "1") (pintype "passive"))
      (node (ref "U19") (pin "24") (pinfunction "GPA3") (pintype "unspecified")))
    (net (code "233") (name "Net-(U19-GPA4)") (class "Default")
      (node (ref "R59") (pin "1") (pintype "passive"))
      (node (ref "U19") (pin "25") (pinfunction "GPA4") (pintype "unspecified")))
    (net (code "234") (name "Net-(U19-GPA5)") (class "Default")
      (node (ref "R58") (pin "1") (pintype "passive"))
      (node (ref "U19") (pin "26") (pinfunction "GPA5") (pintype "unspecified")))
    (net (code "235") (name "Net-(U19-GPA6)") (class "Default")
      (node (ref "R57") (pin "1") (pintype "passive"))
      (node (ref "U19") (pin "27") (pinfunction "GPA6") (pintype "unspecified")))
    (net (code "236") (name "Net-(U19-GPA7)") (class "Default")
      (node (ref "R56") (pin "1") (pintype "passive"))
      (node (ref "U19") (pin "28") (pinfunction "GPA7") (pintype "unspecified")))
    (net (code "237") (name "Net-(U19-GPB0)") (class "Default")
      (node (ref "R63") (pin "2") (pintype "passive"))
      (node (ref "U19") (pin "1") (pinfunction "GPB0") (pintype "unspecified")))
    (net (code "238") (name "Net-(U19-GPB1)") (class "Default")
      (node (ref "R64") (pin "2") (pintype "passive"))
      (node (ref "U19") (pin "2") (pinfunction "GPB1") (pintype "unspecified")))
    (net (code "239") (name "Net-(U19-GPB2)") (class "Default")
      (node (ref "R65") (pin "2") (pintype "passive"))
      (node (ref "U19") (pin "3") (pinfunction "GPB2") (pintype "unspecified")))
    (net (code "240") (name "Net-(U19-GPB3)") (class "Default")
      (node (ref "R66") (pin "2") (pintype "passive"))
      (node (ref "U19") (pin "4") (pinfunction "GPB3") (pintype "unspecified")))
    (net (code "241") (name "Net-(U19-GPB4)") (class "Default")
      (node (ref "R67") (pin "2") (pintype "passive"))
      (node (ref "U19") (pin "5") (pinfunction "GPB4") (pintype "unspecified")))
    (net (code "242") (name "Net-(U19-GPB5)") (class "Default")
      (node (ref "R68") (pin "2") (pintype "passive"))
      (node (ref "U19") (pin "6") (pinfunction "GPB5") (pintype "unspecified")))
    (net (code "243") (name "Net-(U19-RESET#)") (class "Default")
      (node (ref "R55") (pin "1") (pintype "passive"))
      (node (ref "U19") (pin "18") (pinfunction "RESET#") (pintype "unspecified")))
    (net (code "244") (name "Net-(U20-CLK)") (class "Default")
      (node (ref "R69") (pin "2") (pintype "passive"))
      (node (ref "U20") (pin "5") (pinfunction "CLK") (pintype "input")))
    (net (code "245") (name "Net-(V3-Pad1)") (class "Default")
      (node (ref "V3") (pin "1") (pintype "passive"))
      (node (ref "V4") (pin "2") (pintype "passive")))
    (net (code "246") (name "UART_ATMEGA_RX") (class "Default")
      (node (ref "R8") (pin "2") (pintype "passive"))
      (node (ref "U14") (pin "20") (pinfunction "PD2") (pintype "bidirectional")))
    (net (code "247") (name "UART_ATMEGA_TX") (class "Default")
      (node (ref "R9") (pin "2") (pintype "passive"))
      (node (ref "U14") (pin "21") (pinfunction "PD3") (pintype "bidirectional")))
    (net (code "248") (name "unconnected-(J2-DETECT_GND-Pad3)") (class "Default")
      (node (ref "J2") (pin "3") (pinfunction "DETECT_GND") (pintype "passive+no_connect")))
    (net (code "249") (name "unconnected-(J2-DETECT_LEFT-Pad7)") (class "Default")
      (node (ref "J2") (pin "7") (pinfunction "DETECT_LEFT") (pintype "passive+no_connect")))
    (net (code "250") (name "unconnected-(J2-DETECT_R-Pad5)") (class "Default")
      (node (ref "J2") (pin "5") (pinfunction "DETECT_R") (pintype "passive+no_connect")))
    (net (code "251") (name "unconnected-(J5-DETECT_GND-Pad4)") (class "Default")
      (node (ref "J5") (pin "4") (pinfunction "DETECT_GND") (pintype "passive+no_connect")))
    (net (code "252") (name "unconnected-(J8-D+-Pad3)") (class "Default")
      (node (ref "J8") (pin "3") (pinfunction "D+") (pintype "bidirectional+no_connect")))
    (net (code "253") (name "unconnected-(J8-D--Pad2)") (class "Default")
      (node (ref "J8") (pin "2") (pinfunction "D-") (pintype "bidirectional+no_connect")))
    (net (code "254") (name "unconnected-(J9-SBU1-Pad9)") (class "Default")
      (node (ref "J9") (pin "9") (pinfunction "SBU1") (pintype "unspecified+no_connect")))
    (net (code "255") (name "unconnected-(J9-SBU2-Pad3)") (class "Default")
      (node (ref "J9") (pin "3") (pinfunction "SBU2") (pintype "unspecified+no_connect")))
    (net (code "256") (name "unconnected-(J12-P1-Pad1)") (class "Default")
      (node (ref "J12") (pin "1") (pinfunction "P1") (pintype "output+no_connect")))
    (net (code "257") (name "unconnected-(J13-UTILITY{slash}HEAC+-Pad2)") (class "Default")
      (node (ref "J13") (pin "2") (pinfunction "UTILITY/HEAC+") (pintype "passive+no_connect")))
    (net (code "258") (name "unconnected-(J14-UTILITY{slash}HEAC+-Pad2)") (class "Default")
      (node (ref "J14") (pin "2") (pinfunction "UTILITY/HEAC+") (pintype "passive+no_connect")))
    (net (code "259") (name "unconnected-(J15-SBU1-PadA8)") (class "Default")
      (node (ref "J15") (pin "A8") (pinfunction "SBU1") (pintype "unspecified+no_connect")))
    (net (code "260") (name "unconnected-(J15-SBU2-PadB8)") (class "Default")
      (node (ref "J15") (pin "B8") (pinfunction "SBU2") (pintype "unspecified+no_connect")))
    (net (code "261") (name "unconnected-(SW1-A5-Pad5)") (class "Default")
      (node (ref "SW1") (pin "5") (pinfunction "A5") (pintype "input+no_connect")))
    (net (code "262") (name "unconnected-(SW3-Pad3)") (class "Default")
      (node (ref "SW3") (pin "3") (pinfunction "3") (pintype "unspecified+no_connect")))
    (net (code "263") (name "unconnected-(SW3-Pad4)") (class "Default")
      (node (ref "SW3") (pin "4") (pinfunction "4") (pintype "unspecified+no_connect")))
    (net (code "264") (name "unconnected-(SW3-Pad5)") (class "Default")
      (node (ref "SW3") (pin "5") (pinfunction "5") (pintype "unspecified+no_connect")))
    (net (code "265") (name "unconnected-(SW3-Pad6)") (class "Default")
      (node (ref "SW3") (pin "6") (pinfunction "6") (pintype "unspecified+no_connect")))
    (net (code "266") (name "unconnected-(SW3-Pad7)") (class "Default")
      (node (ref "SW3") (pin "7") (pinfunction "7") (pintype "unspecified+no_connect")))
    (net (code "267") (name "unconnected-(SW3-Pad8)") (class "Default")
      (node (ref "SW3") (pin "8") (pinfunction "8") (pintype "unspecified+no_connect")))
    (net (code "268") (name "unconnected-(U1A-CM4_1.8V_Out_1-Pad88)") (class "Default")
      (node (ref "U1") (pin "88") (pinfunction "CM4_1.8V_Out_1") (pintype "power_out+no_connect")))
    (net (code "269") (name "unconnected-(U1A-CM4_1.8V_Out_2-Pad90)") (class "Default")
      (node (ref "U1") (pin "90") (pinfunction "CM4_1.8V_Out_2") (pintype "power_out+no_connect")))
    (net (code "270") (name "unconnected-(U1A-CM4_3.3V_Out_1-Pad84)") (class "Default")
      (node (ref "U1") (pin "84") (pinfunction "CM4_3.3V_Out_1") (pintype "power_out+no_connect")))
    (net (code "271") (name "unconnected-(U1A-CM4_3.3V_Out_2-Pad86)") (class "Default")
      (node (ref "U1") (pin "86") (pinfunction "CM4_3.3V_Out_2") (pintype "power_out+no_connect")))
    (net (code "272") (name "unconnected-(U1B-GPIO2-Pad58)") (class "Default")
      (node (ref "U1") (pin "58") (pinfunction "GPIO2") (pintype "passive+no_connect")))
    (net (code "273") (name "unconnected-(U1B-GPIO3-Pad56)") (class "Default")
      (node (ref "U1") (pin "56") (pinfunction "GPIO3") (pintype "passive+no_connect")))
    (net (code "274") (name "unconnected-(U1B-GPIO4-Pad54)") (class "Default")
      (node (ref "U1") (pin "54") (pinfunction "GPIO4") (pintype "passive+no_connect")))
    (net (code "275") (name "unconnected-(U1B-GPIO5-Pad34)") (class "Default")
      (node (ref "U1") (pin "34") (pinfunction "GPIO5") (pintype "passive+no_connect")))
    (net (code "276") (name "unconnected-(U1B-GPIO6-Pad30)") (class "Default")
      (node (ref "U1") (pin "30") (pinfunction "GPIO6") (pintype "passive+no_connect")))
    (net (code "277") (name "unconnected-(U1B-GPIO7-Pad37)") (class "Default")
      (node (ref "U1") (pin "37") (pinfunction "GPIO7") (pintype "passive+no_connect")))
    (net (code "278") (name "unconnected-(U1B-GPIO8-Pad39)") (class "Default")
      (node (ref "U1") (pin "39") (pinfunction "GPIO8") (pintype "passive+no_connect")))
    (net (code "279") (name "unconnected-(U1B-GPIO9-Pad40)") (class "Default")
      (node (ref "U1") (pin "40") (pinfunction "GPIO9") (pintype "passive+no_connect")))
    (net (code "280") (name "unconnected-(U1B-GPIO10-Pad44)") (class "Default")
      (node (ref "U1") (pin "44") (pinfunction "GPIO10") (pintype "passive+no_connect")))
    (net (code "281") (name "unconnected-(U1B-GPIO11-Pad38)") (class "Default")
      (node (ref "U1") (pin "38") (pinfunction "GPIO11") (pintype "passive+no_connect")))
    (net (code "282") (name "unconnected-(U1B-GPIO12-Pad31)") (class "Default")
      (node (ref "U1") (pin "31") (pinfunction "GPIO12") (pintype "passive+no_connect")))
    (net (code "283") (name "unconnected-(U1B-GPIO13-Pad28)") (class "Default")
      (node (ref "U1") (pin "28") (pinfunction "GPIO13") (pintype "passive+no_connect")))
    (net (code "284") (name "unconnected-(U1B-GPIO16-Pad29)") (class "Default")
      (node (ref "U1") (pin "29") (pinfunction "GPIO16") (pintype "passive+no_connect")))
    (net (code "285") (name "unconnected-(U1B-GPIO17-Pad50)") (class "Default")
      (node (ref "U1") (pin "50") (pinfunction "GPIO17") (pintype "passive+no_connect")))
    (net (code "286") (name "unconnected-(U1B-GPIO20-Pad27)") (class "Default")
      (node (ref "U1") (pin "27") (pinfunction "GPIO20") (pintype "passive+no_connect")))
    (net (code "287") (name "unconnected-(U1B-GPIO22-Pad46)") (class "Default")
      (node (ref "U1") (pin "46") (pinfunction "GPIO22") (pintype "passive+no_connect")))
    (net (code "288") (name "unconnected-(U1B-GPIO23-Pad47)") (class "Default")
      (node (ref "U1") (pin "47") (pinfunction "GPIO23") (pintype "passive+no_connect")))
    (net (code "289") (name "unconnected-(U1B-GPIO24-Pad45)") (class "Default")
      (node (ref "U1") (pin "45") (pinfunction "GPIO24") (pintype "passive+no_connect")))
    (net (code "290") (name "unconnected-(U1B-GPIO25-Pad41)") (class "Default")
      (node (ref "U1") (pin "41") (pinfunction "GPIO25") (pintype "passive+no_connect")))
    (net (code "291") (name "unconnected-(U1B-GPIO26-Pad24)") (class "Default")
      (node (ref "U1") (pin "24") (pinfunction "GPIO26") (pintype "passive+no_connect")))
    (net (code "292") (name "unconnected-(U1B-GPIO27-Pad48)") (class "Default")
      (node (ref "U1") (pin "48") (pinfunction "GPIO27") (pintype "passive+no_connect")))
    (net (code "293") (name "unconnected-(U1B-ID_SC-Pad35)") (class "Default")
      (node (ref "U1") (pin "35") (pinfunction "ID_SC") (pintype "passive+no_connect")))
    (net (code "294") (name "unconnected-(U1B-ID_SD-Pad36)") (class "Default")
      (node (ref "U1") (pin "36") (pinfunction "ID_SD") (pintype "passive+no_connect")))
    (net (code "295") (name "unconnected-(U1C-Ethernet_SYNC_OUT-Pad18)") (class "Default")
      (node (ref "U1") (pin "18") (pinfunction "Ethernet_SYNC_OUT") (pintype "input+no_connect")))
    (net (code "296") (name "unconnected-(U1I-SD_DAT4-Pad68)") (class "Default")
      (node (ref "U1") (pin "68") (pinfunction "SD_DAT4") (pintype "passive+no_connect")))
    (net (code "297") (name "unconnected-(U1I-SD_DAT5-Pad64)") (class "Default")
      (node (ref "U1") (pin "64") (pinfunction "SD_DAT5") (pintype "passive+no_connect")))
    (net (code "298") (name "unconnected-(U1I-SD_DAT6-Pad72)") (class "Default")
      (node (ref "U1") (pin "72") (pinfunction "SD_DAT6") (pintype "passive+no_connect")))
    (net (code "299") (name "unconnected-(U1I-SD_DAT7-Pad70)") (class "Default")
      (node (ref "U1") (pin "70") (pinfunction "SD_DAT7") (pintype "passive+no_connect")))
    (net (code "300") (name "unconnected-(U1I-SD_VDD_Override-Pad73)") (class "Default")
      (node (ref "U1") (pin "73") (pinfunction "SD_VDD_Override") (pintype "input+no_connect")))
    (net (code "301") (name "unconnected-(U1J-CAM_GPIO0-Pad97)") (class "Default")
      (node (ref "U1") (pin "97") (pinfunction "CAM_GPIO0") (pintype "input+no_connect")))
    (net (code "302") (name "unconnected-(U1J-CAM_GPIO1-Pad100)") (class "Default")
      (node (ref "U1") (pin "100") (pinfunction "CAM_GPIO1") (pintype "input+no_connect")))
    (net (code "303") (name "unconnected-(U2-GPIO3{slash}AGNS-Pad15)") (class "Default")
      (node (ref "U2") (pin "15") (pinfunction "GPIO3/AGNS") (pintype "bidirectional+no_connect")))
    (net (code "304") (name "unconnected-(U2-GPIO4{slash}MAST-Pad14)") (class "Default")
      (node (ref "U2") (pin "14") (pinfunction "GPIO4/MAST") (pintype "bidirectional+no_connect")))
    (net (code "305") (name "unconnected-(U2-GPIO5{slash}ATT0-Pad13)") (class "Default")
      (node (ref "U2") (pin "13") (pinfunction "GPIO5/ATT0") (pintype "bidirectional+no_connect")))
    (net (code "306") (name "unconnected-(U2-GPIO6{slash}FLT-Pad19)") (class "Default")
      (node (ref "U2") (pin "19") (pinfunction "GPIO6/FLT") (pintype "bidirectional+no_connect")))
    (net (code "307") (name "unconnected-(U3-FAULT-Pad4)") (class "Default")
      (node (ref "U3") (pin "4") (pinfunction "FAULT") (pintype "unspecified+no_connect")))
    (net (code "308") (name "unconnected-(U4-FAULT-Pad4)") (class "Default")
      (node (ref "U4") (pin "4") (pinfunction "FAULT") (pintype "unspecified+no_connect")))
    (net (code "309") (name "unconnected-(U5-FAULT-Pad4)") (class "Default")
      (node (ref "U5") (pin "4") (pinfunction "FAULT") (pintype "unspecified+no_connect")))
    (net (code "310") (name "unconnected-(U9-FAULT-Pad4)") (class "Default")
      (node (ref "U9") (pin "4") (pinfunction "FAULT") (pintype "unspecified+no_connect")))
    (net (code "311") (name "unconnected-(U10-NC-Pad4)") (class "Default")
      (node (ref "U10") (pin "4") (pinfunction "NC") (pintype "no_connect")))
    (net (code "312") (name "unconnected-(U11-NC-Pad4)") (class "Default")
      (node (ref "U11") (pin "4") (pinfunction "NC") (pintype "no_connect")))
    (net (code "313") (name "unconnected-(U12-CFG3-Pad3)") (class "Default")
      (node (ref "U12") (pin "3") (pinfunction "CFG3") (pintype "passive+no_connect")))
    (net (code "314") (name "unconnected-(U13-ILMT-Pad10)") (class "Default")
      (node (ref "U13") (pin "10") (pinfunction "ILMT") (pintype "unspecified+no_connect")))
    (net (code "315") (name "unconnected-(U14-D+-Pad4)") (class "Default")
      (node (ref "U14") (pin "4") (pinfunction "D+") (pintype "bidirectional+no_connect")))
    (net (code "316") (name "unconnected-(U14-D--Pad3)") (class "Default")
      (node (ref "U14") (pin "3") (pinfunction "D-") (pintype "bidirectional+no_connect")))
    (net (code "317") (name "unconnected-(U16-Y3-Pad6)") (class "Default")
      (node (ref "U16") (pin "6") (pinfunction "Y3") (pintype "unspecified+no_connect")))
    (net (code "318") (name "unconnected-(U16-Y4-Pad5)") (class "Default")
      (node (ref "U16") (pin "5") (pinfunction "Y4") (pintype "unspecified+no_connect")))
    (net (code "319") (name "unconnected-(U16-Y5-Pad4)") (class "Default")
      (node (ref "U16") (pin "4") (pinfunction "Y5") (pintype "unspecified+no_connect")))
    (net (code "320") (name "unconnected-(U16-Y6-Pad3)") (class "Default")
      (node (ref "U16") (pin "3") (pinfunction "Y6") (pintype "unspecified+no_connect")))
    (net (code "321") (name "unconnected-(U16-Y7-Pad2)") (class "Default")
      (node (ref "U16") (pin "2") (pinfunction "Y7") (pintype "unspecified+no_connect")))
    (net (code "322") (name "unconnected-(U16-Y8-Pad23)") (class "Default")
      (node (ref "U16") (pin "23") (pinfunction "Y8") (pintype "unspecified+no_connect")))
    (net (code "323") (name "unconnected-(U16-Y9-Pad22)") (class "Default")
      (node (ref "U16") (pin "22") (pinfunction "Y9") (pintype "unspecified+no_connect")))
    (net (code "324") (name "unconnected-(U16-Y10-Pad21)") (class "Default")
      (node (ref "U16") (pin "21") (pinfunction "Y10") (pintype "unspecified+no_connect")))
    (net (code "325") (name "unconnected-(U16-Y11-Pad20)") (class "Default")
      (node (ref "U16") (pin "20") (pinfunction "Y11") (pintype "unspecified+no_connect")))
    (net (code "326") (name "unconnected-(U16-Y12-Pad19)") (class "Default")
      (node (ref "U16") (pin "19") (pinfunction "Y12") (pintype "unspecified+no_connect")))
    (net (code "327") (name "unconnected-(U16-Y13-Pad18)") (class "Default")
      (node (ref "U16") (pin "18") (pinfunction "Y13") (pintype "unspecified+no_connect")))
    (net (code "328") (name "unconnected-(U16-Y14-Pad17)") (class "Default")
      (node (ref "U16") (pin "17") (pinfunction "Y14") (pintype "unspecified+no_connect")))
    (net (code "329") (name "unconnected-(U16-Y15-Pad16)") (class "Default")
      (node (ref "U16") (pin "16") (pinfunction "Y15") (pintype "unspecified+no_connect")))
    (net (code "330") (name "unconnected-(U17-ADR1{slash}MISO{slash}FMT-Pad24)") (class "Default")
      (node (ref "U17") (pin "24") (pinfunction "ADR1/MISO/FMT") (pintype "bidirectional+no_connect")))
    (net (code "331") (name "unconnected-(U17-ADR2{slash}GPIO2{slash}DOUT-Pad16)") (class "Default")
      (node (ref "U17") (pin "16") (pinfunction "ADR2/GPIO2/DOUT") (pintype "bidirectional+no_connect")))
    (net (code "332") (name "unconnected-(U17-BCK-Pad21)") (class "Default")
      (node (ref "U17") (pin "21") (pinfunction "BCK") (pintype "bidirectional+no_connect")))
    (net (code "333") (name "unconnected-(U17-DIN-Pad22)") (class "Default")
      (node (ref "U17") (pin "22") (pinfunction "DIN") (pintype "input+no_connect")))
    (net (code "334") (name "unconnected-(U17-GPIO3{slash}AGNS-Pad15)") (class "Default")
      (node (ref "U17") (pin "15") (pinfunction "GPIO3/AGNS") (pintype "bidirectional+no_connect")))
    (net (code "335") (name "unconnected-(U17-GPIO4{slash}MAST-Pad14)") (class "Default")
      (node (ref "U17") (pin "14") (pinfunction "GPIO4/MAST") (pintype "bidirectional+no_connect")))
    (net (code "336") (name "unconnected-(U17-GPIO5{slash}ATT0-Pad13)") (class "Default")
      (node (ref "U17") (pin "13") (pinfunction "GPIO5/ATT0") (pintype "bidirectional+no_connect")))
    (net (code "337") (name "unconnected-(U17-GPIO6{slash}FLT-Pad19)") (class "Default")
      (node (ref "U17") (pin "19") (pinfunction "GPIO6/FLT") (pintype "bidirectional+no_connect")))
    (net (code "338") (name "unconnected-(U17-LRCK-Pad23)") (class "Default")
      (node (ref "U17") (pin "23") (pinfunction "LRCK") (pintype "bidirectional+no_connect")))
    (net (code "339") (name "unconnected-(U17-MODE1-Pad17)") (class "Default")
      (node (ref "U17") (pin "17") (pinfunction "MODE1") (pintype "input+no_connect")))
    (net (code "340") (name "unconnected-(U17-MODE2{slash}MS-Pad18)") (class "Default")
      (node (ref "U17") (pin "18") (pinfunction "MODE2/MS") (pintype "input+no_connect")))
    (net (code "341") (name "unconnected-(U17-SCK-Pad20)") (class "Default")
      (node (ref "U17") (pin "20") (pinfunction "SCK") (pintype "input+no_connect")))
    (net (code "342") (name "unconnected-(U17-SCL{slash}MC{slash}ATT1-Pad12)") (class "Default")
      (node (ref "U17") (pin "12") (pinfunction "SCL/MC/ATT1") (pintype "input+no_connect")))
    (net (code "343") (name "unconnected-(U17-SDA{slash}MOSI{slash}ATT2-Pad11)") (class "Default")
      (node (ref "U17") (pin "11") (pinfunction "SDA/MOSI/ATT2") (pintype "bidirectional+no_connect")))
    (net (code "344") (name "unconnected-(U18-NC-Pad11)") (class "Default")
      (node (ref "U18") (pin "11") (pinfunction "NC") (pintype "unspecified+no_connect")))
    (net (code "345") (name "unconnected-(U18-NC-Pad14)") (class "Default")
      (node (ref "U18") (pin "14") (pinfunction "NC") (pintype "unspecified+no_connect")))
    (net (code "346") (name "unconnected-(U19-GPB7-Pad8)") (class "Default")
      (node (ref "U19") (pin "8") (pinfunction "GPB7") (pintype "unspecified+no_connect")))
    (net (code "347") (name "unconnected-(U19-NC-Pad11)") (class "Default")
      (node (ref "U19") (pin "11") (pinfunction "NC") (pintype "unspecified+no_connect")))
    (net (code "348") (name "unconnected-(U19-NC-Pad14)") (class "Default")
      (node (ref "U19") (pin "14") (pinfunction "NC") (pintype "unspecified+no_connect")))
    (net (code "349") (name "unconnected-(U20-CD-Pad9)") (class "Default")
      (node (ref "U20") (pin "9") (pinfunction "CD") (pintype "input+no_connect")))))