(export (version "E")
  (design
    (source "/Users/sam1902/Documents/CustomDJ/CDJ-MainBoard/CDJ-MainBoard.kicad_sch")
    (date "2026-02-13T00:13:02+0100")
    (tool "Eeschema 9.0.7")
    (sheet (number "1") (name "/") (tstamps "/")
      (title_block
        (title "CustomDJ")
        (company "xXxXxXxXxX DJ Rookmachine B.V. XxXxXxXxXx")
        (rev "v1")
        (date "2026-02-08")
        (source "CDJ-MainBoard.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value ""))))
    (sheet (number "2") (name "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/")
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source "audio_outputs.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value ""))))
    (sheet (number "3") (name "/Test Points/") (tstamps "/51b1dfb5-ef32-4d46-aca8-09c1f86f56e0/")
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source "test_points.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value ""))))
    (sheet (number "4") (name "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/")
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source "usb_dj_ports.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value ""))))
    (sheet (number "5") (name "/HDMI and Ethernet/") (tstamps "/97e2c747-925a-451b-94c7-ccaeac2c14a8/")
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source "hdmi.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value ""))))
    (sheet (number "6") (name "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/")
      (title_block
        (title "Power Delivery (20V @ 3A = 60W, peak draw 2.12A / 42.4W)")
        (company)
        (rev)
        (date)
        (source "power.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value ""))))
    (sheet (number "7") (name "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/")
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source "arduino_midi.kicad_sch")
        (comment (number "1") (value ""))
        (comment (number "2") (value ""))
        (comment (number "3") (value ""))
        (comment (number "4") (value ""))
        (comment (number "5") (value ""))
        (comment (number "6") (value ""))
        (comment (number "7") (value ""))
        (comment (number "8") (value ""))
        (comment (number "9") (value "")))))
  (components
    (comp (ref "BT1")
      (value "CR2032-BS-6-1")
      (footprint "JLC2KiCad_lib-footprints:BAT-TH_CR2032-BS-6-1")
      (datasheet "https://item.szlcsc.com/71472.html")
      (fields
        (field (name "LCSC") "C70377")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:BAT-TH_CR2032-BS-6-1")
        (field (name "Datasheet") "https://item.szlcsc.com/71472.html")
        (field (name "Description")))
      (libsource (lib "CR2032-BS-6-1") (part "CR2032-BS-6-1") (description ""))
      (property (name "LCSC") (value "C70377"))
      (property (name "Sheetname") (value "Root"))
      (property (name "Sheetfile") (value "CDJ-MainBoard.kicad_sch"))
      (property (name "ki_keywords") (value "C70377"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "11eda74e-925a-453a-8338-744d6c79ca06"))
    (comp (ref "C42")
      (value "100nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Root"))
      (property (name "Sheetfile") (value "CDJ-MainBoard.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "0eeed2c4-5957-435c-877d-1d6f7a507e90"))
    (comp (ref "D4")
      (value "XL-1608UBC-04")
      (footprint "JLC2KiCad_lib-footprints:LED0603-RD_BLUE")
      (datasheet "https://atta.szlcsc.com/upload/public/pdf/source/20210617/C2837377_50FC585D376FE0CDA016E524346528FF.pdf")
      (fields
        (field (name "LCSC") "C965807")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:LED0603-RD_BLUE")
        (field (name "Datasheet") "https://atta.szlcsc.com/upload/public/pdf/source/20210617/C2837377_50FC585D376FE0CDA016E524346528FF.pdf")
        (field (name "Description")))
      (libsource (lib "XL-1608UBC-04") (part "XL-1608UBC-04") (description ""))
      (property (name "LCSC") (value "C965807"))
      (property (name "Sheetname") (value "Root"))
      (property (name "Sheetfile") (value "CDJ-MainBoard.kicad_sch"))
      (property (name "ki_keywords") (value "C965807"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "7dcaef86-a358-43ee-9ba9-a98c96e1dd84"))
    (comp (ref "D5")
      (value "PSC-1608U52GC-G4")
      (footprint "JLC2KiCad_lib-footprints:LED0603-RD_GREEN")
      (datasheet "https://atta.szlcsc.com/upload/public/pdf/source/20190115/C264450_D840E7E570138F41CCE67133F241C738.pdf")
      (description "green led 780mcd")
      (fields
        (field (name "LCSC") "C22371297")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:LED0603-RD_GREEN")
        (field (name "Datasheet") "https://atta.szlcsc.com/upload/public/pdf/source/20190115/C264450_D840E7E570138F41CCE67133F241C738.pdf")
        (field (name "Description") "green led 780mcd"))
      (libsource (lib "PSC-1608U52GC-G4") (part "PSC-1608U52GC-G4") (description ""))
      (property (name "LCSC") (value "C22371297"))
      (property (name "Sheetname") (value "Root"))
      (property (name "Sheetfile") (value "CDJ-MainBoard.kicad_sch"))
      (property (name "ki_keywords") (value "C22371297"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "dd446156-56f3-4c7b-b2d8-65127bb03476"))
    (comp (ref "J14")
      (value "J_FAN_PWM")
      (footprint "Connector_JST:JST_PH_B4B-PH-K_1x04_P2.00mm_Vertical")
      (datasheet "~")
      (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (fields
        (field (name "Footprint") "Connector_JST:JST_PH_B4B-PH-K_1x04_P2.00mm_Vertical")
        (field (name "Datasheet") "~")
        (field (name "Description") "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (libsource (lib "Connector_Generic") (part "Conn_01x04") (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (property (name "Sheetname") (value "Root"))
      (property (name "Sheetfile") (value "CDJ-MainBoard.kicad_sch"))
      (property (name "ki_keywords") (value "connector"))
      (property (name "ki_fp_filters") (value "Connector*:*_1x??_*"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "d2475d13-fe58-408b-b741-4adff211bb67"))
    (comp (ref "R4")
      (value "2.2kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Root"))
      (property (name "Sheetfile") (value "CDJ-MainBoard.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "a1e64fd2-67c3-4b19-8a84-02841be4d63c"))
    (comp (ref "R6")
      (value "10kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Root"))
      (property (name "Sheetfile") (value "CDJ-MainBoard.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "5cd2ad05-4c2c-4819-9128-66a01d59b2c3"))
    (comp (ref "R7")
      (value "10kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Root"))
      (property (name "Sheetfile") (value "CDJ-MainBoard.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "ad638e09-9e45-4f8f-9e85-22cca33445c5"))
    (comp (ref "R20")
      (value "220Ω")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Root"))
      (property (name "Sheetfile") (value "CDJ-MainBoard.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "3cc517e8-ca8a-41cb-9c02-1005b114990d"))
    (comp (ref "R21")
      (value "220Ω")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Root"))
      (property (name "Sheetfile") (value "CDJ-MainBoard.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "e92bb50a-f91d-4b2c-b448-1c0076131190"))
    (comp (ref "R23")
      (value "10kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Root"))
      (property (name "Sheetfile") (value "CDJ-MainBoard.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "940f0796-96ca-40eb-b2d9-bd78898c4cc6"))
    (comp (ref "R27")
      (value "2.2kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Root"))
      (property (name "Sheetfile") (value "CDJ-MainBoard.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "aae294f9-b3d1-46c3-906a-bfd623ec1b0d"))
    (comp (ref "R28")
      (value "2.2kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Root"))
      (property (name "Sheetfile") (value "CDJ-MainBoard.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "25dc006a-5bcf-4b1a-9319-0f09ecfcf89a"))
    (comp (ref "R29")
      (value "10kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Root"))
      (property (name "Sheetfile") (value "CDJ-MainBoard.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "5c62c550-33c8-4450-a7fc-1eaf52a0f9d3"))
    (comp (ref "R30")
      (value "10kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Root"))
      (property (name "Sheetfile") (value "CDJ-MainBoard.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "34a02dc0-9d04-4018-ab7e-735fede47d03"))
    (comp (ref "R31")
      (value "5.1kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Root"))
      (property (name "Sheetfile") (value "CDJ-MainBoard.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "8663eea9-57be-469f-aeb0-7b60a4ecd127"))
    (comp (ref "R32")
      (value "5.1kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Root"))
      (property (name "Sheetfile") (value "CDJ-MainBoard.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "fb8ba5bd-0e97-4a46-8628-ff0214a6dfa2"))
    (comp (ref "R38")
      (value "3.3kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Root"))
      (property (name "Sheetfile") (value "CDJ-MainBoard.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "42fcc5db-8a46-45d4-a04e-79c52a30d140"))
    (comp (ref "R39")
      (value "100Ω")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Root"))
      (property (name "Sheetfile") (value "CDJ-MainBoard.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "06f4b706-1555-4f31-bf9f-b82ae96d189a"))
    (comp (ref "SW2")
      (value "PWR_BUT_CM5")
      (footprint "PCM_JLCPCB:SW_TS-1088-AR02016")
      (datasheet "~")
      (description "Push button switch, generic, two pins")
      (fields
        (field (name "Footprint") "PCM_JLCPCB:SW_TS-1088-AR02016")
        (field (name "Datasheet") "~")
        (field (name "Description") "Push button switch, generic, two pins"))
      (libsource (lib "Switch") (part "SW_Push") (description "Push button switch, generic, two pins"))
      (property (name "Sheetname") (value "Root"))
      (property (name "Sheetfile") (value "CDJ-MainBoard.kicad_sch"))
      (property (name "ki_keywords") (value "switch normally-open pushbutton push-button"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "d097adbb-1382-4027-acfa-fed5463824eb"))
    (comp (ref "U3")
      (value "Compute_Module_5_Functional")
      (footprint "kicad-thirdparty-footprints:CM5")
      (fields
        (field (name "Footprint") "kicad-thirdparty-footprints:CM5")
        (field (name "Datasheet"))
        (field (name "Description")))
      (libsource (lib "rpi-cm-5") (part "Compute_Module_5_Functional") (description ""))
      (property (name "Sheetname") (value "Root"))
      (property (name "Sheetfile") (value "CDJ-MainBoard.kicad_sch"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "f74f0870-c7a5-4918-ace5-8c39c69355e7" "5f7bfd13-6eda-41ac-bef7-693d73aab286"))
    (comp (ref "U12")
      (value "DSWB04LHGET")
      (footprint "JLC2KiCad_lib-footprints:SW-TH_DSWB04LHGET")
      (datasheet "https://item.szlcsc.com/100632.html")
      (fields
        (field (name "LCSC") "C99418")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:SW-TH_DSWB04LHGET")
        (field (name "Datasheet") "https://item.szlcsc.com/100632.html")
        (field (name "Description")))
      (libsource (lib "DSWB04LHGET") (part "DSWB04LHGET") (description ""))
      (property (name "LCSC") (value "C99418"))
      (property (name "Sheetname") (value "Root"))
      (property (name "Sheetfile") (value "CDJ-MainBoard.kicad_sch"))
      (property (name "ki_keywords") (value "C99418"))
      (sheetpath (names "/") (tstamps "/"))
      (tstamps "0901c184-9958-44d7-93b1-0ae270c641f6"))
    (comp (ref "C12")
      (value "100nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "4f661c28-4201-4914-992b-643824c79e39"))
    (comp (ref "C13")
      (value "100nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "c260e480-2c5d-4e45-b8e0-b11d915de7d4"))
    (comp (ref "C14")
      (value "2.2µF")
      (footprint "Capacitor_SMD:C_0201_0603Metric")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0201_0603Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "5ee22448-be13-4d4e-be11-4b0fd2840d03"))
    (comp (ref "C16")
      (value "2.2µF")
      (footprint "Capacitor_SMD:C_0201_0603Metric")
      (datasheet "~")
      (description "unpolarized ceramic, 2.2µF, X5R, ≥10V")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0201_0603Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "unpolarized ceramic, 2.2µF, X5R, ≥10V"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "ba26e3a1-accd-4553-95e8-556153eb76a8"))
    (comp (ref "C17")
      (value "1µF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "fff78815-9d5f-4b3c-90ec-7f2950b9fd4f"))
    (comp (ref "C18")
      (value "2.2µF")
      (footprint "Capacitor_SMD:C_0201_0603Metric")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0201_0603Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "4e610d57-fd90-47d3-98e1-eed78308c41b"))
    (comp (ref "C19")
      (value "2.2nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "0098216d-cafd-4381-a194-cc23ac8e3f25"))
    (comp (ref "C20")
      (value "2.2µF")
      (footprint "Capacitor_SMD:C_0201_0603Metric")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0201_0603Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "5ab23adb-0b37-495e-81d7-c67484dc4ef8"))
    (comp (ref "C21")
      (value "2.2nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "efb48ce7-aacb-44df-8d4b-f2ecf7890d24"))
    (comp (ref "C22")
      (value "100nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "40ef6e82-9c3c-44d8-bd56-9bf044af3525"))
    (comp (ref "C24")
      (value "10µF")
      (footprint "Capacitor_SMD:C_0805_2012Metric")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0805_2012Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "bd9696e1-d478-4f32-b68f-06fac59537ec"))
    (comp (ref "C34")
      (value "1µF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "04c3f33a-6fbc-4a33-818e-05b243110513"))
    (comp (ref "FB1")
      (value "~")
      (footprint "PCM_JLCPCB:FB_0603")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2310301640_Sunlord-GZ1608D601TF_C1002.pdf")
      (description "450mΩ ±25% 600Ω@100MHz 0603 Ferrite Beads ROHS")
      (fields
        (field (name "LCSC") "C1002")
        (field (name "Stock") "789150")
        (field (name "Price") "0.010USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "6")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Filters/EMI Optimization,Ferrite Beads")
        (field (name "Manufacturer") "Sunlord")
        (field (name "Part") "GZ1608D601TF")
        (field (name "DC Resistance") "450mΩ")
        (field (name "Impedance @ Frequency") "600Ω@100MHz")
        (field (name "Circuits") "1")
        (field (name "Current Rating") "200mA")
        (field (name "Tolerance") "±25%")
        (field (name "Footprint") "PCM_JLCPCB:FB_0603")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2310301640_Sunlord-GZ1608D601TF_C1002.pdf")
        (field (name "Description") "450mΩ ±25% 600Ω@100MHz 0603 Ferrite Beads ROHS"))
      (libsource (lib "PCM_JLCPCB-Inductors") (part "Ferrite,0603") (description "450mΩ ±25% 600Ω@100MHz 0603 Ferrite Beads ROHS"))
      (property (name "LCSC") (value "C1002"))
      (property (name "Stock") (value "789150"))
      (property (name "Price") (value "0.010USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "6"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Filters/EMI Optimization,Ferrite Beads"))
      (property (name "Manufacturer") (value "Sunlord"))
      (property (name "Part") (value "GZ1608D601TF"))
      (property (name "DC Resistance") (value "450mΩ"))
      (property (name "Impedance @ Frequency") (value "600Ω@100MHz"))
      (property (name "Circuits") (value "1"))
      (property (name "Current Rating") (value "200mA"))
      (property (name "Tolerance") (value "±25%"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_fp_filters") (value "FB_*"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "23f23e2b-67f5-4f99-baa1-294ed0c04cb4"))
    (comp (ref "J6")
      (value "J_RCA_L (white)")
      (footprint "JLC2KiCad_lib-footprints:CONN-TH_AV-5")
      (fields
        (field (name "MF") "Same Sky")
        (field (name "Description_1") "Metal Right-Angle, SMT RCA Jack, White Insulator")
        (field (name "Package") "None")
        (field (name "Price") "None")
        (field (name "Check_prices") "https://www.snapeda.com/parts/RCJ-013-SMT-TR/Same+Sky/view-part/?ref=eda")
        (field (name "PART_REV") "B")
        (field (name "STANDARD") "Manufacturer recommendations")
        (field (name "SnapEDA_Link") "https://www.snapeda.com/parts/RCJ-013-SMT-TR/Same+Sky/view-part/?ref=snap")
        (field (name "MP") "RCJ-013-SMT-TR")
        (field (name "Purchase-URL") "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=1316562&manufacturer=Same Sky&part_name=RCJ-013-SMT-TR&search_term=rca jack pcb mount")
        (field (name "Availability") "In Stock")
        (field (name "MANUFACTURER") "CUI Inc")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:CONN-TH_AV-5")
        (field (name "Datasheet"))
        (field (name "Description")))
      (libsource (lib "rca-jack-white") (part "RCJ-013-SMT") (description ""))
      (property (name "MF") (value "Same Sky"))
      (property (name "Description_1") (value "Metal Right-Angle, SMT RCA Jack, White Insulator"))
      (property (name "Package") (value "None"))
      (property (name "Price") (value "None"))
      (property (name "Check_prices") (value "https://www.snapeda.com/parts/RCJ-013-SMT-TR/Same+Sky/view-part/?ref=eda"))
      (property (name "PART_REV") (value "B"))
      (property (name "STANDARD") (value "Manufacturer recommendations"))
      (property (name "SnapEDA_Link") (value "https://www.snapeda.com/parts/RCJ-013-SMT-TR/Same+Sky/view-part/?ref=snap"))
      (property (name "MP") (value "RCJ-013-SMT-TR"))
      (property (name "Purchase-URL") (value "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=1316562&manufacturer=Same Sky&part_name=RCJ-013-SMT-TR&search_term=rca jack pcb mount"))
      (property (name "Availability") (value "In Stock"))
      (property (name "MANUFACTURER") (value "CUI Inc"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "a588bdb6-f08f-42bc-807f-4bfb60c077dd"))
    (comp (ref "J7")
      (value "J_RCA_R (red)")
      (footprint "JLC2KiCad_lib-footprints:CONN-TH_AV-5")
      (fields
        (field (name "MF") "Same Sky")
        (field (name "Description_1") "Metal Right-Angle, SMT RCA Jack, Red Insulator")
        (field (name "Package") "None")
        (field (name "Price") "None")
        (field (name "Check_prices") "https://www.snapeda.com/parts/RCJ-012-SMT-TR/Same+Sky/view-part/?ref=eda")
        (field (name "PART_REV") "B")
        (field (name "STANDARD") "Manufacturer recommendations")
        (field (name "SnapEDA_Link") "https://www.snapeda.com/parts/RCJ-012-SMT-TR/Same+Sky/view-part/?ref=snap")
        (field (name "MP") "RCJ-012-SMT-TR")
        (field (name "Purchase-URL") "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=1316485&manufacturer=Same Sky&part_name=RCJ-012-SMT-TR&search_term=rca jack pcb mount")
        (field (name "Availability") "In Stock")
        (field (name "MANUFACTURER") "CUI Inc")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:CONN-TH_AV-5")
        (field (name "Datasheet"))
        (field (name "Description")))
      (libsource (lib "rca-jack-red") (part "RCJ-012-SMT") (description ""))
      (property (name "MF") (value "Same Sky"))
      (property (name "Description_1") (value "Metal Right-Angle, SMT RCA Jack, Red Insulator"))
      (property (name "Package") (value "None"))
      (property (name "Price") (value "None"))
      (property (name "Check_prices") (value "https://www.snapeda.com/parts/RCJ-012-SMT-TR/Same+Sky/view-part/?ref=eda"))
      (property (name "PART_REV") (value "B"))
      (property (name "STANDARD") (value "Manufacturer recommendations"))
      (property (name "SnapEDA_Link") (value "https://www.snapeda.com/parts/RCJ-012-SMT-TR/Same+Sky/view-part/?ref=snap"))
      (property (name "MP") (value "RCJ-012-SMT-TR"))
      (property (name "Purchase-URL") (value "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=1316485&manufacturer=Same Sky&part_name=RCJ-012-SMT-TR&search_term=rca jack pcb mount"))
      (property (name "Availability") (value "In Stock"))
      (property (name "MANUFACTURER") (value "CUI Inc"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "0fe64348-9aaa-42ab-87f8-1d2a60e96301"))
    (comp (ref "J18")
      (value "PJ-611E 6.35mm jack")
      (footprint "JLC2KiCad_lib-footprints:AUDIO-TH_PJ-611E_1")
      (datasheet "https://item.szlcsc.com/datasheet/PJ-611E/292943.html?spm=sc.it.xds.a&lcsc_vid=EVMNBFVWTlcKUQUCQ1FdVFJSRgcNXgJXE1BbX1ACQlgxVlNQQ1NcUF1RR1VcXjsOAxUeFF5JWA0NAgAHWQIASA%3D%3D")
      (fields
        (field (name "LCSC") "C309282")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:AUDIO-TH_PJ-611E_1")
        (field (name "Datasheet") "https://item.szlcsc.com/datasheet/PJ-611E/292943.html?spm=sc.it.xds.a&lcsc_vid=EVMNBFVWTlcKUQUCQ1FdVFJSRgcNXgJXE1BbX1ACQlgxVlNQQ1NcUF1RR1VcXjsOAxUeFF5JWA0NAgAHWQIASA%3D%3D")
        (field (name "Description")))
      (libsource (lib "PJ-611E jack 6.35mm") (part "PJ-611E") (description ""))
      (property (name "LCSC") (value "C309282"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_keywords") (value "C309282"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "d8972c84-be5a-41b1-a667-1e70daa636ac"))
    (comp (ref "R8")
      (value "47kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "1c3caf85-5cf5-41bb-b440-f9ff940fc829"))
    (comp (ref "R9")
      (value "470Ω")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "ccb187a4-79e3-46e5-8f34-b2e6d3e85dd4"))
    (comp (ref "R10")
      (value "470Ω")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "7e8e8b16-edef-4204-bc6b-9180e174626c"))
    (comp (ref "U5")
      (value "PCM5122PW")
      (footprint "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm")
      (datasheet "http://www.ti.com/lit/ds/symlink/pcm5122.pdf")
      (description "2VRMS DirectPath, 112dB Audio Stereo DAC with 32-bit, 384kHz PCM Interface, TSSOP-28")
      (fields
        (field (name "Footprint") "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm")
        (field (name "Datasheet") "http://www.ti.com/lit/ds/symlink/pcm5122.pdf")
        (field (name "Description") "2VRMS DirectPath, 112dB Audio Stereo DAC with 32-bit, 384kHz PCM Interface, TSSOP-28"))
      (libsource (lib "Audio") (part "PCM5122PW") (description "2VRMS DirectPath, 112dB Audio Stereo DAC with 32-bit, 384kHz PCM Interface, TSSOP-28"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_keywords") (value "audio dac 2ch 32bit 384kHz"))
      (property (name "ki_fp_filters") (value "TSSOP*4.4x9.7mm*P0.65mm*"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "309d9f76-601e-4cd9-ae2a-b0cb670fc820"))
    (comp (ref "U10")
      (value "PJ-320D 3.5mm jack")
      (footprint "JLC2KiCad_lib-footprints:AUDIO-SMD_PJ-320D-1")
      (datasheet "https://atta.szlcsc.com/upload/public/pdf/source/20190925/C431535_8B274506621F6117FB020BF07A197848.pdf")
      (fields
        (field (name "LCSC") "C431535")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:AUDIO-SMD_PJ-320D-1")
        (field (name "Datasheet") "https://atta.szlcsc.com/upload/public/pdf/source/20190925/C431535_8B274506621F6117FB020BF07A197848.pdf")
        (field (name "Description")))
      (libsource (lib "PJ-320D jack 3.5mm") (part "PJ-320D") (description ""))
      (property (name "LCSC") (value "C431535"))
      (property (name "Sheetname") (value "Audio Outputs"))
      (property (name "Sheetfile") (value "audio_outputs.kicad_sch"))
      (property (name "ki_keywords") (value "C431535"))
      (sheetpath (names "/Audio Outputs/") (tstamps "/ab35c504-92bc-4b2f-b3ae-eb295c2b8b5f/"))
      (tstamps "0c486586-4411-4e6a-82f2-92c1d239706d"))
    (comp (ref "H1")
      (value "MountingHole")
      (footprint "MountingHole:MountingHole_3.2mm_M3")
      (datasheet "~")
      (description "Mounting Hole without connection")
      (fields
        (field (name "Footprint") "MountingHole:MountingHole_3.2mm_M3")
        (field (name "Datasheet") "~")
        (field (name "Description") "Mounting Hole without connection"))
      (libsource (lib "Mechanical") (part "MountingHole") (description "Mounting Hole without connection"))
      (property (name "Sheetname") (value "Test Points"))
      (property (name "Sheetfile") (value "test_points.kicad_sch"))
      (property (name "exclude_from_bom"))
      (property (name "ki_keywords") (value "mounting hole"))
      (property (name "ki_fp_filters") (value "MountingHole*"))
      (sheetpath (names "/Test Points/") (tstamps "/51b1dfb5-ef32-4d46-aca8-09c1f86f56e0/"))
      (tstamps "56f74c51-f794-4317-a013-c2963c2bf83e"))
    (comp (ref "H2")
      (value "MountingHole")
      (footprint "MountingHole:MountingHole_3.2mm_M3")
      (datasheet "~")
      (description "Mounting Hole without connection")
      (fields
        (field (name "Footprint") "MountingHole:MountingHole_3.2mm_M3")
        (field (name "Datasheet") "~")
        (field (name "Description") "Mounting Hole without connection"))
      (libsource (lib "Mechanical") (part "MountingHole") (description "Mounting Hole without connection"))
      (property (name "Sheetname") (value "Test Points"))
      (property (name "Sheetfile") (value "test_points.kicad_sch"))
      (property (name "exclude_from_bom"))
      (property (name "ki_keywords") (value "mounting hole"))
      (property (name "ki_fp_filters") (value "MountingHole*"))
      (sheetpath (names "/Test Points/") (tstamps "/51b1dfb5-ef32-4d46-aca8-09c1f86f56e0/"))
      (tstamps "b29d003e-e50d-47ac-b43b-5653327636e5"))
    (comp (ref "H3")
      (value "MountingHole")
      (footprint "MountingHole:MountingHole_3.2mm_M3")
      (datasheet "~")
      (description "Mounting Hole without connection")
      (fields
        (field (name "Footprint") "MountingHole:MountingHole_3.2mm_M3")
        (field (name "Datasheet") "~")
        (field (name "Description") "Mounting Hole without connection"))
      (libsource (lib "Mechanical") (part "MountingHole") (description "Mounting Hole without connection"))
      (property (name "Sheetname") (value "Test Points"))
      (property (name "Sheetfile") (value "test_points.kicad_sch"))
      (property (name "exclude_from_bom"))
      (property (name "ki_keywords") (value "mounting hole"))
      (property (name "ki_fp_filters") (value "MountingHole*"))
      (sheetpath (names "/Test Points/") (tstamps "/51b1dfb5-ef32-4d46-aca8-09c1f86f56e0/"))
      (tstamps "2709749f-f25d-4c6b-8b75-29bc3049cb5e"))
    (comp (ref "H4")
      (value "MountingHole")
      (footprint "MountingHole:MountingHole_3.2mm_M3")
      (datasheet "~")
      (description "Mounting Hole without connection")
      (fields
        (field (name "Footprint") "MountingHole:MountingHole_3.2mm_M3")
        (field (name "Datasheet") "~")
        (field (name "Description") "Mounting Hole without connection"))
      (libsource (lib "Mechanical") (part "MountingHole") (description "Mounting Hole without connection"))
      (property (name "Sheetname") (value "Test Points"))
      (property (name "Sheetfile") (value "test_points.kicad_sch"))
      (property (name "exclude_from_bom"))
      (property (name "ki_keywords") (value "mounting hole"))
      (property (name "ki_fp_filters") (value "MountingHole*"))
      (sheetpath (names "/Test Points/") (tstamps "/51b1dfb5-ef32-4d46-aca8-09c1f86f56e0/"))
      (tstamps "0653b266-e99c-4ae7-b401-ac460769c694"))
    (comp (ref "J16")
      (value "J_I2C")
      (footprint "Connector_JST:JST_PH_B4B-PH-K_1x04_P2.00mm_Vertical")
      (datasheet "~")
      (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (fields
        (field (name "Footprint") "Connector_JST:JST_PH_B4B-PH-K_1x04_P2.00mm_Vertical")
        (field (name "Datasheet") "~")
        (field (name "Description") "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (libsource (lib "Connector_Generic") (part "Conn_01x04") (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (property (name "Sheetname") (value "Test Points"))
      (property (name "Sheetfile") (value "test_points.kicad_sch"))
      (property (name "ki_keywords") (value "connector"))
      (property (name "ki_fp_filters") (value "Connector*:*_1x??_*"))
      (sheetpath (names "/Test Points/") (tstamps "/51b1dfb5-ef32-4d46-aca8-09c1f86f56e0/"))
      (tstamps "902037ab-2e15-4ffa-86c7-cdaf90458176"))
    (comp (ref "J19")
      (value "J_ISP_ATMEGA")
      (footprint "Connector_JST:JST_PH_B6B-PH-K_1x06_P2.00mm_Vertical")
      (datasheet "~")
      (description "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (fields
        (field (name "Footprint") "Connector_JST:JST_PH_B6B-PH-K_1x06_P2.00mm_Vertical")
        (field (name "Datasheet") "~")
        (field (name "Description") "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (libsource (lib "Connector_Generic") (part "Conn_01x06") (description "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (property (name "Sheetname") (value "Test Points"))
      (property (name "Sheetfile") (value "test_points.kicad_sch"))
      (property (name "ki_keywords") (value "connector"))
      (property (name "ki_fp_filters") (value "Connector*:*_1x??_*"))
      (sheetpath (names "/Test Points/") (tstamps "/51b1dfb5-ef32-4d46-aca8-09c1f86f56e0/"))
      (tstamps "163942d0-20bb-4554-8110-898eb11c0d60"))
    (comp (ref "TP1")
      (value "TP_20V_USB")
      (footprint "TestPoint:TestPoint_Pad_2.0x2.0mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Footprint") "TestPoint:TestPoint_Pad_2.0x2.0mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Sheetname") (value "Test Points"))
      (property (name "Sheetfile") (value "test_points.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Test Points/") (tstamps "/51b1dfb5-ef32-4d46-aca8-09c1f86f56e0/"))
      (tstamps "b3836ea7-1cfe-493c-b6c2-d1b308195380"))
    (comp (ref "TP2")
      (value "TP_5V")
      (footprint "TestPoint:TestPoint_Pad_2.0x2.0mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Footprint") "TestPoint:TestPoint_Pad_2.0x2.0mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Sheetname") (value "Test Points"))
      (property (name "Sheetfile") (value "test_points.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Test Points/") (tstamps "/51b1dfb5-ef32-4d46-aca8-09c1f86f56e0/"))
      (tstamps "000c4d62-16fa-4517-8feb-60d44f0a2c5c"))
    (comp (ref "TP3")
      (value "TP_3.3_DGTL")
      (footprint "TestPoint:TestPoint_Pad_2.0x2.0mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Footprint") "TestPoint:TestPoint_Pad_2.0x2.0mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Sheetname") (value "Test Points"))
      (property (name "Sheetfile") (value "test_points.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Test Points/") (tstamps "/51b1dfb5-ef32-4d46-aca8-09c1f86f56e0/"))
      (tstamps "bffa881a-28f6-44b8-93c6-251ff3411913"))
    (comp (ref "TP4")
      (value "TP_3.3_ANALOG")
      (footprint "TestPoint:TestPoint_Pad_2.0x2.0mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Footprint") "TestPoint:TestPoint_Pad_2.0x2.0mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Sheetname") (value "Test Points"))
      (property (name "Sheetfile") (value "test_points.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Test Points/") (tstamps "/51b1dfb5-ef32-4d46-aca8-09c1f86f56e0/"))
      (tstamps "76099a4f-c44b-4008-b8a7-3315ee307196"))
    (comp (ref "TP5")
      (value "TP_GND")
      (footprint "TestPoint:TestPoint_Pad_2.0x2.0mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Footprint") "TestPoint:TestPoint_Pad_2.0x2.0mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Sheetname") (value "Test Points"))
      (property (name "Sheetfile") (value "test_points.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Test Points/") (tstamps "/51b1dfb5-ef32-4d46-aca8-09c1f86f56e0/"))
      (tstamps "a9cb6750-7855-448a-8fef-5da4eec8b027"))
    (comp (ref "TP6")
      (value "TP_I2C_SDA")
      (footprint "TestPoint:TestPoint_Pad_1.5x1.5mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Footprint") "TestPoint:TestPoint_Pad_1.5x1.5mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Sheetname") (value "Test Points"))
      (property (name "Sheetfile") (value "test_points.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Test Points/") (tstamps "/51b1dfb5-ef32-4d46-aca8-09c1f86f56e0/"))
      (tstamps "c8cffb17-742a-4eb5-a83f-456166104239"))
    (comp (ref "TP7")
      (value "TP_I2C_SCL")
      (footprint "TestPoint:TestPoint_Pad_1.5x1.5mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Footprint") "TestPoint:TestPoint_Pad_1.5x1.5mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Sheetname") (value "Test Points"))
      (property (name "Sheetfile") (value "test_points.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Test Points/") (tstamps "/51b1dfb5-ef32-4d46-aca8-09c1f86f56e0/"))
      (tstamps "8373e821-6e2c-4815-b5f4-083d162ee632"))
    (comp (ref "TP8")
      (value "TP_I2S_BCK")
      (footprint "TestPoint:TestPoint_Pad_1.5x1.5mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Footprint") "TestPoint:TestPoint_Pad_1.5x1.5mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Sheetname") (value "Test Points"))
      (property (name "Sheetfile") (value "test_points.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Test Points/") (tstamps "/51b1dfb5-ef32-4d46-aca8-09c1f86f56e0/"))
      (tstamps "c10537b8-5cc7-4ab7-b68e-2bdbbacbaebe"))
    (comp (ref "TP9")
      (value "TP_I2S_LRCK")
      (footprint "TestPoint:TestPoint_Pad_1.5x1.5mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Footprint") "TestPoint:TestPoint_Pad_1.5x1.5mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Sheetname") (value "Test Points"))
      (property (name "Sheetfile") (value "test_points.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Test Points/") (tstamps "/51b1dfb5-ef32-4d46-aca8-09c1f86f56e0/"))
      (tstamps "5c96c9d8-07a0-4b6b-8b3b-43cd8c67e5d9"))
    (comp (ref "TP10")
      (value "TP_I2S_DIN")
      (footprint "TestPoint:TestPoint_Pad_1.5x1.5mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Footprint") "TestPoint:TestPoint_Pad_1.5x1.5mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Sheetname") (value "Test Points"))
      (property (name "Sheetfile") (value "test_points.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Test Points/") (tstamps "/51b1dfb5-ef32-4d46-aca8-09c1f86f56e0/"))
      (tstamps "c2ef8b36-7158-4909-803c-8d9369519cd3"))
    (comp (ref "TP11")
      (value "TP_20V_USB_RAIL")
      (footprint "TestPoint:TestPoint_Pad_2.0x2.0mm")
      (datasheet "~")
      (description "test point")
      (fields
        (field (name "Footprint") "TestPoint:TestPoint_Pad_2.0x2.0mm")
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (libsource (lib "Connector") (part "TestPoint") (description "test point"))
      (property (name "Sheetname") (value "Test Points"))
      (property (name "Sheetfile") (value "test_points.kicad_sch"))
      (property (name "ki_keywords") (value "test point tp"))
      (property (name "ki_fp_filters") (value "Pin* Test*"))
      (sheetpath (names "/Test Points/") (tstamps "/51b1dfb5-ef32-4d46-aca8-09c1f86f56e0/"))
      (tstamps "9b728568-849d-4b2d-b07b-9f5aff9a8a3c"))
    (comp (ref "C44")
      (value "1µF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "d974f2a3-4574-4cf0-9511-6c8ea5d40aa4"))
    (comp (ref "C45")
      (value "1µF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "7e32ea3d-fc47-47a1-a66f-b074d2a27274"))
    (comp (ref "C46")
      (value "1µF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "dac0d2e6-2158-46fb-b346-b816dce74306"))
    (comp (ref "C47")
      (value "1µF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "9bd8f95e-2099-405d-813b-27e00652ee85"))
    (comp (ref "C48")
      (value "100nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "9ff13258-c727-4529-9560-fce4539c02a5"))
    (comp (ref "C49")
      (value "100nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "952ac961-d558-4e7f-9815-286604b478e7"))
    (comp (ref "C52")
      (value "1µF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "1317ff50-e8d1-469f-94a9-ac53cf4dbd3e"))
    (comp (ref "C53")
      (value "1µF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "2a7c94c0-bcdf-420e-aff2-99c492bec02d"))
    (comp (ref "J4")
      (value "USB_DJ_STICK (USB3_A)")
      (footprint "JLC2KiCad_lib-footprints:USB-3.0-A-TH_HC-ST-003-010-L15.0-J-K")
      (datasheet "~")
      (description "USB 3.0 A connector")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:USB-3.0-A-TH_HC-ST-003-010-L15.0-J-K")
        (field (name "Datasheet") "~")
        (field (name "Description") "USB 3.0 A connector"))
      (libsource (lib "Connector") (part "USB3_A") (description "USB 3.0 A connector"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "usb universal serial bus"))
      (property (name "ki_fp_filters") (value "USB3*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "ef5a3171-3d0c-4174-b3a5-dc9ee025bc31"))
    (comp (ref "J5")
      (value "AUX POWER USB_A")
      (footprint "JLC2KiCad_lib-footprints:USB-3.0-A-TH_HC-ST-003-010-L15.0-J-K")
      (datasheet "~")
      (description "USB Type A connector used to light up gadgets using this circuit's power")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:USB-3.0-A-TH_HC-ST-003-010-L15.0-J-K")
        (field (name "Datasheet") "~")
        (field (name "Description") "USB Type A connector used to light up gadgets using this circuit's power"))
      (libsource (lib "Connector") (part "USB_A") (description "USB Type A connector"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "connector USB"))
      (property (name "ki_fp_filters") (value "USB*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "473da71d-55a4-488c-b9b7-d8b63cb7cad2"))
    (comp (ref "J15")
      (value "USB_SCREEN (USB3_A)")
      (footprint "JLC2KiCad_lib-footprints:USB-3.0-A-TH_HC-ST-003-010-L15.0-J-K")
      (datasheet "~")
      (description "USB 3.0 A connector")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:USB-3.0-A-TH_HC-ST-003-010-L15.0-J-K")
        (field (name "Datasheet") "~")
        (field (name "Description") "USB 3.0 A connector"))
      (libsource (lib "Connector") (part "USB3_A") (description "USB 3.0 A connector"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "usb universal serial bus"))
      (property (name "ki_fp_filters") (value "USB3*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "680b1526-22ae-42ac-8b8d-6241e707f287"))
    (comp (ref "J20")
      (value "USB_C_Receptacle_USB2.0_16P")
      (footprint "JLC2KiCad_lib-footprints:USB-C-SMD_TYPE-C-6PIN-2MD-073")
      (datasheet "https://www.usb.org/sites/default/files/documents/usb_type-c.zip")
      (description "USB 2.0-only 16P Type-C Receptacle connector")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:USB-C-SMD_TYPE-C-6PIN-2MD-073")
        (field (name "Datasheet") "https://www.usb.org/sites/default/files/documents/usb_type-c.zip")
        (field (name "Description") "USB 2.0-only 16P Type-C Receptacle connector"))
      (libsource (lib "Connector") (part "USB_C_Receptacle_USB2.0_16P") (description "USB 2.0-only 16P Type-C Receptacle connector"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "usb universal serial bus type-C USB2.0"))
      (property (name "ki_fp_filters") (value "USB*C*Receptacle*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "1fc3a098-7ef9-4b6b-ab84-7ce99e37e2fb"))
    (comp (ref "R2")
      (value "100kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "3022c101-6b08-44e5-bc77-3ad3540171b2"))
    (comp (ref "R3")
      (value "10kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "14d8051b-bbc0-493f-8fe0-f901aeb5ae0e"))
    (comp (ref "R25")
      (value "100kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "2619be51-8473-49aa-ba0e-7068ac1941d6"))
    (comp (ref "R26")
      (value "10kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "d9ff175a-2704-4c17-acd6-6dd3e5c3c4db"))
    (comp (ref "R33")
      (value "100kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "c6ad4673-9612-44de-9ef5-c550341af4d6"))
    (comp (ref "R34")
      (value "5.1kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "ad3b56e0-772d-4498-b1ff-75f301d3d7e5"))
    (comp (ref "R35")
      (value "5.1kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "e2d8225a-ae82-49b0-a512-f4430a13d329"))
    (comp (ref "R36")
      (value "10kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "b13c1d57-75cd-4096-82d9-b5d0b9885562"))
    (comp (ref "R37")
      (value "10kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "18dae2b8-cdad-475c-b519-28ab9f92aa9d"))
    (comp (ref "U8")
      (value "USBLC6-2SC6")
      (footprint "PCM_JLCPCB:SOT-23-6_L2.9-W1.6-P0.95-LS2.8-BR")
      (datasheet "https://www.st.com/resource/en/datasheet/usblc6-2.pdf")
      (description "Very low capacitance ESD protection diode, 2 data-line, SOT-23-6")
      (fields
        (field (name "Footprint") "PCM_JLCPCB:SOT-23-6_L2.9-W1.6-P0.95-LS2.8-BR")
        (field (name "Datasheet") "https://www.st.com/resource/en/datasheet/usblc6-2.pdf")
        (field (name "Description") "Very low capacitance ESD protection diode, 2 data-line, SOT-23-6"))
      (libsource (lib "Power_Protection") (part "USBLC6-2SC6") (description "Very low capacitance ESD protection diode, 2 data-line, SOT-23-6"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "usb ethernet video"))
      (property (name "ki_fp_filters") (value "SOT?23*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "de02911c-e832-4d1b-bece-e9fc3c155ca6"))
    (comp (ref "U9")
      (value "AP2553W6-7")
      (footprint "JLC2KiCad_lib-footprints:SOT-26_L3.0-W1.6-P0.95-LS2.8-BL")
      (datasheet "https://item.szlcsc.com/211080.html")
      (fields
        (field (name "LCSC") "C212302")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:SOT-26_L3.0-W1.6-P0.95-LS2.8-BL")
        (field (name "Datasheet") "https://item.szlcsc.com/211080.html")
        (field (name "Description")))
      (libsource (lib "AP2553W6-7") (part "AP2553W6-7") (description ""))
      (property (name "LCSC") (value "C212302"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "C212302"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "6630d2a6-2dc3-4f86-ae72-a320e95cf006"))
    (comp (ref "U13")
      (value "AP2553W6-7")
      (footprint "JLC2KiCad_lib-footprints:SOT-26_L3.0-W1.6-P0.95-LS2.8-BL")
      (datasheet "https://item.szlcsc.com/211080.html")
      (fields
        (field (name "LCSC") "C212302")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:SOT-26_L3.0-W1.6-P0.95-LS2.8-BL")
        (field (name "Datasheet") "https://item.szlcsc.com/211080.html")
        (field (name "Description")))
      (libsource (lib "AP2553W6-7") (part "AP2553W6-7") (description ""))
      (property (name "LCSC") (value "C212302"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "C212302"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "c6477ae5-d171-4636-97f7-c43bebb35b68"))
    (comp (ref "U14")
      (value "USBLC6-2SC6")
      (footprint "PCM_JLCPCB:SOT-23-6_L2.9-W1.6-P0.95-LS2.8-BR")
      (datasheet "https://www.st.com/resource/en/datasheet/usblc6-2.pdf")
      (description "Very low capacitance ESD protection diode, 2 data-line, SOT-23-6")
      (fields
        (field (name "Footprint") "PCM_JLCPCB:SOT-23-6_L2.9-W1.6-P0.95-LS2.8-BR")
        (field (name "Datasheet") "https://www.st.com/resource/en/datasheet/usblc6-2.pdf")
        (field (name "Description") "Very low capacitance ESD protection diode, 2 data-line, SOT-23-6"))
      (libsource (lib "Power_Protection") (part "USBLC6-2SC6") (description "Very low capacitance ESD protection diode, 2 data-line, SOT-23-6"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "usb ethernet video"))
      (property (name "ki_fp_filters") (value "SOT?23*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "69ebdfe5-ab8d-4881-a8b0-ca4da78d6ae4"))
    (comp (ref "U17")
      (value "USBLC6-2SC6")
      (footprint "PCM_JLCPCB:SOT-23-6_L2.9-W1.6-P0.95-LS2.8-BR")
      (datasheet "https://www.st.com/resource/en/datasheet/usblc6-2.pdf")
      (description "Very low capacitance ESD protection diode, 2 data-line, SOT-23-6")
      (fields
        (field (name "Footprint") "PCM_JLCPCB:SOT-23-6_L2.9-W1.6-P0.95-LS2.8-BR")
        (field (name "Datasheet") "https://www.st.com/resource/en/datasheet/usblc6-2.pdf")
        (field (name "Description") "Very low capacitance ESD protection diode, 2 data-line, SOT-23-6"))
      (libsource (lib "Power_Protection") (part "USBLC6-2SC6") (description "Very low capacitance ESD protection diode, 2 data-line, SOT-23-6"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "usb ethernet video"))
      (property (name "ki_fp_filters") (value "SOT?23*"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "21b38e91-92af-4196-b01f-a53fcbf494c2"))
    (comp (ref "U18")
      (value "AP2553W6-7")
      (footprint "JLC2KiCad_lib-footprints:SOT-26_L3.0-W1.6-P0.95-LS2.8-BL")
      (datasheet "https://item.szlcsc.com/211080.html")
      (fields
        (field (name "LCSC") "C212302")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:SOT-26_L3.0-W1.6-P0.95-LS2.8-BL")
        (field (name "Datasheet") "https://item.szlcsc.com/211080.html")
        (field (name "Description")))
      (libsource (lib "AP2553W6-7") (part "AP2553W6-7") (description ""))
      (property (name "LCSC") (value "C212302"))
      (property (name "Sheetname") (value "USB DJ Ports"))
      (property (name "Sheetfile") (value "usb_dj_ports.kicad_sch"))
      (property (name "ki_keywords") (value "C212302"))
      (sheetpath (names "/USB DJ Ports/") (tstamps "/23bc0d32-2963-402a-a1e9-9d0e27b47670/"))
      (tstamps "47e62c68-9807-4713-881f-5759cfe0c360"))
    (comp (ref "J2")
      (value "PI HDMI_0 (HDMI_D_1.4 micro)")
      (footprint "JLC2KiCad_lib-footprints:HDMI-SMD_HDMI-101S")
      (datasheet "http://pinoutguide.com/PortableDevices/micro_hdmi_type_d_pinout.shtml")
      (description "HDMI 1.4+ type D connector")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:HDMI-SMD_HDMI-101S")
        (field (name "Datasheet") "http://pinoutguide.com/PortableDevices/micro_hdmi_type_d_pinout.shtml")
        (field (name "Description") "HDMI 1.4+ type D connector"))
      (libsource (lib "Connector") (part "HDMI_D_1.4") (description "HDMI 1.4+ type D connector"))
      (property (name "Sheetname") (value "HDMI and Ethernet"))
      (property (name "Sheetfile") (value "hdmi.kicad_sch"))
      (property (name "ki_keywords") (value "hdmi conn"))
      (property (name "ki_fp_filters") (value "HDMI*D*"))
      (sheetpath (names "/HDMI and Ethernet/") (tstamps "/97e2c747-925a-451b-94c7-ccaeac2c14a8/"))
      (tstamps "762e5660-f9ca-4878-8c8d-fe0d1e6ae217"))
    (comp (ref "J3")
      (value "PI HDMI_0 (HDMI_D_1.4 micro)")
      (footprint "JLC2KiCad_lib-footprints:HDMI-SMD_HDMI-101S")
      (datasheet "http://pinoutguide.com/PortableDevices/micro_hdmi_type_d_pinout.shtml")
      (description "HDMI 1.4+ type D connector")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:HDMI-SMD_HDMI-101S")
        (field (name "Datasheet") "http://pinoutguide.com/PortableDevices/micro_hdmi_type_d_pinout.shtml")
        (field (name "Description") "HDMI 1.4+ type D connector"))
      (libsource (lib "Connector") (part "HDMI_D_1.4") (description "HDMI 1.4+ type D connector"))
      (property (name "Sheetname") (value "HDMI and Ethernet"))
      (property (name "Sheetfile") (value "hdmi.kicad_sch"))
      (property (name "ki_keywords") (value "hdmi conn"))
      (property (name "ki_fp_filters") (value "HDMI*D*"))
      (sheetpath (names "/HDMI and Ethernet/") (tstamps "/97e2c747-925a-451b-94c7-ccaeac2c14a8/"))
      (tstamps "49c01394-e7c0-48a0-adc0-5a338f4ebfd9"))
    (comp (ref "R16")
      (value "270Ω")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "HDMI and Ethernet"))
      (property (name "Sheetfile") (value "hdmi.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/HDMI and Ethernet/") (tstamps "/97e2c747-925a-451b-94c7-ccaeac2c14a8/"))
      (tstamps "06ab9de6-e22d-4745-97ea-244260c32cc3"))
    (comp (ref "R17")
      (value "270Ω")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "HDMI and Ethernet"))
      (property (name "Sheetfile") (value "hdmi.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/HDMI and Ethernet/") (tstamps "/97e2c747-925a-451b-94c7-ccaeac2c14a8/"))
      (tstamps "bcacd027-4321-4fa4-a645-21ca24d1c515"))
    (comp (ref "U15")
      (value "HR911130A")
      (footprint "JLC2KiCad_lib-footprints:RJ45-TH_HR911130A")
      (datasheet "https://item.szlcsc.com/55426.html")
      (fields
        (field (name "LCSC") "C54408")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:RJ45-TH_HR911130A")
        (field (name "Datasheet") "https://item.szlcsc.com/55426.html")
        (field (name "Description")))
      (libsource (lib "HR911130A") (part "HR911130A") (description ""))
      (property (name "LCSC") (value "C54408"))
      (property (name "Sheetname") (value "HDMI and Ethernet"))
      (property (name "Sheetfile") (value "hdmi.kicad_sch"))
      (property (name "ki_keywords") (value "C54408"))
      (sheetpath (names "/HDMI and Ethernet/") (tstamps "/97e2c747-925a-451b-94c7-ccaeac2c14a8/"))
      (tstamps "b31857e9-1d6f-42aa-9d98-b323456281ab"))
    (comp (ref "C1")
      (value "1uF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized CERAMIC capacitor")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized CERAMIC capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "18c7cf92-2c72-4fde-a923-6a92f6eb27fa"))
    (comp (ref "C2")
      (value "1uF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized CERAMIC capacitor")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized CERAMIC capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "a32ba231-ee1d-4dc4-85c6-62b5bb173f38"))
    (comp (ref "C3")
      (value "1uF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized CERAMIC capacitor")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized CERAMIC capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "4ab2f267-88b6-4e5a-a319-e73dafbab2e1"))
    (comp (ref "C4")
      (value "1uF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized CERAMIC capacitor")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized CERAMIC capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "f1a4d73a-00ef-4cd9-91e4-dcc4fb9c8771"))
    (comp (ref "C15")
      (value "100nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "b27266aa-f803-4983-8e02-af9e829e835f"))
    (comp (ref "C23")
      (value "100nF/50V")
      (footprint "Capacitor_SMD:C_0603_1608Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0603_1608Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "161aeb7f-2540-4455-b6ae-ce406024cbf2"))
    (comp (ref "C25")
      (value "22µF/50V")
      (footprint "Capacitor_SMD:C_1210_3225Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_1210_3225Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "25a595ab-2927-4637-86ef-38ec138b365c"))
    (comp (ref "C26")
      (value "100nF/50V")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "1af27551-7b77-435a-afb7-88eac174520c"))
    (comp (ref "C36")
      (value "100nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "fd27a5cf-ad66-4de4-9476-d5d177325ff3"))
    (comp (ref "C37")
      (value "100nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "9f879c2e-d42d-4e69-a0ff-3bf00fb76da0"))
    (comp (ref "C38")
      (value "100nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "a4572058-4832-4939-a61e-b7b8c5b75e10"))
    (comp (ref "C39")
      (value "100nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "2c8c9716-88dd-473a-ac06-b3960f3973a2"))
    (comp (ref "C40")
      (value "100nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "ef64d47f-2653-4782-b4aa-e691d42b97a6"))
    (comp (ref "C41")
      (value "100nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "5847a6db-e430-4d77-a224-31efd6343252"))
    (comp (ref "C43")
      (value "10µF/35V")
      (footprint "Capacitor_SMD:C_0805_2012Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0805_2012Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "0527da60-5b8e-4909-a33d-e9d57c569d7b"))
    (comp (ref "C50")
      (value "100nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "72849b12-8f14-45a9-a4b8-c90fd974d959"))
    (comp (ref "C51")
      (value "100nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "944c08c3-81ef-45f5-96c2-11d541ef3edb"))
    (comp (ref "C54")
      (value "100nF")
      (footprint "PCM_JLCPCB:C_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05B104KB54PNC_C307331.pdf")
      (description "50V 100nF X7R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
      (fields
        (field (name "LCSC") "C307331")
        (field (name "Stock") "8389599")
        (field (name "Price") "0.008USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT")
        (field (name "Manufacturer") "Samsung Electro-Mechanics")
        (field (name "Part") "CL05B104KB54PNC")
        (field (name "Voltage Rated") "50V")
        (field (name "Tolerance") "±10%")
        (field (name "Capacitance") "100nF")
        (field (name "Temperature Coefficient") "X7R")
        (field (name "Footprint") "PCM_JLCPCB:C_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05B104KB54PNC_C307331.pdf")
        (field (name "Description") "50V 100nF X7R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (libsource (lib "PCM_JLCPCB-Capacitors") (part "0402,100nF,(2)") (description "50V 100nF X7R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (property (name "LCSC") (value "C307331"))
      (property (name "Stock") (value "8389599"))
      (property (name "Price") (value "0.008USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT"))
      (property (name "Manufacturer") (value "Samsung Electro-Mechanics"))
      (property (name "Part") (value "CL05B104KB54PNC"))
      (property (name "Voltage Rated") (value "50V"))
      (property (name "Tolerance") (value "±10%"))
      (property (name "Capacitance") (value "100nF"))
      (property (name "Temperature Coefficient") (value "X7R"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "24db408b-d71f-4208-a0c3-316afac55655"))
    (comp (ref "C55")
      (value "10uF")
      (footprint "PCM_JLCPCB:C_0805")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2411041759_Murata-Electronics-GRM21BR61H106KE43L_C440198.pdf")
      (description "50V 10uF X5R ±10% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
      (fields
        (field (name "LCSC") "C440198")
        (field (name "Stock") "1422246")
        (field (name "Price") "0.066USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "5")
        (field (name "Attrition Qty") "4")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT")
        (field (name "Manufacturer") "Murata Electronics")
        (field (name "Part") "GRM21BR61H106KE43L")
        (field (name "Voltage Rated") "50V")
        (field (name "Tolerance") "±10%")
        (field (name "Capacitance") "10uF")
        (field (name "Temperature Coefficient") "X5R")
        (field (name "Footprint") "PCM_JLCPCB:C_0805")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2411041759_Murata-Electronics-GRM21BR61H106KE43L_C440198.pdf")
        (field (name "Description") "50V 10uF X5R ±10% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (libsource (lib "PCM_JLCPCB-Capacitors") (part "0805,10uF,(2)") (description "50V 10uF X5R ±10% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (property (name "LCSC") (value "C440198"))
      (property (name "Stock") (value "1422246"))
      (property (name "Price") (value "0.066USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "5"))
      (property (name "Attrition Qty") (value "4"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT"))
      (property (name "Manufacturer") (value "Murata Electronics"))
      (property (name "Part") (value "GRM21BR61H106KE43L"))
      (property (name "Voltage Rated") (value "50V"))
      (property (name "Tolerance") (value "±10%"))
      (property (name "Capacitance") (value "10uF"))
      (property (name "Temperature Coefficient") (value "X5R"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "dea176c5-2154-4356-9b5b-f6e9bd958275"))
    (comp (ref "C56")
      (value "10uF")
      (footprint "PCM_JLCPCB:C_0805")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2411041759_Murata-Electronics-GRM21BR61H106KE43L_C440198.pdf")
      (description "50V 10uF X5R ±10% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
      (fields
        (field (name "LCSC") "C440198")
        (field (name "Stock") "1422246")
        (field (name "Price") "0.066USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "5")
        (field (name "Attrition Qty") "4")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT")
        (field (name "Manufacturer") "Murata Electronics")
        (field (name "Part") "GRM21BR61H106KE43L")
        (field (name "Voltage Rated") "50V")
        (field (name "Tolerance") "±10%")
        (field (name "Capacitance") "10uF")
        (field (name "Temperature Coefficient") "X5R")
        (field (name "Footprint") "PCM_JLCPCB:C_0805")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2411041759_Murata-Electronics-GRM21BR61H106KE43L_C440198.pdf")
        (field (name "Description") "50V 10uF X5R ±10% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (libsource (lib "PCM_JLCPCB-Capacitors") (part "0805,10uF,(2)") (description "50V 10uF X5R ±10% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (property (name "LCSC") (value "C440198"))
      (property (name "Stock") (value "1422246"))
      (property (name "Price") (value "0.066USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "5"))
      (property (name "Attrition Qty") (value "4"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT"))
      (property (name "Manufacturer") (value "Murata Electronics"))
      (property (name "Part") (value "GRM21BR61H106KE43L"))
      (property (name "Voltage Rated") (value "50V"))
      (property (name "Tolerance") (value "±10%"))
      (property (name "Capacitance") (value "10uF"))
      (property (name "Temperature Coefficient") (value "X5R"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "9f808e14-6a86-4527-9ea2-726561d40961"))
    (comp (ref "C57")
      (value "1uF")
      (footprint "PCM_JLCPCB:C_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05A105KA5NQNC_C52923.pdf")
      (description "25V 1uF X5R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
      (fields
        (field (name "LCSC") "C52923")
        (field (name "Stock") "7021828")
        (field (name "Price") "0.006USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT")
        (field (name "Manufacturer") "Samsung Electro-Mechanics")
        (field (name "Part") "CL05A105KA5NQNC")
        (field (name "Voltage Rated") "25V")
        (field (name "Tolerance") "±10%")
        (field (name "Capacitance") "1uF")
        (field (name "Temperature Coefficient") "X5R")
        (field (name "Footprint") "PCM_JLCPCB:C_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05A105KA5NQNC_C52923.pdf")
        (field (name "Description") "25V 1uF X5R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (libsource (lib "PCM_JLCPCB-Capacitors") (part "0402,1uF") (description "25V 1uF X5R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (property (name "LCSC") (value "C52923"))
      (property (name "Stock") (value "7021828"))
      (property (name "Price") (value "0.006USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT"))
      (property (name "Manufacturer") (value "Samsung Electro-Mechanics"))
      (property (name "Part") (value "CL05A105KA5NQNC"))
      (property (name "Voltage Rated") (value "25V"))
      (property (name "Tolerance") (value "±10%"))
      (property (name "Capacitance") (value "1uF"))
      (property (name "Temperature Coefficient") (value "X5R"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "53c7997d-7e56-47f3-b140-1a5a9341c465"))
    (comp (ref "C58")
      (value "100pF")
      (footprint "PCM_JLCPCB:C_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_FH--Guangdong-Fenghua-Advanced-Tech-0402CG101J500NT_C1546.pdf")
      (description "50V 100pF C0G ±5% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
      (fields
        (field (name "LCSC") "C1546")
        (field (name "Stock") "2554383")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT")
        (field (name "Manufacturer") "FH(Guangdong Fenghua Advanced Tech)")
        (field (name "Part") "0402CG101J500NT")
        (field (name "Voltage Rated") "50V")
        (field (name "Tolerance") "±5%")
        (field (name "Capacitance") "100pF")
        (field (name "Temperature Coefficient") "C0G")
        (field (name "Footprint") "PCM_JLCPCB:C_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_FH--Guangdong-Fenghua-Advanced-Tech-0402CG101J500NT_C1546.pdf")
        (field (name "Description") "50V 100pF C0G ±5% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (libsource (lib "PCM_JLCPCB-Capacitors") (part "0402,100pF") (description "50V 100pF C0G ±5% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"))
      (property (name "LCSC") (value "C1546"))
      (property (name "Stock") (value "2554383"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT"))
      (property (name "Manufacturer") (value "FH(Guangdong Fenghua Advanced Tech)"))
      (property (name "Part") (value "0402CG101J500NT"))
      (property (name "Voltage Rated") (value "50V"))
      (property (name "Tolerance") (value "±5%"))
      (property (name "Capacitance") (value "100pF"))
      (property (name "Temperature Coefficient") (value "C0G"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "86a75b04-5225-4e5d-853a-516bc67504b1"))
    (comp (ref "D1")
      (value "KT-0603R")
      (footprint "JLC2KiCad_lib-footprints:LED0603-RD")
      (datasheet "https://item.szlcsc.com/347874.html")
      (fields
        (field (name "LCSC") "C2286")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:LED0603-RD")
        (field (name "Datasheet") "https://item.szlcsc.com/347874.html")
        (field (name "Description")))
      (libsource (lib "KT-0603R") (part "KT-0603R") (description ""))
      (property (name "LCSC") (value "C2286"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "C2286"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "0b7c3e22-e0e1-462a-9cb1-f31aacaab848"))
    (comp (ref "D2")
      (value "BZT52C3V3S")
      (footprint "PCM_JLCPCB:D_SOD-323")
      (datasheet "https://wmsc.lcsc.com/wmsc/upload/file/pdf/v2/lcsc/2403280505_hongjiacheng-BZT52C3V3S_C19077437.pdf")
      (description "Independent Type 200mW 3.1V~3.5V 3.3V SOD-323 Zener Diodes ROHS")
      (fields
        (field (name "LCSC") "C19077437")
        (field (name "Stock") "229387")
        (field (name "Price") "0.018USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Preferred Component")
        (field (name "Category") "Diodes,Zener Diodes")
        (field (name "Manufacturer") "hongjiacheng")
        (field (name "Part") "BZT52C3V3S")
        (field (name "Footprint") "PCM_JLCPCB:D_SOD-323")
        (field (name "Datasheet") "https://wmsc.lcsc.com/wmsc/upload/file/pdf/v2/lcsc/2403280505_hongjiacheng-BZT52C3V3S_C19077437.pdf")
        (field (name "Description") "Independent Type 200mW 3.1V~3.5V 3.3V SOD-323 Zener Diodes ROHS"))
      (libsource (lib "PCM_JLCPCB-Diodes") (part "Zener,BZT52C3V3S") (description "Independent Type 200mW 3.1V~3.5V 3.3V SOD-323 Zener Diodes ROHS"))
      (property (name "LCSC") (value "C19077437"))
      (property (name "Stock") (value "229387"))
      (property (name "Price") (value "0.018USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Preferred Component"))
      (property (name "Category") (value "Diodes,Zener Diodes"))
      (property (name "Manufacturer") (value "hongjiacheng"))
      (property (name "Part") (value "BZT52C3V3S"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_fp_filters") (value "D_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "10b46454-888d-46b7-a6d6-4bb74fc479b5"))
    (comp (ref "D3")
      (value "PSC-1608U52GC-G4")
      (footprint "JLC2KiCad_lib-footprints:LED0603-RD_GREEN")
      (datasheet "https://atta.szlcsc.com/upload/public/pdf/source/20190115/C264450_D840E7E570138F41CCE67133F241C738.pdf")
      (fields
        (field (name "LCSC") "C22371297")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:LED0603-RD_GREEN")
        (field (name "Datasheet") "https://atta.szlcsc.com/upload/public/pdf/source/20190115/C264450_D840E7E570138F41CCE67133F241C738.pdf")
        (field (name "Description")))
      (libsource (lib "PSC-1608U52GC-G4") (part "PSC-1608U52GC-G4") (description ""))
      (property (name "LCSC") (value "C22371297"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "C22371297"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "b681a82d-fc87-48e5-b309-360d34beb59e"))
    (comp (ref "D7")
      (value "KT-0603R")
      (footprint "JLC2KiCad_lib-footprints:LED0603-RD")
      (datasheet "https://item.szlcsc.com/347874.html")
      (fields
        (field (name "LCSC") "C2286")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:LED0603-RD")
        (field (name "Datasheet") "https://item.szlcsc.com/347874.html")
        (field (name "Description")))
      (libsource (lib "KT-0603R") (part "KT-0603R") (description ""))
      (property (name "LCSC") (value "C2286"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "C2286"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "77e40ba0-0b44-4d46-a1ed-e27504b457b8"))
    (comp (ref "J1")
      (value "USB_C_Receptacle_USB2.0_16P")
      (footprint "JLC2KiCad_lib-footprints:USB-C-SMD_TYPE-C-6PIN-2MD-073")
      (datasheet "https://www.usb.org/sites/default/files/documents/usb_type-c.zip")
      (description "USB 2.0-only 16P Type-C Receptacle connector")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:USB-C-SMD_TYPE-C-6PIN-2MD-073")
        (field (name "Datasheet") "https://www.usb.org/sites/default/files/documents/usb_type-c.zip")
        (field (name "Description") "USB 2.0-only 16P Type-C Receptacle connector"))
      (libsource (lib "Connector") (part "USB_C_Receptacle_USB2.0_16P") (description "USB 2.0-only 16P Type-C Receptacle connector"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "usb universal serial bus type-C USB2.0"))
      (property (name "ki_fp_filters") (value "USB*C*Receptacle*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "e64de935-dc00-49be-97b2-00045a5ae731"))
    (comp (ref "L1")
      (value "SL1040-2R2M")
      (footprint "JLC2KiCad_lib-footprints:IND-SMD_SL1040-R47M")
      (datasheet "https://atta.szlcsc.com/upload/public/pdf/source/20240611/8DE7D6BE1273F2E871C82A6D5C20B08D.pdf")
      (fields
        (field (name "LCSC") "C22463836")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:IND-SMD_SL1040-R47M")
        (field (name "Datasheet") "https://atta.szlcsc.com/upload/public/pdf/source/20240611/8DE7D6BE1273F2E871C82A6D5C20B08D.pdf")
        (field (name "Description")))
      (libsource (lib "SL1040-2R2M") (part "SL1040-2R2M") (description ""))
      (property (name "LCSC") (value "C22463836"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "C22463836"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "167f41e6-7955-4ce1-9c4c-81a3b240f3d7"))
    (comp (ref "R1")
      (value "3.3kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "LCSC") "C22978")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "LCSC") (value "C22978"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "4d123850-2a3f-4e48-8856-e7d170a708b8"))
    (comp (ref "R11")
      (value "3.3kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "cd0ffe8b-f9a6-48b6-acd9-a50a5d190c21"))
    (comp (ref "R19")
      (value "1kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "e2046b71-aa3b-4796-8874-d1b096bfde74"))
    (comp (ref "R40")
      (value "200kΩ")
      (footprint "PCM_JLCPCB:R_0603")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010045_UNI-ROYAL-Uniroyal-Elec-0603WAF2003T5E_C25811.pdf")
      (description "100mW Thick Film Resistors 75V ±100ppm/°C ±1% 200kΩ 0603 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C25811")
        (field (name "Stock") "1426208")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0603WAF2003T5E")
        (field (name "Resistance") "200kΩ")
        (field (name "Power(Watts)") "100mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "75V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0603")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010045_UNI-ROYAL-Uniroyal-Elec-0603WAF2003T5E_C25811.pdf")
        (field (name "Description") "100mW Thick Film Resistors 75V ±100ppm/°C ±1% 200kΩ 0603 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0603,200kΩ") (description "100mW Thick Film Resistors 75V ±100ppm/°C ±1% 200kΩ 0603 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C25811"))
      (property (name "Stock") (value "1426208"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0603WAF2003T5E"))
      (property (name "Resistance") (value "200kΩ"))
      (property (name "Power(Watts)") (value "100mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "75V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±100ppm/°C"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "aa8cb6b9-b6db-462e-9782-82fe90959cb0"))
    (comp (ref "R41")
      (value "27kΩ")
      (footprint "PCM_JLCPCB:R_0603")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010130_UNI-ROYAL-Uniroyal-Elec-0603WAF2702T5E_C22967.pdf")
      (description "100mW Thick Film Resistors 75V ±100ppm/°C ±1% 27kΩ 0603 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C22967")
        (field (name "Stock") "708507")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0603WAF2702T5E")
        (field (name "Resistance") "27kΩ")
        (field (name "Power(Watts)") "100mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "75V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0603")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010130_UNI-ROYAL-Uniroyal-Elec-0603WAF2702T5E_C22967.pdf")
        (field (name "Description") "100mW Thick Film Resistors 75V ±100ppm/°C ±1% 27kΩ 0603 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0603,27kΩ") (description "100mW Thick Film Resistors 75V ±100ppm/°C ±1% 27kΩ 0603 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C22967"))
      (property (name "Stock") (value "708507"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0603WAF2702T5E"))
      (property (name "Resistance") (value "27kΩ"))
      (property (name "Power(Watts)") (value "100mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "75V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±100ppm/°C"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "ed5ce352-bf7e-4d1c-858b-2674fd5586dd"))
    (comp (ref "R42")
      (value "10Ω")
      (footprint "PCM_JLCPCB:R_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2411221126_UNI-ROYAL-Uniroyal-Elec-0402WGF100JTCE_C25077.pdf")
      (description "62.5mW Thick Film Resistors 50V ±1% ±200ppm/°C 10Ω 0402 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C25077")
        (field (name "Stock") "4873481")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF100JTCE")
        (field (name "Resistance") "10Ω")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±200ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2411221126_UNI-ROYAL-Uniroyal-Elec-0402WGF100JTCE_C25077.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±1% ±200ppm/°C 10Ω 0402 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0402,10Ω") (description "62.5mW Thick Film Resistors 50V ±1% ±200ppm/°C 10Ω 0402 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C25077"))
      (property (name "Stock") (value "4873481"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0402WGF100JTCE"))
      (property (name "Resistance") (value "10Ω"))
      (property (name "Power(Watts)") (value "62.5mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "50V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±200ppm/°C"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "8d584352-3510-4b24-9048-9fbd1d85a987"))
    (comp (ref "R43")
      (value "100kΩ")
      (footprint "PCM_JLCPCB:R_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010100_UNI-ROYAL-Uniroyal-Elec-0402WGF1003TCE_C25741.pdf")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 100kΩ 0402 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C25741")
        (field (name "Stock") "6969783")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF1003TCE")
        (field (name "Resistance") "100kΩ")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010100_UNI-ROYAL-Uniroyal-Elec-0402WGF1003TCE_C25741.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 100kΩ 0402 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0402,100kΩ") (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 100kΩ 0402 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C25741"))
      (property (name "Stock") (value "6969783"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0402WGF1003TCE"))
      (property (name "Resistance") (value "100kΩ"))
      (property (name "Power(Watts)") (value "62.5mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "50V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±100ppm/°C"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "bae456c1-7699-4980-8e81-19cf6b602a69"))
    (comp (ref "R44")
      (value "100kΩ")
      (footprint "PCM_JLCPCB:R_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010100_UNI-ROYAL-Uniroyal-Elec-0402WGF1003TCE_C25741.pdf")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 100kΩ 0402 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C25741")
        (field (name "Stock") "6969783")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF1003TCE")
        (field (name "Resistance") "100kΩ")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010100_UNI-ROYAL-Uniroyal-Elec-0402WGF1003TCE_C25741.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 100kΩ 0402 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0402,100kΩ") (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 100kΩ 0402 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C25741"))
      (property (name "Stock") (value "6969783"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0402WGF1003TCE"))
      (property (name "Resistance") (value "100kΩ"))
      (property (name "Power(Watts)") (value "62.5mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "50V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±100ppm/°C"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "5c2260b7-4fcf-4a8d-8658-4b9c34b49021"))
    (comp (ref "R45")
      (value "18kΩ")
      (footprint "PCM_JLCPCB:R_0603")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010045_UNI-ROYAL-Uniroyal-Elec-0603WAF1802T5E_C25810.pdf")
      (description "100mW Thick Film Resistors 75V ±100ppm/°C ±1% 18kΩ 0603 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C25810")
        (field (name "Stock") "574660")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0603WAF1802T5E")
        (field (name "Resistance") "18kΩ")
        (field (name "Power(Watts)") "100mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "75V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0603")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010045_UNI-ROYAL-Uniroyal-Elec-0603WAF1802T5E_C25810.pdf")
        (field (name "Description") "100mW Thick Film Resistors 75V ±100ppm/°C ±1% 18kΩ 0603 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0603,18kΩ") (description "100mW Thick Film Resistors 75V ±100ppm/°C ±1% 18kΩ 0603 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C25810"))
      (property (name "Stock") (value "574660"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "10"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0603WAF1802T5E"))
      (property (name "Resistance") (value "18kΩ"))
      (property (name "Power(Watts)") (value "100mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "75V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±100ppm/°C"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "4a7830e6-10c1-403b-ae48-959667f701c6"))
    (comp (ref "R46")
      (value "510Ω")
      (footprint "PCM_JLCPCB:R_0402")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF5100TCE_C25123.pdf")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 510Ω 0402 Chip Resistor - Surface Mount ROHS")
      (fields
        (field (name "LCSC") "C25123")
        (field (name "Stock") "2434473")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "12")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF5100TCE")
        (field (name "Resistance") "510Ω")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF5100TCE_C25123.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 510Ω 0402 Chip Resistor - Surface Mount ROHS"))
      (libsource (lib "PCM_JLCPCB-Resistors") (part "0402,510Ω") (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 510Ω 0402 Chip Resistor - Surface Mount ROHS"))
      (property (name "LCSC") (value "C25123"))
      (property (name "Stock") (value "2434473"))
      (property (name "Price") (value "0.004USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "20"))
      (property (name "Attrition Qty") (value "12"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Resistors,Chip Resistor - Surface Mount"))
      (property (name "Manufacturer") (value "UNI-ROYAL(Uniroyal Elec)"))
      (property (name "Part") (value "0402WGF5100TCE"))
      (property (name "Resistance") (value "510Ω"))
      (property (name "Power(Watts)") (value "62.5mW"))
      (property (name "Type") (value "Thick Film Resistors"))
      (property (name "Overload Voltage (Max)") (value "50V"))
      (property (name "Operating Temperature Range") (value "-55°C~+155°C"))
      (property (name "Tolerance") (value "±1%"))
      (property (name "Temperature Coefficient") (value "±100ppm/°C"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "388c0a69-40e6-408e-b558-59bb7a55cc83"))
    (comp (ref "U0")
      (value "Compute_Module_5_Functional")
      (footprint "kicad-thirdparty-footprints:CM5")
      (fields
        (field (name "Footprint") "kicad-thirdparty-footprints:CM5")
        (field (name "Datasheet"))
        (field (name "Description")))
      (libsource (lib "rpi-cm-5") (part "Compute_Module_5_Functional") (description ""))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "537f0f7a-af00-4939-990e-5b2e1316d355"))
    (comp (ref "U1")
      (value "AP2112K-3.3 DIGITAL PSU LDO")
      (footprint "JLC2KiCad_lib-footprints:SOT-23-5_L2.9-W1.6-P0.95-LS2.8-BR")
      (datasheet "https://www.diodes.com/assets/Datasheets/AP2112.pdf")
      (description "600mA low dropout linear regulator, with enable pin, 3.8V-6V input voltage range, 3.3V fixed positive output, SOT-23-5")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:SOT-23-5_L2.9-W1.6-P0.95-LS2.8-BR")
        (field (name "Datasheet") "https://www.diodes.com/assets/Datasheets/AP2112.pdf")
        (field (name "Description") "600mA low dropout linear regulator, with enable pin, 3.8V-6V input voltage range, 3.3V fixed positive output, SOT-23-5"))
      (libsource (lib "Regulator_Linear") (part "AP2112K-3.3") (description "600mA low dropout linear regulator, with enable pin, 3.8V-6V input voltage range, 3.3V fixed positive output, SOT-23-5"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "linear regulator ldo fixed positive"))
      (property (name "ki_fp_filters") (value "SOT?23?5*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "297d4d38-3986-4bca-b131-1d4a2b954165"))
    (comp (ref "U2")
      (value "AP2112K-3.3 ANALOG AUDIO LDO")
      (footprint "JLC2KiCad_lib-footprints:SOT-23-5_L2.9-W1.6-P0.95-LS2.8-BR")
      (datasheet "https://www.diodes.com/assets/Datasheets/AP2112.pdf")
      (description "clean analog, for PCM5242 analog section only -- 600mA low dropout linear regulator, with enable pin, 3.8V-6V input voltage range, 3.3V fixed positive output, SOT-23-5")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:SOT-23-5_L2.9-W1.6-P0.95-LS2.8-BR")
        (field (name "Datasheet") "https://www.diodes.com/assets/Datasheets/AP2112.pdf")
        (field (name "Description") "clean analog, for PCM5242 analog section only -- 600mA low dropout linear regulator, with enable pin, 3.8V-6V input voltage range, 3.3V fixed positive output, SOT-23-5"))
      (libsource (lib "Regulator_Linear") (part "AP2112K-3.3") (description "600mA low dropout linear regulator, with enable pin, 3.8V-6V input voltage range, 3.3V fixed positive output, SOT-23-5"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "linear regulator ldo fixed positive"))
      (property (name "ki_fp_filters") (value "SOT?23?5*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "e85fefb2-4c9b-413a-9140-54d0ffc66788"))
    (comp (ref "U6")
      (value "CH224K")
      (footprint "JLC2KiCad_lib-footprints:ESSOP-10_L4.9-W3.9-P1.0-LS6.0-TL-EP")
      (datasheet "https://www.wch.cn/downloads/file/301.html")
      (description "100W USB Type-C PD3.0/2.0, BC1.2 Sink Controller, SSOP-10")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:ESSOP-10_L4.9-W3.9-P1.0-LS6.0-TL-EP")
        (field (name "Datasheet") "https://www.wch.cn/downloads/file/301.html")
        (field (name "Description") "100W USB Type-C PD3.0/2.0, BC1.2 Sink Controller, SSOP-10"))
      (libsource (lib "Interface_USB") (part "CH224K") (description "100W USB Type-C PD3.0/2.0, BC1.2 Sink Controller, SSOP-10"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "USB-C WCH powered-device"))
      (property (name "ki_fp_filters") (value "SSOP*3.9x4.9mm*P1mm*EP2.1x3.3mm*"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "d4cab4f1-520c-4755-b9d4-abd2cd18705b"))
    (comp (ref "U11")
      (value "SW_MAIN_POWER")
      (footprint "JLC2KiCad_lib-footprints:SW-TH_PS-22E05")
      (datasheet "https://atta.szlcsc.com/upload/public/pdf/source/20210825/03FED21E2D4F2980BA08F4ED04C13B40.pdf")
      (fields
        (field (name "LCSC") "C19190928")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:SW-TH_PS-22E05")
        (field (name "Datasheet") "https://atta.szlcsc.com/upload/public/pdf/source/20210825/03FED21E2D4F2980BA08F4ED04C13B40.pdf")
        (field (name "Description")))
      (libsource (lib "PS-22E05-S-O-001") (part "PS-22E05-S-O-001") (description ""))
      (property (name "LCSC") (value "C19190928"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "C19190928"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "ad778893-c1fb-4dad-8d17-c591559144e4"))
    (comp (ref "U19")
      (value "SY8368AQQC")
      (footprint "JLC2KiCad_lib-footprints:QFN-12_L3.0-W3.0-P0.45-TL-EP")
      (datasheet "https://atta.szlcsc.com/upload/public/pdf/source/20180224/C178253_15194367790221363788.pdf")
      (fields
        (field (name "LCSC") "C207642")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:QFN-12_L3.0-W3.0-P0.45-TL-EP")
        (field (name "Datasheet") "https://atta.szlcsc.com/upload/public/pdf/source/20180224/C178253_15194367790221363788.pdf")
        (field (name "Description")))
      (libsource (lib "SY8368AQQC") (part "SY8368AQQC") (description ""))
      (property (name "LCSC") (value "C207642"))
      (property (name "Sheetname") (value "Power Delivery"))
      (property (name "Sheetfile") (value "power.kicad_sch"))
      (property (name "ki_keywords") (value "C207642"))
      (sheetpath (names "/Power Delivery/") (tstamps "/a58fdbba-c04e-4f2c-b7ca-3e3943d24e2d/"))
      (tstamps "ad0dd509-8300-48a3-9905-1b707b086243"))
    (comp (ref "C5")
      (value "100nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "7d6b3185-27bd-45c4-9bb8-ec34f3d1a8c6"))
    (comp (ref "C6")
      (value "100nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "f016868c-76f1-4e20-9fb1-468a42b6e24f"))
    (comp (ref "C7")
      (value "100nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "e817a6f3-7c4e-420b-a318-deadfe3abe38"))
    (comp (ref "C8")
      (value "1uF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "980bc064-5e1e-4f0d-9ec7-dbae45398075"))
    (comp (ref "C9")
      (value "15pF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "0a98cc2a-2f3d-477e-858b-9056b4fff403"))
    (comp (ref "C10")
      (value "15pF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "a397d297-62d5-4c44-9d38-68510deb7179"))
    (comp (ref "C11")
      (value "1uF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "b26b00f8-47d3-4d14-a4dc-caf61af2b366"))
    (comp (ref "C31")
      (value "10nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, a trick to reduce ADC noise further. Not massively useful but 0.1 cents addition")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, a trick to reduce ADC noise further. Not massively useful but 0.1 cents addition"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "869a6ff0-2778-49c4-a7d2-469b592af6f1"))
    (comp (ref "C33")
      (value "22nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor, small symbol")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (libsource (lib "Device") (part "C_Small") (description "Unpolarized capacitor, small symbol"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "capacitor cap"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "cae2631b-631a-4ca4-a33a-12f65aa24d88"))
    (comp (ref "C35")
      (value "100nF")
      (footprint "Capacitor_SMD:C_0402_1005Metric")
      (datasheet "~")
      (description "Unpolarized capacitor")
      (fields
        (field (name "Footprint") "Capacitor_SMD:C_0402_1005Metric")
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (libsource (lib "Device") (part "C") (description "Unpolarized capacitor"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "cap capacitor"))
      (property (name "ki_fp_filters") (value "C_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "567e92ac-416d-4662-a5cf-7d3b393490bd"))
    (comp (ref "J8")
      (value "J_JOG")
      (footprint "Connector_JST:JST_PH_B4B-PH-K_1x04_P2.00mm_Vertical")
      (datasheet "~")
      (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (fields
        (field (name "Footprint") "Connector_JST:JST_PH_B4B-PH-K_1x04_P2.00mm_Vertical")
        (field (name "Datasheet") "~")
        (field (name "Description") "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (libsource (lib "Connector_Generic") (part "Conn_01x04") (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "connector"))
      (property (name "ki_fp_filters") (value "Connector*:*_1x??_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "ee5d5991-c195-4781-93e1-b72beea3218f"))
    (comp (ref "J9")
      (value "J_PLAY")
      (footprint "Connector_JST:JST_PH_B6B-PH-K_1x06_P2.00mm_Vertical")
      (datasheet "~")
      (description "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (fields
        (field (name "Footprint") "Connector_JST:JST_PH_B6B-PH-K_1x06_P2.00mm_Vertical")
        (field (name "Datasheet") "~")
        (field (name "Description") "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (libsource (lib "Connector_Generic") (part "Conn_01x06") (description "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "connector"))
      (property (name "ki_fp_filters") (value "Connector*:*_1x??_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "c0500eee-4222-49ef-bb61-01b7e4177910"))
    (comp (ref "J10")
      (value "J_LOOP")
      (footprint "Connector_JST:JST_PH_B8B-PH-K_1x08_P2.00mm_Vertical")
      (datasheet "~")
      (description "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (fields
        (field (name "Footprint") "Connector_JST:JST_PH_B8B-PH-K_1x08_P2.00mm_Vertical")
        (field (name "Datasheet") "~")
        (field (name "Description") "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (libsource (lib "Connector_Generic") (part "Conn_01x08") (description "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "connector"))
      (property (name "ki_fp_filters") (value "Connector*:*_1x??_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "48ecd0e2-6d76-4c8e-8298-bb594e085046"))
    (comp (ref "J11")
      (value "J_MASTER_TEMPO")
      (footprint "Connector_JST:JST_PH_B4B-PH-K_1x04_P2.00mm_Vertical")
      (datasheet "~")
      (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (fields
        (field (name "Footprint") "Connector_JST:JST_PH_B4B-PH-K_1x04_P2.00mm_Vertical")
        (field (name "Datasheet") "~")
        (field (name "Description") "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (libsource (lib "Connector_Generic") (part "Conn_01x04") (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "connector"))
      (property (name "ki_fp_filters") (value "Connector*:*_1x??_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "f38476ad-2935-4a5d-aeba-7cb2d3c60ebc"))
    (comp (ref "J12")
      (value "J_ENCODER_BACK")
      (footprint "Connector_JST:JST_PH_B7B-PH-K_1x07_P2.00mm_Vertical")
      (datasheet "~")
      (description "Generic connector, single row, 01x07, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (fields
        (field (name "Footprint") "Connector_JST:JST_PH_B7B-PH-K_1x07_P2.00mm_Vertical")
        (field (name "Datasheet") "~")
        (field (name "Description") "Generic connector, single row, 01x07, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (libsource (lib "Connector_Generic") (part "Conn_01x07") (description "Generic connector, single row, 01x07, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "connector"))
      (property (name "ki_fp_filters") (value "Connector*:*_1x??_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "e61e7c92-5492-4c6c-bd53-28e434de47bb"))
    (comp (ref "J13")
      (value "J_TEMPO")
      (footprint "Connector_JST:JST_PH_B5B-PH-K_1x05_P2.00mm_Vertical")
      (datasheet "~")
      (description "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (fields
        (field (name "Footprint") "Connector_JST:JST_PH_B5B-PH-K_1x05_P2.00mm_Vertical")
        (field (name "Datasheet") "~")
        (field (name "Description") "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (libsource (lib "Connector_Generic") (part "Conn_01x05") (description "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "connector"))
      (property (name "ki_fp_filters") (value "Connector*:*_1x??_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "0c06c56d-eb36-449b-8fec-e62993c49a0d"))
    (comp (ref "J17")
      (value "J_TOUCH")
      (footprint "Connector_JST:JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical")
      (datasheet "~")
      (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (fields
        (field (name "Footprint") "Connector_JST:JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical")
        (field (name "Datasheet") "~")
        (field (name "Description") "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (libsource (lib "Connector_Generic") (part "Conn_01x02") (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "connector"))
      (property (name "ki_fp_filters") (value "Connector*:*_1x??_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "d4f4db6c-3942-4f72-9022-c7da687a15a4"))
    (comp (ref "R5")
      (value "10kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "d530e05f-1d28-4927-849c-921096553a85"))
    (comp (ref "R18")
      (value "22kΩ")
      (footprint "JLC2KiCad_lib-footprints:R0402")
      (datasheet "~")
      (description "Resistor pull up")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:R0402")
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor pull up"))
      (libsource (lib "Device") (part "R") (description "Resistor"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "R res resistor"))
      (property (name "ki_fp_filters") (value "R_*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "a85aa449-029f-4c47-9326-1c2ea337825a"))
    (comp (ref "SW1")
      (value "RESET_BTN")
      (footprint "PCM_JLCPCB:SW_TS-1088-AR02016")
      (datasheet "~")
      (description "Push button switch, generic, two pins")
      (fields
        (field (name "Footprint") "PCM_JLCPCB:SW_TS-1088-AR02016")
        (field (name "Datasheet") "~")
        (field (name "Description") "Push button switch, generic, two pins"))
      (libsource (lib "Switch") (part "SW_Push") (description "Push button switch, generic, two pins"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "switch normally-open pushbutton push-button"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "c28e212b-0b2e-4b16-8343-2d0b8792eb69"))
    (comp (ref "U4")
      (value "ATmega32U4-A (Arduino MIDI controller)")
      (footprint "JLC2KiCad_lib-footprints:VQFN-44_L7.0-W7.0-P0.50-BL-EP5.2")
      (datasheet "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-7766-8-bit-AVR-ATmega16U4-32U4_Datasheet.pdf")
      (description "16MHz, 32kB Flash, 2.5kB SRAM, 1kB EEPROM, USB 2.0, TQFP-44")
      (fields
        (field (name "Footprint") "JLC2KiCad_lib-footprints:VQFN-44_L7.0-W7.0-P0.50-BL-EP5.2")
        (field (name "Datasheet") "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-7766-8-bit-AVR-ATmega16U4-32U4_Datasheet.pdf")
        (field (name "Description") "16MHz, 32kB Flash, 2.5kB SRAM, 1kB EEPROM, USB 2.0, TQFP-44"))
      (libsource (lib "MCU_Microchip_ATmega") (part "ATmega32U4-A") (description "16MHz, 32kB Flash, 2.5kB SRAM, 1kB EEPROM, USB 2.0, TQFP-44"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "AVR 8bit Microcontroller MegaAVR USB"))
      (property (name "ki_fp_filters") (value "TQFP*10x10mm*P0.8mm*"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "776493bf-cc4f-41f2-8e7a-632ad96677db"))
    (comp (ref "X1")
      (value "X322516MLB4SI")
      (footprint "PCM_JLCPCB:OSC-SMD_4P-L3.2-W2.5-BL")
      (datasheet "https://www.lcsc.com/datasheet/lcsc_datasheet_2403291504_YXC-Crystal-Oscillators-X322516MLB4SI_C13738.pdf")
      (description "16MHz Surface Mount Crystal 9pF ±10ppm ±20ppm SMD3225-4P Crystals ROHS")
      (fields
        (field (name "LCSC") "C13738")
        (field (name "Stock") "162087")
        (field (name "Price") "0.068USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "5")
        (field (name "Attrition Qty") "4")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Crystals/Oscillators/Resonators,Crystals")
        (field (name "Manufacturer") "Yangxing Tech")
        (field (name "Part") "X322516MLB4SI")
        (field (name "Frequency") "16MHz")
        (field (name "Frequency Stability") "±20ppm")
        (field (name "Operating Temperature") "-40°C~+85°C")
        (field (name "Frequency Tolerance") "±10ppm")
        (field (name "Crystal Type") "SMD Crystal Resonator")
        (field (name "Load Capacitance") "9pF")
        (field (name "Normal Temperature Frequency Tolerance") "±10ppm")
        (field (name "Type") "Surface Mount Crystal")
        (field (name "Footprint") "PCM_JLCPCB:OSC-SMD_4P-L3.2-W2.5-BL")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2403291504_YXC-Crystal-Oscillators-X322516MLB4SI_C13738.pdf")
        (field (name "Description") "16MHz Surface Mount Crystal 9pF ±10ppm ±20ppm SMD3225-4P Crystals ROHS"))
      (libsource (lib "PCM_JLCPCB-Crystals") (part "Crystal, 16MHz, 9pF") (description "16MHz Surface Mount Crystal 9pF ±10ppm ±20ppm SMD3225-4P Crystals ROHS"))
      (property (name "LCSC") (value "C13738"))
      (property (name "Stock") (value "162087"))
      (property (name "Price") (value "0.068USD"))
      (property (name "Process") (value "SMT"))
      (property (name "Minimum Qty") (value "5"))
      (property (name "Attrition Qty") (value "4"))
      (property (name "Class") (value "Basic Component"))
      (property (name "Category") (value "Crystals/Oscillators/Resonators,Crystals"))
      (property (name "Manufacturer") (value "Yangxing Tech"))
      (property (name "Part") (value "X322516MLB4SI"))
      (property (name "Frequency") (value "16MHz"))
      (property (name "Frequency Stability") (value "±20ppm"))
      (property (name "Operating Temperature") (value "-40°C~+85°C"))
      (property (name "Frequency Tolerance") (value "±10ppm"))
      (property (name "Crystal Type") (value "SMD Crystal Resonator"))
      (property (name "Load Capacitance") (value "9pF"))
      (property (name "Normal Temperature Frequency Tolerance") (value "±10ppm"))
      (property (name "Type") (value "Surface Mount Crystal"))
      (property (name "Sheetname") (value "Arduino MIDI"))
      (property (name "Sheetfile") (value "arduino_midi.kicad_sch"))
      (property (name "ki_keywords") (value "C13738"))
      (sheetpath (names "/Arduino MIDI/") (tstamps "/73c6762a-885b-46bb-a26f-196c571f1a90/"))
      (tstamps "802b01d0-2016-4734-838a-ab91987a3f82")))
  (libparts
    (libpart (lib "AP2553W6-7") (part "AP2553W6-7")
      (docs "https://item.szlcsc.com/211080.html")
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "AP2553W6-7")
        (field (name "Footprint") "footprint:SOT-26_L3.0-W1.6-P0.95-LS2.8-BL")
        (field (name "Datasheet") "https://item.szlcsc.com/211080.html")
        (field (name "Description"))
        (field (name "LCSC") "C212302"))
      (pins
        (pin (num "1") (name "IN") (type "unspecified"))
        (pin (num "2") (name "GND") (type "unspecified"))
        (pin (num "3") (name "EN") (type "unspecified"))
        (pin (num "4") (name "FAULT") (type "unspecified"))
        (pin (num "5") (name "ILIM") (type "unspecified"))
        (pin (num "6") (name "OUT") (type "unspecified"))))
    (libpart (lib "Audio") (part "PCM5122PW")
      (description "2VRMS DirectPath, 112dB Audio Stereo DAC with 32-bit, 384kHz PCM Interface, TSSOP-28")
      (docs "http://www.ti.com/lit/ds/symlink/pcm5122.pdf")
      (footprints
        (fp "TSSOP*4.4x9.7mm*P0.65mm*"))
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "PCM5122PW")
        (field (name "Footprint") "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm")
        (field (name "Datasheet") "http://www.ti.com/lit/ds/symlink/pcm5122.pdf")
        (field (name "Description") "2VRMS DirectPath, 112dB Audio Stereo DAC with 32-bit, 384kHz PCM Interface, TSSOP-28"))
      (pins
        (pin (num "1") (name "CPVDD") (type "power_in"))
        (pin (num "2") (name "CAPP") (type "passive"))
        (pin (num "3") (name "CPGND") (type "power_in"))
        (pin (num "4") (name "CAPM") (type "passive"))
        (pin (num "5") (name "VNEG") (type "passive"))
        (pin (num "6") (name "OUTL") (type "output"))
        (pin (num "7") (name "OUTR") (type "output"))
        (pin (num "8") (name "AVDD") (type "power_in"))
        (pin (num "9") (name "AGND") (type "power_in"))
        (pin (num "10") (name "VCOM/DEMP") (type "bidirectional"))
        (pin (num "11") (name "SDA/MOSI/ATT2") (type "bidirectional"))
        (pin (num "12") (name "SCL/MC/ATT1") (type "input"))
        (pin (num "13") (name "GPIO5/ATT0") (type "bidirectional"))
        (pin (num "14") (name "GPIO4/MAST") (type "bidirectional"))
        (pin (num "15") (name "GPIO3/AGNS") (type "bidirectional"))
        (pin (num "16") (name "ADR2/GPIO2/DOUT") (type "bidirectional"))
        (pin (num "17") (name "MODE1") (type "input"))
        (pin (num "18") (name "MODE2/MS") (type "input"))
        (pin (num "19") (name "GPIO6/FLT") (type "bidirectional"))
        (pin (num "20") (name "SCK") (type "input"))
        (pin (num "21") (name "BCK") (type "bidirectional"))
        (pin (num "22") (name "DIN") (type "input"))
        (pin (num "23") (name "LRCK") (type "bidirectional"))
        (pin (num "24") (name "ADR1/MISO/FMT") (type "bidirectional"))
        (pin (num "25") (name "XSMT") (type "input"))
        (pin (num "26") (name "LDOO") (type "passive"))
        (pin (num "27") (name "DGND") (type "power_in"))
        (pin (num "28") (name "DVDD") (type "power_in"))))
    (libpart (lib "CR2032-BS-6-1") (part "CR2032-BS-6-1")
      (docs "https://item.szlcsc.com/71472.html")
      (fields
        (field (name "Reference") "B")
        (field (name "Value") "CR2032-BS-6-1")
        (field (name "Footprint") "footprint:BAT-TH_CR2032-BS-6-1")
        (field (name "Datasheet") "https://item.szlcsc.com/71472.html")
        (field (name "Description"))
        (field (name "LCSC") "C70377"))
      (pins
        (pin (num "1") (name "1") (type "input"))
        (pin (num "2") (name "2") (type "input"))))
    (libpart (lib "Connector") (part "HDMI_D_1.4")
      (description "HDMI 1.4+ type D connector")
      (docs "http://pinoutguide.com/PortableDevices/micro_hdmi_type_d_pinout.shtml")
      (footprints
        (fp "HDMI*D*"))
      (fields
        (field (name "Reference") "J")
        (field (name "Value") "HDMI_D_1.4")
        (field (name "Footprint"))
        (field (name "Datasheet") "http://pinoutguide.com/PortableDevices/micro_hdmi_type_d_pinout.shtml")
        (field (name "Description") "HDMI 1.4+ type D connector"))
      (pins
        (pin (num "1") (name "HPD/HEAC-") (type "passive"))
        (pin (num "2") (name "UTILITY/HEAC+") (type "passive"))
        (pin (num "3") (name "D2+") (type "passive"))
        (pin (num "4") (name "D2S") (type "power_in"))
        (pin (num "5") (name "D2-") (type "passive"))
        (pin (num "6") (name "D1+") (type "passive"))
        (pin (num "7") (name "D1S") (type "power_in"))
        (pin (num "8") (name "D1-") (type "passive"))
        (pin (num "9") (name "D0+") (type "passive"))
        (pin (num "10") (name "D0S") (type "power_in"))
        (pin (num "11") (name "D0-") (type "passive"))
        (pin (num "12") (name "CK+") (type "passive"))
        (pin (num "13") (name "CKS") (type "power_in"))
        (pin (num "14") (name "CK-") (type "passive"))
        (pin (num "15") (name "CEC") (type "bidirectional"))
        (pin (num "16") (name "GND") (type "power_in"))
        (pin (num "17") (name "SCL") (type "passive"))
        (pin (num "18") (name "SDA") (type "bidirectional"))
        (pin (num "19") (name "+5V") (type "power_in"))
        (pin (num "SH") (name "SH") (type "passive"))))
    (libpart (lib "Connector") (part "TestPoint")
      (description "test point")
      (docs "~")
      (footprints
        (fp "Pin*")
        (fp "Test*"))
      (fields
        (field (name "Reference") "TP")
        (field (name "Value") "TestPoint")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "test point"))
      (pins
        (pin (num "1") (name "1") (type "passive"))))
    (libpart (lib "Connector") (part "USB3_A")
      (description "USB 3.0 A connector")
      (docs "~")
      (footprints
        (fp "USB3*"))
      (fields
        (field (name "Reference") "J")
        (field (name "Value") "USB3_A")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "USB 3.0 A connector"))
      (pins
        (pin (num "1") (name "VBUS") (type "power_in"))
        (pin (num "2") (name "D-") (type "bidirectional"))
        (pin (num "3") (name "D+") (type "bidirectional"))
        (pin (num "4") (name "GND") (type "power_in"))
        (pin (num "5") (name "SSRX-") (type "output"))
        (pin (num "6") (name "SSRX+") (type "output"))
        (pin (num "7") (name "DRAIN") (type "passive"))
        (pin (num "8") (name "SSTX-") (type "input"))
        (pin (num "9") (name "SSTX+") (type "input"))
        (pin (num "10") (name "SHIELD") (type "passive"))))
    (libpart (lib "Connector") (part "USB_A")
      (description "USB Type A connector")
      (docs "~")
      (footprints
        (fp "USB*"))
      (fields
        (field (name "Reference") "J")
        (field (name "Value") "USB_A")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "USB Type A connector"))
      (pins
        (pin (num "1") (name "VBUS") (type "power_in"))
        (pin (num "2") (name "D-") (type "bidirectional"))
        (pin (num "3") (name "D+") (type "bidirectional"))
        (pin (num "4") (name "GND") (type "power_in"))
        (pin (num "5") (name "Shield") (type "passive"))))
    (libpart (lib "Connector") (part "USB_C_Receptacle_USB2.0_16P")
      (description "USB 2.0-only 16P Type-C Receptacle connector")
      (docs "https://www.usb.org/sites/default/files/documents/usb_type-c.zip")
      (footprints
        (fp "USB*C*Receptacle*"))
      (fields
        (field (name "Reference") "J")
        (field (name "Value") "USB_C_Receptacle_USB2.0_16P")
        (field (name "Footprint"))
        (field (name "Datasheet") "https://www.usb.org/sites/default/files/documents/usb_type-c.zip")
        (field (name "Description") "USB 2.0-only 16P Type-C Receptacle connector"))
      (pins
        (pin (num "A1") (name "GND") (type "passive"))
        (pin (num "A4") (name "VBUS") (type "passive"))
        (pin (num "A5") (name "CC1") (type "bidirectional"))
        (pin (num "A6") (name "D+") (type "bidirectional"))
        (pin (num "A7") (name "D-") (type "bidirectional"))
        (pin (num "A8") (name "SBU1") (type "bidirectional"))
        (pin (num "A9") (name "VBUS") (type "passive"))
        (pin (num "A12") (name "GND") (type "passive"))
        (pin (num "B1") (name "GND") (type "passive"))
        (pin (num "B4") (name "VBUS") (type "passive"))
        (pin (num "B5") (name "CC2") (type "bidirectional"))
        (pin (num "B6") (name "D+") (type "bidirectional"))
        (pin (num "B7") (name "D-") (type "bidirectional"))
        (pin (num "B8") (name "SBU2") (type "bidirectional"))
        (pin (num "B9") (name "VBUS") (type "passive"))
        (pin (num "B12") (name "GND") (type "passive"))
        (pin (num "S1") (name "SHIELD") (type "passive"))))
    (libpart (lib "Connector_Generic") (part "Conn_01x02")
      (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs "~")
      (footprints
        (fp "Connector*:*_1x??_*"))
      (fields
        (field (name "Reference") "J")
        (field (name "Value") "Conn_01x02")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (pins
        (pin (num "1") (name "Pin_1") (type "passive"))
        (pin (num "2") (name "Pin_2") (type "passive"))))
    (libpart (lib "Connector_Generic") (part "Conn_01x04")
      (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs "~")
      (footprints
        (fp "Connector*:*_1x??_*"))
      (fields
        (field (name "Reference") "J")
        (field (name "Value") "Conn_01x04")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (pins
        (pin (num "1") (name "Pin_1") (type "passive"))
        (pin (num "2") (name "Pin_2") (type "passive"))
        (pin (num "3") (name "Pin_3") (type "passive"))
        (pin (num "4") (name "Pin_4") (type "passive"))))
    (libpart (lib "Connector_Generic") (part "Conn_01x05")
      (description "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs "~")
      (footprints
        (fp "Connector*:*_1x??_*"))
      (fields
        (field (name "Reference") "J")
        (field (name "Value") "Conn_01x05")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (pins
        (pin (num "1") (name "Pin_1") (type "passive"))
        (pin (num "2") (name "Pin_2") (type "passive"))
        (pin (num "3") (name "Pin_3") (type "passive"))
        (pin (num "4") (name "Pin_4") (type "passive"))
        (pin (num "5") (name "Pin_5") (type "passive"))))
    (libpart (lib "Connector_Generic") (part "Conn_01x06")
      (description "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs "~")
      (footprints
        (fp "Connector*:*_1x??_*"))
      (fields
        (field (name "Reference") "J")
        (field (name "Value") "Conn_01x06")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (pins
        (pin (num "1") (name "Pin_1") (type "passive"))
        (pin (num "2") (name "Pin_2") (type "passive"))
        (pin (num "3") (name "Pin_3") (type "passive"))
        (pin (num "4") (name "Pin_4") (type "passive"))
        (pin (num "5") (name "Pin_5") (type "passive"))
        (pin (num "6") (name "Pin_6") (type "passive"))))
    (libpart (lib "Connector_Generic") (part "Conn_01x07")
      (description "Generic connector, single row, 01x07, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs "~")
      (footprints
        (fp "Connector*:*_1x??_*"))
      (fields
        (field (name "Reference") "J")
        (field (name "Value") "Conn_01x07")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Generic connector, single row, 01x07, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (pins
        (pin (num "1") (name "Pin_1") (type "passive"))
        (pin (num "2") (name "Pin_2") (type "passive"))
        (pin (num "3") (name "Pin_3") (type "passive"))
        (pin (num "4") (name "Pin_4") (type "passive"))
        (pin (num "5") (name "Pin_5") (type "passive"))
        (pin (num "6") (name "Pin_6") (type "passive"))
        (pin (num "7") (name "Pin_7") (type "passive"))))
    (libpart (lib "Connector_Generic") (part "Conn_01x08")
      (description "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs "~")
      (footprints
        (fp "Connector*:*_1x??_*"))
      (fields
        (field (name "Reference") "J")
        (field (name "Value") "Conn_01x08")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (pins
        (pin (num "1") (name "Pin_1") (type "passive"))
        (pin (num "2") (name "Pin_2") (type "passive"))
        (pin (num "3") (name "Pin_3") (type "passive"))
        (pin (num "4") (name "Pin_4") (type "passive"))
        (pin (num "5") (name "Pin_5") (type "passive"))
        (pin (num "6") (name "Pin_6") (type "passive"))
        (pin (num "7") (name "Pin_7") (type "passive"))
        (pin (num "8") (name "Pin_8") (type "passive"))))
    (libpart (lib "DSWB04LHGET") (part "DSWB04LHGET")
      (docs "https://item.szlcsc.com/100632.html")
      (fields
        (field (name "Reference") "U12")
        (field (name "Value") "DSWB04LHGET")
        (field (name "Footprint") "footprint:SW-TH_DSWB04LHGET")
        (field (name "Datasheet") "https://item.szlcsc.com/100632.html")
        (field (name "Description"))
        (field (name "LCSC") "C99418"))
      (pins
        (pin (num "1") (name "1") (type "passive"))
        (pin (num "2") (name "2") (type "passive"))
        (pin (num "3") (name "3") (type "passive"))
        (pin (num "4") (name "4") (type "passive"))
        (pin (num "5") (name "5") (type "passive"))
        (pin (num "6") (name "6") (type "passive"))
        (pin (num "7") (name "7") (type "passive"))
        (pin (num "8") (name "8") (type "passive"))))
    (libpart (lib "Device") (part "C")
      (description "Unpolarized capacitor")
      (docs "~")
      (footprints
        (fp "C_*"))
      (fields
        (field (name "Reference") "C")
        (field (name "Value") "C")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "Device") (part "C_Small")
      (description "Unpolarized capacitor, small symbol")
      (docs "~")
      (footprints
        (fp "C_*"))
      (fields
        (field (name "Reference") "C")
        (field (name "Value") "C_Small")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Unpolarized capacitor, small symbol"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "Device") (part "R")
      (description "Resistor")
      (docs "~")
      (footprints
        (fp "R_*"))
      (fields
        (field (name "Reference") "R")
        (field (name "Value") "R")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Resistor"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "HR911130A") (part "HR911130A")
      (docs "https://item.szlcsc.com/55426.html")
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "HR911130A")
        (field (name "Footprint") "footprint:RJ45-TH_HR911130A")
        (field (name "Datasheet") "https://item.szlcsc.com/55426.html")
        (field (name "Description"))
        (field (name "LCSC") "C54408"))
      (pins
        (pin (num "11") (name "11") (type "unspecified"))
        (pin (num "12") (name "12") (type "unspecified"))
        (pin (num "13") (name "13") (type "unspecified"))
        (pin (num "14") (name "14") (type "unspecified"))
        (pin (num "MDI0+") (name "MDI0+") (type "unspecified"))
        (pin (num "MDI0-") (name "MDI0-") (type "unspecified"))
        (pin (num "MDI1+") (name "MDI1+") (type "unspecified"))
        (pin (num "MDI1-") (name "MDI1-") (type "unspecified"))
        (pin (num "MDI2+") (name "MDI2+") (type "unspecified"))
        (pin (num "MDI2-") (name "MDI2-") (type "unspecified"))
        (pin (num "MDI3+") (name "MDI3+") (type "unspecified"))
        (pin (num "MDI3-") (name "MDI3-") (type "unspecified"))
        (pin (num "P1") (name "P1") (type "unspecified"))
        (pin (num "P10") (name "P10") (type "unspecified"))
        (pin (num "SHIELD0") (name "SHIELD0") (type "unspecified"))
        (pin (num "SHIELD1") (name "SHIELD1") (type "unspecified"))))
    (libpart (lib "Interface_USB") (part "CH224K")
      (description "100W USB Type-C PD3.0/2.0, BC1.2 Sink Controller, SSOP-10")
      (docs "https://www.wch.cn/downloads/file/301.html")
      (footprints
        (fp "SSOP*3.9x4.9mm*P1mm*EP2.1x3.3mm*"))
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "CH224K")
        (field (name "Footprint") "Package_SO:SSOP-10-1EP_3.9x4.9mm_P1mm_EP2.1x3.3mm")
        (field (name "Datasheet") "https://www.wch.cn/downloads/file/301.html")
        (field (name "Description") "100W USB Type-C PD3.0/2.0, BC1.2 Sink Controller, SSOP-10"))
      (pins
        (pin (num "1") (name "VDD") (type "power_in"))
        (pin (num "2") (name "CFG2") (type "passive"))
        (pin (num "3") (name "CFG3") (type "passive"))
        (pin (num "4") (name "DP") (type "bidirectional"))
        (pin (num "5") (name "DM") (type "bidirectional"))
        (pin (num "6") (name "CC2") (type "bidirectional"))
        (pin (num "7") (name "CC1") (type "bidirectional"))
        (pin (num "8") (name "VBUS") (type "passive"))
        (pin (num "9") (name "CFG1") (type "passive"))
        (pin (num "10") (name "PG") (type "open_collector"))
        (pin (num "11") (name "GND") (type "power_in"))))
    (libpart (lib "KT-0603R") (part "KT-0603R")
      (docs "https://item.szlcsc.com/347874.html")
      (fields
        (field (name "Reference") "LED")
        (field (name "Value") "KT-0603R")
        (field (name "Footprint") "footprint:LED0603-RD")
        (field (name "Datasheet") "https://item.szlcsc.com/347874.html")
        (field (name "Description"))
        (field (name "LCSC") "C2286"))
      (pins
        (pin (num "1") (name "K") (type "unspecified"))
        (pin (num "2") (name "A") (type "unspecified"))))
    (libpart (lib "MCU_Microchip_ATmega") (part "ATmega32U4-A")
      (description "16MHz, 32kB Flash, 2.5kB SRAM, 1kB EEPROM, USB 2.0, TQFP-44")
      (docs "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-7766-8-bit-AVR-ATmega16U4-32U4_Datasheet.pdf")
      (footprints
        (fp "TQFP*10x10mm*P0.8mm*"))
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "ATmega32U4-A")
        (field (name "Footprint") "Package_QFP:TQFP-44_10x10mm_P0.8mm")
        (field (name "Datasheet") "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-7766-8-bit-AVR-ATmega16U4-32U4_Datasheet.pdf")
        (field (name "Description") "16MHz, 32kB Flash, 2.5kB SRAM, 1kB EEPROM, USB 2.0, TQFP-44"))
      (pins
        (pin (num "1") (name "PE6") (type "bidirectional"))
        (pin (num "2") (name "UVCC") (type "power_in"))
        (pin (num "3") (name "D-") (type "bidirectional"))
        (pin (num "4") (name "D+") (type "bidirectional"))
        (pin (num "5") (name "UGND") (type "passive"))
        (pin (num "6") (name "UCAP") (type "passive"))
        (pin (num "7") (name "VBUS") (type "input"))
        (pin (num "8") (name "PB0") (type "bidirectional"))
        (pin (num "9") (name "PB1") (type "bidirectional"))
        (pin (num "10") (name "PB2") (type "bidirectional"))
        (pin (num "11") (name "PB3") (type "bidirectional"))
        (pin (num "12") (name "PB7") (type "bidirectional"))
        (pin (num "13") (name "~{RESET}") (type "input"))
        (pin (num "14") (name "VCC") (type "power_in"))
        (pin (num "15") (name "GND") (type "power_in"))
        (pin (num "16") (name "XTAL2") (type "output"))
        (pin (num "17") (name "XTAL1") (type "input"))
        (pin (num "18") (name "PD0") (type "bidirectional"))
        (pin (num "19") (name "PD1") (type "bidirectional"))
        (pin (num "20") (name "PD2") (type "bidirectional"))
        (pin (num "21") (name "PD3") (type "bidirectional"))
        (pin (num "22") (name "PD5") (type "bidirectional"))
        (pin (num "23") (name "GND") (type "passive"))
        (pin (num "24") (name "AVCC") (type "power_in"))
        (pin (num "25") (name "PD4") (type "bidirectional"))
        (pin (num "26") (name "PD6") (type "bidirectional"))
        (pin (num "27") (name "PD7") (type "bidirectional"))
        (pin (num "28") (name "PB4") (type "bidirectional"))
        (pin (num "29") (name "PB5") (type "bidirectional"))
        (pin (num "30") (name "PB6") (type "bidirectional"))
        (pin (num "31") (name "PC6") (type "bidirectional"))
        (pin (num "32") (name "PC7") (type "bidirectional"))
        (pin (num "33") (name "~{HWB}/PE2") (type "bidirectional"))
        (pin (num "34") (name "VCC") (type "passive"))
        (pin (num "35") (name "GND") (type "passive"))
        (pin (num "36") (name "PF7") (type "bidirectional"))
        (pin (num "37") (name "PF6") (type "bidirectional"))
        (pin (num "38") (name "PF5") (type "bidirectional"))
        (pin (num "39") (name "PF4") (type "bidirectional"))
        (pin (num "40") (name "PF1") (type "bidirectional"))
        (pin (num "41") (name "PF0") (type "bidirectional"))
        (pin (num "42") (name "AREF") (type "passive"))
        (pin (num "43") (name "GND") (type "passive"))
        (pin (num "44") (name "AVCC") (type "passive"))))
    (libpart (lib "Mechanical") (part "MountingHole")
      (description "Mounting Hole without connection")
      (docs "~")
      (footprints
        (fp "MountingHole*"))
      (fields
        (field (name "Reference") "H")
        (field (name "Value") "MountingHole")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Mounting Hole without connection")))
    (libpart (lib "PCM_JLCPCB-Capacitors") (part "0402,100nF,(2)")
      (description "50V 100nF X7R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
      (docs "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05B104KB54PNC_C307331.pdf")
      (footprints
        (fp "C_*"))
      (fields
        (field (name "Reference") "C")
        (field (name "Value") "100nF")
        (field (name "Footprint") "PCM_JLCPCB:C_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05B104KB54PNC_C307331.pdf")
        (field (name "Description") "50V 100nF X7R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
        (field (name "LCSC") "C307331")
        (field (name "Stock") "8389599")
        (field (name "Price") "0.008USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT")
        (field (name "Manufacturer") "Samsung Electro-Mechanics")
        (field (name "Part") "CL05B104KB54PNC")
        (field (name "Voltage Rated") "50V")
        (field (name "Tolerance") "±10%")
        (field (name "Capacitance") "100nF")
        (field (name "Temperature Coefficient") "X7R"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "PCM_JLCPCB-Capacitors") (part "0402,100pF")
      (description "50V 100pF C0G ±5% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
      (docs "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_FH--Guangdong-Fenghua-Advanced-Tech-0402CG101J500NT_C1546.pdf")
      (footprints
        (fp "C_*"))
      (fields
        (field (name "Reference") "C")
        (field (name "Value") "100pF")
        (field (name "Footprint") "PCM_JLCPCB:C_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_FH--Guangdong-Fenghua-Advanced-Tech-0402CG101J500NT_C1546.pdf")
        (field (name "Description") "50V 100pF C0G ±5% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
        (field (name "LCSC") "C1546")
        (field (name "Stock") "2554383")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT")
        (field (name "Manufacturer") "FH(Guangdong Fenghua Advanced Tech)")
        (field (name "Part") "0402CG101J500NT")
        (field (name "Voltage Rated") "50V")
        (field (name "Tolerance") "±5%")
        (field (name "Capacitance") "100pF")
        (field (name "Temperature Coefficient") "C0G"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "PCM_JLCPCB-Capacitors") (part "0402,1uF")
      (description "25V 1uF X5R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
      (docs "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05A105KA5NQNC_C52923.pdf")
      (footprints
        (fp "C_*"))
      (fields
        (field (name "Reference") "C")
        (field (name "Value") "1uF")
        (field (name "Footprint") "PCM_JLCPCB:C_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL05A105KA5NQNC_C52923.pdf")
        (field (name "Description") "25V 1uF X5R ±10% 0402 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
        (field (name "LCSC") "C52923")
        (field (name "Stock") "7021828")
        (field (name "Price") "0.006USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT")
        (field (name "Manufacturer") "Samsung Electro-Mechanics")
        (field (name "Part") "CL05A105KA5NQNC")
        (field (name "Voltage Rated") "25V")
        (field (name "Tolerance") "±10%")
        (field (name "Capacitance") "1uF")
        (field (name "Temperature Coefficient") "X5R"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "PCM_JLCPCB-Capacitors") (part "0805,10uF,(2)")
      (description "50V 10uF X5R ±10% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
      (docs "https://www.lcsc.com/datasheet/lcsc_datasheet_2411041759_Murata-Electronics-GRM21BR61H106KE43L_C440198.pdf")
      (footprints
        (fp "C_*"))
      (fields
        (field (name "Reference") "C")
        (field (name "Value") "10uF")
        (field (name "Footprint") "PCM_JLCPCB:C_0805")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2411041759_Murata-Electronics-GRM21BR61H106KE43L_C440198.pdf")
        (field (name "Description") "50V 10uF X5R ±10% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS")
        (field (name "LCSC") "C440198")
        (field (name "Stock") "1422246")
        (field (name "Price") "0.066USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "5")
        (field (name "Attrition Qty") "4")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT")
        (field (name "Manufacturer") "Murata Electronics")
        (field (name "Part") "GRM21BR61H106KE43L")
        (field (name "Voltage Rated") "50V")
        (field (name "Tolerance") "±10%")
        (field (name "Capacitance") "10uF")
        (field (name "Temperature Coefficient") "X5R"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "PCM_JLCPCB-Crystals") (part "Crystal, 16MHz, 9pF")
      (description "16MHz Surface Mount Crystal 9pF ±10ppm ±20ppm SMD3225-4P Crystals ROHS")
      (docs "https://www.lcsc.com/datasheet/lcsc_datasheet_2403291504_YXC-Crystal-Oscillators-X322516MLB4SI_C13738.pdf")
      (fields
        (field (name "Reference") "X")
        (field (name "Value") "X322516MLB4SI")
        (field (name "Footprint") "PCM_JLCPCB:OSC-SMD_4P-L3.2-W2.5-BL")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2403291504_YXC-Crystal-Oscillators-X322516MLB4SI_C13738.pdf")
        (field (name "Description") "16MHz Surface Mount Crystal 9pF ±10ppm ±20ppm SMD3225-4P Crystals ROHS")
        (field (name "LCSC") "C13738")
        (field (name "Stock") "162087")
        (field (name "Price") "0.068USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "5")
        (field (name "Attrition Qty") "4")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Crystals/Oscillators/Resonators,Crystals")
        (field (name "Manufacturer") "Yangxing Tech")
        (field (name "Part") "X322516MLB4SI")
        (field (name "Frequency") "16MHz")
        (field (name "Frequency Stability") "±20ppm")
        (field (name "Operating Temperature") "-40°C~+85°C")
        (field (name "Frequency Tolerance") "±10ppm")
        (field (name "Crystal Type") "SMD Crystal Resonator")
        (field (name "Load Capacitance") "9pF")
        (field (name "Normal Temperature Frequency Tolerance") "±10ppm")
        (field (name "Type") "Surface Mount Crystal"))
      (pins
        (pin (num "1") (name "OSC") (type "unspecified"))
        (pin (num "2") (name "GND") (type "unspecified"))
        (pin (num "3") (name "OSC") (type "unspecified"))
        (pin (num "4") (name "GND") (type "unspecified"))))
    (libpart (lib "PCM_JLCPCB-Diodes") (part "Zener,BZT52C3V3S")
      (description "Independent Type 200mW 3.1V~3.5V 3.3V SOD-323 Zener Diodes ROHS")
      (docs "https://wmsc.lcsc.com/wmsc/upload/file/pdf/v2/lcsc/2403280505_hongjiacheng-BZT52C3V3S_C19077437.pdf")
      (footprints
        (fp "D_*"))
      (fields
        (field (name "Reference") "D")
        (field (name "Value") "BZT52C3V3S")
        (field (name "Footprint") "PCM_JLCPCB:D_SOD-323")
        (field (name "Datasheet") "https://wmsc.lcsc.com/wmsc/upload/file/pdf/v2/lcsc/2403280505_hongjiacheng-BZT52C3V3S_C19077437.pdf")
        (field (name "Description") "Independent Type 200mW 3.1V~3.5V 3.3V SOD-323 Zener Diodes ROHS")
        (field (name "LCSC") "C19077437")
        (field (name "Stock") "229387")
        (field (name "Price") "0.018USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Preferred Component")
        (field (name "Category") "Diodes,Zener Diodes")
        (field (name "Manufacturer") "hongjiacheng")
        (field (name "Part") "BZT52C3V3S"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "PCM_JLCPCB-Inductors") (part "Ferrite,0603")
      (description "450mΩ ±25% 600Ω@100MHz 0603 Ferrite Beads ROHS")
      (docs "https://www.lcsc.com/datasheet/lcsc_datasheet_2310301640_Sunlord-GZ1608D601TF_C1002.pdf")
      (footprints
        (fp "FB_*"))
      (fields
        (field (name "Reference") "FB")
        (field (name "Value"))
        (field (name "Footprint") "PCM_JLCPCB:FB_0603")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2310301640_Sunlord-GZ1608D601TF_C1002.pdf")
        (field (name "Description") "450mΩ ±25% 600Ω@100MHz 0603 Ferrite Beads ROHS")
        (field (name "LCSC") "C1002")
        (field (name "Stock") "789150")
        (field (name "Price") "0.010USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "6")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Filters/EMI Optimization,Ferrite Beads")
        (field (name "Manufacturer") "Sunlord")
        (field (name "Part") "GZ1608D601TF")
        (field (name "DC Resistance") "450mΩ")
        (field (name "Impedance @ Frequency") "600Ω@100MHz")
        (field (name "Circuits") "1")
        (field (name "Current Rating") "200mA")
        (field (name "Tolerance") "±25%"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "PCM_JLCPCB-Resistors") (part "0402,100kΩ")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 100kΩ 0402 Chip Resistor - Surface Mount ROHS")
      (docs "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010100_UNI-ROYAL-Uniroyal-Elec-0402WGF1003TCE_C25741.pdf")
      (footprints
        (fp "R_*"))
      (fields
        (field (name "Reference") "R")
        (field (name "Value") "100kΩ")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010100_UNI-ROYAL-Uniroyal-Elec-0402WGF1003TCE_C25741.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 100kΩ 0402 Chip Resistor - Surface Mount ROHS")
        (field (name "LCSC") "C25741")
        (field (name "Stock") "6969783")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF1003TCE")
        (field (name "Resistance") "100kΩ")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "PCM_JLCPCB-Resistors") (part "0402,10Ω")
      (description "62.5mW Thick Film Resistors 50V ±1% ±200ppm/°C 10Ω 0402 Chip Resistor - Surface Mount ROHS")
      (docs "https://www.lcsc.com/datasheet/lcsc_datasheet_2411221126_UNI-ROYAL-Uniroyal-Elec-0402WGF100JTCE_C25077.pdf")
      (footprints
        (fp "R_*"))
      (fields
        (field (name "Reference") "R")
        (field (name "Value") "10Ω")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2411221126_UNI-ROYAL-Uniroyal-Elec-0402WGF100JTCE_C25077.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±1% ±200ppm/°C 10Ω 0402 Chip Resistor - Surface Mount ROHS")
        (field (name "LCSC") "C25077")
        (field (name "Stock") "4873481")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF100JTCE")
        (field (name "Resistance") "10Ω")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±200ppm/°C"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "PCM_JLCPCB-Resistors") (part "0402,510Ω")
      (description "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 510Ω 0402 Chip Resistor - Surface Mount ROHS")
      (docs "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF5100TCE_C25123.pdf")
      (footprints
        (fp "R_*"))
      (fields
        (field (name "Reference") "R")
        (field (name "Value") "510Ω")
        (field (name "Footprint") "PCM_JLCPCB:R_0402")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2205311900_UNI-ROYAL-Uniroyal-Elec-0402WGF5100TCE_C25123.pdf")
        (field (name "Description") "62.5mW Thick Film Resistors 50V ±100ppm/°C ±1% 510Ω 0402 Chip Resistor - Surface Mount ROHS")
        (field (name "LCSC") "C25123")
        (field (name "Stock") "2434473")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "12")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0402WGF5100TCE")
        (field (name "Resistance") "510Ω")
        (field (name "Power(Watts)") "62.5mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "50V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "PCM_JLCPCB-Resistors") (part "0603,18kΩ")
      (description "100mW Thick Film Resistors 75V ±100ppm/°C ±1% 18kΩ 0603 Chip Resistor - Surface Mount ROHS")
      (docs "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010045_UNI-ROYAL-Uniroyal-Elec-0603WAF1802T5E_C25810.pdf")
      (footprints
        (fp "R_*"))
      (fields
        (field (name "Reference") "R")
        (field (name "Value") "18kΩ")
        (field (name "Footprint") "PCM_JLCPCB:R_0603")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010045_UNI-ROYAL-Uniroyal-Elec-0603WAF1802T5E_C25810.pdf")
        (field (name "Description") "100mW Thick Film Resistors 75V ±100ppm/°C ±1% 18kΩ 0603 Chip Resistor - Surface Mount ROHS")
        (field (name "LCSC") "C25810")
        (field (name "Stock") "574660")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0603WAF1802T5E")
        (field (name "Resistance") "18kΩ")
        (field (name "Power(Watts)") "100mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "75V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "PCM_JLCPCB-Resistors") (part "0603,200kΩ")
      (description "100mW Thick Film Resistors 75V ±100ppm/°C ±1% 200kΩ 0603 Chip Resistor - Surface Mount ROHS")
      (docs "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010045_UNI-ROYAL-Uniroyal-Elec-0603WAF2003T5E_C25811.pdf")
      (footprints
        (fp "R_*"))
      (fields
        (field (name "Reference") "R")
        (field (name "Value") "200kΩ")
        (field (name "Footprint") "PCM_JLCPCB:R_0603")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010045_UNI-ROYAL-Uniroyal-Elec-0603WAF2003T5E_C25811.pdf")
        (field (name "Description") "100mW Thick Film Resistors 75V ±100ppm/°C ±1% 200kΩ 0603 Chip Resistor - Surface Mount ROHS")
        (field (name "LCSC") "C25811")
        (field (name "Stock") "1426208")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0603WAF2003T5E")
        (field (name "Resistance") "200kΩ")
        (field (name "Power(Watts)") "100mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "75V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "PCM_JLCPCB-Resistors") (part "0603,27kΩ")
      (description "100mW Thick Film Resistors 75V ±100ppm/°C ±1% 27kΩ 0603 Chip Resistor - Surface Mount ROHS")
      (docs "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010130_UNI-ROYAL-Uniroyal-Elec-0603WAF2702T5E_C22967.pdf")
      (footprints
        (fp "R_*"))
      (fields
        (field (name "Reference") "R")
        (field (name "Value") "27kΩ")
        (field (name "Footprint") "PCM_JLCPCB:R_0603")
        (field (name "Datasheet") "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010130_UNI-ROYAL-Uniroyal-Elec-0603WAF2702T5E_C22967.pdf")
        (field (name "Description") "100mW Thick Film Resistors 75V ±100ppm/°C ±1% 27kΩ 0603 Chip Resistor - Surface Mount ROHS")
        (field (name "LCSC") "C22967")
        (field (name "Stock") "708507")
        (field (name "Price") "0.004USD")
        (field (name "Process") "SMT")
        (field (name "Minimum Qty") "20")
        (field (name "Attrition Qty") "10")
        (field (name "Class") "Basic Component")
        (field (name "Category") "Resistors,Chip Resistor - Surface Mount")
        (field (name "Manufacturer") "UNI-ROYAL(Uniroyal Elec)")
        (field (name "Part") "0603WAF2702T5E")
        (field (name "Resistance") "27kΩ")
        (field (name "Power(Watts)") "100mW")
        (field (name "Type") "Thick Film Resistors")
        (field (name "Overload Voltage (Max)") "75V")
        (field (name "Operating Temperature Range") "-55°C~+155°C")
        (field (name "Tolerance") "±1%")
        (field (name "Temperature Coefficient") "±100ppm/°C"))
      (pins
        (pin (num "1") (name "") (type "passive"))
        (pin (num "2") (name "") (type "passive"))))
    (libpart (lib "PJ-320D jack 3.5mm") (part "PJ-320D")
      (docs "https://atta.szlcsc.com/upload/public/pdf/source/20190925/C431535_8B274506621F6117FB020BF07A197848.pdf")
      (fields
        (field (name "Reference") "U10")
        (field (name "Value") "PJ-320D 3.5mm jack")
        (field (name "Footprint") "footprint:AUDIO-SMD_PJ-320D-1")
        (field (name "Datasheet") "https://atta.szlcsc.com/upload/public/pdf/source/20190925/C431535_8B274506621F6117FB020BF07A197848.pdf")
        (field (name "Description"))
        (field (name "LCSC") "C431535"))
      (pins
        (pin (num "1") (name "GND/SHLD") (type "passive"))
        (pin (num "2") (name "LEFT_P") (type "passive"))
        (pin (num "3") (name "RIGHT_P") (type "passive"))
        (pin (num "4") (name "DETECT_GND") (type "passive"))))
    (libpart (lib "PJ-611E jack 6.35mm") (part "PJ-611E")
      (docs "https://item.szlcsc.com/datasheet/PJ-611E/292943.html?spm=sc.it.xds.a&lcsc_vid=EVMNBFVWTlcKUQUCQ1FdVFJSRgcNXgJXE1BbX1ACQlgxVlNQQ1NcUF1RR1VcXjsOAxUeFF5JWA0NAgAHWQIASA%3D%3D")
      (fields
        (field (name "Reference") "J18")
        (field (name "Value") "PJ-611E 6.35mm jack")
        (field (name "Footprint") "footprint:AUDIO-TH_PJ-611E_1")
        (field (name "Datasheet") "https://item.szlcsc.com/datasheet/PJ-611E/292943.html?spm=sc.it.xds.a&lcsc_vid=EVMNBFVWTlcKUQUCQ1FdVFJSRgcNXgJXE1BbX1ACQlgxVlNQQ1NcUF1RR1VcXjsOAxUeFF5JWA0NAgAHWQIASA%3D%3D")
        (field (name "Description"))
        (field (name "LCSC") "C309282"))
      (pins
        (pin (num "2") (name "GND/SHLD") (type "passive"))
        (pin (num "3") (name "DETECT_GND") (type "passive"))
        (pin (num "4") (name "RIGHT_P") (type "passive"))
        (pin (num "5") (name "DETECT_R") (type "passive"))
        (pin (num "6") (name "LEFT_P") (type "passive"))
        (pin (num "7") (name "DETECT_LEFT") (type "passive"))))
    (libpart (lib "PS-22E05-S-O-001") (part "PS-22E05-S-O-001")
      (docs "https://atta.szlcsc.com/upload/public/pdf/source/20210825/03FED21E2D4F2980BA08F4ED04C13B40.pdf")
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "PS-22E05-S-O-001")
        (field (name "Footprint") "footprint:SW-TH_PS-22E05")
        (field (name "Datasheet") "https://atta.szlcsc.com/upload/public/pdf/source/20210825/03FED21E2D4F2980BA08F4ED04C13B40.pdf")
        (field (name "Description"))
        (field (name "LCSC") "C19190928"))
      (pins
        (pin (num "1") (name "1") (type "unspecified"))
        (pin (num "2") (name "2") (type "unspecified"))
        (pin (num "3") (name "3") (type "unspecified"))
        (pin (num "4") (name "4") (type "unspecified"))
        (pin (num "5") (name "5") (type "unspecified"))
        (pin (num "6") (name "6") (type "unspecified"))
        (pin (num "7") (name "7") (type "unspecified"))
        (pin (num "8") (name "8") (type "unspecified"))))
    (libpart (lib "PSC-1608U52GC-G4") (part "PSC-1608U52GC-G4")
      (docs "https://atta.szlcsc.com/upload/public/pdf/source/20190115/C264450_D840E7E570138F41CCE67133F241C738.pdf")
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "PSC-1608U52GC-G4")
        (field (name "Footprint") "footprint:LED0603-RD_GREEN")
        (field (name "Datasheet") "https://atta.szlcsc.com/upload/public/pdf/source/20190115/C264450_D840E7E570138F41CCE67133F241C738.pdf")
        (field (name "Description"))
        (field (name "LCSC") "C22371297"))
      (pins
        (pin (num "1") (name "K") (type "unspecified"))
        (pin (num "2") (name "A") (type "unspecified"))))
    (libpart (lib "Power_Protection") (part "USBLC6-2SC6")
      (description "Very low capacitance ESD protection diode, 2 data-line, SOT-23-6")
      (docs "https://www.st.com/resource/en/datasheet/usblc6-2.pdf")
      (footprints
        (fp "SOT?23*"))
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "USBLC6-2SC6")
        (field (name "Footprint") "Package_TO_SOT_SMD:SOT-23-6")
        (field (name "Datasheet") "https://www.st.com/resource/en/datasheet/usblc6-2.pdf")
        (field (name "Description") "Very low capacitance ESD protection diode, 2 data-line, SOT-23-6"))
      (pins
        (pin (num "1") (name "I/O1") (type "passive"))
        (pin (num "2") (name "GND") (type "passive"))
        (pin (num "3") (name "I/O2") (type "passive"))
        (pin (num "4") (name "I/O2") (type "passive"))
        (pin (num "5") (name "VBUS") (type "passive"))
        (pin (num "6") (name "I/O1") (type "passive"))))
    (libpart (lib "Regulator_Linear") (part "AP2112K-3.3")
      (description "600mA low dropout linear regulator, with enable pin, 3.8V-6V input voltage range, 3.3V fixed positive output, SOT-23-5")
      (docs "https://www.diodes.com/assets/Datasheets/AP2112.pdf")
      (footprints
        (fp "SOT?23?5*"))
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "AP2112K-3.3")
        (field (name "Footprint") "Package_TO_SOT_SMD:SOT-23-5")
        (field (name "Datasheet") "https://www.diodes.com/assets/Datasheets/AP2112.pdf")
        (field (name "Description") "600mA low dropout linear regulator, with enable pin, 3.8V-6V input voltage range, 3.3V fixed positive output, SOT-23-5"))
      (pins
        (pin (num "1") (name "VIN") (type "power_in"))
        (pin (num "2") (name "GND") (type "power_in"))
        (pin (num "3") (name "EN") (type "input"))
        (pin (num "4") (name "NC") (type "no_connect"))
        (pin (num "5") (name "VOUT") (type "power_out"))))
    (libpart (lib "SL1040-2R2M") (part "SL1040-2R2M")
      (docs "https://atta.szlcsc.com/upload/public/pdf/source/20240611/8DE7D6BE1273F2E871C82A6D5C20B08D.pdf")
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "SL1040-2R2M")
        (field (name "Footprint") "footprint:IND-SMD_SL1040-R47M")
        (field (name "Datasheet") "https://atta.szlcsc.com/upload/public/pdf/source/20240611/8DE7D6BE1273F2E871C82A6D5C20B08D.pdf")
        (field (name "Description"))
        (field (name "LCSC") "C22463836"))
      (pins
        (pin (num "1") (name "1") (type "unspecified"))
        (pin (num "2") (name "2") (type "unspecified"))))
    (libpart (lib "SY8368AQQC") (part "SY8368AQQC")
      (docs "https://atta.szlcsc.com/upload/public/pdf/source/20180224/C178253_15194367790221363788.pdf")
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "SY8368AQQC")
        (field (name "Footprint") "footprint:QFN-12_L3.0-W3.0-P0.45-TL-EP")
        (field (name "Datasheet") "https://atta.szlcsc.com/upload/public/pdf/source/20180224/C178253_15194367790221363788.pdf")
        (field (name "Description"))
        (field (name "LCSC") "C207642"))
      (pins
        (pin (num "1") (name "GND") (type "unspecified"))
        (pin (num "2") (name "LX") (type "unspecified"))
        (pin (num "3") (name "GND") (type "unspecified"))
        (pin (num "4") (name "IN") (type "unspecified"))
        (pin (num "5") (name "IN") (type "unspecified"))
        (pin (num "6") (name "IN") (type "unspecified"))
        (pin (num "7") (name "BS") (type "unspecified"))
        (pin (num "8") (name "VCC") (type "unspecified"))
        (pin (num "9") (name "FB") (type "unspecified"))
        (pin (num "10") (name "ILMT") (type "unspecified"))
        (pin (num "11") (name "PG") (type "unspecified"))
        (pin (num "12") (name "EN") (type "unspecified"))))
    (libpart (lib "Switch") (part "SW_Push")
      (description "Push button switch, generic, two pins")
      (docs "~")
      (fields
        (field (name "Reference") "SW")
        (field (name "Value") "SW_Push")
        (field (name "Footprint"))
        (field (name "Datasheet") "~")
        (field (name "Description") "Push button switch, generic, two pins"))
      (pins
        (pin (num "1") (name "1") (type "passive"))
        (pin (num "2") (name "2") (type "passive"))))
    (libpart (lib "XL-1608UBC-04") (part "XL-1608UBC-04")
      (docs "https://atta.szlcsc.com/upload/public/pdf/source/20210617/C2837377_50FC585D376FE0CDA016E524346528FF.pdf")
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "XL-1608UBC-04")
        (field (name "Footprint") "footprint:LED0603-RD_BLUE")
        (field (name "Datasheet") "https://atta.szlcsc.com/upload/public/pdf/source/20210617/C2837377_50FC585D376FE0CDA016E524346528FF.pdf")
        (field (name "Description"))
        (field (name "LCSC") "C965807"))
      (pins
        (pin (num "1") (name "K") (type "unspecified"))
        (pin (num "2") (name "A") (type "unspecified"))))
    (libpart (lib "rca-jack-red") (part "RCJ-012-SMT")
      (fields
        (field (name "Reference") "J7")
        (field (name "Value") "J_RCA_R (red)")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:CONN-TH_AV-5")
        (field (name "Datasheet"))
        (field (name "Description"))
        (field (name "MF") "Same Sky")
        (field (name "Description_1") "Metal Right-Angle, SMT RCA Jack, Red Insulator")
        (field (name "Package") "None")
        (field (name "Price") "None")
        (field (name "Check_prices") "https://www.snapeda.com/parts/RCJ-012-SMT-TR/Same+Sky/view-part/?ref=eda")
        (field (name "PART_REV") "B")
        (field (name "STANDARD") "Manufacturer recommendations")
        (field (name "SnapEDA_Link") "https://www.snapeda.com/parts/RCJ-012-SMT-TR/Same+Sky/view-part/?ref=snap")
        (field (name "MP") "RCJ-012-SMT-TR")
        (field (name "Purchase-URL") "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=1316485&manufacturer=Same Sky&part_name=RCJ-012-SMT-TR&search_term=rca jack pcb mount")
        (field (name "Availability") "In Stock")
        (field (name "MANUFACTURER") "CUI Inc"))
      (pins
        (pin (num "1A") (name "SHLD") (type "passive"))
        (pin (num "1B") (name "SHLD") (type "passive"))
        (pin (num "1C") (name "SHLD") (type "passive"))
        (pin (num "2") (name "SIGNL") (type "passive"))))
    (libpart (lib "rca-jack-white") (part "RCJ-013-SMT")
      (fields
        (field (name "Reference") "J6")
        (field (name "Value") "J_RCA_L (white)")
        (field (name "Footprint") "JLC2KiCad_lib-footprints:CONN-TH_AV-5")
        (field (name "Datasheet"))
        (field (name "Description"))
        (field (name "MF") "Same Sky")
        (field (name "Description_1") "Metal Right-Angle, SMT RCA Jack, White Insulator")
        (field (name "Package") "None")
        (field (name "Price") "None")
        (field (name "Check_prices") "https://www.snapeda.com/parts/RCJ-013-SMT-TR/Same+Sky/view-part/?ref=eda")
        (field (name "PART_REV") "B")
        (field (name "STANDARD") "Manufacturer recommendations")
        (field (name "SnapEDA_Link") "https://www.snapeda.com/parts/RCJ-013-SMT-TR/Same+Sky/view-part/?ref=snap")
        (field (name "MP") "RCJ-013-SMT-TR")
        (field (name "Purchase-URL") "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=1316562&manufacturer=Same Sky&part_name=RCJ-013-SMT-TR&search_term=rca jack pcb mount")
        (field (name "Availability") "In Stock")
        (field (name "MANUFACTURER") "CUI Inc"))
      (pins
        (pin (num "1A") (name "SHLD") (type "passive"))
        (pin (num "1B") (name "SHLD") (type "passive"))
        (pin (num "1C") (name "SHLD") (type "passive"))
        (pin (num "2") (name "SIGNL") (type "passive"))))
    (libpart (lib "rpi-cm-5") (part "Compute_Module_5_Functional")
      (fields
        (field (name "Reference") "U")
        (field (name "Value") "Compute_Module_5_Functional")
        (field (name "Footprint") "CM5:CM5")
        (field (name "Datasheet"))
        (field (name "Description")))
      (pins
        (pin (num "1") (name "GND[51]") (type "power_in"))
        (pin (num "2") (name "GND[51]") (type "power_in"))
        (pin (num "3") (name "Ethernet_Pair3_P") (type "passive"))
        (pin (num "4") (name "Ethernet_Pair1_P") (type "passive"))
        (pin (num "5") (name "Ethernet_Pair3_N") (type "passive"))
        (pin (num "6") (name "Ethernet_Pair1_N") (type "passive"))
        (pin (num "7") (name "GND[51]") (type "power_in"))
        (pin (num "8") (name "GND[51]") (type "power_in"))
        (pin (num "9") (name "Ethernet_Pair2_N") (type "passive"))
        (pin (num "10") (name "Ethernet_Pair0_N") (type "passive"))
        (pin (num "11") (name "Ethernet_Pair2_P") (type "passive"))
        (pin (num "12") (name "Ethernet_Pair0_P") (type "passive"))
        (pin (num "13") (name "GND[51]") (type "power_in"))
        (pin (num "14") (name "GND[51]") (type "power_in"))
        (pin (num "15") (name "~{Ethernet_nLED3}") (type "output"))
        (pin (num "16") (name "Fan_tacho") (type "input"))
        (pin (num "17") (name "~{Ethernet_nLED2}") (type "output"))
        (pin (num "18") (name "Ethernet_SYNC_OUT") (type "input"))
        (pin (num "19") (name "Fan_PWM") (type "output"))
        (pin (num "20") (name "EEPROM_nWP") (type "input"))
        (pin (num "21") (name "~{Pi_nLED_Activity}") (type "open_collector"))
        (pin (num "22") (name "GND[51]") (type "power_in"))
        (pin (num "23") (name "GND[51]") (type "power_in"))
        (pin (num "24") (name "GPIO26") (type "passive"))
        (pin (num "25") (name "GPIO21") (type "passive"))
        (pin (num "26") (name "GPIO19") (type "passive"))
        (pin (num "27") (name "GPIO20") (type "passive"))
        (pin (num "28") (name "GPIO13") (type "passive"))
        (pin (num "29") (name "GPIO16") (type "passive"))
        (pin (num "30") (name "GPIO6") (type "passive"))
        (pin (num "31") (name "GPIO12") (type "passive"))
        (pin (num "32") (name "GND[51]") (type "power_in"))
        (pin (num "33") (name "GND[51]") (type "power_in"))
        (pin (num "34") (name "GPIO5") (type "passive"))
        (pin (num "35") (name "ID_SC") (type "passive"))
        (pin (num "36") (name "ID_SD") (type "passive"))
        (pin (num "37") (name "GPIO7") (type "passive"))
        (pin (num "38") (name "GPIO11") (type "passive"))
        (pin (num "39") (name "GPIO8") (type "passive"))
        (pin (num "40") (name "GPIO9") (type "passive"))
        (pin (num "41") (name "GPIO25") (type "passive"))
        (pin (num "42") (name "GND[51]") (type "power_in"))
        (pin (num "43") (name "GND[51]") (type "power_in"))
        (pin (num "44") (name "GPIO10") (type "passive"))
        (pin (num "45") (name "GPIO24") (type "passive"))
        (pin (num "46") (name "GPIO22") (type "passive"))
        (pin (num "47") (name "GPIO23") (type "passive"))
        (pin (num "48") (name "GPIO27") (type "passive"))
        (pin (num "49") (name "GPIO18") (type "passive"))
        (pin (num "50") (name "GPIO17") (type "passive"))
        (pin (num "51") (name "GPIO15") (type "passive"))
        (pin (num "52") (name "GND[51]") (type "power_in"))
        (pin (num "53") (name "GND[51]") (type "power_in"))
        (pin (num "54") (name "GPIO4") (type "passive"))
        (pin (num "55") (name "GPIO14") (type "passive"))
        (pin (num "56") (name "GPIO3") (type "passive"))
        (pin (num "57") (name "SD_CLK") (type "passive"))
        (pin (num "58") (name "GPIO2") (type "passive"))
        (pin (num "59") (name "GND[51]") (type "power_in"))
        (pin (num "60") (name "GND[51]") (type "power_in"))
        (pin (num "61") (name "SD_DAT3") (type "passive"))
        (pin (num "62") (name "SD_CMD") (type "passive"))
        (pin (num "63") (name "SD_DAT0") (type "passive"))
        (pin (num "64") (name "SD_DAT5") (type "passive"))
        (pin (num "65") (name "GND[51]") (type "power_in"))
        (pin (num "66") (name "GND[51]") (type "power_in"))
        (pin (num "67") (name "SD_DAT1") (type "passive"))
        (pin (num "68") (name "SD_DAT4") (type "passive"))
        (pin (num "69") (name "SD_DAT2") (type "passive"))
        (pin (num "70") (name "SD_DAT7") (type "passive"))
        (pin (num "71") (name "GND[51]") (type "power_in"))
        (pin (num "72") (name "SD_DAT6") (type "passive"))
        (pin (num "73") (name "SD_VDD_Override") (type "input"))
        (pin (num "74") (name "GND[51]") (type "power_in"))
        (pin (num "75") (name "SD_PWR_ON") (type "output"))
        (pin (num "76") (name "VBAT") (type "input"))
        (pin (num "77") (name "+5V") (type "power_in"))
        (pin (num "78") (name "GPIO_VREF") (type "power_in"))
        (pin (num "79") (name "+5V") (type "power_in"))
        (pin (num "80") (name "I2C_SCL0") (type "bidirectional"))
        (pin (num "81") (name "+5V") (type "power_in"))
        (pin (num "82") (name "I2C_SDA0") (type "bidirectional"))
        (pin (num "83") (name "+5V") (type "power_in"))
        (pin (num "84") (name "CM4_3.3V_Out_1") (type "power_out"))
        (pin (num "85") (name "+5V") (type "power_in"))
        (pin (num "86") (name "CM4_3.3V_Out_2") (type "power_out"))
        (pin (num "87") (name "+5V") (type "power_in"))
        (pin (num "88") (name "CM4_1.8V_Out_1") (type "power_out"))
        (pin (num "89") (name "~{WL_nDisable}") (type "input"))
        (pin (num "90") (name "CM4_1.8V_Out_2") (type "power_out"))
        (pin (num "91") (name "~{BT_nDisable}") (type "input"))
        (pin (num "92") (name "PWR_Button") (type "passive"))
        (pin (num "93") (name "~{nRPIBOOT}") (type "input"))
        (pin (num "94") (name "CC1") (type "bidirectional"))
        (pin (num "95") (name "~{PI_LED_nPWR}") (type "output"))
        (pin (num "96") (name "CC2") (type "bidirectional"))
        (pin (num "97") (name "CAM_GPIO0") (type "input"))
        (pin (num "98") (name "GND[51]") (type "power_in"))
        (pin (num "99") (name "PMIC_ENABLE") (type "input"))
        (pin (num "100") (name "CAM_GPIO1") (type "input"))
        (pin (num "101") (name "USB_OTG_ID") (type "input"))
        (pin (num "102") (name "~{PCIe_CLK_nREQ}") (type "input"))
        (pin (num "103") (name "USB_N") (type "passive"))
        (pin (num "104") (name "PCIE_DET_nWAKE") (type "passive"))
        (pin (num "105") (name "USB_P") (type "passive"))
        (pin (num "106") (name "PCIE_PWR_EN") (type "passive"))
        (pin (num "107") (name "GND[51]") (type "power_in"))
        (pin (num "108") (name "GND[51]") (type "power_in"))
        (pin (num "109") (name "~{PCIe_nRST}") (type "output"))
        (pin (num "110") (name "PCIe_CLK_P") (type "output"))
        (pin (num "111") (name "VBUS_EN") (type "input"))
        (pin (num "112") (name "PCIe_CLK_N") (type "output"))
        (pin (num "113") (name "GND[51]") (type "power_in"))
        (pin (num "114") (name "GND[51]") (type "power_in"))
        (pin (num "115") (name "MIPI0_D0_N") (type "input"))
        (pin (num "116") (name "PCIe_RX_P") (type "input"))
        (pin (num "117") (name "MIPI0_D0_P") (type "input"))
        (pin (num "118") (name "PCIe_RX_N") (type "input"))
        (pin (num "119") (name "GND[51]") (type "power_in"))
        (pin (num "120") (name "GND[51]") (type "power_in"))
        (pin (num "121") (name "MIPI0_D1_N") (type "input"))
        (pin (num "122") (name "PCIe_TX_P") (type "output"))
        (pin (num "123") (name "MIPI0_D1_P") (type "input"))
        (pin (num "124") (name "PCIe_TX_N") (type "output"))
        (pin (num "125") (name "GND[51]") (type "power_in"))
        (pin (num "126") (name "GND[51]") (type "power_in"))
        (pin (num "127") (name "MIPI0_C_N") (type "input"))
        (pin (num "128") (name "USB3-0-RX_N") (type "input"))
        (pin (num "129") (name "MIPI0_C_P") (type "input"))
        (pin (num "130") (name "USB3-0-RX_P") (type "input"))
        (pin (num "131") (name "GND[51]") (type "power_in"))
        (pin (num "132") (name "GND[51]") (type "power_in"))
        (pin (num "133") (name "MIPI0_D2_N") (type "input"))
        (pin (num "134") (name "USB3-0-DP") (type "bidirectional"))
        (pin (num "135") (name "MIPI0_D2_P") (type "input"))
        (pin (num "136") (name "USB3-0-DM") (type "bidirectional"))
        (pin (num "137") (name "GND[51]") (type "power_in"))
        (pin (num "138") (name "GND[51]") (type "power_in"))
        (pin (num "139") (name "MIPI0_D3_N") (type "input"))
        (pin (num "140") (name "USB3-0-TX_N") (type "output"))
        (pin (num "141") (name "MIPI0_D3_P") (type "input"))
        (pin (num "142") (name "USB3-0-TX_P") (type "output"))
        (pin (num "143") (name "HDMI1_HOTPLUG") (type "input"))
        (pin (num "144") (name "GND[51]") (type "power_in"))
        (pin (num "145") (name "HDMI1_SDA") (type "bidirectional"))
        (pin (num "146") (name "HDMI1_TX2_P") (type "output"))
        (pin (num "147") (name "HDMI1_SCL") (type "open_collector"))
        (pin (num "148") (name "HDMI1_TX2_N") (type "output"))
        (pin (num "149") (name "HDMI1_CEC") (type "open_collector"))
        (pin (num "150") (name "GND[51]") (type "power_in"))
        (pin (num "151") (name "HDMI0_CEC") (type "open_collector"))
        (pin (num "152") (name "HDMI1_TX1_P") (type "output"))
        (pin (num "153") (name "HDMI0_HOTPLUG") (type "input"))
        (pin (num "154") (name "HDMI1_TX1_N") (type "output"))
        (pin (num "155") (name "GND[51]") (type "power_in"))
        (pin (num "156") (name "GND[51]") (type "power_in"))
        (pin (num "157") (name "USB3-1-RX_N") (type "input"))
        (pin (num "158") (name "HDMI1_TX0_P") (type "output"))
        (pin (num "159") (name "USB3-1-RX_P") (type "input"))
        (pin (num "160") (name "HDMI1_TX0_N") (type "output"))
        (pin (num "161") (name "GND[51]") (type "power_in"))
        (pin (num "162") (name "GND[51]") (type "power_in"))
        (pin (num "163") (name "USB3-1-DP") (type "bidirectional"))
        (pin (num "164") (name "HDMI1_CLK_P") (type "output"))
        (pin (num "165") (name "USB3-1-DM") (type "bidirectional"))
        (pin (num "166") (name "HDMI1_CLK_N") (type "output"))
        (pin (num "167") (name "GND[51]") (type "power_in"))
        (pin (num "168") (name "GND[51]") (type "power_in"))
        (pin (num "169") (name "USB3-1-TX_N") (type "output"))
        (pin (num "170") (name "HDMI0_TX2_P") (type "output"))
        (pin (num "171") (name "USB3-1-TX_P") (type "output"))
        (pin (num "172") (name "HDMI0_TX2_N") (type "output"))
        (pin (num "173") (name "GND[51]") (type "power_in"))
        (pin (num "174") (name "GND[51]") (type "power_in"))
        (pin (num "175") (name "MIPI1_D0_N") (type "output"))
        (pin (num "176") (name "HDMI0_TX1_P") (type "output"))
        (pin (num "177") (name "MIPI1_D0_P") (type "output"))
        (pin (num "178") (name "HDMI0_TX1_N") (type "output"))
        (pin (num "179") (name "GND[51]") (type "power_in"))
        (pin (num "180") (name "GND[51]") (type "power_in"))
        (pin (num "181") (name "MIPI1_D1_N") (type "output"))
        (pin (num "182") (name "HDMI0_TX0_P") (type "output"))
        (pin (num "183") (name "MIPI1_D1_P") (type "output"))
        (pin (num "184") (name "HDMI0_TX0_N") (type "output"))
        (pin (num "185") (name "GND[51]") (type "power_in"))
        (pin (num "186") (name "GND[51]") (type "power_in"))
        (pin (num "187") (name "MIPI1_C_N") (type "output"))
        (pin (num "188") (name "HDMI0_CLK_P") (type "output"))
        (pin (num "189") (name "MIPI1_C_P") (type "output"))
        (pin (num "190") (name "HDMI0_CLK_N") (type "output"))
        (pin (num "191") (name "GND[51]") (type "power_in"))
        (pin (num "192") (name "GND[51]") (type "power_in"))
        (pin (num "193") (name "MIPI1_D2_N") (type "output"))
        (pin (num "194") (name "MIPI1_D3_N") (type "output"))
        (pin (num "195") (name "MIPI1_D2_P") (type "output"))
        (pin (num "196") (name "MIPI1_D3_P") (type "output"))
        (pin (num "197") (name "GND[51]") (type "power_in"))
        (pin (num "198") (name "GND[51]") (type "power_in"))
        (pin (num "199") (name "HDMI0_SDA") (type "bidirectional"))
        (pin (num "200") (name "HDMI0_SCL") (type "open_collector")))))
  (libraries
    (library (logical "AP2553W6-7")
      (uri "/Users/sam1902/Documents/CustomDJ/JLC2KiCad_lib/symbol/AP2553W6-7.kicad_sym"))
    (library (logical "Audio")
      (uri "/Applications/KiCad/KiCad.app/Contents/SharedSupport/symbols//Audio.kicad_sym"))
    (library (logical "CR2032-BS-6-1")
      (uri "/Users/sam1902/Documents/CustomDJ/JLC2KiCad_lib/symbol/CR2032-BS-6-1.kicad_sym"))
    (library (logical "Connector")
      (uri "/Applications/KiCad/KiCad.app/Contents/SharedSupport/symbols//Connector.kicad_sym"))
    (library (logical "Connector_Generic")
      (uri "/Applications/KiCad/KiCad.app/Contents/SharedSupport/symbols//Connector_Generic.kicad_sym"))
    (library (logical "DSWB04LHGET")
      (uri "/Users/sam1902/Documents/CustomDJ/JLC2KiCad_lib/symbol/DSWB04LHGET.kicad_sym"))
    (library (logical "Device")
      (uri "/Applications/KiCad/KiCad.app/Contents/SharedSupport/symbols//Device.kicad_sym"))
    (library (logical "HR911130A")
      (uri "/Users/sam1902/Documents/CustomDJ/JLC2KiCad_lib/symbol/HR911130A.kicad_sym"))
    (library (logical "Interface_USB")
      (uri "/Applications/KiCad/KiCad.app/Contents/SharedSupport/symbols//Interface_USB.kicad_sym"))
    (library (logical "KT-0603R")
      (uri "/Users/sam1902/Documents/CustomDJ/JLC2KiCad_lib/symbol/KT-0603R.kicad_sym"))
    (library (logical "MCU_Microchip_ATmega")
      (uri "/Applications/KiCad/KiCad.app/Contents/SharedSupport/symbols//MCU_Microchip_ATmega.kicad_sym"))
    (library (logical "Mechanical")
      (uri "/Applications/KiCad/KiCad.app/Contents/SharedSupport/symbols//Mechanical.kicad_sym"))
    (library (logical "PCM_JLCPCB-Capacitors")
      (uri "/Users/sam1902/Documents/KiCad/9.0/3rdparty//symbols/com_github_CDFER_JLCPCB-Kicad-Library/JLCPCB-Capacitors.kicad_sym"))
    (library (logical "PCM_JLCPCB-Crystals")
      (uri "/Users/sam1902/Documents/KiCad/9.0/3rdparty//symbols/com_github_CDFER_JLCPCB-Kicad-Library/JLCPCB-Crystals.kicad_sym"))
    (library (logical "PCM_JLCPCB-Diodes")
      (uri "/Users/sam1902/Documents/KiCad/9.0/3rdparty//symbols/com_github_CDFER_JLCPCB-Kicad-Library/JLCPCB-Diodes.kicad_sym"))
    (library (logical "PCM_JLCPCB-Inductors")
      (uri "/Users/sam1902/Documents/KiCad/9.0/3rdparty//symbols/com_github_CDFER_JLCPCB-Kicad-Library/JLCPCB-Inductors.kicad_sym"))
    (library (logical "PCM_JLCPCB-Resistors")
      (uri "/Users/sam1902/Documents/KiCad/9.0/3rdparty//symbols/com_github_CDFER_JLCPCB-Kicad-Library/JLCPCB-Resistors.kicad_sym"))
    (library (logical "PJ-320D jack 3.5mm")
      (uri "/Users/sam1902/Documents/CustomDJ/JLC2KiCad_lib/symbol/PJ-320D.kicad_sym"))
    (library (logical "PJ-611E jack 6.35mm")
      (uri "/Users/sam1902/Documents/CustomDJ/JLC2KiCad_lib/symbol/PJ-611E.kicad_sym"))
    (library (logical "PS-22E05-S-O-001")
      (uri "/Users/sam1902/Documents/CustomDJ/JLC2KiCad_lib/symbol/PS-22E05-S-O-001.kicad_sym"))
    (library (logical "PSC-1608U52GC-G4")
      (uri "/Users/sam1902/Documents/CustomDJ/JLC2KiCad_lib/symbol/PSC-1608U52GC-G4.kicad_sym"))
    (library (logical "Power_Protection")
      (uri "/Applications/KiCad/KiCad.app/Contents/SharedSupport/symbols//Power_Protection.kicad_sym"))
    (library (logical "Regulator_Linear")
      (uri "/Applications/KiCad/KiCad.app/Contents/SharedSupport/symbols//Regulator_Linear.kicad_sym"))
    (library (logical "SL1040-2R2M")
      (uri "/Users/sam1902/Documents/CustomDJ/JLC2KiCad_lib/symbol/SL1040-2R2M.kicad_sym"))
    (library (logical "SY8368AQQC")
      (uri "/Users/sam1902/Documents/CustomDJ/JLC2KiCad_lib/symbol/SY8368AQQC.kicad_sym"))
    (library (logical "Switch")
      (uri "/Applications/KiCad/KiCad.app/Contents/SharedSupport/symbols//Switch.kicad_sym"))
    (library (logical "XL-1608UBC-04")
      (uri "/Users/sam1902/Documents/CustomDJ/JLC2KiCad_lib/symbol/XL-1608UBC-04.kicad_sym"))
    (library (logical "rca-jack-red")
      (uri "/Users/sam1902/Documents/CustomDJ/kicad-thirdparty-footprints/RCJ-012-SMT.kicad_sym"))
    (library (logical "rca-jack-white")
      (uri "/Users/sam1902/Documents/CustomDJ/kicad-thirdparty-footprints/RCJ-013-SMT.kicad_sym"))
    (library (logical "rpi-cm-5")
      (uri "/Users/sam1902/Documents/CustomDJ/kicad-thirdparty-footprints/CM5.kicad_sym")))
  (nets
    (net (code "1") (name "+3.3V") (class "Default")
      (node (ref "C1") (pin "1") (pintype "passive"))
      (node (ref "C13") (pin "2") (pintype "passive"))
      (node (ref "C24") (pin "2") (pintype "passive"))
      (node (ref "C42") (pin "1") (pintype "passive"))
      (node (ref "J16") (pin "4") (pinfunction "Pin_4") (pintype "passive"))
      (node (ref "R16") (pin "2") (pintype "passive"))
      (node (ref "R17") (pin "2") (pintype "passive"))
      (node (ref "R27") (pin "2") (pintype "passive"))
      (node (ref "R28") (pin "2") (pintype "passive"))
      (node (ref "R29") (pin "1") (pintype "passive"))
      (node (ref "R30") (pin "2") (pintype "passive"))
      (node (ref "R7") (pin "1") (pintype "passive"))
      (node (ref "R8") (pin "2") (pintype "passive"))
      (node (ref "TP3") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U1") (pin "5") (pinfunction "VOUT") (pintype "power_out"))
      (node (ref "U12") (pin "5") (pinfunction "5") (pintype "passive"))
      (node (ref "U15") (pin "P10") (pinfunction "P10") (pintype "unspecified"))
      (node (ref "U3") (pin "78") (pinfunction "GPIO_VREF") (pintype "power_in"))
      (node (ref "U5") (pin "28") (pinfunction "DVDD") (pintype "power_in")))
    (net (code "2") (name "+3.3V_ANALOG") (class "Default")
      (node (ref "C12") (pin "2") (pintype "passive"))
      (node (ref "C4") (pin "1") (pintype "passive"))
      (node (ref "FB1") (pin "2") (pintype "passive"))
      (node (ref "TP4") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U2") (pin "5") (pinfunction "VOUT") (pintype "power_out"))
      (node (ref "U5") (pin "1") (pinfunction "CPVDD") (pintype "power_in"))
      (node (ref "U5") (pin "8") (pinfunction "AVDD") (pintype "power_in")))
    (net (code "3") (name "+5V") (class "Default")
      (node (ref "C11") (pin "2") (pintype "passive"))
      (node (ref "C2") (pin "1") (pintype "passive"))
      (node (ref "C3") (pin "1") (pintype "passive"))
      (node (ref "C36") (pin "1") (pintype "passive"))
      (node (ref "C37") (pin "1") (pintype "passive"))
      (node (ref "C38") (pin "1") (pintype "passive"))
      (node (ref "C39") (pin "1") (pintype "passive"))
      (node (ref "C40") (pin "1") (pintype "passive"))
      (node (ref "C41") (pin "1") (pintype "passive"))
      (node (ref "C44") (pin "2") (pintype "passive"))
      (node (ref "C46") (pin "2") (pintype "passive"))
      (node (ref "C52") (pin "2") (pintype "passive"))
      (node (ref "C58") (pin "2") (pintype "passive"))
      (node (ref "C6") (pin "2") (pintype "passive"))
      (node (ref "C7") (pin "2") (pintype "passive"))
      (node (ref "J10") (pin "8") (pinfunction "Pin_8") (pintype "passive"))
      (node (ref "J11") (pin "4") (pinfunction "Pin_4") (pintype "passive"))
      (node (ref "J12") (pin "7") (pinfunction "Pin_7") (pintype "passive"))
      (node (ref "J13") (pin "3") (pinfunction "Pin_3") (pintype "passive"))
      (node (ref "J14") (pin "2") (pinfunction "Pin_2") (pintype "passive"))
      (node (ref "J19") (pin "2") (pinfunction "Pin_2") (pintype "passive"))
      (node (ref "J2") (pin "19") (pinfunction "+5V") (pintype "power_in"))
      (node (ref "J3") (pin "19") (pinfunction "+5V") (pintype "power_in"))
      (node (ref "J5") (pin "1") (pinfunction "VBUS") (pintype "power_in"))
      (node (ref "J8") (pin "3") (pinfunction "Pin_3") (pintype "passive"))
      (node (ref "J9") (pin "6") (pinfunction "Pin_6") (pintype "passive"))
      (node (ref "L1") (pin "1") (pinfunction "1") (pintype "unspecified"))
      (node (ref "R18") (pin "1") (pintype "passive"))
      (node (ref "R23") (pin "1") (pintype "passive"))
      (node (ref "R40") (pin "2") (pintype "passive"))
      (node (ref "R43") (pin "2") (pintype "passive"))
      (node (ref "R46") (pin "1") (pintype "passive"))
      (node (ref "R5") (pin "2") (pintype "passive"))
      (node (ref "TP2") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U0") (pin "77") (pinfunction "+5V") (pintype "power_in"))
      (node (ref "U0") (pin "79") (pinfunction "+5V") (pintype "power_in"))
      (node (ref "U0") (pin "81") (pinfunction "+5V") (pintype "power_in"))
      (node (ref "U0") (pin "83") (pinfunction "+5V") (pintype "power_in"))
      (node (ref "U0") (pin "85") (pinfunction "+5V") (pintype "power_in"))
      (node (ref "U0") (pin "87") (pinfunction "+5V") (pintype "power_in"))
      (node (ref "U1") (pin "1") (pinfunction "VIN") (pintype "power_in"))
      (node (ref "U1") (pin "3") (pinfunction "EN") (pintype "input"))
      (node (ref "U13") (pin "1") (pinfunction "IN") (pintype "unspecified"))
      (node (ref "U14") (pin "5") (pinfunction "VBUS") (pintype "passive"))
      (node (ref "U17") (pin "5") (pinfunction "VBUS") (pintype "passive"))
      (node (ref "U18") (pin "1") (pinfunction "IN") (pintype "unspecified"))
      (node (ref "U2") (pin "1") (pinfunction "VIN") (pintype "power_in"))
      (node (ref "U2") (pin "3") (pinfunction "EN") (pintype "input"))
      (node (ref "U4") (pin "14") (pinfunction "VCC") (pintype "power_in"))
      (node (ref "U4") (pin "2") (pinfunction "UVCC") (pintype "power_in"))
      (node (ref "U4") (pin "24") (pinfunction "AVCC") (pintype "power_in"))
      (node (ref "U4") (pin "34") (pinfunction "VCC") (pintype "passive"))
      (node (ref "U4") (pin "44") (pinfunction "AVCC") (pintype "passive"))
      (node (ref "U4") (pin "7") (pinfunction "VBUS") (pintype "input"))
      (node (ref "U8") (pin "5") (pinfunction "VBUS") (pintype "passive"))
      (node (ref "U9") (pin "1") (pinfunction "IN") (pintype "unspecified")))
    (net (code "4") (name "+20V_USB") (class "Default")
      (node (ref "C25") (pin "2") (pintype "passive"))
      (node (ref "C26") (pin "1") (pintype "passive"))
      (node (ref "C55") (pin "1") (pintype "passive"))
      (node (ref "C56") (pin "1") (pintype "passive"))
      (node (ref "R11") (pin "2") (pintype "passive"))
      (node (ref "R44") (pin "1") (pintype "passive"))
      (node (ref "TP1") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U11") (pin "1") (pinfunction "1") (pintype "unspecified"))
      (node (ref "U19") (pin "4") (pinfunction "IN") (pintype "unspecified"))
      (node (ref "U19") (pin "5") (pinfunction "IN") (pintype "unspecified"))
      (node (ref "U19") (pin "6") (pinfunction "IN") (pintype "unspecified")))
    (net (code "5") (name "+20V_USB_RAIL") (class "Default")
      (node (ref "C23") (pin "1") (pintype "passive"))
      (node (ref "C43") (pin "1") (pintype "passive"))
      (node (ref "J1") (pin "A4") (pinfunction "VBUS") (pintype "passive"))
      (node (ref "J1") (pin "A9") (pinfunction "VBUS") (pintype "passive"))
      (node (ref "J1") (pin "B4") (pinfunction "VBUS") (pintype "passive"))
      (node (ref "J1") (pin "B9") (pinfunction "VBUS") (pintype "passive"))
      (node (ref "R1") (pin "1") (pintype "passive"))
      (node (ref "TP11") (pin "1") (pinfunction "1") (pintype "passive")))
    (net (code "6") (name "/Arduino MIDI/BTN_BACK") (class "Default")
      (node (ref "J12") (pin "5") (pinfunction "Pin_5") (pintype "passive"))
      (node (ref "U4") (pin "37") (pinfunction "PF6") (pintype "bidirectional")))
    (net (code "7") (name "/Arduino MIDI/BTN_LOOP_IN") (class "Default")
      (node (ref "J10") (pin "2") (pinfunction "Pin_2") (pintype "passive"))
      (node (ref "U4") (pin "29") (pinfunction "PB5") (pintype "bidirectional")))
    (net (code "8") (name "/Arduino MIDI/BTN_LOOP_OUT") (class "Default")
      (node (ref "J10") (pin "3") (pinfunction "Pin_3") (pintype "passive"))
      (node (ref "U4") (pin "30") (pinfunction "PB6") (pintype "bidirectional")))
    (net (code "9") (name "/Arduino MIDI/BTN_MTEMPO") (class "Default")
      (node (ref "J11") (pin "2") (pinfunction "Pin_2") (pintype "passive"))
      (node (ref "U4") (pin "25") (pinfunction "PD4") (pintype "bidirectional")))
    (net (code "10") (name "/Arduino MIDI/BTN_RELOOP") (class "Default")
      (node (ref "J10") (pin "4") (pinfunction "Pin_4") (pintype "passive"))
      (node (ref "U4") (pin "12") (pinfunction "PB7") (pintype "bidirectional")))
    (net (code "11") (name "/Arduino MIDI/BTN_TEMPO_RST") (class "Default")
      (node (ref "J13") (pin "4") (pinfunction "Pin_4") (pintype "passive"))
      (node (ref "U4") (pin "33") (pinfunction "~{HWB}/PE2") (pintype "bidirectional")))
    (net (code "12") (name "/Arduino MIDI/BTN_TOUCH") (class "Default")
      (node (ref "C33") (pin "1") (pintype "passive"))
      (node (ref "J17") (pin "1") (pinfunction "Pin_1") (pintype "passive"))
      (node (ref "R18") (pin "2") (pintype "passive"))
      (node (ref "U4") (pin "22") (pinfunction "PD5") (pintype "bidirectional")))
    (net (code "13") (name "/Arduino MIDI/ENC_A") (class "Default")
      (node (ref "J12") (pin "2") (pinfunction "Pin_2") (pintype "passive"))
      (node (ref "U4") (pin "40") (pinfunction "PF1") (pintype "bidirectional")))
    (net (code "14") (name "/Arduino MIDI/ENC_B") (class "Default")
      (node (ref "J12") (pin "3") (pinfunction "Pin_3") (pintype "passive"))
      (node (ref "U4") (pin "39") (pinfunction "PF4") (pintype "bidirectional")))
    (net (code "15") (name "/Arduino MIDI/ENC_SW") (class "Default")
      (node (ref "J12") (pin "4") (pinfunction "Pin_4") (pintype "passive"))
      (node (ref "U4") (pin "38") (pinfunction "PF5") (pintype "bidirectional")))
    (net (code "16") (name "/Arduino MIDI/FADER_ADIN") (class "Default")
      (node (ref "J13") (pin "2") (pinfunction "Pin_2") (pintype "passive"))
      (node (ref "U4") (pin "41") (pinfunction "PF0") (pintype "bidirectional")))
    (net (code "17") (name "/Arduino MIDI/JOG1") (class "Default")
      (node (ref "J8") (pin "2") (pinfunction "Pin_2") (pintype "passive"))
      (node (ref "U4") (pin "19") (pinfunction "PD1") (pintype "bidirectional")))
    (net (code "18") (name "/Arduino MIDI/JOG2") (class "Default")
      (node (ref "J8") (pin "1") (pinfunction "Pin_1") (pintype "passive"))
      (node (ref "U4") (pin "18") (pinfunction "PD0") (pintype "bidirectional")))
    (net (code "19") (name "/Arduino MIDI/LED_BACK") (class "Default")
      (node (ref "J12") (pin "6") (pinfunction "Pin_6") (pintype "passive"))
      (node (ref "U4") (pin "36") (pinfunction "PF7") (pintype "bidirectional")))
    (net (code "20") (name "/Arduino MIDI/LED_CUE") (class "Default")
      (node (ref "J9") (pin "5") (pinfunction "Pin_5") (pintype "passive"))
      (node (ref "U4") (pin "28") (pinfunction "PB4") (pintype "bidirectional")))
    (net (code "21") (name "/Arduino MIDI/LED_LOOP_IN") (class "Default")
      (node (ref "J10") (pin "5") (pinfunction "Pin_5") (pintype "passive"))
      (node (ref "U4") (pin "31") (pinfunction "PC6") (pintype "bidirectional")))
    (net (code "22") (name "/Arduino MIDI/LED_LOOP_OUT") (class "Default")
      (node (ref "J10") (pin "6") (pinfunction "Pin_6") (pintype "passive"))
      (node (ref "U4") (pin "32") (pinfunction "PC7") (pintype "bidirectional")))
    (net (code "23") (name "/Arduino MIDI/LED_MTEMPO") (class "Default")
      (node (ref "J11") (pin "3") (pinfunction "Pin_3") (pintype "passive"))
      (node (ref "U4") (pin "27") (pinfunction "PD7") (pintype "bidirectional")))
    (net (code "24") (name "/Arduino MIDI/LED_RELOOP") (class "Default")
      (node (ref "J10") (pin "7") (pinfunction "Pin_7") (pintype "passive"))
      (node (ref "U4") (pin "26") (pinfunction "PD6") (pintype "bidirectional")))
    (net (code "25") (name "/Arduino MIDI/LED_TEMPO_RST") (class "Default")
      (node (ref "J13") (pin "5") (pinfunction "Pin_5") (pintype "passive"))
      (node (ref "U4") (pin "1") (pinfunction "PE6") (pintype "bidirectional")))
    (net (code "26") (name "/Audio Outputs/RCA_LEFT") (class "Default")
      (node (ref "C19") (pin "1") (pintype "passive"))
      (node (ref "J18") (pin "6") (pinfunction "LEFT_P") (pintype "passive"))
      (node (ref "J6") (pin "2") (pinfunction "SIGNL") (pintype "passive"))
      (node (ref "R9") (pin "2") (pintype "passive"))
      (node (ref "U10") (pin "2") (pinfunction "LEFT_P") (pintype "passive")))
    (net (code "27") (name "/Audio Outputs/RCA_RIGHT") (class "Default")
      (node (ref "C21") (pin "1") (pintype "passive"))
      (node (ref "J18") (pin "4") (pinfunction "RIGHT_P") (pintype "passive"))
      (node (ref "J7") (pin "2") (pinfunction "SIGNL") (pintype "passive"))
      (node (ref "R10") (pin "2") (pintype "passive"))
      (node (ref "U10") (pin "3") (pinfunction "RIGHT_P") (pintype "passive")))
    (net (code "28") (name "/HDMI and Ethernet/eth_nled_2") (class "Default")
      (node (ref "U15") (pin "13") (pinfunction "13") (pintype "unspecified"))
      (node (ref "U3") (pin "17") (pinfunction "~{Ethernet_nLED2}") (pintype "output")))
    (net (code "29") (name "/HDMI and Ethernet/eth_nled_3") (class "Default")
      (node (ref "U15") (pin "12") (pinfunction "12") (pintype "unspecified"))
      (node (ref "U3") (pin "15") (pinfunction "~{Ethernet_nLED3}") (pintype "output")))
    (net (code "30") (name "/HDMI and Ethernet/eth_p0_n") (class "Default")
      (node (ref "U15") (pin "MDI0-") (pinfunction "MDI0-") (pintype "unspecified"))
      (node (ref "U3") (pin "10") (pinfunction "Ethernet_Pair0_N") (pintype "passive")))
    (net (code "31") (name "/HDMI and Ethernet/eth_p0_p") (class "Default")
      (node (ref "U15") (pin "MDI0+") (pinfunction "MDI0+") (pintype "unspecified"))
      (node (ref "U3") (pin "12") (pinfunction "Ethernet_Pair0_P") (pintype "passive")))
    (net (code "32") (name "/HDMI and Ethernet/eth_p1_n") (class "Default")
      (node (ref "U15") (pin "MDI1-") (pinfunction "MDI1-") (pintype "unspecified"))
      (node (ref "U3") (pin "6") (pinfunction "Ethernet_Pair1_N") (pintype "passive")))
    (net (code "33") (name "/HDMI and Ethernet/eth_p1_p") (class "Default")
      (node (ref "U15") (pin "MDI1+") (pinfunction "MDI1+") (pintype "unspecified"))
      (node (ref "U3") (pin "4") (pinfunction "Ethernet_Pair1_P") (pintype "passive")))
    (net (code "34") (name "/HDMI and Ethernet/eth_p2_n") (class "Default")
      (node (ref "U15") (pin "MDI2-") (pinfunction "MDI2-") (pintype "unspecified"))
      (node (ref "U3") (pin "9") (pinfunction "Ethernet_Pair2_N") (pintype "passive")))
    (net (code "35") (name "/HDMI and Ethernet/eth_p2_p") (class "Default")
      (node (ref "U15") (pin "MDI2+") (pinfunction "MDI2+") (pintype "unspecified"))
      (node (ref "U3") (pin "11") (pinfunction "Ethernet_Pair2_P") (pintype "passive")))
    (net (code "36") (name "/HDMI and Ethernet/eth_p3_n") (class "Default")
      (node (ref "U15") (pin "MDI3-") (pinfunction "MDI3-") (pintype "unspecified"))
      (node (ref "U3") (pin "5") (pinfunction "Ethernet_Pair3_N") (pintype "passive")))
    (net (code "37") (name "/HDMI and Ethernet/eth_p3_p") (class "Default")
      (node (ref "U15") (pin "MDI3+") (pinfunction "MDI3+") (pintype "unspecified"))
      (node (ref "U3") (pin "3") (pinfunction "Ethernet_Pair3_P") (pintype "passive")))
    (net (code "38") (name "/S_EEPROM_WP_UP") (class "Default")
      (node (ref "R6") (pin "1") (pintype "passive"))
      (node (ref "U12") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U3") (pin "20") (pinfunction "EEPROM_nWP") (pintype "input")))
    (net (code "39") (name "/USB DJ Ports/USB_C_DJ_DM") (class "Default")
      (node (ref "U14") (pin "6") (pinfunction "I/O1") (pintype "passive"))
      (node (ref "U3") (pin "103") (pinfunction "USB_N") (pintype "passive")))
    (net (code "40") (name "/USB DJ Ports/USB_C_DJ_DP") (class "Default")
      (node (ref "U14") (pin "4") (pinfunction "I/O2") (pintype "passive"))
      (node (ref "U3") (pin "105") (pinfunction "USB_P") (pintype "passive")))
    (net (code "41") (name "/USB DJ Ports/USB_C_DJ_VBUS") (class "Default")
      (node (ref "C47") (pin "2") (pintype "passive"))
      (node (ref "J20") (pin "A4") (pinfunction "VBUS") (pintype "passive"))
      (node (ref "J20") (pin "A9") (pinfunction "VBUS") (pintype "passive"))
      (node (ref "J20") (pin "B4") (pinfunction "VBUS") (pintype "passive"))
      (node (ref "J20") (pin "B9") (pinfunction "VBUS") (pintype "passive"))
      (node (ref "U13") (pin "6") (pinfunction "OUT") (pintype "unspecified")))
    (net (code "42") (name "/USB DJ Ports/USB_DJ_DM") (class "Default")
      (node (ref "U3") (pin "136") (pinfunction "USB3-0-DM") (pintype "bidirectional"))
      (node (ref "U8") (pin "6") (pinfunction "I/O1") (pintype "passive")))
    (net (code "43") (name "/USB DJ Ports/USB_DJ_DP") (class "Default")
      (node (ref "U3") (pin "134") (pinfunction "USB3-0-DP") (pintype "bidirectional"))
      (node (ref "U8") (pin "4") (pinfunction "I/O2") (pintype "passive")))
    (net (code "44") (name "/USB DJ Ports/USB_DJ_SSRXM") (class "Default")
      (node (ref "J4") (pin "5") (pinfunction "SSRX-") (pintype "output"))
      (node (ref "U3") (pin "128") (pinfunction "USB3-0-RX_N") (pintype "input")))
    (net (code "45") (name "/USB DJ Ports/USB_DJ_SSRXP") (class "Default")
      (node (ref "J4") (pin "6") (pinfunction "SSRX+") (pintype "output"))
      (node (ref "U3") (pin "130") (pinfunction "USB3-0-RX_P") (pintype "input")))
    (net (code "46") (name "/USB DJ Ports/USB_DJ_SSTXM") (class "Default")
      (node (ref "J4") (pin "8") (pinfunction "SSTX-") (pintype "input"))
      (node (ref "U3") (pin "140") (pinfunction "USB3-0-TX_N") (pintype "output")))
    (net (code "47") (name "/USB DJ Ports/USB_DJ_SSTXP") (class "Default")
      (node (ref "J4") (pin "9") (pinfunction "SSTX+") (pintype "input"))
      (node (ref "U3") (pin "142") (pinfunction "USB3-0-TX_P") (pintype "output")))
    (net (code "48") (name "/USB DJ Ports/USB_DJ_VBUS") (class "Default")
      (node (ref "C45") (pin "2") (pintype "passive"))
      (node (ref "J4") (pin "1") (pinfunction "VBUS") (pintype "power_in"))
      (node (ref "U9") (pin "6") (pinfunction "OUT") (pintype "unspecified")))
    (net (code "49") (name "/USB DJ Ports/USB_DJ_VBUS_EN") (class "Default")
      (node (ref "R25") (pin "2") (pintype "passive"))
      (node (ref "R33") (pin "2") (pintype "passive"))
      (node (ref "U13") (pin "3") (pinfunction "EN") (pintype "unspecified"))
      (node (ref "U3") (pin "111") (pinfunction "VBUS_EN") (pintype "input"))
      (node (ref "U9") (pin "3") (pinfunction "EN") (pintype "unspecified")))
    (net (code "50") (name "/USB DJ Ports/USB_SCR_DM") (class "Default")
      (node (ref "U17") (pin "6") (pinfunction "I/O1") (pintype "passive"))
      (node (ref "U3") (pin "165") (pinfunction "USB3-1-DM") (pintype "bidirectional")))
    (net (code "51") (name "/USB DJ Ports/USB_SCR_DP") (class "Default")
      (node (ref "U17") (pin "4") (pinfunction "I/O2") (pintype "passive"))
      (node (ref "U3") (pin "163") (pinfunction "USB3-1-DP") (pintype "bidirectional")))
    (net (code "52") (name "/USB DJ Ports/USB_SCR_SSRXM") (class "Default")
      (node (ref "J15") (pin "5") (pinfunction "SSRX-") (pintype "output"))
      (node (ref "U3") (pin "157") (pinfunction "USB3-1-RX_N") (pintype "input")))
    (net (code "53") (name "/USB DJ Ports/USB_SCR_SSRXP") (class "Default")
      (node (ref "J15") (pin "6") (pinfunction "SSRX+") (pintype "output"))
      (node (ref "U3") (pin "159") (pinfunction "USB3-1-RX_P") (pintype "input")))
    (net (code "54") (name "/USB DJ Ports/USB_SCR_SSTXM") (class "Default")
      (node (ref "J15") (pin "8") (pinfunction "SSTX-") (pintype "input"))
      (node (ref "U3") (pin "169") (pinfunction "USB3-1-TX_N") (pintype "output")))
    (net (code "55") (name "/USB DJ Ports/USB_SCR_SSTXP") (class "Default")
      (node (ref "J15") (pin "9") (pinfunction "SSTX+") (pintype "input"))
      (node (ref "U3") (pin "171") (pinfunction "USB3-1-TX_P") (pintype "output")))
    (net (code "56") (name "/USB DJ Ports/USB_SCR_VBUS") (class "Default")
      (node (ref "C53") (pin "2") (pintype "passive"))
      (node (ref "J15") (pin "1") (pinfunction "VBUS") (pintype "power_in"))
      (node (ref "U18") (pin "6") (pinfunction "OUT") (pintype "unspecified")))
    (net (code "57") (name "GND") (class "Default")
      (node (ref "BT1") (pin "2") (pinfunction "2") (pintype "input"))
      (node (ref "C1") (pin "2") (pintype "passive"))
      (node (ref "C10") (pin "1") (pintype "passive"))
      (node (ref "C11") (pin "1") (pintype "passive"))
      (node (ref "C12") (pin "1") (pintype "passive"))
      (node (ref "C13") (pin "1") (pintype "passive"))
      (node (ref "C14") (pin "1") (pintype "passive"))
      (node (ref "C15") (pin "2") (pintype "passive"))
      (node (ref "C17") (pin "2") (pintype "passive"))
      (node (ref "C19") (pin "2") (pintype "passive"))
      (node (ref "C2") (pin "2") (pintype "passive"))
      (node (ref "C21") (pin "2") (pintype "passive"))
      (node (ref "C22") (pin "2") (pintype "passive"))
      (node (ref "C23") (pin "2") (pintype "passive"))
      (node (ref "C24") (pin "1") (pintype "passive"))
      (node (ref "C25") (pin "1") (pintype "passive"))
      (node (ref "C26") (pin "2") (pintype "passive"))
      (node (ref "C3") (pin "2") (pintype "passive"))
      (node (ref "C33") (pin "2") (pintype "passive"))
      (node (ref "C34") (pin "2") (pintype "passive"))
      (node (ref "C35") (pin "1") (pintype "passive"))
      (node (ref "C36") (pin "2") (pintype "passive"))
      (node (ref "C37") (pin "2") (pintype "passive"))
      (node (ref "C38") (pin "2") (pintype "passive"))
      (node (ref "C39") (pin "2") (pintype "passive"))
      (node (ref "C4") (pin "2") (pintype "passive"))
      (node (ref "C40") (pin "2") (pintype "passive"))
      (node (ref "C41") (pin "2") (pintype "passive"))
      (node (ref "C42") (pin "2") (pintype "passive"))
      (node (ref "C43") (pin "2") (pintype "passive"))
      (node (ref "C44") (pin "1") (pintype "passive"))
      (node (ref "C45") (pin "1") (pintype "passive"))
      (node (ref "C46") (pin "1") (pintype "passive"))
      (node (ref "C47") (pin "1") (pintype "passive"))
      (node (ref "C48") (pin "2") (pintype "passive"))
      (node (ref "C49") (pin "2") (pintype "passive"))
      (node (ref "C5") (pin "1") (pintype "passive"))
      (node (ref "C50") (pin "2") (pintype "passive"))
      (node (ref "C51") (pin "2") (pintype "passive"))
      (node (ref "C52") (pin "1") (pintype "passive"))
      (node (ref "C53") (pin "1") (pintype "passive"))
      (node (ref "C55") (pin "2") (pintype "passive"))
      (node (ref "C56") (pin "2") (pintype "passive"))
      (node (ref "C57") (pin "1") (pintype "passive"))
      (node (ref "C6") (pin "1") (pintype "passive"))
      (node (ref "C7") (pin "1") (pintype "passive"))
      (node (ref "C8") (pin "2") (pintype "passive"))
      (node (ref "C9") (pin "2") (pintype "passive"))
      (node (ref "D1") (pin "1") (pinfunction "K") (pintype "unspecified"))
      (node (ref "D2") (pin "1") (pintype "passive"))
      (node (ref "D3") (pin "1") (pinfunction "K") (pintype "unspecified"))
      (node (ref "D4") (pin "1") (pinfunction "K") (pintype "unspecified"))
      (node (ref "D5") (pin "1") (pinfunction "K") (pintype "unspecified"))
      (node (ref "J1") (pin "A1") (pinfunction "GND") (pintype "passive"))
      (node (ref "J1") (pin "A12") (pinfunction "GND") (pintype "passive"))
      (node (ref "J1") (pin "B1") (pinfunction "GND") (pintype "passive"))
      (node (ref "J1") (pin "B12") (pinfunction "GND") (pintype "passive"))
      (node (ref "J1") (pin "S1") (pinfunction "SHIELD") (pintype "passive"))
      (node (ref "J10") (pin "1") (pinfunction "Pin_1") (pintype "passive"))
      (node (ref "J11") (pin "1") (pinfunction "Pin_1") (pintype "passive"))
      (node (ref "J12") (pin "1") (pinfunction "Pin_1") (pintype "passive"))
      (node (ref "J13") (pin "1") (pinfunction "Pin_1") (pintype "passive"))
      (node (ref "J14") (pin "1") (pinfunction "Pin_1") (pintype "passive"))
      (node (ref "J15") (pin "10") (pinfunction "SHIELD") (pintype "passive"))
      (node (ref "J15") (pin "4") (pinfunction "GND") (pintype "power_in"))
      (node (ref "J15") (pin "7") (pinfunction "DRAIN") (pintype "passive"))
      (node (ref "J16") (pin "1") (pinfunction "Pin_1") (pintype "passive"))
      (node (ref "J17") (pin "2") (pinfunction "Pin_2") (pintype "passive"))
      (node (ref "J18") (pin "2") (pinfunction "GND/SHLD") (pintype "passive"))
      (node (ref "J19") (pin "6") (pinfunction "Pin_6") (pintype "passive"))
      (node (ref "J2") (pin "10") (pinfunction "D0S") (pintype "power_in"))
      (node (ref "J2") (pin "13") (pinfunction "CKS") (pintype "power_in"))
      (node (ref "J2") (pin "16") (pinfunction "GND") (pintype "power_in"))
      (node (ref "J2") (pin "4") (pinfunction "D2S") (pintype "power_in"))
      (node (ref "J2") (pin "7") (pinfunction "D1S") (pintype "power_in"))
      (node (ref "J2") (pin "SH") (pinfunction "SH") (pintype "passive"))
      (node (ref "J20") (pin "A1") (pinfunction "GND") (pintype "passive"))
      (node (ref "J20") (pin "A12") (pinfunction "GND") (pintype "passive"))
      (node (ref "J20") (pin "B1") (pinfunction "GND") (pintype "passive"))
      (node (ref "J20") (pin "B12") (pinfunction "GND") (pintype "passive"))
      (node (ref "J20") (pin "S1") (pinfunction "SHIELD") (pintype "passive"))
      (node (ref "J3") (pin "10") (pinfunction "D0S") (pintype "power_in"))
      (node (ref "J3") (pin "13") (pinfunction "CKS") (pintype "power_in"))
      (node (ref "J3") (pin "16") (pinfunction "GND") (pintype "power_in"))
      (node (ref "J3") (pin "4") (pinfunction "D2S") (pintype "power_in"))
      (node (ref "J3") (pin "7") (pinfunction "D1S") (pintype "power_in"))
      (node (ref "J3") (pin "SH") (pinfunction "SH") (pintype "passive"))
      (node (ref "J4") (pin "10") (pinfunction "SHIELD") (pintype "passive"))
      (node (ref "J4") (pin "4") (pinfunction "GND") (pintype "power_in"))
      (node (ref "J4") (pin "7") (pinfunction "DRAIN") (pintype "passive"))
      (node (ref "J5") (pin "4") (pinfunction "GND") (pintype "power_in"))
      (node (ref "J5") (pin "5") (pinfunction "Shield") (pintype "passive"))
      (node (ref "J6") (pin "1A") (pinfunction "SHLD") (pintype "passive"))
      (node (ref "J6") (pin "1B") (pinfunction "SHLD") (pintype "passive"))
      (node (ref "J6") (pin "1C") (pinfunction "SHLD") (pintype "passive"))
      (node (ref "J7") (pin "1A") (pinfunction "SHLD") (pintype "passive"))
      (node (ref "J7") (pin "1B") (pinfunction "SHLD") (pintype "passive"))
      (node (ref "J7") (pin "1C") (pinfunction "SHLD") (pintype "passive"))
      (node (ref "J8") (pin "4") (pinfunction "Pin_4") (pintype "passive"))
      (node (ref "J9") (pin "1") (pinfunction "Pin_1") (pintype "passive"))
      (node (ref "R2") (pin "1") (pintype "passive"))
      (node (ref "R25") (pin "1") (pintype "passive"))
      (node (ref "R26") (pin "2") (pintype "passive"))
      (node (ref "R3") (pin "1") (pintype "passive"))
      (node (ref "R31") (pin "1") (pintype "passive"))
      (node (ref "R32") (pin "1") (pintype "passive"))
      (node (ref "R33") (pin "1") (pintype "passive"))
      (node (ref "R34") (pin "2") (pintype "passive"))
      (node (ref "R35") (pin "2") (pintype "passive"))
      (node (ref "R36") (pin "1") (pintype "passive"))
      (node (ref "R37") (pin "1") (pintype "passive"))
      (node (ref "R38") (pin "1") (pintype "passive"))
      (node (ref "R41") (pin "2") (pintype "passive"))
      (node (ref "R45") (pin "2") (pintype "passive"))
      (node (ref "R6") (pin "2") (pintype "passive"))
      (node (ref "SW1") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "SW2") (pin "2") (pinfunction "2") (pintype "passive"))
      (node (ref "TP5") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U0") (pin "1") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "107") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "108") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "113") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "114") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "119") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "120") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "125") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "126") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "13") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "131") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "132") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "137") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "138") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "14") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "144") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "150") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "155") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "156") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "161") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "162") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "167") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "168") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "173") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "174") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "179") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "180") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "185") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "186") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "191") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "192") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "197") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "198") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "2") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "22") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "23") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "32") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "33") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "42") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "43") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "52") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "53") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "59") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "60") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "65") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "66") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "7") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "71") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "74") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "8") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U0") (pin "98") (pinfunction "GND[51]") (pintype "power_in"))
      (node (ref "U1") (pin "2") (pinfunction "GND") (pintype "power_in"))
      (node (ref "U10") (pin "1") (pinfunction "GND/SHLD") (pintype "passive"))
      (node (ref "U12") (pin "2") (pinfunction "2") (pintype "passive"))
      (node (ref "U12") (pin "3") (pinfunction "3") (pintype "passive"))
      (node (ref "U12") (pin "4") (pinfunction "4") (pintype "passive"))
      (node (ref "U13") (pin "2") (pinfunction "GND") (pintype "unspecified"))
      (node (ref "U14") (pin "2") (pinfunction "GND") (pintype "passive"))
      (node (ref "U15") (pin "SHIELD0") (pinfunction "SHIELD0") (pintype "unspecified"))
      (node (ref "U15") (pin "SHIELD1") (pinfunction "SHIELD1") (pintype "unspecified"))
      (node (ref "U17") (pin "2") (pinfunction "GND") (pintype "passive"))
      (node (ref "U18") (pin "2") (pinfunction "GND") (pintype "unspecified"))
      (node (ref "U19") (pin "1") (pinfunction "GND") (pintype "unspecified"))
      (node (ref "U19") (pin "3") (pinfunction "GND") (pintype "unspecified"))
      (node (ref "U2") (pin "2") (pinfunction "GND") (pintype "power_in"))
      (node (ref "U3") (pin "89") (pinfunction "~{WL_nDisable}") (pintype "input"))
      (node (ref "U3") (pin "91") (pinfunction "~{BT_nDisable}") (pintype "input"))
      (node (ref "U3") (pin "93") (pinfunction "~{nRPIBOOT}") (pintype "input"))
      (node (ref "U4") (pin "15") (pinfunction "GND") (pintype "power_in"))
      (node (ref "U4") (pin "23") (pinfunction "GND") (pintype "passive"))
      (node (ref "U4") (pin "35") (pinfunction "GND") (pintype "passive"))
      (node (ref "U4") (pin "43") (pinfunction "GND") (pintype "passive"))
      (node (ref "U4") (pin "5") (pinfunction "UGND") (pintype "passive"))
      (node (ref "U5") (pin "16") (pinfunction "ADR2/GPIO2/DOUT") (pintype "bidirectional"))
      (node (ref "U5") (pin "17") (pinfunction "MODE1") (pintype "input"))
      (node (ref "U5") (pin "18") (pinfunction "MODE2/MS") (pintype "input"))
      (node (ref "U5") (pin "20") (pinfunction "SCK") (pintype "input"))
      (node (ref "U5") (pin "24") (pinfunction "ADR1/MISO/FMT") (pintype "bidirectional"))
      (node (ref "U5") (pin "27") (pinfunction "DGND") (pintype "power_in"))
      (node (ref "U5") (pin "3") (pinfunction "CPGND") (pintype "power_in"))
      (node (ref "U5") (pin "9") (pinfunction "AGND") (pintype "power_in"))
      (node (ref "U6") (pin "11") (pinfunction "GND") (pintype "power_in"))
      (node (ref "U6") (pin "2") (pinfunction "CFG2") (pintype "passive"))
      (node (ref "U6") (pin "9") (pinfunction "CFG1") (pintype "passive"))
      (node (ref "U8") (pin "2") (pinfunction "GND") (pintype "passive"))
      (node (ref "U9") (pin "2") (pinfunction "GND") (pintype "unspecified"))
      (node (ref "X1") (pin "2") (pinfunction "GND") (pintype "unspecified"))
      (node (ref "X1") (pin "4") (pinfunction "GND") (pintype "unspecified")))
    (net (code "58") (name "I2C_SCL") (class "Default")
      (node (ref "J16") (pin "3") (pinfunction "Pin_3") (pintype "passive"))
      (node (ref "R27") (pin "1") (pintype "passive"))
      (node (ref "TP7") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U3") (pin "82") (pinfunction "I2C_SDA0") (pintype "bidirectional"))
      (node (ref "U5") (pin "12") (pinfunction "SCL/MC/ATT1") (pintype "input")))
    (net (code "59") (name "I2C_SDA") (class "Default")
      (node (ref "J16") (pin "2") (pinfunction "Pin_2") (pintype "passive"))
      (node (ref "R28") (pin "1") (pintype "passive"))
      (node (ref "TP6") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U3") (pin "80") (pinfunction "I2C_SCL0") (pintype "bidirectional"))
      (node (ref "U5") (pin "11") (pinfunction "SDA/MOSI/ATT2") (pintype "bidirectional")))
    (net (code "60") (name "I2S_BCK") (class "Default")
      (node (ref "TP8") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U3") (pin "49") (pinfunction "GPIO18") (pintype "passive"))
      (node (ref "U5") (pin "21") (pinfunction "BCK") (pintype "bidirectional")))
    (net (code "61") (name "I2S_DIN") (class "Default")
      (node (ref "TP10") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U3") (pin "25") (pinfunction "GPIO21") (pintype "passive"))
      (node (ref "U5") (pin "22") (pinfunction "DIN") (pintype "input")))
    (net (code "62") (name "I2S_LRCLK") (class "Default")
      (node (ref "TP9") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U3") (pin "26") (pinfunction "GPIO19") (pintype "passive"))
      (node (ref "U5") (pin "23") (pinfunction "LRCK") (pintype "bidirectional")))
    (net (code "63") (name "ISP_MISO") (class "Default")
      (node (ref "J19") (pin "1") (pinfunction "Pin_1") (pintype "passive"))
      (node (ref "J9") (pin "4") (pinfunction "Pin_4") (pintype "passive"))
      (node (ref "U4") (pin "11") (pinfunction "PB3") (pintype "bidirectional")))
    (net (code "64") (name "ISP_MOSI") (class "Default")
      (node (ref "J19") (pin "4") (pinfunction "Pin_4") (pintype "passive"))
      (node (ref "J9") (pin "3") (pinfunction "Pin_3") (pintype "passive"))
      (node (ref "U4") (pin "10") (pinfunction "PB2") (pintype "bidirectional")))
    (net (code "65") (name "ISP_RESET") (class "Default")
      (node (ref "C35") (pin "2") (pintype "passive"))
      (node (ref "J19") (pin "3") (pinfunction "Pin_3") (pintype "passive"))
      (node (ref "R5") (pin "1") (pintype "passive"))
      (node (ref "SW1") (pin "2") (pinfunction "2") (pintype "passive"))
      (node (ref "U4") (pin "13") (pinfunction "~{RESET}") (pintype "input")))
    (net (code "66") (name "ISP_SCK") (class "Default")
      (node (ref "J19") (pin "5") (pinfunction "Pin_5") (pintype "passive"))
      (node (ref "J9") (pin "2") (pinfunction "Pin_2") (pintype "passive"))
      (node (ref "U4") (pin "9") (pinfunction "PB1") (pintype "bidirectional")))
    (net (code "67") (name "Net-(C14-Pad2)") (class "Default")
      (node (ref "C14") (pin "2") (pintype "passive"))
      (node (ref "FB1") (pin "1") (pintype "passive")))
    (net (code "68") (name "Net-(C18-Pad2)") (class "Default")
      (node (ref "C18") (pin "2") (pintype "passive"))
      (node (ref "R9") (pin "1") (pintype "passive")))
    (net (code "69") (name "Net-(C20-Pad2)") (class "Default")
      (node (ref "C20") (pin "2") (pintype "passive"))
      (node (ref "R10") (pin "1") (pintype "passive")))
    (net (code "70") (name "Net-(C31-Pad1)") (class "Default")
      (node (ref "C31") (pin "1") (pintype "passive"))
      (node (ref "C5") (pin "2") (pintype "passive")))
    (net (code "71") (name "Net-(C58-Pad1)") (class "Default")
      (node (ref "C58") (pin "1") (pintype "passive"))
      (node (ref "R42") (pin "2") (pintype "passive")))
    (net (code "72") (name "Net-(D1-A)") (class "Default")
      (node (ref "D1") (pin "2") (pinfunction "A") (pintype "unspecified"))
      (node (ref "R11") (pin "1") (pintype "passive")))
    (net (code "73") (name "Net-(D3-A)") (class "Default")
      (node (ref "D3") (pin "2") (pinfunction "A") (pintype "unspecified"))
      (node (ref "R19") (pin "2") (pintype "passive")))
    (net (code "74") (name "Net-(D4-A)") (class "Default")
      (node (ref "D4") (pin "2") (pinfunction "A") (pintype "unspecified"))
      (node (ref "R21") (pin "2") (pintype "passive")))
    (net (code "75") (name "Net-(D5-A)") (class "Default")
      (node (ref "D5") (pin "2") (pinfunction "A") (pintype "unspecified"))
      (node (ref "R20") (pin "1") (pintype "passive")))
    (net (code "76") (name "Net-(D7-A)") (class "Default")
      (node (ref "D7") (pin "2") (pinfunction "A") (pintype "unspecified"))
      (node (ref "R46") (pin "2") (pintype "passive")))
    (net (code "77") (name "Net-(D7-K)") (class "Default")
      (node (ref "D7") (pin "1") (pinfunction "K") (pintype "unspecified"))
      (node (ref "R43") (pin "1") (pintype "passive"))
      (node (ref "U19") (pin "11") (pinfunction "PG") (pintype "unspecified")))
    (net (code "78") (name "Net-(J1-CC1)") (class "Default")
      (node (ref "C51") (pin "1") (pintype "passive"))
      (node (ref "J1") (pin "A5") (pinfunction "CC1") (pintype "bidirectional"))
      (node (ref "U6") (pin "7") (pinfunction "CC1") (pintype "bidirectional")))
    (net (code "79") (name "Net-(J1-CC2)") (class "Default")
      (node (ref "C50") (pin "1") (pintype "passive"))
      (node (ref "J1") (pin "B5") (pinfunction "CC2") (pintype "bidirectional"))
      (node (ref "U6") (pin "6") (pinfunction "CC2") (pintype "bidirectional")))
    (net (code "80") (name "Net-(J2-CEC)") (class "Default")
      (node (ref "J2") (pin "15") (pinfunction "CEC") (pintype "bidirectional"))
      (node (ref "U3") (pin "149") (pinfunction "HDMI1_CEC") (pintype "open_collector")))
    (net (code "81") (name "Net-(J2-CK+)") (class "Default")
      (node (ref "J2") (pin "12") (pinfunction "CK+") (pintype "passive"))
      (node (ref "U3") (pin "164") (pinfunction "HDMI1_CLK_P") (pintype "output")))
    (net (code "82") (name "Net-(J2-CK-)") (class "Default")
      (node (ref "J2") (pin "14") (pinfunction "CK-") (pintype "passive"))
      (node (ref "U3") (pin "166") (pinfunction "HDMI1_CLK_N") (pintype "output")))
    (net (code "83") (name "Net-(J2-D0+)") (class "Default")
      (node (ref "J2") (pin "9") (pinfunction "D0+") (pintype "passive"))
      (node (ref "U3") (pin "158") (pinfunction "HDMI1_TX0_P") (pintype "output")))
    (net (code "84") (name "Net-(J2-D0-)") (class "Default")
      (node (ref "J2") (pin "11") (pinfunction "D0-") (pintype "passive"))
      (node (ref "U3") (pin "160") (pinfunction "HDMI1_TX0_N") (pintype "output")))
    (net (code "85") (name "Net-(J2-D1+)") (class "Default")
      (node (ref "J2") (pin "6") (pinfunction "D1+") (pintype "passive"))
      (node (ref "U3") (pin "152") (pinfunction "HDMI1_TX1_P") (pintype "output")))
    (net (code "86") (name "Net-(J2-D1-)") (class "Default")
      (node (ref "J2") (pin "8") (pinfunction "D1-") (pintype "passive"))
      (node (ref "U3") (pin "154") (pinfunction "HDMI1_TX1_N") (pintype "output")))
    (net (code "87") (name "Net-(J2-D2+)") (class "Default")
      (node (ref "J2") (pin "3") (pinfunction "D2+") (pintype "passive"))
      (node (ref "U3") (pin "146") (pinfunction "HDMI1_TX2_P") (pintype "output")))
    (net (code "88") (name "Net-(J2-D2-)") (class "Default")
      (node (ref "J2") (pin "5") (pinfunction "D2-") (pintype "passive"))
      (node (ref "U3") (pin "148") (pinfunction "HDMI1_TX2_N") (pintype "output")))
    (net (code "89") (name "Net-(J2-HPD{slash}HEAC-)") (class "Default")
      (node (ref "J2") (pin "1") (pinfunction "HPD/HEAC-") (pintype "passive"))
      (node (ref "U3") (pin "143") (pinfunction "HDMI1_HOTPLUG") (pintype "input")))
    (net (code "90") (name "Net-(J2-SCL)") (class "Default")
      (node (ref "J2") (pin "17") (pinfunction "SCL") (pintype "passive"))
      (node (ref "U3") (pin "147") (pinfunction "HDMI1_SCL") (pintype "open_collector")))
    (net (code "91") (name "Net-(J2-SDA)") (class "Default")
      (node (ref "J2") (pin "18") (pinfunction "SDA") (pintype "bidirectional"))
      (node (ref "U3") (pin "145") (pinfunction "HDMI1_SDA") (pintype "bidirectional")))
    (net (code "92") (name "Net-(J3-CEC)") (class "Default")
      (node (ref "J3") (pin "15") (pinfunction "CEC") (pintype "bidirectional"))
      (node (ref "U3") (pin "151") (pinfunction "HDMI0_CEC") (pintype "open_collector")))
    (net (code "93") (name "Net-(J3-CK+)") (class "Default")
      (node (ref "J3") (pin "12") (pinfunction "CK+") (pintype "passive"))
      (node (ref "U3") (pin "188") (pinfunction "HDMI0_CLK_P") (pintype "output")))
    (net (code "94") (name "Net-(J3-CK-)") (class "Default")
      (node (ref "J3") (pin "14") (pinfunction "CK-") (pintype "passive"))
      (node (ref "U3") (pin "190") (pinfunction "HDMI0_CLK_N") (pintype "output")))
    (net (code "95") (name "Net-(J3-D0+)") (class "Default")
      (node (ref "J3") (pin "9") (pinfunction "D0+") (pintype "passive"))
      (node (ref "U3") (pin "182") (pinfunction "HDMI0_TX0_P") (pintype "output")))
    (net (code "96") (name "Net-(J3-D0-)") (class "Default")
      (node (ref "J3") (pin "11") (pinfunction "D0-") (pintype "passive"))
      (node (ref "U3") (pin "184") (pinfunction "HDMI0_TX0_N") (pintype "output")))
    (net (code "97") (name "Net-(J3-D1+)") (class "Default")
      (node (ref "J3") (pin "6") (pinfunction "D1+") (pintype "passive"))
      (node (ref "U3") (pin "176") (pinfunction "HDMI0_TX1_P") (pintype "output")))
    (net (code "98") (name "Net-(J3-D1-)") (class "Default")
      (node (ref "J3") (pin "8") (pinfunction "D1-") (pintype "passive"))
      (node (ref "U3") (pin "178") (pinfunction "HDMI0_TX1_N") (pintype "output")))
    (net (code "99") (name "Net-(J3-D2+)") (class "Default")
      (node (ref "J3") (pin "3") (pinfunction "D2+") (pintype "passive"))
      (node (ref "U3") (pin "170") (pinfunction "HDMI0_TX2_P") (pintype "output")))
    (net (code "100") (name "Net-(J3-D2-)") (class "Default")
      (node (ref "J3") (pin "5") (pinfunction "D2-") (pintype "passive"))
      (node (ref "U3") (pin "172") (pinfunction "HDMI0_TX2_N") (pintype "output")))
    (net (code "101") (name "Net-(J3-HPD{slash}HEAC-)") (class "Default")
      (node (ref "J3") (pin "1") (pinfunction "HPD/HEAC-") (pintype "passive"))
      (node (ref "U3") (pin "153") (pinfunction "HDMI0_HOTPLUG") (pintype "input")))
    (net (code "102") (name "Net-(J3-SCL)") (class "Default")
      (node (ref "J3") (pin "17") (pinfunction "SCL") (pintype "passive"))
      (node (ref "U3") (pin "200") (pinfunction "HDMI0_SCL") (pintype "open_collector")))
    (net (code "103") (name "Net-(J3-SDA)") (class "Default")
      (node (ref "J3") (pin "18") (pinfunction "SDA") (pintype "bidirectional"))
      (node (ref "U3") (pin "199") (pinfunction "HDMI0_SDA") (pintype "bidirectional")))
    (net (code "104") (name "Net-(J4-D+)") (class "Default")
      (node (ref "J4") (pin "3") (pinfunction "D+") (pintype "bidirectional"))
      (node (ref "U8") (pin "3") (pinfunction "I/O2") (pintype "passive")))
    (net (code "105") (name "Net-(J4-D-)") (class "Default")
      (node (ref "J4") (pin "2") (pinfunction "D-") (pintype "bidirectional"))
      (node (ref "U8") (pin "1") (pinfunction "I/O1") (pintype "passive")))
    (net (code "106") (name "Net-(J14-Pin_3)") (class "Default")
      (node (ref "J14") (pin "3") (pinfunction "Pin_3") (pintype "passive"))
      (node (ref "U3") (pin "16") (pinfunction "Fan_tacho") (pintype "input")))
    (net (code "107") (name "Net-(J14-Pin_4)") (class "Default")
      (node (ref "J14") (pin "4") (pinfunction "Pin_4") (pintype "passive"))
      (node (ref "U3") (pin "19") (pinfunction "Fan_PWM") (pintype "output")))
    (net (code "108") (name "Net-(J15-D+)") (class "Default")
      (node (ref "J15") (pin "3") (pinfunction "D+") (pintype "bidirectional"))
      (node (ref "U17") (pin "3") (pinfunction "I/O2") (pintype "passive")))
    (net (code "109") (name "Net-(J15-D-)") (class "Default")
      (node (ref "J15") (pin "2") (pinfunction "D-") (pintype "bidirectional"))
      (node (ref "U17") (pin "1") (pinfunction "I/O1") (pintype "passive")))
    (net (code "110") (name "Net-(J20-CC1)") (class "Default")
      (node (ref "C48") (pin "1") (pintype "passive"))
      (node (ref "J20") (pin "A5") (pinfunction "CC1") (pintype "bidirectional"))
      (node (ref "R35") (pin "1") (pintype "passive")))
    (net (code "111") (name "Net-(J20-CC2)") (class "Default")
      (node (ref "C49") (pin "1") (pintype "passive"))
      (node (ref "J20") (pin "B5") (pinfunction "CC2") (pintype "bidirectional"))
      (node (ref "R34") (pin "1") (pintype "passive")))
    (net (code "112") (name "Net-(J20-D+-PadA6)") (class "Default")
      (node (ref "J20") (pin "A6") (pinfunction "D+") (pintype "bidirectional"))
      (node (ref "J20") (pin "B6") (pinfunction "D+") (pintype "bidirectional"))
      (node (ref "U14") (pin "3") (pinfunction "I/O2") (pintype "passive")))
    (net (code "113") (name "Net-(J20-D--PadA7)") (class "Default")
      (node (ref "J20") (pin "A7") (pinfunction "D-") (pintype "bidirectional"))
      (node (ref "J20") (pin "B7") (pinfunction "D-") (pintype "bidirectional"))
      (node (ref "U14") (pin "1") (pinfunction "I/O1") (pintype "passive")))
    (net (code "114") (name "Net-(R7-Pad2)") (class "Default")
      (node (ref "R7") (pin "2") (pintype "passive"))
      (node (ref "U12") (pin "6") (pinfunction "6") (pintype "passive")))
    (net (code "115") (name "Net-(R16-Pad1)") (class "Default")
      (node (ref "R16") (pin "1") (pintype "passive"))
      (node (ref "U15") (pin "14") (pinfunction "14") (pintype "unspecified")))
    (net (code "116") (name "Net-(R17-Pad1)") (class "Default")
      (node (ref "R17") (pin "1") (pintype "passive"))
      (node (ref "U15") (pin "11") (pinfunction "11") (pintype "unspecified")))
    (net (code "117") (name "Net-(R29-Pad2)") (class "Default")
      (node (ref "R29") (pin "2") (pintype "passive"))
      (node (ref "U12") (pin "7") (pinfunction "7") (pintype "passive")))
    (net (code "118") (name "Net-(R30-Pad1)") (class "Default")
      (node (ref "R30") (pin "1") (pintype "passive"))
      (node (ref "U12") (pin "8") (pinfunction "8") (pintype "passive")))
    (net (code "119") (name "Net-(U3B-GPIO14)") (class "Default")
      (node (ref "R39") (pin "1") (pintype "passive"))
      (node (ref "U3") (pin "55") (pinfunction "GPIO14") (pintype "passive")))
    (net (code "120") (name "Net-(U3B-GPIO15)") (class "Default")
      (node (ref "R38") (pin "2") (pintype "passive"))
      (node (ref "R4") (pin "1") (pintype "passive"))
      (node (ref "U3") (pin "51") (pinfunction "GPIO15") (pintype "passive")))
    (net (code "121") (name "Net-(U3D-USB_OTG_ID)") (class "Default")
      (node (ref "R26") (pin "1") (pintype "passive"))
      (node (ref "U3") (pin "101") (pinfunction "USB_OTG_ID") (pintype "input")))
    (net (code "122") (name "Net-(U3J-CC1)") (class "Default")
      (node (ref "R31") (pin "2") (pintype "passive"))
      (node (ref "U3") (pin "94") (pinfunction "CC1") (pintype "bidirectional")))
    (net (code "123") (name "Net-(U3J-CC2)") (class "Default")
      (node (ref "R32") (pin "2") (pintype "passive"))
      (node (ref "U3") (pin "96") (pinfunction "CC2") (pintype "bidirectional")))
    (net (code "124") (name "Net-(U3J-PMIC_ENABLE)") (class "Default")
      (node (ref "R23") (pin "2") (pintype "passive"))
      (node (ref "U3") (pin "99") (pinfunction "PMIC_ENABLE") (pintype "input")))
    (net (code "125") (name "Net-(U3J-PWR_Button)") (class "Default")
      (node (ref "SW2") (pin "1") (pinfunction "1") (pintype "passive"))
      (node (ref "U3") (pin "92") (pinfunction "PWR_Button") (pintype "passive")))
    (net (code "126") (name "Net-(U3J-VBAT)") (class "Default")
      (node (ref "BT1") (pin "1") (pinfunction "1") (pintype "input"))
      (node (ref "U3") (pin "76") (pinfunction "VBAT") (pintype "input")))
    (net (code "127") (name "Net-(U3J-~{PI_LED_nPWR})") (class "Default")
      (node (ref "R21") (pin "1") (pintype "passive"))
      (node (ref "U3") (pin "95") (pinfunction "~{PI_LED_nPWR}") (pintype "output")))
    (net (code "128") (name "Net-(U3J-~{Pi_nLED_Activity})") (class "Default")
      (node (ref "R20") (pin "2") (pintype "passive"))
      (node (ref "U3") (pin "21") (pinfunction "~{Pi_nLED_Activity}") (pintype "open_collector")))
    (net (code "129") (name "Net-(U4-AREF)") (class "Default")
      (node (ref "C31") (pin "2") (pintype "passive"))
      (node (ref "U4") (pin "42") (pinfunction "AREF") (pintype "passive")))
    (net (code "130") (name "Net-(U4-UCAP)") (class "Default")
      (node (ref "C8") (pin "1") (pintype "passive"))
      (node (ref "U4") (pin "6") (pinfunction "UCAP") (pintype "passive")))
    (net (code "131") (name "Net-(U4-XTAL1)") (class "Default")
      (node (ref "C10") (pin "2") (pintype "passive"))
      (node (ref "U4") (pin "17") (pinfunction "XTAL1") (pintype "input"))
      (node (ref "X1") (pin "3") (pinfunction "OSC") (pintype "unspecified")))
    (net (code "132") (name "Net-(U4-XTAL2)") (class "Default")
      (node (ref "C9") (pin "1") (pintype "passive"))
      (node (ref "U4") (pin "16") (pinfunction "XTAL2") (pintype "output"))
      (node (ref "X1") (pin "1") (pinfunction "OSC") (pintype "unspecified")))
    (net (code "133") (name "Net-(U5-CAPM)") (class "Default")
      (node (ref "C16") (pin "1") (pintype "passive"))
      (node (ref "U5") (pin "4") (pinfunction "CAPM") (pintype "passive")))
    (net (code "134") (name "Net-(U5-CAPP)") (class "Default")
      (node (ref "C16") (pin "2") (pintype "passive"))
      (node (ref "U5") (pin "2") (pinfunction "CAPP") (pintype "passive")))
    (net (code "135") (name "Net-(U5-LDOO)") (class "Default")
      (node (ref "C22") (pin "1") (pintype "passive"))
      (node (ref "U5") (pin "26") (pinfunction "LDOO") (pintype "passive")))
    (net (code "136") (name "Net-(U5-OUTL)") (class "Default")
      (node (ref "C18") (pin "1") (pintype "passive"))
      (node (ref "U5") (pin "6") (pinfunction "OUTL") (pintype "output")))
    (net (code "137") (name "Net-(U5-OUTR)") (class "Default")
      (node (ref "C20") (pin "1") (pintype "passive"))
      (node (ref "U5") (pin "7") (pinfunction "OUTR") (pintype "output")))
    (net (code "138") (name "Net-(U5-VCOM{slash}DEMP)") (class "Default")
      (node (ref "C34") (pin "1") (pintype "passive"))
      (node (ref "U5") (pin "10") (pinfunction "VCOM/DEMP") (pintype "bidirectional")))
    (net (code "139") (name "Net-(U5-VNEG)") (class "Default")
      (node (ref "C17") (pin "1") (pintype "passive"))
      (node (ref "U5") (pin "5") (pinfunction "VNEG") (pintype "passive")))
    (net (code "140") (name "Net-(U5-XSMT)") (class "Default")
      (node (ref "R8") (pin "1") (pintype "passive"))
      (node (ref "U5") (pin "25") (pinfunction "XSMT") (pintype "input")))
    (net (code "141") (name "Net-(U6-DM)") (class "Default")
      (node (ref "J1") (pin "A7") (pinfunction "D-") (pintype "bidirectional"))
      (node (ref "J1") (pin "B7") (pinfunction "D-") (pintype "bidirectional"))
      (node (ref "U6") (pin "5") (pinfunction "DM") (pintype "bidirectional")))
    (net (code "142") (name "Net-(U6-DP)") (class "Default")
      (node (ref "J1") (pin "A6") (pinfunction "D+") (pintype "bidirectional"))
      (node (ref "J1") (pin "B6") (pinfunction "D+") (pintype "bidirectional"))
      (node (ref "U6") (pin "4") (pinfunction "DP") (pintype "bidirectional")))
    (net (code "143") (name "Net-(U6-PG)") (class "Default")
      (node (ref "R19") (pin "1") (pintype "passive"))
      (node (ref "U6") (pin "10") (pinfunction "PG") (pintype "open_collector")))
    (net (code "144") (name "Net-(U6-VBUS)") (class "Default")
      (node (ref "U11") (pin "2") (pinfunction "2") (pintype "unspecified"))
      (node (ref "U6") (pin "8") (pinfunction "VBUS") (pintype "passive")))
    (net (code "145") (name "Net-(U6-VDD)") (class "Default")
      (node (ref "C15") (pin "1") (pintype "passive"))
      (node (ref "D2") (pin "2") (pintype "passive"))
      (node (ref "R1") (pin "2") (pintype "passive"))
      (node (ref "U6") (pin "1") (pinfunction "VDD") (pintype "power_in")))
    (net (code "146") (name "Net-(U9-ILIM)") (class "Default")
      (node (ref "R36") (pin "2") (pintype "passive"))
      (node (ref "U9") (pin "5") (pinfunction "ILIM") (pintype "unspecified")))
    (net (code "147") (name "Net-(U13-ILIM)") (class "Default")
      (node (ref "R37") (pin "2") (pintype "passive"))
      (node (ref "U13") (pin "5") (pinfunction "ILIM") (pintype "unspecified")))
    (net (code "148") (name "Net-(U18-EN)") (class "Default")
      (node (ref "R2") (pin "2") (pintype "passive"))
      (node (ref "U18") (pin "3") (pinfunction "EN") (pintype "unspecified")))
    (net (code "149") (name "Net-(U18-ILIM)") (class "Default")
      (node (ref "R3") (pin "2") (pintype "passive"))
      (node (ref "U18") (pin "5") (pinfunction "ILIM") (pintype "unspecified")))
    (net (code "150") (name "Net-(U19-BS)") (class "Default")
      (node (ref "C54") (pin "2") (pintype "passive"))
      (node (ref "U19") (pin "7") (pinfunction "BS") (pintype "unspecified")))
    (net (code "151") (name "Net-(U19-EN)") (class "Default")
      (node (ref "R44") (pin "2") (pintype "passive"))
      (node (ref "R45") (pin "1") (pintype "passive"))
      (node (ref "U19") (pin "12") (pinfunction "EN") (pintype "unspecified")))
    (net (code "152") (name "Net-(U19-FB)") (class "Default")
      (node (ref "R40") (pin "1") (pintype "passive"))
      (node (ref "R41") (pin "1") (pintype "passive"))
      (node (ref "R42") (pin "1") (pintype "passive"))
      (node (ref "U19") (pin "9") (pinfunction "FB") (pintype "unspecified")))
    (net (code "153") (name "Net-(U19-LX)") (class "Default")
      (node (ref "C54") (pin "1") (pintype "passive"))
      (node (ref "L1") (pin "2") (pinfunction "2") (pintype "unspecified"))
      (node (ref "U19") (pin "2") (pinfunction "LX") (pintype "unspecified")))
    (net (code "154") (name "Net-(U19-VCC)") (class "Default")
      (node (ref "C57") (pin "2") (pintype "passive"))
      (node (ref "U19") (pin "8") (pinfunction "VCC") (pintype "unspecified")))
    (net (code "155") (name "UART_ATMEGA_RX") (class "Default")
      (node (ref "R39") (pin "2") (pintype "passive"))
      (node (ref "U4") (pin "20") (pinfunction "PD2") (pintype "bidirectional")))
    (net (code "156") (name "UART_ATMEGA_TX") (class "Default")
      (node (ref "R4") (pin "2") (pintype "passive"))
      (node (ref "U4") (pin "21") (pinfunction "PD3") (pintype "bidirectional")))
    (net (code "157") (name "unconnected-(J1-SBU1-PadA8)") (class "Default")
      (node (ref "J1") (pin "A8") (pinfunction "SBU1") (pintype "bidirectional+no_connect")))
    (net (code "158") (name "unconnected-(J1-SBU2-PadB8)") (class "Default")
      (node (ref "J1") (pin "B8") (pinfunction "SBU2") (pintype "bidirectional+no_connect")))
    (net (code "159") (name "unconnected-(J2-UTILITY{slash}HEAC+-Pad2)") (class "Default")
      (node (ref "J2") (pin "2") (pinfunction "UTILITY/HEAC+") (pintype "passive+no_connect")))
    (net (code "160") (name "unconnected-(J3-UTILITY{slash}HEAC+-Pad2)") (class "Default")
      (node (ref "J3") (pin "2") (pinfunction "UTILITY/HEAC+") (pintype "passive+no_connect")))
    (net (code "161") (name "unconnected-(J5-D+-Pad3)") (class "Default")
      (node (ref "J5") (pin "3") (pinfunction "D+") (pintype "bidirectional+no_connect")))
    (net (code "162") (name "unconnected-(J5-D--Pad2)") (class "Default")
      (node (ref "J5") (pin "2") (pinfunction "D-") (pintype "bidirectional+no_connect")))
    (net (code "163") (name "unconnected-(J18-DETECT_GND-Pad3)") (class "Default")
      (node (ref "J18") (pin "3") (pinfunction "DETECT_GND") (pintype "passive+no_connect")))
    (net (code "164") (name "unconnected-(J18-DETECT_LEFT-Pad7)") (class "Default")
      (node (ref "J18") (pin "7") (pinfunction "DETECT_LEFT") (pintype "passive+no_connect")))
    (net (code "165") (name "unconnected-(J18-DETECT_R-Pad5)") (class "Default")
      (node (ref "J18") (pin "5") (pinfunction "DETECT_R") (pintype "passive+no_connect")))
    (net (code "166") (name "unconnected-(J20-SBU1-PadA8)") (class "Default")
      (node (ref "J20") (pin "A8") (pinfunction "SBU1") (pintype "bidirectional+no_connect")))
    (net (code "167") (name "unconnected-(J20-SBU2-PadB8)") (class "Default")
      (node (ref "J20") (pin "B8") (pinfunction "SBU2") (pintype "bidirectional+no_connect")))
    (net (code "168") (name "unconnected-(U0A-CM4_1.8V_Out_1-Pad88)") (class "Default")
      (node (ref "U0") (pin "88") (pinfunction "CM4_1.8V_Out_1") (pintype "power_out+no_connect")))
    (net (code "169") (name "unconnected-(U0A-CM4_1.8V_Out_2-Pad90)") (class "Default")
      (node (ref "U0") (pin "90") (pinfunction "CM4_1.8V_Out_2") (pintype "power_out+no_connect")))
    (net (code "170") (name "unconnected-(U0A-CM4_3.3V_Out_1-Pad84)") (class "Default")
      (node (ref "U0") (pin "84") (pinfunction "CM4_3.3V_Out_1") (pintype "power_out+no_connect")))
    (net (code "171") (name "unconnected-(U0A-CM4_3.3V_Out_2-Pad86)") (class "Default")
      (node (ref "U0") (pin "86") (pinfunction "CM4_3.3V_Out_2") (pintype "power_out+no_connect")))
    (net (code "172") (name "unconnected-(U1-NC-Pad4)") (class "Default")
      (node (ref "U1") (pin "4") (pinfunction "NC") (pintype "no_connect")))
    (net (code "173") (name "unconnected-(U2-NC-Pad4)") (class "Default")
      (node (ref "U2") (pin "4") (pinfunction "NC") (pintype "no_connect")))
    (net (code "174") (name "unconnected-(U3B-GPIO2-Pad58)") (class "Default")
      (node (ref "U3") (pin "58") (pinfunction "GPIO2") (pintype "passive+no_connect")))
    (net (code "175") (name "unconnected-(U3B-GPIO3-Pad56)") (class "Default")
      (node (ref "U3") (pin "56") (pinfunction "GPIO3") (pintype "passive+no_connect")))
    (net (code "176") (name "unconnected-(U3B-GPIO4-Pad54)") (class "Default")
      (node (ref "U3") (pin "54") (pinfunction "GPIO4") (pintype "passive+no_connect")))
    (net (code "177") (name "unconnected-(U3B-GPIO5-Pad34)") (class "Default")
      (node (ref "U3") (pin "34") (pinfunction "GPIO5") (pintype "passive+no_connect")))
    (net (code "178") (name "unconnected-(U3B-GPIO6-Pad30)") (class "Default")
      (node (ref "U3") (pin "30") (pinfunction "GPIO6") (pintype "passive+no_connect")))
    (net (code "179") (name "unconnected-(U3B-GPIO7-Pad37)") (class "Default")
      (node (ref "U3") (pin "37") (pinfunction "GPIO7") (pintype "passive+no_connect")))
    (net (code "180") (name "unconnected-(U3B-GPIO8-Pad39)") (class "Default")
      (node (ref "U3") (pin "39") (pinfunction "GPIO8") (pintype "passive+no_connect")))
    (net (code "181") (name "unconnected-(U3B-GPIO9-Pad40)") (class "Default")
      (node (ref "U3") (pin "40") (pinfunction "GPIO9") (pintype "passive+no_connect")))
    (net (code "182") (name "unconnected-(U3B-GPIO10-Pad44)") (class "Default")
      (node (ref "U3") (pin "44") (pinfunction "GPIO10") (pintype "passive+no_connect")))
    (net (code "183") (name "unconnected-(U3B-GPIO11-Pad38)") (class "Default")
      (node (ref "U3") (pin "38") (pinfunction "GPIO11") (pintype "passive+no_connect")))
    (net (code "184") (name "unconnected-(U3B-GPIO12-Pad31)") (class "Default")
      (node (ref "U3") (pin "31") (pinfunction "GPIO12") (pintype "passive+no_connect")))
    (net (code "185") (name "unconnected-(U3B-GPIO13-Pad28)") (class "Default")
      (node (ref "U3") (pin "28") (pinfunction "GPIO13") (pintype "passive+no_connect")))
    (net (code "186") (name "unconnected-(U3B-GPIO16-Pad29)") (class "Default")
      (node (ref "U3") (pin "29") (pinfunction "GPIO16") (pintype "passive+no_connect")))
    (net (code "187") (name "unconnected-(U3B-GPIO17-Pad50)") (class "Default")
      (node (ref "U3") (pin "50") (pinfunction "GPIO17") (pintype "passive+no_connect")))
    (net (code "188") (name "unconnected-(U3B-GPIO20-Pad27)") (class "Default")
      (node (ref "U3") (pin "27") (pinfunction "GPIO20") (pintype "passive+no_connect")))
    (net (code "189") (name "unconnected-(U3B-GPIO22-Pad46)") (class "Default")
      (node (ref "U3") (pin "46") (pinfunction "GPIO22") (pintype "passive+no_connect")))
    (net (code "190") (name "unconnected-(U3B-GPIO23-Pad47)") (class "Default")
      (node (ref "U3") (pin "47") (pinfunction "GPIO23") (pintype "passive+no_connect")))
    (net (code "191") (name "unconnected-(U3B-GPIO24-Pad45)") (class "Default")
      (node (ref "U3") (pin "45") (pinfunction "GPIO24") (pintype "passive+no_connect")))
    (net (code "192") (name "unconnected-(U3B-GPIO25-Pad41)") (class "Default")
      (node (ref "U3") (pin "41") (pinfunction "GPIO25") (pintype "passive+no_connect")))
    (net (code "193") (name "unconnected-(U3B-GPIO26-Pad24)") (class "Default")
      (node (ref "U3") (pin "24") (pinfunction "GPIO26") (pintype "passive+no_connect")))
    (net (code "194") (name "unconnected-(U3B-GPIO27-Pad48)") (class "Default")
      (node (ref "U3") (pin "48") (pinfunction "GPIO27") (pintype "passive+no_connect")))
    (net (code "195") (name "unconnected-(U3B-ID_SC-Pad35)") (class "Default")
      (node (ref "U3") (pin "35") (pinfunction "ID_SC") (pintype "passive+no_connect")))
    (net (code "196") (name "unconnected-(U3B-ID_SD-Pad36)") (class "Default")
      (node (ref "U3") (pin "36") (pinfunction "ID_SD") (pintype "passive+no_connect")))
    (net (code "197") (name "unconnected-(U3C-Ethernet_SYNC_OUT-Pad18)") (class "Default")
      (node (ref "U3") (pin "18") (pinfunction "Ethernet_SYNC_OUT") (pintype "input+no_connect")))
    (net (code "198") (name "unconnected-(U3J-CAM_GPIO0-Pad97)") (class "Default")
      (node (ref "U3") (pin "97") (pinfunction "CAM_GPIO0") (pintype "input+no_connect")))
    (net (code "199") (name "unconnected-(U3J-CAM_GPIO1-Pad100)") (class "Default")
      (node (ref "U3") (pin "100") (pinfunction "CAM_GPIO1") (pintype "input+no_connect")))
    (net (code "200") (name "unconnected-(U4-D+-Pad4)") (class "Default")
      (node (ref "U4") (pin "4") (pinfunction "D+") (pintype "bidirectional+no_connect")))
    (net (code "201") (name "unconnected-(U4-D--Pad3)") (class "Default")
      (node (ref "U4") (pin "3") (pinfunction "D-") (pintype "bidirectional+no_connect")))
    (net (code "202") (name "unconnected-(U4-PB0-Pad8)") (class "Default")
      (node (ref "U4") (pin "8") (pinfunction "PB0") (pintype "bidirectional+no_connect")))
    (net (code "203") (name "unconnected-(U5-GPIO3{slash}AGNS-Pad15)") (class "Default")
      (node (ref "U5") (pin "15") (pinfunction "GPIO3/AGNS") (pintype "bidirectional+no_connect")))
    (net (code "204") (name "unconnected-(U5-GPIO4{slash}MAST-Pad14)") (class "Default")
      (node (ref "U5") (pin "14") (pinfunction "GPIO4/MAST") (pintype "bidirectional+no_connect")))
    (net (code "205") (name "unconnected-(U5-GPIO5{slash}ATT0-Pad13)") (class "Default")
      (node (ref "U5") (pin "13") (pinfunction "GPIO5/ATT0") (pintype "bidirectional+no_connect")))
    (net (code "206") (name "unconnected-(U5-GPIO6{slash}FLT-Pad19)") (class "Default")
      (node (ref "U5") (pin "19") (pinfunction "GPIO6/FLT") (pintype "bidirectional+no_connect")))
    (net (code "207") (name "unconnected-(U6-CFG3-Pad3)") (class "Default")
      (node (ref "U6") (pin "3") (pinfunction "CFG3") (pintype "passive+no_connect")))
    (net (code "208") (name "unconnected-(U9-FAULT-Pad4)") (class "Default")
      (node (ref "U9") (pin "4") (pinfunction "FAULT") (pintype "unspecified+no_connect")))
    (net (code "209") (name "unconnected-(U10-DETECT_GND-Pad4)") (class "Default")
      (node (ref "U10") (pin "4") (pinfunction "DETECT_GND") (pintype "passive+no_connect")))
    (net (code "210") (name "unconnected-(U11-Pad3)") (class "Default")
      (node (ref "U11") (pin "3") (pinfunction "3") (pintype "unspecified+no_connect")))
    (net (code "211") (name "unconnected-(U11-Pad4)") (class "Default")
      (node (ref "U11") (pin "4") (pinfunction "4") (pintype "unspecified+no_connect")))
    (net (code "212") (name "unconnected-(U11-Pad5)") (class "Default")
      (node (ref "U11") (pin "5") (pinfunction "5") (pintype "unspecified+no_connect")))
    (net (code "213") (name "unconnected-(U11-Pad6)") (class "Default")
      (node (ref "U11") (pin "6") (pinfunction "6") (pintype "unspecified+no_connect")))
    (net (code "214") (name "unconnected-(U11-Pad7)") (class "Default")
      (node (ref "U11") (pin "7") (pinfunction "7") (pintype "unspecified+no_connect")))
    (net (code "215") (name "unconnected-(U11-Pad8)") (class "Default")
      (node (ref "U11") (pin "8") (pinfunction "8") (pintype "unspecified+no_connect")))
    (net (code "216") (name "unconnected-(U13-FAULT-Pad4)") (class "Default")
      (node (ref "U13") (pin "4") (pinfunction "FAULT") (pintype "unspecified+no_connect")))
    (net (code "217") (name "unconnected-(U15-PadP1)") (class "Default")
      (node (ref "U15") (pin "P1") (pinfunction "P1") (pintype "unspecified+no_connect")))
    (net (code "218") (name "unconnected-(U18-FAULT-Pad4)") (class "Default")
      (node (ref "U18") (pin "4") (pinfunction "FAULT") (pintype "unspecified+no_connect")))
    (net (code "219") (name "unconnected-(U19-ILMT-Pad10)") (class "Default")
      (node (ref "U19") (pin "10") (pinfunction "ILMT") (pintype "unspecified+no_connect")))))