
(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "RCJ-013-SMT" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "J" (id 0) (at -2.54144 3.81216 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Value" "RCJ-013-SMT" (id 1) (at -2.54136 -6.35341 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Footprint" "RCJ-013-SMT:CUI_RCJ-013-SMT" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MF" "Same Sky" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Description" "\n                        \n                            Metal Right-Angle, SMT RCA Jack, White Insulator\n                        \n" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Package" "None" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Price" "None" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Check_prices" "https://www.snapeda.com/parts/RCJ-013-SMT-TR/Same+Sky/view-part/?ref=eda" (id 8) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "PART_REV" "B" (id 9) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "STANDARD" "Manufacturer recommendations" (id 10) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/RCJ-013-SMT-TR/Same+Sky/view-part/?ref=snap" (id 11) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MP" "RCJ-013-SMT-TR" (id 12) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=1316562&manufacturer=Same Sky&part_name=RCJ-013-SMT-TR&search_term=rca jack pcb mount" (id 13) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Availability" "In Stock" (id 14) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MANUFACTURER" "CUI Inc" (id 15) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (symbol "RCJ-013-SMT_0_0"
      (polyline
        (pts (xy 5.08 2.54) (xy -2.54 2.54)) (stroke (width 0.1524))
      )
      (polyline
        (pts (xy -2.54 2.54) (xy -2.54 1.27)) (stroke (width 0.1524))
      )
      (polyline
        (pts (xy 5.08 -2.54) (xy 2.54 -2.54)) (stroke (width 0.1524))
      )
      (polyline
        (pts (xy 2.54 -2.54) (xy 0.762 -2.54)) (stroke (width 0.1524))
      )
      (polyline
        (pts (xy 0.762 -2.54) (xy 0.0 -1.016)) (stroke (width 0.1524))
      )
      (polyline
        (pts (xy 0.0 -1.016) (xy -0.762 -2.54)) (stroke (width 0.1524))
      )
      (rectangle (start -3.30257 -2.54044) (end -1.778 1.27)
        (stroke (width 0.1)) (fill (type outline))
      )
      (pin passive line (at 7.62 2.54 180.0) (length 2.54)
        (name "1"
          (effects (font (size 1.016 1.016)))
        )
        (number "1A"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at 7.62 2.54 180.0) (length 2.54) hide
        (name "1"
          (effects (font (size 1.016 1.016)))
        )
        (number "1B"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at 7.62 2.54 180.0) (length 2.54) hide
        (name "1"
          (effects (font (size 1.016 1.016)))
        )
        (number "1C"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at 7.62 -2.54 180.0) (length 2.54)
        (name "2"
          (effects (font (size 1.016 1.016)))
        )
        (number "2"
          (effects (font (size 1.016 1.016)))
        )
      )
    )
  )
)