(kicad_symbol_lib (version 20210201) (generator TousstNicolas/JLC2KiCad_lib)
  (symbol "ATMEGA32U4-MU"   (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "ATMEGA32U4-MU" (id 1) (at 0 -2.54 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "footprint:VQFN-44_L7.0-W7.0-P0.50-BL-EP5.2" (id 2) (at 0 -10.16 0)
      (effects (font (size 1.27 1.27) italic) hide)
    )
    (property "Datasheet" "https://item.szlcsc.com/1427808.html" (id 3) (at -2.286 0.127 0)
      (effects (font (size 1.27 1.27)) (justify left) hide)
    )
    (property "ki_keywords" "C112161" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "LCSC" "C112161" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    
    (symbol "ATMEGA32U4-MU_0_1"
      (rectangle
        (start -49.530099060198125 30.48006096012192)
        (end 49.530099060198125 -30.48006096012192)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (circle
        (center -48.260096520193045 29.21005842011684)
        (radius 0.381000762001524)
        (stroke (width 0) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin unspecified line
        (at -52.07 25.4 0)
        (length 2.54)
        (name "PE6(INT.6/AIN0)" (effects (font (size 1 1))))
        (number "1" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at -52.07 22.86 0)
        (length 2.54)
        (name "UVcc" (effects (font (size 1 1))))
        (number "2" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at -52.07 20.32 0)
        (length 2.54)
        (name "D-" (effects (font (size 1 1))))
        (number "3" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at -52.07 17.78 0)
        (length 2.54)
        (name "D+" (effects (font (size 1 1))))
        (number "4" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at -52.07 15.24 0)
        (length 2.54)
        (name "UGnd" (effects (font (size 1 1))))
        (number "5" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at -52.07 12.7 0)
        (length 2.54)
        (name "UCap" (effects (font (size 1 1))))
        (number "6" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at -52.07 10.16 0)
        (length 2.54)
        (name "VBus" (effects (font (size 1 1))))
        (number "7" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at -52.07 7.62 0)
        (length 2.54)
        (name "PB0(SS/PCINT0)" (effects (font (size 1 1))))
        (number "8" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at -52.07 5.08 0)
        (length 2.54)
        (name "PB1(PCINT1/SCLK)" (effects (font (size 1 1))))
        (number "9" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at -52.07 2.54 0)
        (length 2.54)
        (name "PB2(PDI/PCINT2/MOSI)" (effects (font (size 1 1))))
        (number "10" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at -52.07 -0.0 0)
        (length 2.54)
        (name "PB3(PDO/PCINT3/MISO)" (effects (font (size 1 1))))
        (number "11" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at -52.07 -2.54 0)
        (length 2.54)
        (name "PB7(PCINT7/OC0A/OC1C/RTS#)" (effects (font (size 1 1))))
        (number "12" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at -52.07 -5.08 0)
        (length 2.54)
        (name "RESET#" (effects (font (size 1 1))))
        (number "13" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at -52.07 -7.62 0)
        (length 2.54)
        (name "VCC" (effects (font (size 1 1))))
        (number "14" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at -52.07 -10.16 0)
        (length 2.54)
        (name "GND" (effects (font (size 1 1))))
        (number "15" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at -52.07 -12.7 0)
        (length 2.54)
        (name "XTAL2" (effects (font (size 1 1))))
        (number "16" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at -52.07 -15.24 0)
        (length 2.54)
        (name "XTAL1" (effects (font (size 1 1))))
        (number "17" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at -52.07 -17.78 0)
        (length 2.54)
        (name "PD0(OC0B/SCL/INT0)" (effects (font (size 1 1))))
        (number "18" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at -52.07 -20.32 0)
        (length 2.54)
        (name "PD1(SDA/INT1)" (effects (font (size 1 1))))
        (number "19" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at -52.07 -22.86 0)
        (length 2.54)
        (name "PD2(RXD1/INT2)" (effects (font (size 1 1))))
        (number "20" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at -52.07 -25.4 0)
        (length 2.54)
        (name "PD3(TXD1/INT3)" (effects (font (size 1 1))))
        (number "21" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at -52.07 -27.94 0)
        (length 2.54)
        (name "PD5(XCK1/CTS#)" (effects (font (size 1 1))))
        (number "22" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at 52.07 -27.94 180)
        (length 2.54)
        (name "GND" (effects (font (size 1 1))))
        (number "23" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at 52.07 -25.4 180)
        (length 2.54)
        (name "AVCC" (effects (font (size 1 1))))
        (number "24" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at 52.07 -22.86 180)
        (length 2.54)
        (name "PD4(ICP1/ADC8)" (effects (font (size 1 1))))
        (number "25" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at 52.07 -20.32 180)
        (length 2.54)
        (name "PD6(T1/OC4D#/ADC9)" (effects (font (size 1 1))))
        (number "26" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at 52.07 -17.78 180)
        (length 2.54)
        (name "PD7(T0/OC4D/ADC10)" (effects (font (size 1 1))))
        (number "27" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at 52.07 -15.24 180)
        (length 2.54)
        (name "PB4(PCINT4/ADC11)" (effects (font (size 1 1))))
        (number "28" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at 52.07 -12.7 180)
        (length 2.54)
        (name "PB5(PCINT5/OC1A/OC4B#/ADC12)" (effects (font (size 1 1))))
        (number "29" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at 52.07 -10.16 180)
        (length 2.54)
        (name "PB6(PCINT6/OC1B/OC4B/ADC13)" (effects (font (size 1 1))))
        (number "30" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at 52.07 -7.62 180)
        (length 2.54)
        (name "PC6(OC3A/OC4A#)" (effects (font (size 1 1))))
        (number "31" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at 52.07 -5.08 180)
        (length 2.54)
        (name "PC7(ICP3/CLK0/OC4A)" (effects (font (size 1 1))))
        (number "32" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at 52.07 -2.54 180)
        (length 2.54)
        (name "PE2(HWB#)" (effects (font (size 1 1))))
        (number "33" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at 52.07 -0.0 180)
        (length 2.54)
        (name "VCC" (effects (font (size 1 1))))
        (number "34" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at 52.07 2.54 180)
        (length 2.54)
        (name "GND" (effects (font (size 1 1))))
        (number "35" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at 52.07 5.08 180)
        (length 2.54)
        (name "PF7(ADC7/TDI)" (effects (font (size 1 1))))
        (number "36" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at 52.07 7.62 180)
        (length 2.54)
        (name "PF6(ADC6/TDO)" (effects (font (size 1 1))))
        (number "37" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at 52.07 10.16 180)
        (length 2.54)
        (name "PF5(ADC5/TMS)" (effects (font (size 1 1))))
        (number "38" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at 52.07 12.7 180)
        (length 2.54)
        (name "PF4(ADC4/TCK)" (effects (font (size 1 1))))
        (number "39" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at 52.07 15.24 180)
        (length 2.54)
        (name "PF1(ADC1)" (effects (font (size 1 1))))
        (number "40" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at 52.07 17.78 180)
        (length 2.54)
        (name "PF0(ADC0)" (effects (font (size 1 1))))
        (number "41" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at 52.07 20.32 180)
        (length 2.54)
        (name "AREF" (effects (font (size 1 1))))
        (number "42" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at 52.07 22.86 180)
        (length 2.54)
        (name "GND" (effects (font (size 1 1))))
        (number "43" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at 52.07 25.4 180)
        (length 2.54)
        (name "AVCC" (effects (font (size 1 1))))
        (number "44" (effects (font (size 1 1))))
      )
      (pin unspecified line
        (at 52.07 27.94 180)
        (length 2.54)
        (name "EP" (effects (font (size 1 1))))
        (number "45" (effects (font (size 1 1))))
      )
    )
  )
)
